<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="4.2926" y1="29.3243" x2="4.2926" y2="24.7523" width="0" layer="20"/>
<wire x1="4.2926" y1="24.7523" x2="3.1496" y2="23.7363" width="0" layer="20"/>
<wire x1="3.1496" y1="23.7363" x2="3.1496" y2="22.2123" width="0" layer="20"/>
<wire x1="3.1496" y1="22.2123" x2="3.6576" y2="22.2123" width="0" layer="20"/>
<wire x1="3.6576" y1="22.2123" x2="3.6576" y2="20.6883" width="0" layer="20"/>
<wire x1="3.6576" y1="20.6883" x2="3.1496" y2="20.1803" width="0" layer="20"/>
<wire x1="13.9446" y1="29.3243" x2="13.4366" y2="29.8323" width="0" layer="20" curve="90"/>
<wire x1="13.4366" y1="29.8323" x2="4.8006" y2="29.8323" width="0" layer="20"/>
<wire x1="4.8006" y1="29.8323" x2="4.2926" y2="29.3243" width="0" layer="20" curve="90"/>
<wire x1="13.9446" y1="29.3243" x2="13.9446" y2="5.6388" width="0" layer="20"/>
<text>(BOBRICIUS)
ATMEGA328
CARD</text>
<wire x1="3.1496" y1="20.1803" x2="3.1496" y2="5.6769" width="0" layer="20"/>
<wire x1="3.1496" y1="5.6769" x2="4.6228" y2="4.2037" width="0" layer="20"/>
<wire x1="4.6228" y1="4.2037" x2="12.2682" y2="4.2037" width="0" layer="20"/>
<wire x1="12.2682" y1="4.2037" x2="13.9446" y2="5.6388" width="0" layer="20"/>
<text>www.
PEMI.
TECHNOLOGY</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="MICRO-SDCARD">
</package>
</packages>
</library>
<library name="rc-master-smd">
<packages>
<package name="C0603">
<description>&lt;b&gt;SMD CHIP CAP&lt;/b&gt; - 0603</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="R0603@1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3_TEST_POINTS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun" package="MICRO-SDCARD" value="MICRO-SDCARD"/>
<element name="C1" library="rc-master-smd" package="C0603" value="100n"/>
<element name="RRST" library="rcl" package="R0603@1" value="10k"/>
<element name="IC1" library="atmel" package="TQFP32-08" value="ATMEGA328P">
<attribute name="OC_FARNELL" value="9171371"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA8-16AU"/>
<attribute name="OC_NEWARK" value="73M8863"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="2X3_TEST_POINTS" value="AVR_SPI_PRG_6TESTPOINTS"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="GND"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="21"/>
<contactref element="C1" pad="1"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="VCC"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="18"/>
<contactref element="RRST" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="IC1" pad="17"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="16"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="IC1" pad="15"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="RESET">
<contactref element="IC1" pad="29"/>
<contactref element="RRST" pad="1"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="SDA">
<contactref element="IC1" pad="27"/>
<contactref element="U1" pad="DAT0"/>
</signal>
<signal name="SCL">
<contactref element="IC1" pad="28"/>
<contactref element="U1" pad="CLK"/>
</signal>
<signal name="PB6">
<contactref element="IC1" pad="7"/>
</signal>
<signal name="PB7">
<contactref element="IC1" pad="8"/>
</signal>
<signal name="A0">
<contactref element="IC1" pad="23"/>
</signal>
<signal name="AREF">
<contactref element="IC1" pad="20"/>
</signal>
<signal name="D9">
<contactref element="IC1" pad="13"/>
</signal>
<signal name="A2">
<contactref element="IC1" pad="25"/>
<contactref element="U1" pad="CD/DAT3"/>
</signal>
<signal name="A3">
<contactref element="IC1" pad="26"/>
<contactref element="U1" pad="CMD"/>
</signal>
<signal name="D4">
<contactref element="IC1" pad="2"/>
</signal>
<signal name="D8">
<contactref element="IC1" pad="12"/>
</signal>
<signal name="D3">
<contactref element="IC1" pad="1"/>
<contactref element="U1" pad="DAT1"/>
</signal>
<signal name="A1">
<contactref element="IC1" pad="24"/>
<contactref element="U1" pad="DAT2"/>
</signal>
<signal name="D5">
<contactref element="IC1" pad="9"/>
</signal>
<signal name="D6">
<contactref element="IC1" pad="10"/>
</signal>
<signal name="D7">
<contactref element="IC1" pad="11"/>
</signal>
<signal name="RXD">
<contactref element="IC1" pad="30"/>
</signal>
<signal name="TXD">
<contactref element="IC1" pad="31"/>
</signal>
<signal name="D2">
<contactref element="IC1" pad="32"/>
</signal>
<signal name="D10">
<contactref element="IC1" pad="14"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
