(kicad_pcb (version 20171130) (host pcbnew 5.1.5-52549c5~84~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 30)
    (tracks 472)
    (zones 0)
    (modules 14)
    (nets 33)
  )
  (page A3)
  (title_block
    (title "ALERT scintillator module row")
    (date 2018-12-12)
    (rev v1.0)
    (comment 4 "Author: Whitney Armstrong")
  )
  (layers
    (0 F.Cu signal)
    (1 G2L.Cu signal)
    (2 G3L.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref true)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 /p5_P)
  (net 2 /p5_N)
  (net 3 /p1_N)
  (net 4 /p1_P)
  (net 5 /p2_P)
  (net 6 /p2_N)
  (net 7 /p3_N)
  (net 8 /p3_P)
  (net 9 /p4_P)
  (net 10 /p4_N)
  (net 11 /p6_P)
  (net 12 /p6_N)
  (net 13 /p7_P)
  (net 14 /p7_N)
  (net 15 /p8_P)
  (net 16 /p8_N)
  (net 17 /p9_P)
  (net 18 /p9_N)
  (net 19 /p10_P)
  (net 20 /p10_N)
  (net 21 /p16_P)
  (net 22 /p16_N)
  (net 23 /p15_P)
  (net 24 /p15_N)
  (net 25 /p14_P)
  (net 26 /p14_N)
  (net 27 /p13_P)
  (net 28 /p13_N)
  (net 29 /p12_P)
  (net 30 /p12_N)
  (net 31 /p11_P)
  (net 32 /p11_N)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.2032)
    (add_net /p10_N)
    (add_net /p10_P)
    (add_net /p11_N)
    (add_net /p11_P)
    (add_net /p12_N)
    (add_net /p12_P)
    (add_net /p13_N)
    (add_net /p13_P)
    (add_net /p14_N)
    (add_net /p14_P)
    (add_net /p15_N)
    (add_net /p15_P)
    (add_net /p16_N)
    (add_net /p16_P)
    (add_net /p1_N)
    (add_net /p1_P)
    (add_net /p2_N)
    (add_net /p2_P)
    (add_net /p3_N)
    (add_net /p3_P)
    (add_net /p4_N)
    (add_net /p4_P)
    (add_net /p5_N)
    (add_net /p5_P)
    (add_net /p6_N)
    (add_net /p6_P)
    (add_net /p7_N)
    (add_net /p7_P)
    (add_net /p8_N)
    (add_net /p8_P)
    (add_net /p9_N)
    (add_net /p9_P)
  )
  (module photo_detectors:SiPM_6050VE (layer F.Cu) (tedit 5D5A2F30)
    (at 335.75 126.5)
    (fp_text reference D1 (at 0 4) (layer F.SilkS))
    (fp_text value D_SiPM (at 0.25 -4.5) (layer F.Fab))
    (fp_text user cathode (at 2.8194 -0.0254 -90) (layer F.SilkS))
    (fp_text user anode (at 0.5588 0.0254 -90) (layer F.SilkS))
    (pad 2 smd circle (at 1.25 -1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 12 /p6_N))
    (pad 2 smd circle (at 1.25 1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 12 /p6_N))
    (pad 2 smd circle (at -1.25 1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 12 /p6_N))
    (pad 2 smd circle (at -1.25 -1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 12 /p6_N))
    (pad 1 smd circle (at 2.5 -2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 11 /p6_P))
    (pad 1 smd circle (at 2.5 2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 11 /p6_P))
    (pad 1 smd circle (at -2.5 -2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 11 /p6_P))
    (pad 1 smd circle (at -2.5 2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 11 /p6_P))
    (model ${MY_DESIGNS}/kicad_libs/footprints/photo_detectors.pretty/sipm_shape.step
      (offset (xyz -3 3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module photo_detectors:SiPM_6050VE (layer F.Cu) (tedit 5D5A2F30)
    (at 306.75 126.5)
    (fp_text reference D2 (at 0 4) (layer F.SilkS))
    (fp_text value D_SiPM (at 0.25 -4.5) (layer F.Fab))
    (fp_text user anode (at 0.5588 0.0254 -90) (layer F.SilkS))
    (fp_text user cathode (at 2.8194 -0.0254 -90) (layer F.SilkS))
    (pad 1 smd circle (at -2.5 2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 13 /p7_P))
    (pad 1 smd circle (at -2.5 -2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 13 /p7_P))
    (pad 1 smd circle (at 2.5 2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 13 /p7_P))
    (pad 1 smd circle (at 2.5 -2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 13 /p7_P))
    (pad 2 smd circle (at -1.25 -1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 14 /p7_N))
    (pad 2 smd circle (at -1.25 1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 14 /p7_N))
    (pad 2 smd circle (at 1.25 1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 14 /p7_N))
    (pad 2 smd circle (at 1.25 -1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 14 /p7_N))
    (model ${MY_DESIGNS}/kicad_libs/footprints/photo_detectors.pretty/sipm_shape.step
      (offset (xyz -3 3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module photo_detectors:SiPM_6050VE (layer F.Cu) (tedit 5D5A2F30)
    (at 276.75 126.5)
    (fp_text reference D3 (at 0 4) (layer F.SilkS))
    (fp_text value D_SiPM (at 0.25 -4.5) (layer F.Fab))
    (fp_text user cathode (at 2.8194 -0.0254 -90) (layer F.SilkS))
    (fp_text user anode (at 0.5588 0.0254 -90) (layer F.SilkS))
    (pad 2 smd circle (at 1.25 -1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 /p8_N))
    (pad 2 smd circle (at 1.25 1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 /p8_N))
    (pad 2 smd circle (at -1.25 1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 /p8_N))
    (pad 2 smd circle (at -1.25 -1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 /p8_N))
    (pad 1 smd circle (at 2.5 -2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 15 /p8_P))
    (pad 1 smd circle (at 2.5 2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 15 /p8_P))
    (pad 1 smd circle (at -2.5 -2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 15 /p8_P))
    (pad 1 smd circle (at -2.5 2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 15 /p8_P))
    (model ${MY_DESIGNS}/kicad_libs/footprints/photo_detectors.pretty/sipm_shape.step
      (offset (xyz -3 3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module photo_detectors:SiPM_6050VE (layer F.Cu) (tedit 5D5A2F30)
    (at 250.75 126.5)
    (fp_text reference D4 (at 0 4) (layer F.SilkS))
    (fp_text value D_SiPM (at 0.25 -4.5) (layer F.Fab))
    (fp_text user anode (at 0.5588 0.0254 -90) (layer F.SilkS))
    (fp_text user cathode (at 2.8194 -0.0254 -90) (layer F.SilkS))
    (pad 1 smd circle (at -2.5 2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 17 /p9_P))
    (pad 1 smd circle (at -2.5 -2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 17 /p9_P))
    (pad 1 smd circle (at 2.5 2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 17 /p9_P))
    (pad 1 smd circle (at 2.5 -2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 17 /p9_P))
    (pad 2 smd circle (at -1.25 -1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 18 /p9_N))
    (pad 2 smd circle (at -1.25 1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 18 /p9_N))
    (pad 2 smd circle (at 1.25 1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 18 /p9_N))
    (pad 2 smd circle (at 1.25 -1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 18 /p9_N))
    (model ${MY_DESIGNS}/kicad_libs/footprints/photo_detectors.pretty/sipm_shape.step
      (offset (xyz -3 3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module photo_detectors:SiPM_6050VE (layer F.Cu) (tedit 5D5A2F30)
    (at 224.75 126.5)
    (fp_text reference D5 (at 0 4) (layer F.SilkS))
    (fp_text value D_SiPM (at 0.25 -4.5) (layer F.Fab))
    (fp_text user cathode (at 2.8194 -0.0254 -90) (layer F.SilkS))
    (fp_text user anode (at 0.5588 0.0254 -90) (layer F.SilkS))
    (pad 2 smd circle (at 1.25 -1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 20 /p10_N))
    (pad 2 smd circle (at 1.25 1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 20 /p10_N))
    (pad 2 smd circle (at -1.25 1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 20 /p10_N))
    (pad 2 smd circle (at -1.25 -1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 20 /p10_N))
    (pad 1 smd circle (at 2.5 -2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 19 /p10_P))
    (pad 1 smd circle (at 2.5 2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 19 /p10_P))
    (pad 1 smd circle (at -2.5 -2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 19 /p10_P))
    (pad 1 smd circle (at -2.5 2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 19 /p10_P))
    (model ${MY_DESIGNS}/kicad_libs/footprints/photo_detectors.pretty/sipm_shape.step
      (offset (xyz -3 3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module photo_detectors:SiPM_6050VE (layer F.Cu) (tedit 5D5A2F30)
    (at 194.75 126.5)
    (fp_text reference D6 (at 0 4) (layer F.SilkS))
    (fp_text value D_SiPM (at 0.25 -4.5) (layer F.Fab))
    (fp_text user cathode (at 2.8194 -0.0254 -90) (layer F.SilkS))
    (fp_text user anode (at 0.5588 0.0254 -90) (layer F.SilkS))
    (pad 2 smd circle (at 1.25 -1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 /p1_N))
    (pad 2 smd circle (at 1.25 1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 /p1_N))
    (pad 2 smd circle (at -1.25 1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 /p1_N))
    (pad 2 smd circle (at -1.25 -1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 /p1_N))
    (pad 1 smd circle (at 2.5 -2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 /p1_P))
    (pad 1 smd circle (at 2.5 2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 /p1_P))
    (pad 1 smd circle (at -2.5 -2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 /p1_P))
    (pad 1 smd circle (at -2.5 2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 /p1_P))
    (model ${MY_DESIGNS}/kicad_libs/footprints/photo_detectors.pretty/sipm_shape.step
      (offset (xyz -3 3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module photo_detectors:SiPM_6050VE (layer F.Cu) (tedit 5D5A2F30)
    (at 166.75 126.5)
    (fp_text reference D7 (at 0 4) (layer F.SilkS))
    (fp_text value D_SiPM (at 0.25 -4.5) (layer F.Fab))
    (fp_text user anode (at 0.5588 0.0254 -90) (layer F.SilkS))
    (fp_text user cathode (at 2.8194 -0.0254 -90) (layer F.SilkS))
    (pad 1 smd circle (at -2.5 2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 5 /p2_P))
    (pad 1 smd circle (at -2.5 -2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 5 /p2_P))
    (pad 1 smd circle (at 2.5 2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 5 /p2_P))
    (pad 1 smd circle (at 2.5 -2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 5 /p2_P))
    (pad 2 smd circle (at -1.25 -1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 6 /p2_N))
    (pad 2 smd circle (at -1.25 1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 6 /p2_N))
    (pad 2 smd circle (at 1.25 1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 6 /p2_N))
    (pad 2 smd circle (at 1.25 -1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 6 /p2_N))
    (model ${MY_DESIGNS}/kicad_libs/footprints/photo_detectors.pretty/sipm_shape.step
      (offset (xyz -3 3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module photo_detectors:SiPM_6050VE (layer F.Cu) (tedit 5D5A2F30)
    (at 137.75 126.5)
    (fp_text reference D8 (at 0 4) (layer F.SilkS))
    (fp_text value D_SiPM (at 0.25 -4.5) (layer F.Fab))
    (fp_text user cathode (at 2.8194 -0.0254 -90) (layer F.SilkS))
    (fp_text user anode (at 0.5588 1 -90) (layer F.SilkS))
    (pad 2 smd circle (at 1.25 -1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 7 /p3_N))
    (pad 2 smd circle (at 1.25 1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 7 /p3_N))
    (pad 2 smd circle (at -1.25 1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 7 /p3_N))
    (pad 2 smd circle (at -1.25 -1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 7 /p3_N))
    (pad 1 smd circle (at 2.5 -2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 8 /p3_P))
    (pad 1 smd circle (at 2.5 2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 8 /p3_P))
    (pad 1 smd circle (at -2.5 -2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 8 /p3_P))
    (pad 1 smd circle (at -2.5 2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 8 /p3_P))
    (model ${MY_DESIGNS}/kicad_libs/footprints/photo_detectors.pretty/sipm_shape.step
      (offset (xyz -3 3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module photo_detectors:SiPM_6050VE (layer F.Cu) (tedit 5D5A2F30)
    (at 109.75 126.5)
    (fp_text reference D9 (at 0 4) (layer F.SilkS))
    (fp_text value D_SiPM (at 0.25 -4.5) (layer F.Fab))
    (fp_text user anode (at 0.5588 0 -90) (layer F.SilkS))
    (fp_text user cathode (at 2.8194 -0.0254 -90) (layer F.SilkS))
    (pad 1 smd circle (at -2.5 2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 9 /p4_P))
    (pad 1 smd circle (at -2.5 -2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 9 /p4_P))
    (pad 1 smd circle (at 2.5 2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 9 /p4_P))
    (pad 1 smd circle (at 2.5 -2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 9 /p4_P))
    (pad 2 smd circle (at -1.25 -1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 10 /p4_N))
    (pad 2 smd circle (at -1.25 1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 10 /p4_N))
    (pad 2 smd circle (at 1.25 1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 10 /p4_N))
    (pad 2 smd circle (at 1.25 -1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 10 /p4_N))
    (model ${MY_DESIGNS}/kicad_libs/footprints/photo_detectors.pretty/sipm_shape.step
      (offset (xyz -3 3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module photo_detectors:SiPM_6050VE (layer F.Cu) (tedit 5D5A2F30)
    (at 81.75 126.5)
    (fp_text reference D10 (at 0 4) (layer F.SilkS))
    (fp_text value D_SiPM (at 0.25 -4.5) (layer F.Fab))
    (fp_text user anode (at 0.5588 0.0254 -90) (layer F.SilkS))
    (fp_text user cathode (at 2.8194 -0.0254 -90) (layer F.SilkS))
    (pad 1 smd circle (at -2.5 2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 /p5_P))
    (pad 1 smd circle (at -2.5 -2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 /p5_P))
    (pad 1 smd circle (at 2.5 2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 /p5_P))
    (pad 1 smd circle (at 2.5 -2.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 /p5_P))
    (pad 2 smd circle (at -1.25 -1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 /p5_N))
    (pad 2 smd circle (at -1.25 1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 /p5_N))
    (pad 2 smd circle (at 1.25 1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 /p5_N))
    (pad 2 smd circle (at 1.25 -1.25) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 /p5_N))
    (model ${MY_DESIGNS}/kicad_libs/footprints/photo_detectors.pretty/sipm_shape.step
      (offset (xyz -3 3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x16_Pitch2.54mm_SMD (layer B.Cu) (tedit 59650533)
    (at 206.98 126.475 270)
    (descr "surface-mounted straight pin header, 2x16, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x16 2.54mm double row")
    (attr smd)
    (fp_text reference J1 (at 0 21.38 90) (layer B.SilkS))
    (fp_text value Conn_02x16_Odd_Even (at 0 -21.38 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 32 smd rect (at 2.525 -19.05 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 21 /p16_P))
    (pad 31 smd rect (at -2.525 -19.05 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 22 /p16_N))
    (pad 30 smd rect (at 2.525 -16.51 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 23 /p15_P))
    (pad 29 smd rect (at -2.525 -16.51 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 24 /p15_N))
    (pad 28 smd rect (at 2.525 -13.97 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 25 /p14_P))
    (pad 27 smd rect (at -2.525 -13.97 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 26 /p14_N))
    (pad 26 smd rect (at 2.525 -11.43 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 27 /p13_P))
    (pad 25 smd rect (at -2.525 -11.43 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 28 /p13_N))
    (pad 24 smd rect (at 2.525 -8.89 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 29 /p12_P))
    (pad 23 smd rect (at -2.525 -8.89 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 30 /p12_N))
    (pad 22 smd rect (at 2.525 -6.35 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 31 /p11_P))
    (pad 21 smd rect (at -2.525 -6.35 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 32 /p11_N))
    (pad 20 smd rect (at 2.525 -3.81 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 19 /p10_P))
    (pad 19 smd rect (at -2.525 -3.81 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 20 /p10_N))
    (pad 18 smd rect (at 2.525 -1.27 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 17 /p9_P))
    (pad 17 smd rect (at -2.525 -1.27 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 18 /p9_N))
    (pad 16 smd rect (at 2.525 1.27 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 15 /p8_P))
    (pad 15 smd rect (at -2.525 1.27 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 16 /p8_N))
    (pad 14 smd rect (at 2.525 3.81 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 13 /p7_P))
    (pad 13 smd rect (at -2.525 3.81 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 14 /p7_N))
    (pad 12 smd rect (at 2.525 6.35 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 11 /p6_P))
    (pad 11 smd rect (at -2.525 6.35 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 12 /p6_N))
    (pad 10 smd rect (at 2.525 8.89 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 1 /p5_P))
    (pad 9 smd rect (at -2.525 8.89 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 2 /p5_N))
    (pad 8 smd rect (at 2.525 11.43 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 9 /p4_P))
    (pad 7 smd rect (at -2.525 11.43 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 10 /p4_N))
    (pad 6 smd rect (at 2.525 13.97 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 8 /p3_P))
    (pad 5 smd rect (at -2.525 13.97 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 7 /p3_N))
    (pad 4 smd rect (at 2.525 16.51 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 5 /p2_P))
    (pad 3 smd rect (at -2.525 16.51 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 6 /p2_N))
    (pad 2 smd rect (at 2.525 19.05 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 4 /p1_P))
    (pad 1 smd rect (at -2.525 19.05 270) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 3 /p1_N))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x16_Pitch2.54mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x02_Pitch2.54mm_SMD (layer B.Cu) (tedit 59650532)
    (at 323.75 126 180)
    (descr "surface-mounted straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x02 2.54mm double row")
    (attr smd)
    (fp_text reference J2 (at 0 3.6) (layer B.SilkS))
    (fp_text value Conn_02x02_Odd_Even (at 0 -3.6) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 4 smd rect (at 2.525 -1.27 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 22 /p16_N))
    (pad 3 smd rect (at -2.525 -1.27 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 21 /p16_P))
    (pad 2 smd rect (at 2.525 1.27 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 24 /p15_N))
    (pad 1 smd rect (at -2.525 1.27 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 23 /p15_P))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x02_Pitch2.54mm_SMD (layer F.Cu) (tedit 59650532)
    (at 352 126)
    (descr "surface-mounted straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x02 2.54mm double row")
    (attr smd)
    (fp_text reference J3 (at 0 -3.6) (layer F.SilkS))
    (fp_text value Conn_02x02_Odd_Even (at 0 3.6) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.525 -1.27) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 27 /p13_P))
    (pad 2 smd rect (at 2.525 -1.27) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 28 /p13_N))
    (pad 3 smd rect (at -2.525 1.27) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 25 /p14_P))
    (pad 4 smd rect (at 2.525 1.27) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 26 /p14_N))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x02_Pitch2.54mm_SMD (layer F.Cu) (tedit 59650532)
    (at 63.5 126.25)
    (descr "surface-mounted straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x02 2.54mm double row")
    (attr smd)
    (fp_text reference J4 (at 0 -3.6) (layer F.SilkS))
    (fp_text value Conn_02x02_Odd_Even (at 0 3.6) (layer F.Fab))
    (fp_text user %R (at 0 0 -270) (layer F.Fab))
    (pad 4 smd rect (at 2.525 1.27) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 30 /p12_N))
    (pad 3 smd rect (at -2.525 1.27) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 29 /p12_P))
    (pad 2 smd rect (at 2.525 -1.27) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 32 /p11_N))
    (pad 1 smd rect (at -2.525 -1.27) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 31 /p11_P))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 57.75 131.5) (end 67.75 131.5) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 57.75 121.5) (end 57.75 131.5) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 67.75 121.5) (end 57.75 121.5) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 357.75 131.5) (end 347.75 131.5) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 357.75 121.5) (end 357.75 131.5) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 347.75 121.5) (end 357.75 121.5) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 347.75 121.5) (end 67.75 121.5) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 67.75 131.5) (end 347.75 131.5) (layer Edge.Cuts) (width 0.0254))
)
