(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 55)
    (no_connects 2)
    (area 33.3375 31.4325 218.757501 168.592501)
    (thickness 1.6)
    (drawings 59)
    (tracks 226)
    (zones 0)
    (modules 16)
    (nets 32)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 Earth)
  (net 2 /MOSI)
  (net 3 /Clock)
  (net 4 /MISO)
  (net 5 /CS)
  (net 6 /QTI_R)
  (net 7 /QTI_RR)
  (net 8 /QTI_LL)
  (net 9 /QTI_L)
  (net 10 "Net-(B1-Pad15)")
  (net 11 "Net-(B1-Pad6)")
  (net 12 "Net-(B1-Pad14)")
  (net 13 "Net-(B1-Pad7)")
  (net 14 "Net-(B1-Pad13)")
  (net 15 /SONAR)
  (net 16 "Net-(B1-Pad9)")
  (net 17 "Net-(B1-Pad11)")
  (net 18 +5V)
  (net 19 /IR_1)
  (net 20 /IR_2)
  (net 21 /RN1.4)
  (net 22 /LED_AH)
  (net 23 /LED_BG)
  (net 24 /RN1.3)
  (net 25 /RN1.2)
  (net 26 /LED_CF)
  (net 27 /LED_DE)
  (net 28 /RN1.1)
  (net 29 /BATTERY_READ)
  (net 30 "Net-(U1-Pad1)")
  (net 31 "Net-(B1-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /BATTERY_READ)
    (add_net /CS)
    (add_net /Clock)
    (add_net /IR_1)
    (add_net /IR_2)
    (add_net /LED_AH)
    (add_net /LED_BG)
    (add_net /LED_CF)
    (add_net /LED_DE)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /QTI_L)
    (add_net /QTI_LL)
    (add_net /QTI_R)
    (add_net /QTI_RR)
    (add_net /RN1.1)
    (add_net /RN1.2)
    (add_net /RN1.3)
    (add_net /RN1.4)
    (add_net /SONAR)
    (add_net Earth)
    (add_net "Net-(B1-Pad11)")
    (add_net "Net-(B1-Pad13)")
    (add_net "Net-(B1-Pad14)")
    (add_net "Net-(B1-Pad15)")
    (add_net "Net-(B1-Pad6)")
    (add_net "Net-(B1-Pad7)")
    (add_net "Net-(B1-Pad8)")
    (add_net "Net-(B1-Pad9)")
    (add_net "Net-(U1-Pad1)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A662F95)
    (at 106.68 99.06 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value LL (at 0 -3.048 180) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /QTI_LL))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 +5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A662FA1)
    (at 106.68 106.68 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value RR (at 0 -3.048 180) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /QTI_RR))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 +5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A66317E)
    (at 116.84 109.22 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 0 -2.286 90) (layer F.Fab) hide)
    (fp_text value SNR (at 0.508 -2.54 90) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /SONAR))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A663092)
    (at 116.84 101.6 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value 2 (at 1.016 -2.286 180) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 +5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /IR_2))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCAD-Footprints:BOE (layer F.Cu) (tedit 5A2EC149)
    (at 129.413 97.917)
    (fp_text reference B1 (at 0.127 -14.007) (layer F.SilkS) hide)
    (fp_text value BOE-BOARD (at 3.937 1.397 270) (layer F.Fab))
    (pad 20 thru_hole oval (at 1.397 -11.557 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 1 thru_hole oval (at -1.143 -11.557 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 19 thru_hole oval (at 1.397 -9.017 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 /MOSI))
    (pad 2 thru_hole oval (at -1.143 -9.017 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Clock))
    (pad 18 thru_hole oval (at 1.397 -6.477 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 /MISO))
    (pad 3 thru_hole oval (at -1.143 -6.477 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 /CS))
    (pad 17 thru_hole oval (at 1.397 -3.937 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 /QTI_R))
    (pad 4 thru_hole oval (at -1.143 -3.937 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 /QTI_RR))
    (pad 16 thru_hole oval (at 1.397 -1.397 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 /QTI_LL))
    (pad 5 thru_hole oval (at -1.143 -1.397 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 9 /QTI_L))
    (pad 15 thru_hole oval (at 1.397 1.143 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(B1-Pad15)"))
    (pad 6 thru_hole oval (at -1.143 1.143 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(B1-Pad6)"))
    (pad 14 thru_hole oval (at 1.397 3.683 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(B1-Pad14)"))
    (pad 7 thru_hole oval (at -1.143 3.683 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(B1-Pad7)"))
    (pad 13 thru_hole oval (at 1.397 6.223 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(B1-Pad13)"))
    (pad 8 thru_hole oval (at -1.143 6.223 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(B1-Pad8)"))
    (pad 12 thru_hole oval (at 1.397 8.763 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 15 /SONAR))
    (pad 9 thru_hole oval (at -1.143 8.763 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(B1-Pad9)"))
    (pad 11 thru_hole oval (at 1.397 11.303 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(B1-Pad11)"))
    (pad 10 thru_hole oval (at -1.143 11.303 270) (size 1.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 18 +5V))
  )
  (module Capacitors_THT:CP_Radial_D4.0mm_P1.50mm (layer F.Cu) (tedit 5A3AACC4)
    (at 110.617 78.637 270)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference C1 (at 0.75 -3.31 270) (layer F.SilkS) hide)
    (fp_text value C (at 0.738 2.0955 270) (layer F.Fab))
    (fp_text user %R (at 1.27 0 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 18 +5V))
    (pad 2 thru_hole circle (at 1.5 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 Earth))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D4.0mm_P1.50mm (layer F.Cu) (tedit 5A3AACBE)
    (at 110.6805 89.154 270)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference C2 (at 0.75 -3.31 270) (layer F.SilkS) hide)
    (fp_text value C (at 0.6985 2.032 270) (layer F.Fab))
    (fp_text user %R (at 1.27 0 450) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 18 +5V))
    (pad 2 thru_hole circle (at 1.5 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 Earth))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCAD-Footprints:LTL-2820G (layer F.Cu) (tedit 5A2EC490)
    (at 129.54 96.52 270)
    (fp_text reference L1 (at -11.34 0 360) (layer F.SilkS) hide)
    (fp_text value LTL-2820G (at 0 0 270) (layer F.SilkS) hide)
    (pad 16 thru_hole oval (at -8.89 -3.81 270) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 21 /RN1.4))
    (pad 1 thru_hole oval (at -8.89 3.81 270) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 21 /RN1.4))
    (pad 15 thru_hole oval (at -6.35 -3.81 270) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 22 /LED_AH))
    (pad 2 thru_hole oval (at -6.35 3.81 270) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 22 /LED_AH))
    (pad 14 thru_hole oval (at -3.81 -3.81 270) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 23 /LED_BG))
    (pad 3 thru_hole oval (at -3.81 3.81 270) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 23 /LED_BG))
    (pad 13 thru_hole oval (at -1.27 -3.81 270) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 24 /RN1.3))
    (pad 4 thru_hole oval (at -1.27 3.81 270) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 24 /RN1.3))
    (pad 12 thru_hole oval (at 1.27 -3.81 270) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 25 /RN1.2))
    (pad 5 thru_hole oval (at 1.27 3.81 270) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 25 /RN1.2))
    (pad 11 thru_hole oval (at 3.81 -3.81 270) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 26 /LED_CF))
    (pad 6 thru_hole oval (at 3.81 3.81 270) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 26 /LED_CF))
    (pad 10 thru_hole oval (at 6.35 -3.81 270) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 27 /LED_DE))
    (pad 7 thru_hole oval (at 6.35 3.81 270) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 27 /LED_DE))
    (pad 9 thru_hole oval (at 8.89 -3.81 270) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 28 /RN1.1))
    (pad 8 thru_hole oval (at 8.89 3.81 270) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 28 /RN1.1))
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5A394466)
    (at 114.3635 82.042)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.81 2.31) (layer B.SilkS) hide)
    (fp_text value 1MΩR (at 3.683 0) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /BATTERY_READ))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(B1-Pad11)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5A39446A)
    (at 122.047 92.71 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 3.8735 2.159 180) (layer B.SilkS) hide)
    (fp_text value 1MΩR (at 3.937 -0.0635 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /BATTERY_READ))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A663094)
    (at 116.84 104.14 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value 1 (at -1.016 -2.286 180) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 +5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /IR_1))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A662FA6)
    (at 106.68 101.6 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value L (at 0 -3.048 180) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /QTI_L))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 +5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A662FA3)
    (at 106.68 104.14 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 -3.048 180) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /QTI_R))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 +5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Array_SIP5 (layer F.Cu) (tedit 5A394435)
    (at 137.033 90.17 270)
    (descr "5-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at 6.35 -2.4 270) (layer F.SilkS) hide)
    (fp_text value 180ΩR (at 6.35 2.4 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /RN1.4))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /RN1.3))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /RN1.2))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /RN1.1))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Array_SIP5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket (layer F.Cu) (tedit 5A622E3B)
    (at 114.427 85.852 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U1 (at 3.81 -2.33 90) (layer F.SilkS) hide)
    (fp_text value TINY (at 2.8575 -2.4765 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(U1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /LED_BG))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /LED_DE))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /LED_AH))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /LED_CF))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /BATTERY_READ))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket (layer F.Cu) (tedit 5A622E44)
    (at 114.427 96.393 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U2 (at 3.81 -2.33 90) (layer F.SilkS) hide)
    (fp_text value ADC (at 3.6195 -2.032 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /CS))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /MOSI))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /IR_1))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /MISO))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /IR_2))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /Clock))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text - (at 119.126 99.06) (layer F.SilkS))
  (gr_line (start 123.825 77.1525) (end 123.825 78.105) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 107.442 78.6765) (end 107.442 92.075) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 123.3805 76.708) (end 109.2835 76.708) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 123.3805 77.1525) (end 123.3805 76.708) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 109.347 78.613) (end 107.442 78.6765) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.537 93.98) (end 104.775 93.98) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 105.537 92.075) (end 107.442 92.075) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.632 111.125) (end 137.16 111.125) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.505 93.98) (end 104.775 93.98) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 102.108 109.601) (end 102.108 95.631) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 103.632 95.504) (end 102.108 95.631) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 103.632 109.601) (end 103.632 111.125) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text W (at 121.92 107.188) (layer F.SilkS))
  (gr_text R (at 119.38 107.188) (layer F.SilkS))
  (gr_text B (at 116.84 107.188) (layer F.SilkS))
  (gr_text Sig (at 121.92 99.06) (layer F.SilkS))
  (gr_text + (at 116.586 99.06) (layer F.SilkS))
  (gr_text IR (at 114.3 102.87) (layer F.SilkS))
  (gr_line (start 132.08 78.74) (end 124.46 78.74) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 124.46 78.105) (end 124.46 78.74) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "Daniel M.\nDimitry K.\nMichelle K." (at 129.16 81.88) (layer F.SilkS))
  (gr_line (start 139.065 86.995) (end 139.065 109.22) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.89 85.09) (end 137.16 85.09) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.985 80.645) (end 133.985 83.185) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 137.16 109.22) (end 139.065 109.22) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 137.16 86.995) (end 137.16 85.09) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 135.89 83.185) (end 135.89 85.09) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 132.08 80.645) (end 132.08 78.74) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text TEJ4M (at 135.636 109.728) (layer F.SilkS))
  (gr_text WCSS (at 135.6995 107.95) (layer F.SilkS))
  (gr_text W (at 111.0615 109.22) (layer F.SilkS))
  (gr_text R (at 108.331 109.22) (layer F.SilkS))
  (gr_text B (at 105.791 109.22) (layer F.SilkS))
  (gr_text QTI (at 108.5215 95.9485) (layer F.SilkS))
  (zone (net 1) (net_name Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.9575 89.8525) (xy 58.7375 33.9725) (xy 119.6975 31.4325) (xy 195.8975 36.5125) (xy 218.7575 105.0925)
        (xy 208.5975 160.9725) (xy 127.3175 168.5925) (xy 33.3375 155.8925) (xy 40.9575 94.9325)
      )
    )
  )
)
