<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="37.751371875" y1="19.04" x2="4.25731875" y2="19.04" width="0" layer="20"/>
<wire x1="4.25731875" y1="19.04" x2="2.54" y2="17.32268125" width="0" layer="20" curve="90"/>
<wire x1="2.54" y1="17.32268125" x2="2.54" y2="1.3008" width="0" layer="20"/>
<wire x1="2.54" y1="1.3008" x2="3.8408" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3.8408" y1="0" x2="37.74" y2="0" width="0" layer="20"/>
<wire x1="37.74" y1="0" x2="39.421" y2="1.681" width="0" layer="20" curve="90"/>
<wire x1="39.421" y1="1.681" x2="39.421" y2="17.370371875" width="0" layer="20"/>
<wire x1="39.421" y1="17.370371875" x2="37.751371875" y2="19.04" width="0" layer="20" curve="90"/>
<text>RV-Project.Com
Test Board SB4A
1-9-2021</text>
<hole x="11.43" y="13.97" drill="2.54"/>
<hole x="5.08" y="13.97" drill="2.54"/>
<hole x="11.43" y="5.08" drill="2.54"/>
<hole x="5.08" y="5.08" drill="2.54"/>
</plain>
<libraries>
<library name="a-lib_Connectors">
<description>Thru-Hole Connectors (Connectors, Terminals)</description>
<packages>
<package name="KEYSTONE_4919">
</package>
<package name="MO1-18AWG">
</package>
</packages>
</library>
<library name="a-lib_Passives">
<description>Thru-Hole Passives (Resistors, Capacitors)</description>
<packages>
<package name="2-SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="TB1" library="a-lib_Connectors" package="KEYSTONE_4919" value=""/>
<element name="TB2" library="a-lib_Connectors" package="KEYSTONE_4919" value=""/>
<element name="TB3" library="a-lib_Connectors" package="MO1-18AWG" value=""/>
<element name="TB4" library="a-lib_Connectors" package="MO1-18AWG" value=""/>
<element name="F1" library="a-lib_Passives" package="2-SMD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$5">
</signal>
<signal name="N$6">
</signal>
<signal name="N$1">
<contactref element="TB3" pad="P$1"/>
<contactref element="TB1" pad="T1"/>
<contactref element="TB1" pad="T2"/>
</signal>
<signal name="N$2">
<contactref element="F1" pad="P$1"/>
<contactref element="TB4" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="TB2" pad="T2"/>
<contactref element="TB2" pad="T1"/>
<contactref element="F1" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
