<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="-33.02" y1="-7.62" x2="-33.02" y2="10.16" width="0.1524" layer="20"/>
<wire x1="-33.02" y1="10.16" x2="-30.48" y2="13.462" width="0.1524" layer="20" curve="-90"/>
<wire x1="-30.48" y1="13.462" x2="50.8" y2="13.462" width="0.1524" layer="20"/>
<wire x1="50.8" y1="13.462" x2="53.34" y2="10.16" width="0.1524" layer="20" curve="-90"/>
<wire x1="53.34" y1="10.16" x2="55.88" y2="7.62" width="0.1524" layer="20" curve="90"/>
<wire x1="55.88" y1="7.62" x2="58.42" y2="10.16" width="0.1524" layer="20" curve="90"/>
<wire x1="58.42" y1="10.16" x2="60.706" y2="13.462" width="0.1524" layer="20" curve="-90"/>
<wire x1="60.706" y1="13.462" x2="78.486" y2="13.462" width="0.1524" layer="20"/>
<wire x1="78.486" y1="13.462" x2="81.28" y2="10.16" width="0.1524" layer="20" curve="-90"/>
<wire x1="81.28" y1="10.16" x2="81.28" y2="-7.62" width="0.1524" layer="20"/>
<wire x1="81.28" y1="-7.62" x2="78.74" y2="-10.922" width="0.1524" layer="20" curve="-90"/>
<wire x1="78.74" y1="-10.922" x2="60.96" y2="-10.922" width="0.1524" layer="20"/>
<wire x1="60.96" y1="-10.922" x2="58.42" y2="-7.62" width="0.1524" layer="20" curve="-90"/>
<wire x1="58.42" y1="-7.62" x2="55.88" y2="-5.08" width="0.1524" layer="20" curve="90"/>
<wire x1="55.88" y1="-5.08" x2="53.34" y2="-7.62" width="0.1524" layer="20" curve="90"/>
<wire x1="53.34" y1="-7.62" x2="51.308" y2="-10.922" width="0.1524" layer="20" curve="-90"/>
<wire x1="51.308" y1="-10.922" x2="-29.972" y2="-10.922" width="0.1524" layer="20"/>
<wire x1="-29.972" y1="-10.922" x2="-33.02" y2="-7.62" width="0.1524" layer="20" curve="-90"/>
<text>R</text>
<text>L</text>
<text>BTN</text>
<text>3.3V</text>
<text>3.3V</text>
<text>3.3V</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>5V</text>
<text>DAT</text>
<text>1</text>
<text>2</text>
<text>8</text>
<text>5V</text>
<text>IO12</text>
<text>IO27</text>
<text>IO27</text>
<text>IO12</text>
<text>5V</text>
<text>GND</text>
<text>3.3V</text>
<text>IO33</text>
<text>IO15</text>
<text>3.3V</text>
<text>L</text>
<text>R</text>
<text>BTN</text>
<text>3.3V</text>
<text>3.3V</text>
<text>BTN</text>
<text>L</text>
<text>R</text>
<text>BEN'S</text>
<text>BUTTON SUPPORT</text>
<text>REV A</text>
<text>BEN'S</text>
<text>MONITOR RISER</text>
<circle x="54.1274" y="-2.54" radius="0.259028125" width="0.381" layer="46"/>
<circle x="54.1274" y="-1.27" radius="0.259028125" width="0.381" layer="46"/>
<circle x="54.1274" y="0" radius="0.259028125" width="0.381" layer="46"/>
<circle x="54.1274" y="2.54" radius="0.259028125" width="0.381" layer="46"/>
<circle x="54.1274" y="5.08" radius="0.259028125" width="0.381" layer="46"/>
<circle x="54.1274" y="3.7846" radius="0.259028125" width="0.381" layer="46"/>
<circle x="54.1274" y="1.27" radius="0.259028125" width="0.381" layer="46"/>
<text>R</text>
<text>L</text>
<text>BTN</text>
<text>3.3V</text>
<text>REV A</text>
</plain>
<libraries>
<library name="74xx-us">
<description>&lt;b&gt;TTL Devices, 74xx Series with US Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="personal">
<packages>
<package name="CAP1000UF_0807_0304">
</package>
<package name="ROTARYENCODER">
</package>
<package name="FEATHER32">
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1,6/0,9">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="74*125" library="74xx-us" package="DIL14" value="74125N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="470">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="CAP1" library="personal" package="CAP1000UF_0807_0304" value="1000uF"/>
<element name="LED1" library="wirepad" package="1,6/0,9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="wirepad" package="1,6/0,9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="wirepad" package="1,6/0,9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="wirepad" package="1,6/0,9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ONBOARD_ROT" library="personal" package="ROTARYENCODER" value="ROTARYENCODER"/>
<element name="OFFBOARD_ROT" library="personal" package="ROTARYENCODER" value="ROTARYENCODER"/>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="330">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3" value="330">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.3" value="330">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.3" value="470">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="AXIAL-0.3" value="470">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="AXIAL-0.3" value="470">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="personal" package="FEATHER32" value="FEATHER32"/>
<element name="BTN2" library="wirepad" package="1,6/0,9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LPIN" library="wirepad" package="1,6/0,9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RPIN" library="wirepad" package="1,6/0,9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LRVAL" library="wirepad" package="1,6/0,9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="74*125" pad="7"/>
<contactref element="74*125" pad="1"/>
<contactref element="74*125" pad="4"/>
<contactref element="74*125" pad="10"/>
<contactref element="74*125" pad="13"/>
<contactref element="LED1" pad="1"/>
<contactref element="LED2" pad="1"/>
<contactref element="CAP1" pad="NEG"/>
<contactref element="R5" pad="P$1"/>
<contactref element="R7" pad="P$2"/>
<contactref element="R6" pad="P$2"/>
<contactref element="U$1" pad="GND"/>
</signal>
<signal name="VCC">
<contactref element="74*125" pad="14"/>
<contactref element="LED3" pad="1"/>
<contactref element="CAP1" pad="POS"/>
<contactref element="U$1" pad="VCC"/>
</signal>
<signal name="3.3V">
<contactref element="ONBOARD_ROT" pad="BTN1"/>
<contactref element="ONBOARD_ROT" pad="LRVAL"/>
<contactref element="U$1" pad="3.3V"/>
</signal>
<signal name="N$1">
<contactref element="74*125" pad="3"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="DAT5V">
<contactref element="R1" pad="P$2"/>
<contactref element="LED4" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="P$2"/>
<contactref element="ONBOARD_ROT" pad="BTN2"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="P$1"/>
<contactref element="ONBOARD_ROT" pad="RPIN"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="P$1"/>
<contactref element="ONBOARD_ROT" pad="LPIN"/>
</signal>
<signal name="IO12">
<contactref element="74*125" pad="2"/>
<contactref element="U$1" pad="IO12_A11"/>
</signal>
<signal name="IO27">
<contactref element="R7" pad="P$1"/>
<contactref element="R3" pad="P$2"/>
<contactref element="U$1" pad="IO27_A10"/>
</signal>
<signal name="IO33">
<contactref element="R6" pad="P$1"/>
<contactref element="R4" pad="P$2"/>
<contactref element="U$1" pad="IO33_A9"/>
</signal>
<signal name="IO15">
<contactref element="R5" pad="P$2"/>
<contactref element="R2" pad="P$1"/>
<contactref element="U$1" pad="IO15_A8"/>
</signal>
<signal name="N$5">
<contactref element="OFFBOARD_ROT" pad="BTN1"/>
<contactref element="OFFBOARD_ROT" pad="LRVAL"/>
<contactref element="LRVAL" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="BTN2" pad="1"/>
<contactref element="OFFBOARD_ROT" pad="BTN2"/>
</signal>
<signal name="N$8">
<contactref element="LPIN" pad="1"/>
<contactref element="OFFBOARD_ROT" pad="LPIN"/>
</signal>
<signal name="N$9">
<contactref element="RPIN" pad="1"/>
<contactref element="OFFBOARD_ROT" pad="RPIN"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
