(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "MiniNDP 256")
    (date "2023-11-13")
    (rev "014")
    (company "Brian K. White - b.kenyon.w@gmail.com")
    (comment 1 "github.com/bkw777/NODE_DATAPAC")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "ENIG")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 121.95 86.025)
    (grid_origin 151.95 115.025)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "GERBER_${TITLE}_${REVISION}")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "VMEM")
  (net 3 "VBUS")
  (net 4 "/AD0")
  (net 5 "/AD1")
  (net 6 "/AD2")
  (net 7 "/AD3")
  (net 8 "/AD4")
  (net 9 "/AD5")
  (net 10 "/AD6")
  (net 11 "/AD7")
  (net 12 "/A8")
  (net 13 "/A9")
  (net 14 "/A10")
  (net 15 "/A11")
  (net 16 "/A12")
  (net 17 "/A13")
  (net 18 "/A14")
  (net 19 "/A15")
  (net 20 "/~{RD}")
  (net 21 "/RAMRST")
  (net 22 "/~{Y0}")
  (net 23 "/(A)")
  (net 24 "unconnected-(J1-Pin_39-Pad39)")
  (net 25 "unconnected-(J1-Pin_40-Pad40)")
  (net 26 "unconnected-(J1-Pin_30-Pad30)")
  (net 27 "unconnected-(J1-Pin_31-Pad31)")
  (net 28 "unconnected-(J1-Pin_37-Pad37)")
  (net 29 "/~{BLOCK}")
  (net 30 "/~{BYTE}")
  (net 31 "/CARRY0")
  (net 32 "unconnected-(U4-O7-Pad7)")
  (net 33 "unconnected-(U4-O6-Pad9)")
  (net 34 "unconnected-(U4-O5-Pad10)")
  (net 35 "unconnected-(U4-O4-Pad11)")
  (net 36 "unconnected-(U4-O2-Pad13)")
  (net 37 "unconnected-(U4-O0-Pad15)")
  (net 38 "/SLEEP")
  (net 39 "/A5")
  (net 40 "/A6")
  (net 41 "/CARRY1")
  (net 42 "/~{CE}")
  (net 43 "/A7")
  (net 44 "/BATT+")
  (net 45 "/BUS_A8")
  (net 46 "/BUS_A9")
  (net 47 "/A16")
  (net 48 "/A17")
  (net 49 "/A0")
  (net 50 "/A1")
  (net 51 "/A2")
  (net 52 "/A3")
  (net 53 "/A4")
  (net 54 "unconnected-(J1-Pin_15-Pad15)")
  (net 55 "unconnected-(J1-Pin_16-Pad16)")
  (net 56 "unconnected-(J1-Pin_17-Pad17)")
  (net 57 "unconnected-(J1-Pin_18-Pad18)")
  (net 58 "unconnected-(J1-Pin_19-Pad19)")
  (net 59 "unconnected-(J1-Pin_20-Pad20)")
  (net 60 "unconnected-(J1-Pin_25-Pad25)")
  (net 61 "unconnected-(J1-Pin_26-Pad26)")
  (net 62 "unconnected-(J1-Pin_27-Pad27)")
  (net 63 "unconnected-(J1-Pin_28-Pad28)")
  (net 64 "unconnected-(J1-Pin_33-Pad33)")
  (net 65 "unconnected-(J1-Pin_34-Pad34)")
  (net 66 "unconnected-(U3-Q3-Pad11)")
  (net 67 "unconnected-(U3-Q2-Pad12)")
  (net 68 "unconnected-(U3-TC-Pad15)")
  (net 69 "/~{WR}")
  (net 70 "unconnected-(DA1B-A-Pad5)")
  (net 71 "Net-(C1-Pad1)")
  (footprint "000_LOCAL:CP_6032" (layer "F.Cu")
    (at 152.331 110.85 180)
    (descr "Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "Sheetfile" "MiniNDP_256.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor, small symbol")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 3.75 0.6 unlocked) (layer "F.SilkS"))
    (fp_text value "220u10v" (at 3.75 -0.75 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.4625 0 180) (size 2.075 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1204819277)
      (net 71 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.4625 0 180) (size 2.075 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1204819277)
      (net 1 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CP_6032-28.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CP_6032-15.step" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "000_LOCAL:MountHole_M2.5" (layer "F.Cu")
    (at 179.45 88.525)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, ISO7380")
    (tags "mounting hole 2.7mm no annular m2.5 iso7380")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "M1" (at 0 -3.25) (layer "F.SilkS") hide)
    (fp_text value "MountHole_M2.5" (at 0 3.25) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.6) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (solder_mask_margin -0.1))
  )
  (footprint "000_LOCAL:Fiducial_0.75_1.5" (layer "F.Cu")
    (at 175.95 88.025)
    (descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
    (tags "fiducial")
    (zone_connect 0)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "F1" (at 0 -2) (layer "F.SilkS") hide)
    (fp_text value "Fiducial_0.75_1.5" (at 0 2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "" smd circle (at 0 0) (size 0.75 0.75) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.375) (clearance 0.375))
  )
  (footprint "000_LOCAL:MountHole_M2.5" (layer "F.Cu")
    (at 124.45 117.525)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, ISO7380")
    (tags "mounting hole 2.7mm no annular m2.5 iso7380")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "M3" (at 0 -3.25) (layer "F.SilkS") hide)
    (fp_text value "MountHole_M2.5" (at 0 3.25) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.6) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (solder_mask_margin -0.1))
  )
  (footprint "000_LOCAL:TSSOP-16" (layer "F.Cu")
    (at 139.15 108.55 180)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "MiniNDP_256.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Decoder 3 to 8 active low outputs")
    (property "ki_keywords" "TTL DECOD DECOD8")
    (attr smd)
    (fp_text reference "U4" (at -1.25 -1 90 unlocked) (layer "F.SilkS"))
    (fp_text value "74138" (at 1 0 90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "/BUS_A8") (pinfunction "A0") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.625 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "/BUS_A9") (pinfunction "A1") (pintype "input"))
    (pad "3" smd roundrect (at -2.8625 -0.975 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "A2") (pintype "input"))
    (pad "4" smd roundrect (at -2.8625 -0.325 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "E1") (pintype "input"))
    (pad "5" smd roundrect (at -2.8625 0.325 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/~{Y0}") (pinfunction "E2") (pintype "input"))
    (pad "6" smd roundrect (at -2.8625 0.975 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/(A)") (pinfunction "E3") (pintype "input"))
    (pad "7" smd roundrect (at -2.8625 1.625 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "unconnected-(U4-O7-Pad7)") (pinfunction "O7") (pintype "output+no_connect"))
    (pad "8" smd roundrect (at -2.8625 2.275 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" smd roundrect (at 2.8625 2.275 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "unconnected-(U4-O6-Pad9)") (pinfunction "O6") (pintype "output+no_connect"))
    (pad "10" smd roundrect (at 2.8625 1.625 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "unconnected-(U4-O5-Pad10)") (pinfunction "O5") (pintype "output+no_connect"))
    (pad "11" smd roundrect (at 2.8625 0.975 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "unconnected-(U4-O4-Pad11)") (pinfunction "O4") (pintype "output+no_connect"))
    (pad "12" smd roundrect (at 2.8625 0.325 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/~{BYTE}") (pinfunction "O3") (pintype "output"))
    (pad "13" smd roundrect (at 2.8625 -0.325 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "unconnected-(U4-O2-Pad13)") (pinfunction "O2") (pintype "output+no_connect"))
    (pad "14" smd roundrect (at 2.8625 -0.975 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/~{BLOCK}") (pinfunction "O1") (pintype "output"))
    (pad "15" smd roundrect (at 2.8625 -1.625 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "unconnected-(U4-O0-Pad15)") (pinfunction "O0") (pintype "output+no_connect"))
    (pad "16" smd roundrect (at 2.8625 -2.275 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "VBUS") (pinfunction "VCC") (pintype "power_in"))
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSSOP-16.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "000_LOCAL:Fiducial_0.75_1.5" (layer "F.Cu")
    (at 179.95 114.025)
    (descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
    (tags "fiducial")
    (zone_connect 0)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "F2" (at 0 -2) (layer "F.SilkS") hide)
    (fp_text value "Fiducial_0.75_1.5" (at 0 2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "" smd circle (at 0 0) (size 0.75 0.75) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.375) (clearance 0.375))
  )
  (footprint "000_LOCAL:MountHole_M2.5" (layer "F.Cu")
    (at 179.45 117.525)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, ISO7380")
    (tags "mounting hole 2.7mm no annular m2.5 iso7380")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "M2" (at 0 -3.25) (layer "F.SilkS") hide)
    (fp_text value "MountHole_M2.5" (at 0 3.25) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.6) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (solder_mask_margin -0.1))
  )
  (footprint "000_LOCAL:TSSOP-16" (layer "F.Cu")
    (at 139.15 91.825)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "MiniNDP_256.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Synchronous 4-bit programmable binary Counter")
    (property "ki_keywords" "TTL CNT CNT4")
    (attr smd)
    (fp_text reference "U2" (at -1.25 -1 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "74161" (at 1 0 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/~{BLOCK}") (pinfunction "~{MR}") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/~{BYTE}") (pinfunction "CP") (pintype "input"))
    (pad "3" smd roundrect (at -2.8625 -0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "D0") (pintype "input"))
    (pad "4" smd roundrect (at -2.8625 -0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "D1") (pintype "input"))
    (pad "5" smd roundrect (at -2.8625 0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "D2") (pintype "input"))
    (pad "6" smd roundrect (at -2.8625 0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "D3") (pintype "input"))
    (pad "7" smd roundrect (at -2.8625 1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/CARRY0") (pinfunction "CEP") (pintype "input"))
    (pad "8" smd roundrect (at -2.8625 2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" smd roundrect (at 2.8625 2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "VBUS") (pinfunction "~{PE}") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/CARRY0") (pinfunction "CET") (pintype "input"))
    (pad "11" smd roundrect (at 2.8625 0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "/A7") (pinfunction "Q3") (pintype "output"))
    (pad "12" smd roundrect (at 2.8625 0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/A6") (pinfunction "Q2") (pintype "output"))
    (pad "13" smd roundrect (at 2.8625 -0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/A5") (pinfunction "Q1") (pintype "output"))
    (pad "14" smd roundrect (at 2.8625 -0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "/A4") (pinfunction "Q0") (pintype "output"))
    (pad "15" smd roundrect (at 2.8625 -1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/CARRY1") (pinfunction "TC") (pintype "output"))
    (pad "16" smd roundrect (at 2.8625 -2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "VBUS") (pinfunction "VCC") (pintype "power_in"))
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSSOP-16.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "000_LOCAL:C_0805" (layer "F.Cu")
    (at 133.75 110.425 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MiniNDP_256.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C3" (at 0.5 -1.025 unlocked) (layer "F.SilkS"))
    (fp_text value "1u" (at -0.7 -1.025 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "VBUS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "000_LOCAL:SOT-363_SC-70-6_symmetric" (layer "F.Cu")
    (at 149.35 107.375 90)
    (descr "SOT-363, SC-70-6")
    (tags "SOT-363 SC-70-6")
    (property "Sheetfile" "MiniNDP_256.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 250mA high-speed switching diodes, dual common cathode, SOT-363")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "DA1" (at 1.8 0 180) (layer "F.SilkS"))
    (fp_text value "BAS70DW-05" (at 2.85 1.15 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 -0.65 90) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "VBUS") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at -0.95 0 90) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "/BATT+") (pinfunction "A") (pintype "passive"))
    (pad "3" smd roundrect (at -0.95 0.65 90) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/RAMRST") (pinfunction "K") (pintype "passive"))
    (pad "4" smd roundrect (at 0.95 0.65 90) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/SLEEP") (pinfunction "A") (pintype "passive"))
    (pad "5" smd roundrect (at 0.95 0 90) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "unconnected-(DA1B-A-Pad5)") (pinfunction "A") (pintype "passive+no_connect"))
    (pad "6" smd roundrect (at 0.95 -0.65 90) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VMEM") (pinfunction "K") (pintype "passive"))
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/SOT-363_SC-70-6.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "000_LOCAL:C_0805" (layer "F.Cu")
    (at 156.525 106.025 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MiniNDP_256.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C2" (at 0.975 0.975 unlocked) (layer "F.SilkS"))
    (fp_text value "1u" (at -0.15 0.975 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VMEM") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "000_LOCAL:R_0805" (layer "F.Cu")
    (at 157.146 110.975 -90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (property "Sheetfile" "MiniNDP_256.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R2" (at -0.649 -1.027 unlocked) (layer "F.SilkS"))
    (fp_text value "1k" (at 0.494 -1.027 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 0.7 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 2 "VMEM") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 0.7 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 71 "Net-(C1-Pad1)") (pintype "passive"))
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "000_LOCAL:SOT-353_SC-70-5" (layer "F.Cu")
    (at 145.35 106.525)
    (descr "SOT-353, SC-70-5")
    (tags "SOT-353 SC-70-5")
    (property "Sheetfile" "MiniNDP_256.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single OR Gate, Low-Voltage CMOS")
    (property "ki_keywords" "Single Gate OR LVC CMOS")
    (attr smd)
    (fp_text reference "U7" (at -0.9 -1.8 unlocked) (layer "F.SilkS"))
    (fp_text value "741G32" (at 0 2 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 -0.65) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/~{BYTE}") (pintype "input"))
    (pad "2" smd roundrect (at -0.95 0) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/SLEEP") (pintype "input"))
    (pad "3" smd roundrect (at -0.95 0.65) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd roundrect (at 0.95 0.65) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/~{CE}") (pintype "output"))
    (pad "5" smd roundrect (at 0.95 -0.65) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VMEM") (pinfunction "VCC") (pintype "power_in"))
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/SOT-353_SC-70-5.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "000_LOCAL:R_0805" (layer "F.Cu")
    (at 152.5 106.825 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (property "Sheetfile" "MiniNDP_256.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R1" (at -1.375 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "240k" (at 0.025 -1.625 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 0.7 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 2 "VMEM") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 0.7 1.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 38 "/SLEEP") (pintype "passive"))
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "000_LOCAL:C_0805" (layer "F.Cu")
    (at 129.25 88.45 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MiniNDP_256.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C5" (at -1.75 0.525 unlocked) (layer "F.SilkS"))
    (fp_text value "1u" (at -1.75 -0.625 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "VBUS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "000_LOCAL:TSSOP-16" (layer "F.Cu")
    (at 152.75 92.025)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "MiniNDP_256.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Synchronous 4-bit programmable binary Counter")
    (property "ki_keywords" "TTL CNT CNT4")
    (attr smd)
    (fp_text reference "U3" (at -1.25 -1 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "74161" (at 1 0 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/~{BLOCK}") (pinfunction "~{MR}") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/~{BYTE}") (pinfunction "CP") (pintype "input"))
    (pad "3" smd roundrect (at -2.8625 -0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "D0") (pintype "input"))
    (pad "4" smd roundrect (at -2.8625 -0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "D1") (pintype "input"))
    (pad "5" smd roundrect (at -2.8625 0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "D2") (pintype "input"))
    (pad "6" smd roundrect (at -2.8625 0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "D3") (pintype "input"))
    (pad "7" smd roundrect (at -2.8625 1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/CARRY1") (pinfunction "CEP") (pintype "input"))
    (pad "8" smd roundrect (at -2.8625 2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" smd roundrect (at 2.8625 2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "VBUS") (pinfunction "~{PE}") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/CARRY1") (pinfunction "CET") (pintype "input"))
    (pad "11" smd roundrect (at 2.8625 0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "unconnected-(U3-Q3-Pad11)") (pinfunction "Q3") (pintype "output+no_connect"))
    (pad "12" smd roundrect (at 2.8625 0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "unconnected-(U3-Q2-Pad12)") (pinfunction "Q2") (pintype "output+no_connect"))
    (pad "13" smd roundrect (at 2.8625 -0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/A8") (pinfunction "Q1") (pintype "output"))
    (pad "14" smd roundrect (at 2.8625 -0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/A9") (pinfunction "Q0") (pintype "output"))
    (pad "15" smd roundrect (at 2.8625 -1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "unconnected-(U3-TC-Pad15)") (pinfunction "TC") (pintype "output+no_connect"))
    (pad "16" smd roundrect (at 2.8625 -2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "VBUS") (pinfunction "VCC") (pintype "power_in"))
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSSOP-16.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "000_LOCAL:Fiducial_0.75_1.5" (layer "F.Cu")
    (at 123.95 114.025)
    (descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
    (tags "fiducial")
    (zone_connect 0)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "F3" (at 0 -2) (layer "F.SilkS") hide)
    (fp_text value "Fiducial_0.75_1.5" (at 0 2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "" smd circle (at 0 0) (size 0.75 0.75) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.375) (clearance 0.375))
  )
  (footprint "000_LOCAL:MountHole_M2.5" (layer "F.Cu")
    (at 124.45 88.525)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, ISO7380")
    (tags "mounting hole 2.7mm no annular m2.5 iso7380")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "M4" (at 0 -3.25) (layer "F.SilkS") hide)
    (fp_text value "MountHole_M2.5" (at 0 3.25) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.6) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (solder_mask_margin -0.1))
  )
  (footprint "000_LOCAL:Keystone_3028_3034" (layer "F.Cu")
    (at 169.7 99.775 90)
    (descr "Keystone 3034 SMD battery holder for 2020, 2025 and 2032 coincell batteries. http://www.keyelco.com/product-pdf.cfm?p=798")
    (tags "Keystone type 3034 coin cell retainer")
    (property "Sheetfile" "MiniNDP_256.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single-cell battery")
    (property "ki_keywords" "battery cell")
    (attr smd)
    (fp_text reference "BT1" (at 8.475 -5.825 45) (layer "F.SilkS"))
    (fp_text value "Keystone_3034" (at 9.575 0 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -2.9 90) (layer "F.Fab"))
    (pad "1" smd oval (at -11.35 0 90) (size 2 6.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "/BATT+") (pinfunction "+") (pintype "passive"))
    (pad "1" smd oval (at 11.35 0 90) (size 2 6.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "/BATT+") (pinfunction "+") (pintype "passive"))
    (pad "2" smd circle (at 0 0 90) (size 18 18) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "-") (pintype "passive"))
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2032_holder_Keystone_3034.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2016_holder_BAT-HLD-002-SMT.STEP" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2012_holder_Keystone_3028.step" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2012_blank.step" hide
      (offset (xyz 0 0 1.2))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 0))
    )
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2016_blank.step" hide
      (offset (xyz 0 0 1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 0))
    )
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2032_blank.step"
      (offset (xyz 0 0 3.2))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 0))
    )
  )
  (footprint "000_LOCAL:TSOP32-dual" (layer "F.Cu")
    (at 145.95 99.825 180)
    (descr "Module CMS TSOP 32 pins")
    (tags "CMS TSOP")
    (property "Sheetfile" "MiniNDP_256.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "256K x 8 Static RAM, TSOP-32")
    (property "ki_keywords" "RAM SRAM CMOS MEMORY")
    (attr smd)
    (fp_text reference "U6" (at -2.95 -2.550001 180 unlocked) (layer "F.SilkS"))
    (fp_text value "AS6C2008A" (at -2.95 0 180 unlocked) (layer "F.SilkS"))
    (fp_text user "AS6C4008" (at -2.95 1.75 180 unlocked) (layer "F.SilkS"))
    (pad "1" smd roundrect (at -9.85 -3.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/A11") (pinfunction "A11") (pintype "input"))
    (pad "2" smd roundrect (at -9.85 -3.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/A9") (pinfunction "A9") (pintype "input"))
    (pad "3" smd roundrect (at -9.85 -2.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/A8") (pinfunction "A8") (pintype "input"))
    (pad "4" smd roundrect (at -9.85 -2.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/A13") (pinfunction "A13") (pintype "input"))
    (pad "5" smd roundrect (at -9.85 -1.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "/~{WR}") (pinfunction "~{WE}") (pintype "input"))
    (pad "6" smd roundrect (at -9.85 -1.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "VBUS") (pinfunction "CE2") (pintype "input"))
    (pad "7" smd roundrect (at -9.85 -0.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/A15") (pinfunction "A15") (pintype "input"))
    (pad "8" smd roundrect (at -9.85 -0.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VMEM") (pinfunction "VCC") (pintype "power_in"))
    (pad "9" smd roundrect (at -9.85 0.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "/A17") (pinfunction "A17") (pintype "input"))
    (pad "10" smd roundrect (at -9.85 0.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "/A16") (pinfunction "A16") (pintype "input"))
    (pad "11" smd roundrect (at -9.85 1.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/A14") (pinfunction "A14") (pintype "input"))
    (pad "12" smd roundrect (at -9.85 1.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/A12") (pinfunction "A12") (pintype "input"))
    (pad "13" smd roundrect (at -9.85 2.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "/A7") (pinfunction "A7") (pintype "input"))
    (pad "14" smd roundrect (at -9.85 2.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/A6") (pinfunction "A6") (pintype "input"))
    (pad "15" smd roundrect (at -9.85 3.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/A5") (pinfunction "A5") (pintype "input"))
    (pad "16" smd roundrect (at -9.85 3.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "/A4") (pinfunction "A4") (pintype "input"))
    (pad "17" smd roundrect (at 3.85 3.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "/A3") (pinfunction "A3") (pintype "input"))
    (pad "17" smd roundrect (at 9.85 3.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "/A3") (pinfunction "A3") (pintype "input"))
    (pad "18" smd roundrect (at 3.85 3.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "/A2") (pinfunction "A2") (pintype "input"))
    (pad "18" smd roundrect (at 9.85 3.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "/A2") (pinfunction "A2") (pintype "input"))
    (pad "19" smd roundrect (at 3.85 2.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "/A1") (pinfunction "A1") (pintype "input"))
    (pad "19" smd roundrect (at 9.85 2.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "/A1") (pinfunction "A1") (pintype "input"))
    (pad "20" smd roundrect (at 3.85 2.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "/A0") (pinfunction "A0") (pintype "input"))
    (pad "20" smd roundrect (at 9.85 2.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "/A0") (pinfunction "A0") (pintype "input"))
    (pad "21" smd roundrect (at 3.85 1.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/AD0") (pinfunction "Q0") (pintype "tri_state"))
    (pad "21" smd roundrect (at 9.85 1.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/AD0") (pinfunction "Q0") (pintype "tri_state"))
    (pad "22" smd roundrect (at 3.85 1.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/AD1") (pinfunction "Q1") (pintype "tri_state"))
    (pad "22" smd roundrect (at 9.85 1.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/AD1") (pinfunction "Q1") (pintype "tri_state"))
    (pad "23" smd roundrect (at 3.85 0.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/AD2") (pinfunction "Q2") (pintype "tri_state"))
    (pad "23" smd roundrect (at 9.85 0.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/AD2") (pinfunction "Q2") (pintype "tri_state"))
    (pad "24" smd roundrect (at 3.85 0.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "24" smd roundrect (at 9.85 0.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "25" smd roundrect (at 3.85 -0.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/AD3") (pinfunction "Q3") (pintype "tri_state"))
    (pad "25" smd roundrect (at 9.85 -0.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/AD3") (pinfunction "Q3") (pintype "tri_state"))
    (pad "26" smd roundrect (at 3.85 -0.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/AD4") (pinfunction "Q4") (pintype "tri_state"))
    (pad "26" smd roundrect (at 9.85 -0.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/AD4") (pinfunction "Q4") (pintype "tri_state"))
    (pad "27" smd roundrect (at 3.85 -1.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/AD5") (pinfunction "Q5") (pintype "tri_state"))
    (pad "27" smd roundrect (at 9.85 -1.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/AD5") (pinfunction "Q5") (pintype "tri_state"))
    (pad "28" smd roundrect (at 3.85 -1.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/AD6") (pinfunction "Q6") (pintype "tri_state"))
    (pad "28" smd roundrect (at 9.85 -1.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/AD6") (pinfunction "Q6") (pintype "tri_state"))
    (pad "29" smd roundrect (at 3.85 -2.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/AD7") (pinfunction "Q7") (pintype "tri_state"))
    (pad "29" smd roundrect (at 9.85 -2.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/AD7") (pinfunction "Q7") (pintype "tri_state"))
    (pad "30" smd roundrect (at 3.85 -2.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/~{CE}") (pinfunction "~{CE}") (pintype "input"))
    (pad "30" smd roundrect (at 9.85 -2.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/~{CE}") (pinfunction "~{CE}") (pintype "input"))
    (pad "31" smd roundrect (at 3.85 -3.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/A10") (pinfunction "A10") (pintype "input"))
    (pad "31" smd roundrect (at 9.85 -3.25 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/A10") (pinfunction "A10") (pintype "input"))
    (pad "32" smd roundrect (at 3.85 -3.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/~{RD}") (pinfunction "~{OE}") (pintype "input"))
    (pad "32" smd roundrect (at 9.85 -3.75 90) (size 0.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/~{RD}") (pinfunction "~{OE}") (pintype "input"))
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSOP32_8x14.step" hide
      (offset (xyz -3 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSOP32_8X20.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "000_LOCAL:TSSOP-16" (layer "F.Cu")
    (at 127.45 94.2575)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "MiniNDP_256.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Synchronous 4-bit programmable binary Counter")
    (property "ki_keywords" "TTL CNT CNT4")
    (attr smd)
    (fp_text reference "U1" (at -1.25 -1 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "74161" (at 1 0 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/~{BLOCK}") (pinfunction "~{MR}") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/~{BYTE}") (pinfunction "CP") (pintype "input"))
    (pad "3" smd roundrect (at -2.8625 -0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "D0") (pintype "input"))
    (pad "4" smd roundrect (at -2.8625 -0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "D1") (pintype "input"))
    (pad "5" smd roundrect (at -2.8625 0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "D2") (pintype "input"))
    (pad "6" smd roundrect (at -2.8625 0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "D3") (pintype "input"))
    (pad "7" smd roundrect (at -2.8625 1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "VBUS") (pinfunction "CEP") (pintype "input"))
    (pad "8" smd roundrect (at -2.8625 2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" smd roundrect (at 2.8625 2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "VBUS") (pinfunction "~{PE}") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "VBUS") (pinfunction "CET") (pintype "input"))
    (pad "11" smd roundrect (at 2.8625 0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "/A0") (pinfunction "Q3") (pintype "output"))
    (pad "12" smd roundrect (at 2.8625 0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "/A1") (pinfunction "Q2") (pintype "output"))
    (pad "13" smd roundrect (at 2.8625 -0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "/A2") (pinfunction "Q1") (pintype "output"))
    (pad "14" smd roundrect (at 2.8625 -0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "/A3") (pinfunction "Q0") (pintype "output"))
    (pad "15" smd roundrect (at 2.8625 -1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/CARRY0") (pinfunction "TC") (pintype "output"))
    (pad "16" smd roundrect (at 2.8625 -2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "VBUS") (pinfunction "VCC") (pintype "power_in"))
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSSOP-16.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "000_LOCAL:C_0805" (layer "F.Cu")
    (at 146.925 89.675 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MiniNDP_256.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C6" (at -0.5 1 unlocked) (layer "F.SilkS"))
    (fp_text value "1u" (at 0.65 1 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "VBUS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "000_LOCAL:C_0805" (layer "F.Cu")
    (at 128.65 107.1)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MiniNDP_256.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C4" (at 1.75 -0.55 unlocked) (layer "F.SilkS"))
    (fp_text value "1u" (at 1.75 0.6 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "VBUS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "000_LOCAL:TSSOP-20" (layer "F.Cu")
    (at 127.45 101.425)
    (descr "TSSOP, 20 Pin (JEDEC MO-153 Var AC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "MiniNDP_256.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "8-bit Register, 3-state outputs")
    (property "ki_keywords" "TTL DFF DFF8 REG 3State")
    (attr smd)
    (fp_text reference "U5" (at -1.25 -1.5 270 unlocked) (layer "F.SilkS"))
    (fp_text value "74374" (at 1 0 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.925) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "OE") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/A11") (pinfunction "O0") (pintype "tri_state"))
    (pad "3" smd roundrect (at -2.8625 -1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/AD0") (pinfunction "D0") (pintype "input"))
    (pad "4" smd roundrect (at -2.8625 -0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/AD1") (pinfunction "D1") (pintype "input"))
    (pad "5" smd roundrect (at -2.8625 -0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/A13") (pinfunction "O1") (pintype "tri_state"))
    (pad "6" smd roundrect (at -2.8625 0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/A12") (pinfunction "O2") (pintype "tri_state"))
    (pad "7" smd roundrect (at -2.8625 0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/AD3") (pinfunction "D2") (pintype "input"))
    (pad "8" smd roundrect (at -2.8625 1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/AD2") (pinfunction "D3") (pintype "input"))
    (pad "9" smd roundrect (at -2.8625 2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/A10") (pinfunction "O3") (pintype "tri_state"))
    (pad "10" smd roundrect (at -2.8625 2.925) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "11" smd roundrect (at 2.8625 2.925) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/~{BLOCK}") (pinfunction "Cp") (pintype "input"))
    (pad "12" smd roundrect (at 2.8625 2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/A14") (pinfunction "O4") (pintype "tri_state"))
    (pad "13" smd roundrect (at 2.8625 1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/AD7") (pinfunction "D4") (pintype "input"))
    (pad "14" smd roundrect (at 2.8625 0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/AD6") (pinfunction "D5") (pintype "input"))
    (pad "15" smd roundrect (at 2.8625 0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "/A17") (pinfunction "O5") (pintype "tri_state"))
    (pad "16" smd roundrect (at 2.8625 -0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/A15") (pinfunction "O6") (pintype "tri_state"))
    (pad "17" smd roundrect (at 2.8625 -0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/AD5") (pinfunction "D6") (pintype "input"))
    (pad "18" smd roundrect (at 2.8625 -1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/AD4") (pinfunction "D7") (pintype "input"))
    (pad "19" smd roundrect (at 2.8625 -2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "/A16") (pinfunction "O7") (pintype "tri_state"))
    (pad "20" smd roundrect (at 2.8625 -2.925) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "VBUS") (pinfunction "VCC") (pintype "power_in"))
    (model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSSOP-20.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "000_LOCAL:IDC-Header_2x20_P2.54mm_Vertical" (layer "B.Cu")
    (at 127.82 113.755 -90)
    (descr "Through hole IDC box header, 2x20, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x20 2.54mm double row")
    (property "Sheetfile" "MiniNDP_256.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at -0.42 2.61 90) (layer "B.SilkS"))
    (fp_text value "Conn_02x20_Odd_Even" (at 1.27 -24.003) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -1.905 -24.13) (layer "B.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1470588235)
      (net 3 "VBUS") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "VBUS") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_3") (pintype "passive") (zone_connect 1) (thermal_bridge_width 0.4) (thermal_gap 0.25))
    (pad "4" thru_hole circle (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive") (zone_connect 1) (thermal_bridge_width 0.4) (thermal_gap 0.25))
    (pad "5" thru_hole circle (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "/AD1") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "/AD0") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "/AD3") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at 2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "/AD2") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "/AD5") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at 2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "/AD4") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole circle (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "/AD7") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole circle (at 2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "/AD6") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole circle (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 46 "/BUS_A9") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole circle (at 2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 45 "/BUS_A8") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole circle (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 54 "unconnected-(J1-Pin_15-Pad15)") (pinfunction "Pin_15") (pintype "passive+no_connect"))
    (pad "16" thru_hole circle (at 2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 55 "unconnected-(J1-Pin_16-Pad16)") (pinfunction "Pin_16") (pintype "passive+no_connect"))
    (pad "17" thru_hole circle (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 56 "unconnected-(J1-Pin_17-Pad17)") (pinfunction "Pin_17") (pintype "passive+no_connect"))
    (pad "18" thru_hole circle (at 2.54 -20.32 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 57 "unconnected-(J1-Pin_18-Pad18)") (pinfunction "Pin_18") (pintype "passive+no_connect"))
    (pad "19" thru_hole circle (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 58 "unconnected-(J1-Pin_19-Pad19)") (pinfunction "Pin_19") (pintype "passive+no_connect"))
    (pad "20" thru_hole circle (at 2.54 -22.86 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 59 "unconnected-(J1-Pin_20-Pad20)") (pinfunction "Pin_20") (pintype "passive+no_connect"))
    (pad "21" thru_hole circle (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_21") (pintype "passive") (zone_connect 1) (thermal_bridge_width 0.4) (thermal_gap 0.25))
    (pad "22" thru_hole circle (at 2.54 -25.4 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_22") (pintype "passive") (zone_connect 1) (thermal_bridge_width 0.4) (thermal_gap 0.25))
    (pad "23" thru_hole circle (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 69 "/~{WR}") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole circle (at 2.54 -27.94 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "/~{RD}") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole circle (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 60 "unconnected-(J1-Pin_25-Pad25)") (pinfunction "Pin_25") (pintype "passive+no_connect"))
    (pad "26" thru_hole circle (at 2.54 -30.48 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 61 "unconnected-(J1-Pin_26-Pad26)") (pinfunction "Pin_26") (pintype "passive+no_connect"))
    (pad "27" thru_hole circle (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 62 "unconnected-(J1-Pin_27-Pad27)") (pinfunction "Pin_27") (pintype "passive+no_connect"))
    (pad "28" thru_hole circle (at 2.54 -33.02 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 63 "unconnected-(J1-Pin_28-Pad28)") (pinfunction "Pin_28") (pintype "passive+no_connect"))
    (pad "29" thru_hole circle (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "/~{Y0}") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole circle (at 2.54 -35.56 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 26 "unconnected-(J1-Pin_30-Pad30)") (pinfunction "Pin_30") (pintype "passive+no_connect"))
    (pad "31" thru_hole circle (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 27 "unconnected-(J1-Pin_31-Pad31)") (pinfunction "Pin_31") (pintype "passive+no_connect"))
    (pad "32" thru_hole circle (at 2.54 -38.1 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "/(A)") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" thru_hole circle (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 64 "unconnected-(J1-Pin_33-Pad33)") (pinfunction "Pin_33") (pintype "passive+no_connect"))
    (pad "34" thru_hole circle (at 2.54 -40.64 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 65 "unconnected-(J1-Pin_34-Pad34)") (pinfunction "Pin_34") (pintype "passive+no_connect"))
    (pad "35" thru_hole circle (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_35") (pintype "passive") (zone_connect 1) (thermal_bridge_width 0.4) (thermal_gap 0.25))
    (pad "36" thru_hole circle (at 2.54 -43.18 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_36") (pintype "passive") (zone_connect 1) (thermal_bridge_width 0.4) (thermal_gap 0.25))
    (pad "37" thru_hole circle (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 28 "unconnected-(J1-Pin_37-Pad37)") (pinfunction "Pin_37") (pintype "passive+no_connect"))
    (pad "38" thru_hole circle (at 2.54 -45.72 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "/RAMRST") (pinfunction "Pin_38") (pintype "passive"))
    (pad "39" thru_hole circle (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 24 "unconnected-(J1-Pin_39-Pad39)") (pinfunction "Pin_39") (pintype "passive+no_connect"))
    (pad "40" thru_hole circle (at 2.54 -48.26 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "unconnected-(J1-Pin_40-Pad40)") (pinfunction "Pin_40") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x20_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 180.95 86.025) (mid 181.657107 86.317893) (end 181.95 87.025)
    (layer "Edge.Cuts"))
  (gr_line (start 122.95 86.025) (end 180.95 86.025)
    (layer "Edge.Cuts"))
  (gr_arc (start 121.95 87.025) (mid 122.242893 86.317893) (end 122.95 86.025)
    (layer "Edge.Cuts"))
  (gr_line (start 180.95 120.025) (end 122.95 120.025)
    (layer "Edge.Cuts"))
  (gr_arc (start 181.95 119.025) (mid 181.657107 119.732107) (end 180.95 120.025)
    (layer "Edge.Cuts"))
  (gr_line (start 181.95 87.025) (end 181.95 119.025)
    (layer "Edge.Cuts"))
  (gr_arc (start 122.95 120.025) (mid 122.242893 119.732107) (end 121.95 119.025)
    (layer "Edge.Cuts"))
  (gr_line (start 121.95 119.025) (end 121.95 87.025)
    (layer "Edge.Cuts"))
  (gr_text "MiniNDP 256" (at 151.95 99.15) (layer "B.SilkS"))
  (gr_text "${COMMENT1} - ${REVISION}" (at 151.95 102.96) (layer "B.SilkS"))
  (zone (net 40) (net_name "/A6") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30061)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.95 92.05)
        (xy 142.897653 92.043522)
        (xy 142.845307 92.031044)
        (xy 142.79296 92.012567)
        (xy 142.740614 91.988089)
        (xy 142.688268 91.957612)
        (xy 142.0115 92.15)
        (xy 142.688268 92.342388)
        (xy 142.740614 92.31191)
        (xy 142.79296 92.287432)
        (xy 142.845307 92.268955)
        (xy 142.897653 92.256477)
        (xy 142.95 92.25)
      )
    )
  )
  (zone (net 12) (net_name "/A8") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30178)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 156.4 102.475)
        (xy 156.36074 102.472141)
        (xy 156.32148 102.466283)
        (xy 156.28222 102.457425)
        (xy 156.24296 102.445567)
        (xy 156.203701 102.430709)
        (xy 155.799 102.575)
        (xy 156.203701 102.719291)
        (xy 156.24296 102.704432)
        (xy 156.28222 102.692574)
        (xy 156.32148 102.683716)
        (xy 156.36074 102.677858)
        (xy 156.4 102.675)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30009)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.525 111.875)
        (xy 132.778303 111.851)
        (xy 133.031606 111.839)
        (xy 133.284909 111.839)
        (xy 133.538212 111.851)
        (xy 133.791516 111.875)
        (xy 133.751 111.375)
        (xy 133.078232 110.97814)
        (xy 132.967585 111.061511)
        (xy 132.856939 111.132883)
        (xy 132.746292 111.192256)
        (xy 132.635646 111.239628)
        (xy 132.525 111.275)
      )
    )
  )
  (zone (net 5) (net_name "/AD1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30146)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.5 98.675)
        (xy 135.539259 98.677858)
        (xy 135.578519 98.683716)
        (xy 135.617779 98.692574)
        (xy 135.657039 98.704432)
        (xy 135.696299 98.719291)
        (xy 136.101 98.575)
        (xy 135.696299 98.430709)
        (xy 135.657039 98.445567)
        (xy 135.617779 98.457425)
        (xy 135.578519 98.466283)
        (xy 135.539259 98.472141)
        (xy 135.5 98.475)
      )
    )
  )
  (zone (net 10) (net_name "/AD6") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30043)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.25 102.3)
        (xy 131.197653 102.293522)
        (xy 131.145307 102.281044)
        (xy 131.09296 102.262567)
        (xy 131.040614 102.238089)
        (xy 130.988268 102.207612)
        (xy 130.3115 102.4)
        (xy 130.988268 102.592388)
        (xy 131.040614 102.56191)
        (xy 131.09296 102.537432)
        (xy 131.145307 102.518955)
        (xy 131.197653 102.506477)
        (xy 131.25 102.5)
      )
    )
  )
  (zone (net 4) (net_name "/AD0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30152)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.5 98.175)
        (xy 135.539259 98.177858)
        (xy 135.578519 98.183716)
        (xy 135.617779 98.192574)
        (xy 135.657039 98.204432)
        (xy 135.696299 98.219291)
        (xy 136.101 98.075)
        (xy 135.696299 97.930709)
        (xy 135.657039 97.945567)
        (xy 135.617779 97.957425)
        (xy 135.578519 97.966283)
        (xy 135.539259 97.972141)
        (xy 135.5 97.975)
      )
    )
  )
  (zone (net 46) (net_name "/BUS_A9") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30093)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.65 110.275)
        (xy 142.754804 110.280813)
        (xy 142.827582 110.29768)
        (xy 142.888392 110.324737)
        (xy 142.957288 110.361121)
        (xy 143.054329 110.40597)
        (xy 143.151 110.175)
        (xy 143.054329 109.94403)
        (xy 142.957288 109.988878)
        (xy 142.888392 110.025262)
        (xy 142.827582 110.052319)
        (xy 142.754804 110.069186)
        (xy 142.65 110.075)
      )
    )
  )
  (zone (net 41) (net_name "/CARRY1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30060)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 150.825 93.55)
        (xy 150.772653 93.543522)
        (xy 150.720307 93.531044)
        (xy 150.66796 93.512567)
        (xy 150.615614 93.488089)
        (xy 150.563268 93.457612)
        (xy 149.8865 93.65)
        (xy 150.563268 93.842388)
        (xy 150.615614 93.81191)
        (xy 150.66796 93.787432)
        (xy 150.720307 93.768955)
        (xy 150.772653 93.756477)
        (xy 150.825 93.75)
      )
    )
  )
  (zone (net 4) (net_name "/AD0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30186)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 136.7 97.975001)
        (xy 136.66074 97.972142)
        (xy 136.62148 97.966284)
        (xy 136.58222 97.957425)
        (xy 136.54296 97.945567)
        (xy 136.503701 97.930709)
        (xy 136.099001 98.075)
        (xy 136.503701 98.219291)
        (xy 136.54296 98.204432)
        (xy 136.58222 98.192574)
        (xy 136.621479 98.183716)
        (xy 136.660739 98.177858)
        (xy 136.699999 98.175)
      )
    )
  )
  (zone (net 7) (net_name "/AD3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30133)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 136.7 100.025)
        (xy 136.667475 100.01819)
        (xy 136.63495 100.00838)
        (xy 136.602426 99.995571)
        (xy 136.569901 99.979761)
        (xy 136.537377 99.960952)
        (xy 136.099 100.075)
        (xy 136.092766 100.225)
        (xy 136.214212 100.219)
        (xy 136.335659 100.216)
        (xy 136.457106 100.216)
        (xy 136.578553 100.219)
        (xy 136.7 100.225)
      )
    )
  )
  (zone (net 21) (net_name "/RAMRST") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30007)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 172.267208 115.163629)
        (xy 172.498234 115.455544)
        (xy 172.588769 115.706624)
        (xy 172.61254 115.957412)
        (xy 172.643275 116.24845)
        (xy 172.754702 116.620281)
        (xy 173.540707 116.295707)
        (xy 173.865281 115.509702)
        (xy 173.49345 115.398275)
        (xy 173.202412 115.36754)
        (xy 172.951624 115.343769)
        (xy 172.700544 115.253234)
        (xy 172.408629 115.022208)
      )
    )
  )
  (zone (net 44) (net_name "/BATT+") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30022)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 161.15 108.175)
        (xy 161.274358 108.1802)
        (xy 161.362179 108.1926)
        (xy 161.43782 108.2074)
        (xy 161.52564 108.2198)
        (xy 161.65 108.225)
        (xy 161.651 107.975)
        (xy 161.65 107.725)
        (xy 161.52564 107.7302)
        (xy 161.43782 107.7426)
        (xy 161.362179 107.7574)
        (xy 161.274358 107.7698)
        (xy 161.15 107.775)
      )
    )
  )
  (zone (net 38) (net_name "/SLEEP") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30124)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 150.1 106.95)
        (xy 150.118477 106.885653)
        (xy 150.136955 106.827307)
        (xy 150.155432 106.77496)
        (xy 150.17391 106.728614)
        (xy 150.192388 106.688268)
        (xy 150 106.424)
        (xy 149.807612 106.688268)
        (xy 149.826089 106.728614)
        (xy 149.844567 106.77496)
        (xy 149.863044 106.827307)
        (xy 149.881522 106.885653)
        (xy 149.9 106.95)
      )
    )
  )
  (zone (net 44) (net_name "/BATT+") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30001)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 165.4 111.425)
        (xy 165.723463 111.465776)
        (xy 166.046926 111.548552)
        (xy 166.37039 111.673328)
        (xy 166.693853 111.840104)
        (xy 167.017317 112.04888)
        (xy 169.701 111.125)
        (xy 167.017317 110.20112)
        (xy 166.693853 110.409896)
        (xy 166.37039 110.576672)
        (xy 166.046926 110.701448)
        (xy 165.723463 110.784224)
        (xy 165.4 110.825)
      )
    )
  )
  (zone (net 30) (net_name "/~{BYTE}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30117)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 143.875 105.875)
        (xy 143.917254 105.891749)
        (xy 143.959509 105.914499)
        (xy 144.001763 105.943248)
        (xy 144.044018 105.977998)
        (xy 144.086273 106.018748)
        (xy 144.401 105.875)
        (xy 144.419843 105.675)
        (xy 144.310874 105.687)
        (xy 144.201905 105.693)
        (xy 144.092937 105.693)
        (xy 143.983968 105.687)
        (xy 143.875 105.675)
      )
    )
  )
  (zone (net 20) (net_name "/~{RD}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30184)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.5 103.674999)
        (xy 141.539259 103.677857)
        (xy 141.578519 103.683715)
        (xy 141.617779 103.692574)
        (xy 141.657039 103.704432)
        (xy 141.696299 103.719291)
        (xy 142.100999 103.575)
        (xy 141.696299 103.430709)
        (xy 141.657039 103.445567)
        (xy 141.617779 103.457425)
        (xy 141.57852 103.466283)
        (xy 141.53926 103.472141)
        (xy 141.500001 103.475)
      )
    )
  )
  (zone (net 8) (net_name "/AD4") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30047)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.25 99.7)
        (xy 131.197653 99.693522)
        (xy 131.145307 99.681044)
        (xy 131.09296 99.662567)
        (xy 131.040614 99.638089)
        (xy 130.988268 99.607612)
        (xy 130.3115 99.8)
        (xy 130.988268 99.992388)
        (xy 131.040614 99.96191)
        (xy 131.09296 99.937432)
        (xy 131.145307 99.918955)
        (xy 131.197653 99.906477)
        (xy 131.25 99.9)
      )
    )
  )
  (zone (net 11) (net_name "/AD7") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30108)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.02 101.975)
        (xy 140.915195 101.969186)
        (xy 140.842416 101.952319)
        (xy 140.781607 101.925262)
        (xy 140.71271 101.888878)
        (xy 140.615671 101.84403)
        (xy 140.519 102.075)
        (xy 140.615671 102.30597)
        (xy 140.71271 102.261121)
        (xy 140.781607 102.224737)
        (xy 140.842416 102.19768)
        (xy 140.915195 102.180813)
        (xy 141.02 102.175)
      )
    )
  )
  (zone (net 4) (net_name "/AD0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30120)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.944669 97.075)
        (xy 131.861331 97.063328)
        (xy 131.810295 97.030913)
        (xy 131.77414 96.981656)
        (xy 131.735441 96.919459)
        (xy 131.676777 96.848223)
        (xy 131.499 97.025)
        (xy 131.5 97.275)
        (xy 131.610277 97.275)
        (xy 131.688539 97.275)
        (xy 131.756128 97.275)
        (xy 131.83439 97.275)
        (xy 131.944669 97.275)
      )
    )
  )
  (zone (net 10) (net_name "/AD6") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30147)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.5 101.675)
        (xy 135.539259 101.677858)
        (xy 135.578519 101.683716)
        (xy 135.617779 101.692574)
        (xy 135.657039 101.704432)
        (xy 135.696299 101.719291)
        (xy 136.101 101.575)
        (xy 135.696299 101.430709)
        (xy 135.657039 101.445567)
        (xy 135.617779 101.457425)
        (xy 135.578519 101.466283)
        (xy 135.539259 101.472141)
        (xy 135.5 101.475)
      )
    )
  )
  (zone (net 5) (net_name "/AD1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30067)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 125.525 100.35)
        (xy 125.472653 100.343522)
        (xy 125.420307 100.331044)
        (xy 125.36796 100.312567)
        (xy 125.315614 100.288089)
        (xy 125.263268 100.257612)
        (xy 124.5865 100.45)
        (xy 125.263268 100.642388)
        (xy 125.315614 100.61191)
        (xy 125.36796 100.587432)
        (xy 125.420307 100.568955)
        (xy 125.472653 100.556477)
        (xy 125.525 100.55)
      )
    )
  )
  (zone (net 16) (net_name "/A12") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30019)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 125.525 101.55)
        (xy 125.335175 101.562)
        (xy 125.14535 101.568)
        (xy 124.955526 101.568)
        (xy 124.765701 101.562)
        (xy 124.575877 101.55)
        (xy 124.5865 101.75)
        (xy 125.320439 101.872928)
        (xy 125.361351 101.836342)
        (xy 125.402263 101.805756)
        (xy 125.443175 101.781171)
        (xy 125.484087 101.762585)
        (xy 125.525 101.75)
      )
    )
  )
  (zone (net 14) (net_name "/A10") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30167)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.5 103.175)
        (xy 141.539259 103.177858)
        (xy 141.578519 103.183716)
        (xy 141.617779 103.192574)
        (xy 141.657039 103.204432)
        (xy 141.696299 103.219291)
        (xy 142.101 103.075)
        (xy 141.696299 102.930709)
        (xy 141.657039 102.945567)
        (xy 141.617779 102.957425)
        (xy 141.578519 102.966283)
        (xy 141.539259 102.972141)
        (xy 141.5 102.975)
      )
    )
  )
  (zone (net 18) (net_name "/A14") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30145)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 155.2 98.675)
        (xy 155.239259 98.677858)
        (xy 155.278519 98.683716)
        (xy 155.317779 98.692574)
        (xy 155.357039 98.704432)
        (xy 155.396299 98.719291)
        (xy 155.801 98.575)
        (xy 155.396299 98.430709)
        (xy 155.357039 98.445567)
        (xy 155.317779 98.457425)
        (xy 155.278519 98.466283)
        (xy 155.239259 98.472141)
        (xy 155.2 98.475)
      )
    )
  )
  (zone (net 29) (net_name "/~{BLOCK}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30122)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.694669 108.525)
        (xy 132.58439 108.525)
        (xy 132.506128 108.525)
        (xy 132.438539 108.525)
        (xy 132.360277 108.525)
        (xy 132.25 108.525)
        (xy 132.249 108.775)
        (xy 132.426777 108.951777)
        (xy 132.485441 108.88054)
        (xy 132.52414 108.818342)
        (xy 132.560295 108.769086)
        (xy 132.611331 108.736671)
        (xy 132.694669 108.725)
      )
    )
  )
  (zone (net 9) (net_name "/AD5") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30128)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.5 101.225)
        (xy 141.621446 101.219)
        (xy 141.742893 101.216)
        (xy 141.86434 101.216)
        (xy 141.985787 101.219)
        (xy 142.107234 101.225)
        (xy 142.101 101.075)
        (xy 141.662622 100.960952)
        (xy 141.630097 100.979761)
        (xy 141.597573 100.995571)
        (xy 141.565048 101.00838)
        (xy 141.532524 101.01819)
        (xy 141.5 101.025)
      )
    )
  )
  (zone (net 6) (net_name "/AD2") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30137)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.5 99.125)
        (xy 141.532524 99.131809)
        (xy 141.565048 99.141618)
        (xy 141.597573 99.154428)
        (xy 141.630097 99.170237)
        (xy 141.662622 99.189047)
        (xy 142.101 99.075)
        (xy 142.107234 98.925)
        (xy 141.985787 98.931)
        (xy 141.86434 98.934)
        (xy 141.742893 98.934)
        (xy 141.621446 98.931)
        (xy 141.5 98.925)
      )
    )
  )
  (zone (net 16) (net_name "/A12") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30096)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 126.167157 101.299264)
        (xy 126.245376 101.229266)
        (xy 126.308764 101.18973)
        (xy 126.370895 101.165864)
        (xy 126.445339 101.142874)
        (xy 126.545671 101.10597)
        (xy 126.450707 100.874293)
        (xy 126.21903 100.779329)
        (xy 126.182124 100.879659)
        (xy 126.159135 100.954104)
        (xy 126.135268 101.016234)
        (xy 126.095732 101.079623)
        (xy 126.025736 101.157843)
      )
    )
  )
  (zone (net 13) (net_name "/A9") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30176)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 156.4 102.975)
        (xy 156.36074 102.972141)
        (xy 156.32148 102.966283)
        (xy 156.28222 102.957425)
        (xy 156.24296 102.945567)
        (xy 156.203701 102.930709)
        (xy 155.799 103.075)
        (xy 156.203701 103.219291)
        (xy 156.24296 103.204432)
        (xy 156.28222 103.192574)
        (xy 156.32148 103.183716)
        (xy 156.36074 103.177858)
        (xy 156.4 103.175)
      )
    )
  )
  (zone (net 5) (net_name "/AD1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30166)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.5 98.675)
        (xy 141.539259 98.677858)
        (xy 141.578519 98.683716)
        (xy 141.617779 98.692574)
        (xy 141.657039 98.704432)
        (xy 141.696299 98.719291)
        (xy 142.101 98.575)
        (xy 141.696299 98.430709)
        (xy 141.657039 98.445567)
        (xy 141.617779 98.457425)
        (xy 141.578519 98.466283)
        (xy 141.539259 98.472141)
        (xy 141.5 98.475)
      )
    )
  )
  (zone (net 17) (net_name "/A13") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30075)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 123.728033 101.288388)
        (xy 123.772426 101.27871)
        (xy 123.816819 101.275032)
        (xy 123.861213 101.277355)
        (xy 123.905606 101.285677)
        (xy 123.95 101.3)
        (xy 124.588207 101.099293)
        (xy 123.851721 100.991344)
        (xy 123.798699 101.034468)
        (xy 123.745677 101.071593)
        (xy 123.692655 101.102717)
        (xy 123.639633 101.127842)
        (xy 123.586612 101.146967)
      )
    )
  )
  (zone (net 29) (net_name "/~{BLOCK}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30039)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 137.225 89.45)
        (xy 137.172653 89.443522)
        (xy 137.120307 89.431044)
        (xy 137.06796 89.412567)
        (xy 137.015614 89.388089)
        (xy 136.963268 89.357612)
        (xy 136.2865 89.55)
        (xy 136.963268 89.742388)
        (xy 137.015614 89.71191)
        (xy 137.06796 89.687432)
        (xy 137.120307 89.668955)
        (xy 137.172653 89.656477)
        (xy 137.225 89.65)
      )
    )
  )
  (zone (net 47) (net_name "/A16") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30083)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 146.580896 98.014475)
        (xy 146.518089 97.928403)
        (xy 146.502133 97.852509)
        (xy 146.507587 97.776135)
        (xy 146.509012 97.688627)
        (xy 146.48097 97.579329)
        (xy 146.249293 97.674293)
        (xy 146.073223 97.851777)
        (xy 146.159786 97.931878)
        (xy 146.22638 97.983063)
        (xy 146.286317 98.024609)
        (xy 146.352911 98.075794)
        (xy 146.439475 98.155896)
      )
    )
  )
  (zone (net 71) (net_name "Net-(C1-Pad1)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30014)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 156.146 112.025)
        (xy 156.216 112.044369)
        (xy 156.286 112.066738)
        (xy 156.355999 112.092108)
        (xy 156.425999 112.120477)
        (xy 156.496 112.151847)
        (xy 157.147 111.925)
        (xy 157.181625 111.575)
        (xy 156.9745 111.551)
        (xy 156.767375 111.524)
        (xy 156.560249 111.494)
        (xy 156.353124 111.461)
        (xy 156.146 111.425)
      )
    )
  )
  (zone (net 52) (net_name "/A3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30188)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 136.699999 95.975001)
        (xy 136.660739 95.972142)
        (xy 136.621479 95.966284)
        (xy 136.58222 95.957425)
        (xy 136.54296 95.945567)
        (xy 136.503701 95.930709)
        (xy 136.099001 96.075)
        (xy 136.503701 96.219291)
        (xy 136.54296 96.204432)
        (xy 136.58222 96.192574)
        (xy 136.62148 96.183716)
        (xy 136.66074 96.177858)
        (xy 136.7 96.175)
      )
    )
  )
  (zone (net 45) (net_name "/BUS_A8") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30112)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 143.839946 110.925)
        (xy 143.940408 110.926025)
        (xy 144.012169 110.931314)
        (xy 144.073137 110.944188)
        (xy 144.141221 110.967966)
        (xy 144.234329 111.00597)
        (xy 144.331 110.775)
        (xy 144.234329 110.54403)
        (xy 144.13717 110.594733)
        (xy 144.071397 110.643599)
        (xy 144.014767 110.68521)
        (xy 143.945031 110.714149)
        (xy 143.839946 110.725)
      )
    )
  )
  (zone (net 9) (net_name "/AD5") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30091)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 137.48 101.175)
        (xy 137.584804 101.180813)
        (xy 137.657582 101.19768)
        (xy 137.718392 101.224737)
        (xy 137.787288 101.261121)
        (xy 137.884329 101.30597)
        (xy 137.981 101.075)
        (xy 137.884329 100.84403)
        (xy 137.787288 100.888878)
        (xy 137.718392 100.925262)
        (xy 137.657582 100.952319)
        (xy 137.584804 100.969186)
        (xy 137.48 100.975)
      )
    )
  )
  (zone (net 38) (net_name "/SLEEP") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30141)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 144.925 106.425)
        (xy 144.872653 106.418522)
        (xy 144.820307 106.406044)
        (xy 144.76796 106.387567)
        (xy 144.715614 106.363089)
        (xy 144.663268 106.332612)
        (xy 144.399 106.525)
        (xy 144.663268 106.717388)
        (xy 144.715614 106.68691)
        (xy 144.76796 106.662432)
        (xy 144.820307 106.643955)
        (xy 144.872653 106.631477)
        (xy 144.925 106.625)
      )
    )
  )
  (zone (net 30) (net_name "/~{BYTE}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30065)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 137.225 90.1)
        (xy 137.172653 90.093522)
        (xy 137.120307 90.081044)
        (xy 137.06796 90.062567)
        (xy 137.015614 90.038089)
        (xy 136.963268 90.007612)
        (xy 136.2865 90.2)
        (xy 136.963268 90.392388)
        (xy 137.015614 90.36191)
        (xy 137.06796 90.337432)
        (xy 137.120307 90.318955)
        (xy 137.172653 90.306477)
        (xy 137.225 90.3)
      )
    )
  )
  (zone (net 2) (net_name "VMEM") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30074)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 156.459946 100.225)
        (xy 156.581845 100.2302)
        (xy 156.667912 100.2426)
        (xy 156.742033 100.2574)
        (xy 156.8281 100.2698)
        (xy 156.95 100.275)
        (xy 156.951 100.025)
        (xy 156.854329 99.79403)
        (xy 156.759545 99.838184)
        (xy 156.692417 99.874481)
        (xy 156.633243 99.901798)
        (xy 156.56232 99.919012)
        (xy 156.459946 99.925)
      )
    )
  )
  (zone (net 6) (net_name "/AD2") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30071)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 125.525 102.95)
        (xy 125.472653 102.943522)
        (xy 125.420307 102.931044)
        (xy 125.36796 102.912567)
        (xy 125.315614 102.888089)
        (xy 125.263268 102.857612)
        (xy 124.5865 103.05)
        (xy 125.263268 103.242388)
        (xy 125.315614 103.21191)
        (xy 125.36796 103.187432)
        (xy 125.420307 103.168955)
        (xy 125.472653 103.156477)
        (xy 125.525 103.15)
      )
    )
  )
  (zone (net 23) (net_name "/(A)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30038)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.95 107.475)
        (xy 142.897653 107.468522)
        (xy 142.845307 107.456044)
        (xy 142.79296 107.437567)
        (xy 142.740614 107.413089)
        (xy 142.688268 107.382612)
        (xy 142.0115 107.575)
        (xy 142.688268 107.767388)
        (xy 142.740614 107.73691)
        (xy 142.79296 107.712432)
        (xy 142.845307 107.693955)
        (xy 142.897653 107.681477)
        (xy 142.95 107.675)
      )
    )
  )
  (zone (net 50) (net_name "/A1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30052)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.25 94.4825)
        (xy 131.197653 94.476022)
        (xy 131.145307 94.463544)
        (xy 131.09296 94.445067)
        (xy 131.040614 94.420589)
        (xy 130.988268 94.390112)
        (xy 130.3115 94.5825)
        (xy 130.988268 94.774888)
        (xy 131.040614 94.74441)
        (xy 131.09296 94.719932)
        (xy 131.145307 94.701455)
        (xy 131.197653 94.688977)
        (xy 131.25 94.6825)
      )
    )
  )
  (zone (net 29) (net_name "/~{BLOCK}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30072)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.35 89.675)
        (xy 135.402346 89.676477)
        (xy 135.454692 89.683955)
        (xy 135.507039 89.697432)
        (xy 135.559385 89.71691)
        (xy 135.611732 89.742388)
        (xy 136.2885 89.55)
        (xy 135.595606 89.368386)
        (xy 135.546484 89.401708)
        (xy 135.497363 89.429031)
        (xy 135.448242 89.450354)
        (xy 135.399121 89.465677)
        (xy 135.35 89.475)
      )
    )
  )
  (zone (net 10) (net_name "/AD6") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30089)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.433 101.674999)
        (xy 142.537804 101.680812)
        (xy 142.610582 101.697679)
        (xy 142.671392 101.724736)
        (xy 142.740288 101.76112)
        (xy 142.837329 101.805969)
        (xy 142.934 101.574999)
        (xy 142.837329 101.344029)
        (xy 142.740288 101.388877)
        (xy 142.671392 101.425261)
        (xy 142.610582 101.452318)
        (xy 142.537804 101.469185)
        (xy 142.433 101.474999)
      )
    )
  )
  (zone (net 29) (net_name "/~{BLOCK}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30044)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.25 104.25)
        (xy 131.197653 104.243522)
        (xy 131.145307 104.231044)
        (xy 131.09296 104.212567)
        (xy 131.040614 104.188089)
        (xy 130.988268 104.157612)
        (xy 130.3115 104.35)
        (xy 130.988268 104.542388)
        (xy 131.040614 104.51191)
        (xy 131.09296 104.487432)
        (xy 131.145307 104.468955)
        (xy 131.197653 104.456477)
        (xy 131.25 104.45)
      )
    )
  )
  (zone (net 42) (net_name "/~{CE}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30113)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 145.809946 102.675)
        (xy 145.910408 102.676025)
        (xy 145.982169 102.681314)
        (xy 146.043137 102.694188)
        (xy 146.111221 102.717966)
        (xy 146.204329 102.75597)
        (xy 146.301 102.525)
        (xy 146.204329 102.29403)
        (xy 146.10717 102.344733)
        (xy 146.041397 102.393599)
        (xy 145.984767 102.43521)
        (xy 145.915031 102.464149)
        (xy 145.809946 102.475)
      )
    )
  )
  (zone (net 7) (net_name "/AD3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30092)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 134.8 100.175)
        (xy 134.904804 100.180813)
        (xy 134.977582 100.19768)
        (xy 135.038392 100.224737)
        (xy 135.107288 100.261121)
        (xy 135.204329 100.30597)
        (xy 135.301 100.075)
        (xy 135.204329 99.84403)
        (xy 135.107288 99.888878)
        (xy 135.038392 99.925262)
        (xy 134.977582 99.952319)
        (xy 134.904804 99.969186)
        (xy 134.8 99.975)
      )
    )
  )
  (zone (net 2) (net_name "VMEM") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30008)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 155.3 107.475)
        (xy 155.553303 107.451)
        (xy 155.806606 107.439)
        (xy 156.059909 107.439)
        (xy 156.313212 107.451)
        (xy 156.566516 107.475)
        (xy 156.526 106.975)
        (xy 155.853232 106.57814)
        (xy 155.742585 106.661511)
        (xy 155.631939 106.732883)
        (xy 155.521292 106.792256)
        (xy 155.410646 106.839628)
        (xy 155.3 106.875)
      )
    )
  )
  (zone (net 19) (net_name "/A15") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30046)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.25 101)
        (xy 131.197653 100.993522)
        (xy 131.145307 100.981044)
        (xy 131.09296 100.962567)
        (xy 131.040614 100.938089)
        (xy 130.988268 100.907612)
        (xy 130.3115 101.1)
        (xy 130.988268 101.292388)
        (xy 131.040614 101.26191)
        (xy 131.09296 101.237432)
        (xy 131.145307 101.218955)
        (xy 131.197653 101.206477)
        (xy 131.25 101.2)
      )
    )
  )
  (zone (net 16) (net_name "/A12") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30170)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 155.2 98.175)
        (xy 155.239259 98.177858)
        (xy 155.278519 98.183716)
        (xy 155.317779 98.192574)
        (xy 155.357039 98.204432)
        (xy 155.396299 98.219291)
        (xy 155.801 98.075)
        (xy 155.396299 97.930709)
        (xy 155.357039 97.945567)
        (xy 155.317779 97.957425)
        (xy 155.278519 97.966283)
        (xy 155.239259 97.972141)
        (xy 155.2 97.975)
      )
    )
  )
  (zone (net 11) (net_name "/AD7") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30179)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 136.7 101.975)
        (xy 136.66074 101.972141)
        (xy 136.62148 101.966283)
        (xy 136.58222 101.957425)
        (xy 136.54296 101.945567)
        (xy 136.503701 101.930709)
        (xy 136.099 102.075)
        (xy 136.503701 102.219291)
        (xy 136.54296 102.204432)
        (xy 136.58222 102.192574)
        (xy 136.62148 102.183716)
        (xy 136.66074 102.177858)
        (xy 136.7 102.175)
      )
    )
  )
  (zone (net 6) (net_name "/AD2") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30084)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.546448 98.975)
        (xy 135.420508 98.978078)
        (xy 135.331217 98.988997)
        (xy 135.255684 99.010279)
        (xy 135.171017 99.044449)
        (xy 135.054329 99.09403)
        (xy 135.149 99.325)
        (xy 135.326777 99.501777)
        (xy 135.384179 99.414334)
        (xy 135.40754 99.326611)
        (xy 135.424166 99.249932)
        (xy 135.461366 99.19562)
        (xy 135.546448 99.175)
      )
    )
  )
  (zone (net 31) (net_name "/CARRY0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30027)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.075 93.55)
        (xy 141.127346 93.556477)
        (xy 141.179692 93.568955)
        (xy 141.232039 93.587432)
        (xy 141.284385 93.61191)
        (xy 141.336732 93.642388)
        (xy 142.0135 93.45)
        (xy 141.336732 93.257612)
        (xy 141.284385 93.288089)
        (xy 141.232039 93.312567)
        (xy 141.179692 93.331044)
        (xy 141.127346 93.343522)
        (xy 141.075 93.35)
      )
    )
  )
  (zone (net 20) (net_name "/~{RD}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30187)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 136.7 103.475)
        (xy 136.66074 103.472141)
        (xy 136.62148 103.466283)
        (xy 136.58222 103.457425)
        (xy 136.54296 103.445567)
        (xy 136.503701 103.430709)
        (xy 136.099001 103.575)
        (xy 136.503701 103.719291)
        (xy 136.54296 103.704432)
        (xy 136.58222 103.692574)
        (xy 136.621479 103.683715)
        (xy 136.660739 103.677857)
        (xy 136.699999 103.674999)
      )
    )
  )
  (zone (net 31) (net_name "/CARRY0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30028)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.35 93.55)
        (xy 135.402346 93.556477)
        (xy 135.454692 93.568955)
        (xy 135.507039 93.587432)
        (xy 135.559385 93.61191)
        (xy 135.611732 93.642388)
        (xy 136.2885 93.45)
        (xy 135.611732 93.257612)
        (xy 135.559385 93.288089)
        (xy 135.507039 93.312567)
        (xy 135.454692 93.331044)
        (xy 135.402346 93.343522)
        (xy 135.35 93.35)
      )
    )
  )
  (zone (net 10) (net_name "/AD6") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30130)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 136.7 101.525)
        (xy 136.667475 101.51819)
        (xy 136.63495 101.50838)
        (xy 136.602426 101.495571)
        (xy 136.569901 101.479761)
        (xy 136.537377 101.460952)
        (xy 136.099 101.575)
        (xy 136.092766 101.725)
        (xy 136.214212 101.719)
        (xy 136.335659 101.716)
        (xy 136.457106 101.716)
        (xy 136.578553 101.719)
        (xy 136.7 101.725)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30035)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 129.375 95.9825)
        (xy 129.427346 95.988977)
        (xy 129.479692 96.001455)
        (xy 129.532039 96.019932)
        (xy 129.584385 96.04441)
        (xy 129.636732 96.074888)
        (xy 130.3135 95.8825)
        (xy 129.636732 95.690112)
        (xy 129.584385 95.720589)
        (xy 129.532039 95.745067)
        (xy 129.479692 95.763544)
        (xy 129.427346 95.776022)
        (xy 129.375 95.7825)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30013)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.2 88.425)
        (xy 131.099999 88.377822)
        (xy 130.999999 88.318644)
        (xy 130.9 88.247467)
        (xy 130.8 88.164289)
        (xy 130.7 88.069112)
        (xy 130.199 88.45)
        (xy 130.635657 89.088486)
        (xy 130.748525 89.051788)
        (xy 130.861394 89.027091)
        (xy 130.974262 89.014394)
        (xy 131.087131 89.013697)
        (xy 131.2 89.025)
      )
    )
  )
  (zone (net 10) (net_name "/AD6") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30136)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.5 101.625)
        (xy 141.532524 101.631809)
        (xy 141.565048 101.641618)
        (xy 141.597573 101.654428)
        (xy 141.630097 101.670237)
        (xy 141.662622 101.689047)
        (xy 142.101 101.575)
        (xy 142.107234 101.425)
        (xy 141.985787 101.431)
        (xy 141.86434 101.434)
        (xy 141.742893 101.434)
        (xy 141.621446 101.431)
        (xy 141.5 101.425)
      )
    )
  )
  (zone (net 7) (net_name "/AD3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30143)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.5 100.175)
        (xy 135.539259 100.177858)
        (xy 135.578519 100.183716)
        (xy 135.617779 100.192574)
        (xy 135.657039 100.204432)
        (xy 135.696299 100.219291)
        (xy 136.101 100.075)
        (xy 135.696299 99.930709)
        (xy 135.657039 99.945567)
        (xy 135.617779 99.957425)
        (xy 135.578519 99.966283)
        (xy 135.539259 99.972141)
        (xy 135.5 99.975)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30189)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 130.2125 96.1325)
        (xy 130.1925 96.1845)
        (xy 130.1725 96.2305)
        (xy 130.152499 96.270499)
        (xy 130.132499 96.304499)
        (xy 130.1125 96.3325)
        (xy 130.3125 96.5335)
        (xy 130.5125 96.3325)
        (xy 130.4925 96.304499)
        (xy 130.4725 96.270499)
        (xy 130.452499 96.2305)
        (xy 130.432499 96.1845)
        (xy 130.4125 96.1325)
      )
    )
  )
  (zone (net 53) (net_name "/A4") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30150)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 155.2 96.175)
        (xy 155.239259 96.177858)
        (xy 155.278519 96.183716)
        (xy 155.317779 96.192574)
        (xy 155.357039 96.204432)
        (xy 155.396299 96.219291)
        (xy 155.801 96.075)
        (xy 155.396299 95.930709)
        (xy 155.357039 95.945567)
        (xy 155.317779 95.957425)
        (xy 155.278519 95.966283)
        (xy 155.239259 95.972141)
        (xy 155.2 95.975)
      )
    )
  )
  (zone (net 41) (net_name "/CARRY1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30059)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.95 90.1)
        (xy 142.897653 90.093522)
        (xy 142.845307 90.081044)
        (xy 142.79296 90.062567)
        (xy 142.740614 90.038089)
        (xy 142.688268 90.007612)
        (xy 142.0115 90.2)
        (xy 142.688268 90.392388)
        (xy 142.740614 90.36191)
        (xy 142.79296 90.337432)
        (xy 142.845307 90.318955)
        (xy 142.897653 90.306477)
        (xy 142.95 90.3)
      )
    )
  )
  (zone (net 49) (net_name "/A0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30174)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 136.7 97.475)
        (xy 136.66074 97.472141)
        (xy 136.62148 97.466283)
        (xy 136.58222 97.457425)
        (xy 136.54296 97.445567)
        (xy 136.503701 97.430709)
        (xy 136.099 97.575)
        (xy 136.503701 97.719291)
        (xy 136.54296 97.704432)
        (xy 136.58222 97.692574)
        (xy 136.62148 97.683716)
        (xy 136.66074 97.677858)
        (xy 136.7 97.675)
      )
    )
  )
  (zone (net 47) (net_name "/A16") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30095)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132 99.25)
        (xy 132.104804 99.255813)
        (xy 132.177582 99.27268)
        (xy 132.238392 99.299737)
        (xy 132.307288 99.336121)
        (xy 132.404329 99.38097)
        (xy 132.501 99.15)
        (xy 132.404329 98.91903)
        (xy 132.307288 98.963878)
        (xy 132.238392 99.000262)
        (xy 132.177582 99.027319)
        (xy 132.104804 99.044186)
        (xy 132 99.05)
      )
    )
  )
  (zone (net 50) (net_name "/A1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30160)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.5 97.175)
        (xy 135.539259 97.177858)
        (xy 135.578519 97.183716)
        (xy 135.617779 97.192574)
        (xy 135.657039 97.204432)
        (xy 135.696299 97.219291)
        (xy 136.101 97.075)
        (xy 135.696299 96.930709)
        (xy 135.657039 96.945567)
        (xy 135.617779 96.957425)
        (xy 135.578519 96.966283)
        (xy 135.539259 96.972141)
        (xy 135.5 96.975)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30023)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 154.85 89.55)
        (xy 154.72564 89.5448)
        (xy 154.63782 89.5324)
        (xy 154.562179 89.5176)
        (xy 154.474358 89.5052)
        (xy 154.35 89.5)
        (xy 154.349 89.75)
        (xy 154.35 90)
        (xy 154.474358 89.9948)
        (xy 154.562179 89.9824)
        (xy 154.63782 89.9676)
        (xy 154.72564 89.9552)
        (xy 154.85 89.95)
      )
    )
  )
  (zone (net 8) (net_name "/AD4") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30102)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.2 100.475)
        (xy 140.095195 100.469186)
        (xy 140.022416 100.452319)
        (xy 139.961607 100.425262)
        (xy 139.89271 100.388878)
        (xy 139.795671 100.34403)
        (xy 139.699 100.575)
        (xy 139.795671 100.80597)
        (xy 139.89271 100.761121)
        (xy 139.961607 100.724737)
        (xy 140.022416 100.69768)
        (xy 140.095195 100.680813)
        (xy 140.2 100.675)
      )
    )
  )
  (zone (net 14) (net_name "/A10") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30127)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.5 103.225)
        (xy 135.621446 103.219)
        (xy 135.742893 103.216)
        (xy 135.86434 103.216)
        (xy 135.985787 103.219)
        (xy 136.107234 103.225)
        (xy 136.101 103.075)
        (xy 135.662622 102.960952)
        (xy 135.630097 102.979761)
        (xy 135.597573 102.995571)
        (xy 135.565048 103.00838)
        (xy 135.532524 103.01819)
        (xy 135.5 103.025)
      )
    )
  )
  (zone (net 51) (net_name "/A2") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30155)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.5 96.675)
        (xy 141.539259 96.677858)
        (xy 141.578519 96.683716)
        (xy 141.617779 96.692574)
        (xy 141.657039 96.704432)
        (xy 141.696299 96.719291)
        (xy 142.101 96.575)
        (xy 141.696299 96.430709)
        (xy 141.657039 96.445567)
        (xy 141.617779 96.457425)
        (xy 141.578519 96.466283)
        (xy 141.539259 96.472141)
        (xy 141.5 96.475)
      )
    )
  )
  (zone (net 17) (net_name "/A13") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30125)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 155.2 102.225)
        (xy 155.321446 102.219)
        (xy 155.442893 102.216)
        (xy 155.56434 102.216)
        (xy 155.685787 102.219)
        (xy 155.807234 102.225)
        (xy 155.801 102.075)
        (xy 155.362622 101.960952)
        (xy 155.330097 101.979761)
        (xy 155.297573 101.995571)
        (xy 155.265048 102.00838)
        (xy 155.232524 102.01819)
        (xy 155.2 102.025)
      )
    )
  )
  (zone (net 9) (net_name "/AD5") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30114)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 138.470054 101.025)
        (xy 138.364967 101.014149)
        (xy 138.295232 100.98521)
        (xy 138.238601 100.943599)
        (xy 138.172829 100.894733)
        (xy 138.075671 100.84403)
        (xy 137.979 101.075)
        (xy 138.075671 101.30597)
        (xy 138.168778 101.267966)
        (xy 138.236861 101.244188)
        (xy 138.297829 101.231314)
        (xy 138.369591 101.226025)
        (xy 138.470054 101.225)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30002)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 128.12 115.455)
        (xy 128.226194 115.188134)
        (xy 128.332388 114.954268)
        (xy 128.438582 114.753402)
        (xy 128.544776 114.585536)
        (xy 128.65097 114.450671)
        (xy 127.82 113.754)
        (xy 126.98903 114.450671)
        (xy 127.095224 114.585536)
        (xy 127.201418 114.753402)
        (xy 127.307612 114.954268)
        (xy 127.413806 115.188134)
        (xy 127.52 115.455)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30011)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 145.7 89.025)
        (xy 145.830865 89.037193)
        (xy 145.961731 89.061387)
        (xy 146.092597 89.097582)
        (xy 146.223463 89.145776)
        (xy 146.354329 89.20597)
        (xy 146.926 88.725)
        (xy 146.354329 88.24403)
        (xy 146.223463 88.304223)
        (xy 146.092597 88.352417)
        (xy 145.961731 88.388612)
        (xy 145.830865 88.412806)
        (xy 145.7 88.425)
      )
    )
  )
  (zone (net 43) (net_name "/A7") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30048)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.95 92.7)
        (xy 142.897653 92.693522)
        (xy 142.845307 92.681044)
        (xy 142.79296 92.662567)
        (xy 142.740614 92.638089)
        (xy 142.688268 92.607612)
        (xy 142.0115 92.8)
        (xy 142.688268 92.992388)
        (xy 142.740614 92.96191)
        (xy 142.79296 92.937432)
        (xy 142.845307 92.918955)
        (xy 142.897653 92.906477)
        (xy 142.95 92.9)
      )
    )
  )
  (zone (net 38) (net_name "/SLEEP") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30017)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 150.85 107.175)
        (xy 150.92 107.181582)
        (xy 150.99 107.199551)
        (xy 151.059999 107.228905)
        (xy 151.129999 107.269644)
        (xy 151.2 107.32177)
        (xy 151.551 106.825)
        (xy 151.2 106.578586)
        (xy 151.129999 106.687868)
        (xy 151.059999 106.782151)
        (xy 150.99 106.861434)
        (xy 150.92 106.925717)
        (xy 150.85 106.975)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30021)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 128.562132 92.330025)
        (xy 128.470519 92.414283)
        (xy 128.399652 92.467613)
        (xy 128.335701 92.510634)
        (xy 128.264834 92.563964)
        (xy 128.173223 92.648223)
        (xy 128.349293 92.825707)
        (xy 128.526777 93.001777)
        (xy 128.611035 92.910164)
        (xy 128.664365 92.839297)
        (xy 128.707386 92.775346)
        (xy 128.760716 92.704479)
        (xy 128.844975 92.612868)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30149)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 155.2 101.175)
        (xy 155.239259 101.177858)
        (xy 155.278519 101.183716)
        (xy 155.317779 101.192574)
        (xy 155.357039 101.204432)
        (xy 155.396299 101.219291)
        (xy 155.801 101.075)
        (xy 155.396299 100.930709)
        (xy 155.357039 100.945567)
        (xy 155.317779 100.957425)
        (xy 155.278519 100.966283)
        (xy 155.239259 100.972141)
        (xy 155.2 100.975)
      )
    )
  )
  (zone (net 42) (net_name "/~{CE}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30181)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.7 102.475)
        (xy 142.66074 102.472141)
        (xy 142.62148 102.466283)
        (xy 142.58222 102.457425)
        (xy 142.54296 102.445567)
        (xy 142.503701 102.430709)
        (xy 142.099 102.575)
        (xy 142.503701 102.719291)
        (xy 142.54296 102.704432)
        (xy 142.58222 102.692574)
        (xy 142.62148 102.683716)
        (xy 142.66074 102.677858)
        (xy 142.7 102.675)
      )
    )
  )
  (zone (net 9) (net_name "/AD5") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30158)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.5 101.175)
        (xy 135.539259 101.177858)
        (xy 135.578519 101.183716)
        (xy 135.617779 101.192574)
        (xy 135.657039 101.204432)
        (xy 135.696299 101.219291)
        (xy 136.101 101.075)
        (xy 135.696299 100.930709)
        (xy 135.657039 100.945567)
        (xy 135.617779 100.957425)
        (xy 135.578519 100.966283)
        (xy 135.539259 100.972141)
        (xy 135.5 100.975)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30107)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.35 94)
        (xy 141.245195 93.994186)
        (xy 141.172416 93.977319)
        (xy 141.111607 93.950262)
        (xy 141.04271 93.913878)
        (xy 140.945671 93.86903)
        (xy 140.849 94.1)
        (xy 140.945671 94.33097)
        (xy 141.04271 94.286121)
        (xy 141.111607 94.249737)
        (xy 141.172416 94.22268)
        (xy 141.245195 94.205813)
        (xy 141.35 94.2)
      )
    )
  )
  (zone (net 19) (net_name "/A15") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30132)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 156.4 100.525)
        (xy 156.367475 100.51819)
        (xy 156.33495 100.50838)
        (xy 156.302426 100.495571)
        (xy 156.269901 100.479761)
        (xy 156.237377 100.460952)
        (xy 155.799 100.575)
        (xy 155.792766 100.725)
        (xy 155.914212 100.719)
        (xy 156.035659 100.716)
        (xy 156.157106 100.716)
        (xy 156.278553 100.719)
        (xy 156.4 100.725)
      )
    )
  )
  (zone (net 40) (net_name "/A6") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30153)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 155.2 97.175)
        (xy 155.239259 97.177858)
        (xy 155.278519 97.183716)
        (xy 155.317779 97.192574)
        (xy 155.357039 97.204432)
        (xy 155.396299 97.219291)
        (xy 155.801 97.075)
        (xy 155.396299 96.930709)
        (xy 155.357039 96.945567)
        (xy 155.317779 96.957425)
        (xy 155.278519 96.966283)
        (xy 155.239259 96.972141)
        (xy 155.2 96.975)
      )
    )
  )
  (zone (net 39) (net_name "/A5") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30062)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.95 91.4)
        (xy 142.897653 91.393522)
        (xy 142.845307 91.381044)
        (xy 142.79296 91.362567)
        (xy 142.740614 91.338089)
        (xy 142.688268 91.307612)
        (xy 142.0115 91.5)
        (xy 142.688268 91.692388)
        (xy 142.740614 91.66191)
        (xy 142.79296 91.637432)
        (xy 142.845307 91.618955)
        (xy 142.897653 91.606477)
        (xy 142.95 91.6)
      )
    )
  )
  (zone (net 31) (net_name "/CARRY0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30085)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.425736 93.142157)
        (xy 132.495732 93.220376)
        (xy 132.535268 93.283764)
        (xy 132.559135 93.345895)
        (xy 132.582124 93.420339)
        (xy 132.61903 93.520671)
        (xy 132.850707 93.425707)
        (xy 132.945671 93.19403)
        (xy 132.845339 93.157124)
        (xy 132.770895 93.134135)
        (xy 132.708764 93.110268)
        (xy 132.645376 93.070732)
        (xy 132.567157 93.000736)
      )
    )
  )
  (zone (net 14) (net_name "/A10") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30040)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 125.525 103.6)
        (xy 125.472653 103.593522)
        (xy 125.420307 103.581044)
        (xy 125.36796 103.562567)
        (xy 125.315614 103.538089)
        (xy 125.263268 103.507612)
        (xy 124.5865 103.7)
        (xy 125.263268 103.892388)
        (xy 125.315614 103.86191)
        (xy 125.36796 103.837432)
        (xy 125.420307 103.818955)
        (xy 125.472653 103.806477)
        (xy 125.525 103.8)
      )
    )
  )
  (zone (net 52) (net_name "/A3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30154)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.5 96.175)
        (xy 135.539259 96.177858)
        (xy 135.578519 96.183716)
        (xy 135.617779 96.192574)
        (xy 135.657039 96.204432)
        (xy 135.696299 96.219291)
        (xy 136.101 96.075)
        (xy 135.696299 95.930709)
        (xy 135.657039 95.945567)
        (xy 135.617779 95.957425)
        (xy 135.578519 95.966283)
        (xy 135.539259 95.972141)
        (xy 135.5 95.975)
      )
    )
  )
  (zone (net 69) (net_name "/~{WR}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30148)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 155.2 101.675)
        (xy 155.239259 101.677858)
        (xy 155.278519 101.683716)
        (xy 155.317779 101.692574)
        (xy 155.357039 101.704432)
        (xy 155.396299 101.719291)
        (xy 155.801 101.575)
        (xy 155.396299 101.430709)
        (xy 155.357039 101.445567)
        (xy 155.317779 101.457425)
        (xy 155.278519 101.466283)
        (xy 155.239259 101.472141)
        (xy 155.2 101.475)
      )
    )
  )
  (zone (net 30) (net_name "/~{BYTE}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30058)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 125.525 92.5325)
        (xy 125.472653 92.526022)
        (xy 125.420307 92.513544)
        (xy 125.36796 92.495067)
        (xy 125.315614 92.470589)
        (xy 125.263268 92.440112)
        (xy 124.5865 92.6325)
        (xy 125.263268 92.824888)
        (xy 125.315614 92.79441)
        (xy 125.36796 92.769932)
        (xy 125.420307 92.751455)
        (xy 125.472653 92.738977)
        (xy 125.525 92.7325)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30070)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 125.525 95.7825)
        (xy 125.472653 95.776022)
        (xy 125.420307 95.763544)
        (xy 125.36796 95.745067)
        (xy 125.315614 95.720589)
        (xy 125.263268 95.690112)
        (xy 124.5865 95.8825)
        (xy 125.263268 96.074888)
        (xy 125.315614 96.04441)
        (xy 125.36796 96.019932)
        (xy 125.420307 96.001455)
        (xy 125.472653 95.988977)
        (xy 125.525 95.9825)
      )
    )
  )
  (zone (net 20) (net_name "/~{RD}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30119)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 152.905331 103.225)
        (xy 153.015608 103.225)
        (xy 153.09387 103.225)
        (xy 153.161459 103.225)
        (xy 153.239721 103.225)
        (xy 153.35 103.225)
        (xy 153.351 102.975)
        (xy 153.173223 102.798223)
        (xy 153.114557 102.869459)
        (xy 153.075858 102.931656)
        (xy 153.039703 102.980913)
        (xy 152.988668 103.013328)
        (xy 152.905331 103.025)
      )
    )
  )
  (zone (net 30) (net_name "/~{BYTE}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30032)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.35 108.325)
        (xy 135.402346 108.331477)
        (xy 135.454692 108.343955)
        (xy 135.507039 108.362432)
        (xy 135.559385 108.38691)
        (xy 135.611732 108.417388)
        (xy 136.2885 108.225)
        (xy 135.611732 108.032612)
        (xy 135.559385 108.063089)
        (xy 135.507039 108.087567)
        (xy 135.454692 108.106044)
        (xy 135.402346 108.118522)
        (xy 135.35 108.125)
      )
    )
  )
  (zone (net 5) (net_name "/AD1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30172)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 136.7 98.475)
        (xy 136.66074 98.472141)
        (xy 136.62148 98.466283)
        (xy 136.58222 98.457425)
        (xy 136.54296 98.445567)
        (xy 136.503701 98.430709)
        (xy 136.099 98.575)
        (xy 136.503701 98.719291)
        (xy 136.54296 98.704432)
        (xy 136.58222 98.692574)
        (xy 136.62148 98.683716)
        (xy 136.66074 98.677858)
        (xy 136.7 98.675)
      )
    )
  )
  (zone (net 29) (net_name "/~{BLOCK}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30025)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.301257 109.442677)
        (xy 135.351005 109.463068)
        (xy 135.400754 109.48946)
        (xy 135.450502 109.521852)
        (xy 135.500251 109.560244)
        (xy 135.55 109.604636)
        (xy 136.288207 109.525707)
        (xy 136.300658 109.325)
        (xy 136.129061 109.332251)
        (xy 135.957465 109.333502)
        (xy 135.785869 109.328754)
        (xy 135.614273 109.318005)
        (xy 135.442677 109.301257)
      )
    )
  )
  (zone (net 49) (net_name "/A0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30164)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.5 97.675)
        (xy 141.539259 97.677858)
        (xy 141.578519 97.683716)
        (xy 141.617779 97.692574)
        (xy 141.657039 97.704432)
        (xy 141.696299 97.719291)
        (xy 142.101 97.575)
        (xy 141.696299 97.430709)
        (xy 141.657039 97.445567)
        (xy 141.617779 97.457425)
        (xy 141.578519 97.466283)
        (xy 141.539259 97.472141)
        (xy 141.5 97.475)
      )
    )
  )
  (zone (net 31) (net_name "/CARRY0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30063)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.25 92.5325)
        (xy 131.197653 92.526022)
        (xy 131.145307 92.513544)
        (xy 131.09296 92.495067)
        (xy 131.040614 92.470589)
        (xy 130.988268 92.440112)
        (xy 130.3115 92.6325)
        (xy 130.988268 92.824888)
        (xy 131.040614 92.79441)
        (xy 131.09296 92.769932)
        (xy 131.145307 92.751455)
        (xy 131.197653 92.738977)
        (xy 131.25 92.7325)
      )
    )
  )
  (zone (net 30) (net_name "/~{BYTE}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30066)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 137.225 108.125)
        (xy 137.172653 108.118522)
        (xy 137.120307 108.106044)
        (xy 137.06796 108.087567)
        (xy 137.015614 108.063089)
        (xy 136.963268 108.032612)
        (xy 136.2865 108.225)
        (xy 136.963268 108.417388)
        (xy 137.015614 108.38691)
        (xy 137.06796 108.362432)
        (xy 137.120307 108.343955)
        (xy 137.172653 108.331477)
        (xy 137.225 108.325)
      )
    )
  )
  (zone (net 29) (net_name "/~{BLOCK}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30098)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.8 89.475)
        (xy 132.695195 89.469186)
        (xy 132.622416 89.452319)
        (xy 132.561607 89.425262)
        (xy 132.49271 89.388878)
        (xy 132.395671 89.34403)
        (xy 132.299 89.575)
        (xy 132.395671 89.80597)
        (xy 132.49271 89.761121)
        (xy 132.561607 89.724737)
        (xy 132.622416 89.69768)
        (xy 132.695195 89.680813)
        (xy 132.8 89.675)
      )
    )
  )
  (zone (net 19) (net_name "/A15") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30088)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.2 101.2)
        (xy 131.304804 101.205813)
        (xy 131.377582 101.22268)
        (xy 131.438392 101.249737)
        (xy 131.507288 101.286121)
        (xy 131.604329 101.33097)
        (xy 131.701 101.1)
        (xy 131.604329 100.86903)
        (xy 131.507288 100.913878)
        (xy 131.438392 100.950262)
        (xy 131.377582 100.977319)
        (xy 131.304804 100.994186)
        (xy 131.2 101)
      )
    )
  )
  (zone (net 30) (net_name "/~{BYTE}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30080)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 130.235082 90.1)
        (xy 130.129537 90.086671)
        (xy 130.061462 90.051774)
        (xy 130.007218 90.002945)
        (xy 129.943167 89.947818)
        (xy 129.845671 89.89403)
        (xy 129.749 90.125)
        (xy 129.75 90.375)
        (xy 129.871129 90.3672)
        (xy 129.956089 90.3486)
        (xy 130.028991 90.3264)
        (xy 130.113951 90.3078)
        (xy 130.235082 90.3)
      )
    )
  )
  (zone (net 52) (net_name "/A3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30183)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.500001 96.175)
        (xy 141.53926 96.177858)
        (xy 141.57852 96.183716)
        (xy 141.617779 96.192574)
        (xy 141.657039 96.204432)
        (xy 141.696299 96.219291)
        (xy 142.100999 96.075)
        (xy 141.696299 95.930709)
        (xy 141.657039 95.945567)
        (xy 141.617779 95.957425)
        (xy 141.578519 95.966284)
        (xy 141.539259 95.972142)
        (xy 141.5 95.975001)
      )
    )
  )
  (zone (net 41) (net_name "/CARRY1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30030)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 154.675 93.75)
        (xy 154.727346 93.756477)
        (xy 154.779692 93.768955)
        (xy 154.832039 93.787432)
        (xy 154.884385 93.81191)
        (xy 154.936732 93.842388)
        (xy 155.6135 93.65)
        (xy 154.936732 93.457612)
        (xy 154.884385 93.488089)
        (xy 154.832039 93.512567)
        (xy 154.779692 93.531044)
        (xy 154.727346 93.543522)
        (xy 154.675 93.55)
      )
    )
  )
  (zone (net 8) (net_name "/AD4") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30139)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 136.7 100.425)
        (xy 136.578553 100.431)
        (xy 136.457106 100.434)
        (xy 136.335659 100.434)
        (xy 136.214212 100.431)
        (xy 136.092766 100.425)
        (xy 136.099 100.575)
        (xy 136.537377 100.689047)
        (xy 136.569901 100.670237)
        (xy 136.602426 100.654428)
        (xy 136.63495 100.641618)
        (xy 136.667475 100.631809)
        (xy 136.7 100.625)
      )
    )
  )
  (zone (net 41) (net_name "/CARRY1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30033)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 148.95 93.75)
        (xy 149.002346 93.756477)
        (xy 149.054692 93.768955)
        (xy 149.107039 93.787432)
        (xy 149.159385 93.81191)
        (xy 149.211732 93.842388)
        (xy 149.8885 93.65)
        (xy 149.211732 93.457612)
        (xy 149.159385 93.488089)
        (xy 149.107039 93.512567)
        (xy 149.054692 93.531044)
        (xy 149.002346 93.543522)
        (xy 148.95 93.55)
      )
    )
  )
  (zone (net 49) (net_name "/A0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30162)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.5 97.675)
        (xy 135.539259 97.677858)
        (xy 135.578519 97.683716)
        (xy 135.617779 97.692574)
        (xy 135.657039 97.704432)
        (xy 135.696299 97.719291)
        (xy 136.101 97.575)
        (xy 135.696299 97.430709)
        (xy 135.657039 97.445567)
        (xy 135.617779 97.457425)
        (xy 135.578519 97.466283)
        (xy 135.539259 97.472141)
        (xy 135.5 97.475)
      )
    )
  )
  (zone (net 45) (net_name "/BUS_A8") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30057)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.95 110.725)
        (xy 142.897653 110.718522)
        (xy 142.845307 110.706044)
        (xy 142.79296 110.687567)
        (xy 142.740614 110.663089)
        (xy 142.688268 110.632612)
        (xy 142.0115 110.825)
        (xy 142.688268 111.017388)
        (xy 142.740614 110.98691)
        (xy 142.79296 110.962432)
        (xy 142.845307 110.943955)
        (xy 142.897653 110.931477)
        (xy 142.95 110.925)
      )
    )
  )
  (zone (net 50) (net_name "/A1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30177)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 136.7 96.975)
        (xy 136.66074 96.972141)
        (xy 136.62148 96.966283)
        (xy 136.58222 96.957425)
        (xy 136.54296 96.945567)
        (xy 136.503701 96.930709)
        (xy 136.099 97.075)
        (xy 136.503701 97.219291)
        (xy 136.54296 97.204432)
        (xy 136.58222 97.192574)
        (xy 136.62148 97.183716)
        (xy 136.66074 97.177858)
        (xy 136.7 97.175)
      )
    )
  )
  (zone (net 52) (net_name "/A3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30050)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.25 93.1825)
        (xy 131.197653 93.176022)
        (xy 131.145307 93.163544)
        (xy 131.09296 93.145067)
        (xy 131.040614 93.120589)
        (xy 130.988268 93.090112)
        (xy 130.3115 93.2825)
        (xy 130.988268 93.474888)
        (xy 131.040614 93.44441)
        (xy 131.09296 93.419932)
        (xy 131.145307 93.401455)
        (xy 131.197653 93.388977)
        (xy 131.25 93.3825)
      )
    )
  )
  (zone (net 2) (net_name "VMEM") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30016)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 154.15 106.875)
        (xy 154.079999 106.827809)
        (xy 154.009999 106.777619)
        (xy 153.94 106.724429)
        (xy 153.87 106.668239)
        (xy 153.8 106.609049)
        (xy 153.449 106.825)
        (xy 153.8 107.39145)
        (xy 153.87 107.40216)
        (xy 153.94 107.41587)
        (xy 154.009999 107.43258)
        (xy 154.079999 107.45229)
        (xy 154.15 107.475)
      )
    )
  )
  (zone (net 18) (net_name "/A14") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30109)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 147.874264 98.407843)
        (xy 147.804266 98.329623)
        (xy 147.76473 98.266234)
        (xy 147.740864 98.204104)
        (xy 147.717874 98.129659)
        (xy 147.68097 98.029329)
        (xy 147.449293 98.124293)
        (xy 147.354329 98.35597)
        (xy 147.454659 98.392874)
        (xy 147.529104 98.415864)
        (xy 147.591234 98.43973)
        (xy 147.654623 98.479266)
        (xy 147.732843 98.549264)
      )
    )
  )
  (zone (net 21) (net_name "/RAMRST") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30142)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 150.4 108.425)
        (xy 150.359999 108.39235)
        (xy 150.319999 108.353701)
        (xy 150.28 108.309051)
        (xy 150.24 108.258402)
        (xy 150.2 108.201753)
        (xy 149.999 108.325)
        (xy 150.159205 108.628398)
        (xy 150.207364 108.615718)
        (xy 150.255523 108.609038)
        (xy 150.303682 108.608359)
        (xy 150.351841 108.613679)
        (xy 150.4 108.625)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30010)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 134.975 111.275)
        (xy 134.864353 111.239628)
        (xy 134.753706 111.192256)
        (xy 134.64306 111.132883)
        (xy 134.532413 111.061511)
        (xy 134.421767 110.97814)
        (xy 133.749 111.375)
        (xy 133.708484 111.875)
        (xy 133.961787 111.851)
        (xy 134.21509 111.839)
        (xy 134.468393 111.839)
        (xy 134.721696 111.851)
        (xy 134.975 111.875)
      )
    )
  )
  (zone (net 16) (net_name "/A12") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30123)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 126.587344 93.533735)
        (xy 126.509415 93.611701)
        (xy 126.454143 93.667064)
        (xy 126.406423 93.714892)
        (xy 126.351151 93.770256)
        (xy 126.273223 93.848223)
        (xy 126.449293 94.025707)
        (xy 126.7 94.025)
        (xy 126.691077 93.933133)
        (xy 126.674382 93.861775)
        (xy 126.665025 93.801366)
        (xy 126.678116 93.742346)
        (xy 126.728765 93.675156)
      )
    )
  )
  (zone (net 2) (net_name "VMEM") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30015)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 152.731595 106.089437)
        (xy 152.805276 106.239445)
        (xy 152.878957 106.398453)
        (xy 152.952637 106.566462)
        (xy 153.026318 106.74347)
        (xy 153.1 106.929479)
        (xy 153.450707 106.825707)
        (xy 153.441425 106.175)
        (xy 153.356027 106.119318)
        (xy 153.270629 106.054637)
        (xy 153.185232 105.980957)
        (xy 153.099834 105.898276)
        (xy 153.014437 105.806595)
      )
    )
  )
  (zone (net 23) (net_name "/(A)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30005)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 164.647208 115.163629)
        (xy 164.878234 115.455544)
        (xy 164.968769 115.706624)
        (xy 164.99254 115.957412)
        (xy 165.023275 116.24845)
        (xy 165.134702 116.620281)
        (xy 165.920707 116.295707)
        (xy 166.245281 115.509702)
        (xy 165.87345 115.398275)
        (xy 165.582412 115.36754)
        (xy 165.331624 115.343769)
        (xy 165.080544 115.253234)
        (xy 164.788629 115.022208)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30190)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 130.4125 96.2825)
        (xy 130.432499 96.230499)
        (xy 130.452499 96.184499)
        (xy 130.4725 96.1445)
        (xy 130.4925 96.1105)
        (xy 130.5125 96.0825)
        (xy 130.3125 95.8815)
        (xy 130.1125 96.0825)
        (xy 130.132499 96.1105)
        (xy 130.152499 96.1445)
        (xy 130.1725 96.184499)
        (xy 130.1925 96.230499)
        (xy 130.2125 96.2825)
      )
    )
  )
  (zone (net 12) (net_name "/A8") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30076)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 156.613388 91.746967)
        (xy 156.560366 91.727842)
        (xy 156.507344 91.702717)
        (xy 156.454322 91.671593)
        (xy 156.4013 91.634468)
        (xy 156.348278 91.591344)
        (xy 155.611793 91.699293)
        (xy 156.25 91.9)
        (xy 156.294393 91.885677)
        (xy 156.338786 91.877355)
        (xy 156.38318 91.875032)
        (xy 156.427573 91.87871)
        (xy 156.471967 91.888388)
      )
    )
  )
  (zone (net 4) (net_name "/AD0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30118)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.055331 97.275)
        (xy 131.165608 97.275)
        (xy 131.24387 97.275)
        (xy 131.311459 97.275)
        (xy 131.389721 97.275)
        (xy 131.5 97.275)
        (xy 131.501 97.025)
        (xy 131.323223 96.848223)
        (xy 131.264557 96.919459)
        (xy 131.225858 96.981656)
        (xy 131.189703 97.030913)
        (xy 131.138668 97.063328)
        (xy 131.055331 97.075)
      )
    )
  )
  (zone (net 18) (net_name "/A14") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30087)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.8 103.8)
        (xy 131.904804 103.805813)
        (xy 131.977582 103.82268)
        (xy 132.038392 103.849737)
        (xy 132.107288 103.886121)
        (xy 132.204329 103.93097)
        (xy 132.301 103.7)
        (xy 132.204329 103.46903)
        (xy 132.107288 103.513878)
        (xy 132.038392 103.550262)
        (xy 131.977582 103.577319)
        (xy 131.904804 103.594186)
        (xy 131.8 103.6)
      )
    )
  )
  (zone (net 8) (net_name "/AD4") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30144)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.5 100.675)
        (xy 141.539259 100.677858)
        (xy 141.578519 100.683716)
        (xy 141.617779 100.692574)
        (xy 141.657039 100.704432)
        (xy 141.696299 100.719291)
        (xy 142.101 100.575)
        (xy 141.696299 100.430709)
        (xy 141.657039 100.445567)
        (xy 141.617779 100.457425)
        (xy 141.578519 100.466283)
        (xy 141.539259 100.472141)
        (xy 141.5 100.475)
      )
    )
  )
  (zone (net 69) (net_name "/~{WR}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30082)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 155.128077 101.475)
        (xy 155.009138 101.4698)
        (xy 154.925184 101.4574)
        (xy 154.852892 101.4426)
        (xy 154.768938 101.4302)
        (xy 154.65 101.425)
        (xy 154.649 101.675)
        (xy 154.745671 101.90597)
        (xy 154.843243 101.849124)
        (xy 154.905097 101.78774)
        (xy 154.956407 101.731682)
        (xy 155.022342 101.690814)
        (xy 155.128077 101.675)
      )
    )
  )
  (zone (net 20) (net_name "/~{RD}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30180)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.7 103.475)
        (xy 142.66074 103.472141)
        (xy 142.62148 103.466283)
        (xy 142.58222 103.457425)
        (xy 142.54296 103.445567)
        (xy 142.503701 103.430709)
        (xy 142.099 103.575)
        (xy 142.503701 103.719291)
        (xy 142.54296 103.704432)
        (xy 142.58222 103.692574)
        (xy 142.62148 103.683716)
        (xy 142.66074 103.677858)
        (xy 142.7 103.675)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30106)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 154.85 94.2)
        (xy 154.745195 94.194186)
        (xy 154.672416 94.177319)
        (xy 154.611607 94.150262)
        (xy 154.54271 94.113878)
        (xy 154.445671 94.06903)
        (xy 154.349 94.3)
        (xy 154.445671 94.53097)
        (xy 154.54271 94.486121)
        (xy 154.611607 94.449737)
        (xy 154.672416 94.42268)
        (xy 154.745195 94.405813)
        (xy 154.85 94.4)
      )
    )
  )
  (zone (net 49) (net_name "/A0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30053)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.25 95.1325)
        (xy 131.197653 95.126022)
        (xy 131.145307 95.113544)
        (xy 131.09296 95.095067)
        (xy 131.040614 95.070589)
        (xy 130.988268 95.040112)
        (xy 130.3115 95.2325)
        (xy 130.988268 95.424888)
        (xy 131.040614 95.39441)
        (xy 131.09296 95.369932)
        (xy 131.145307 95.351455)
        (xy 131.197653 95.338977)
        (xy 131.25 95.3325)
      )
    )
  )
  (zone (net 14) (net_name "/A10") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30175)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 136.7 102.975)
        (xy 136.66074 102.972141)
        (xy 136.62148 102.966283)
        (xy 136.58222 102.957425)
        (xy 136.54296 102.945567)
        (xy 136.503701 102.930709)
        (xy 136.099 103.075)
        (xy 136.503701 103.219291)
        (xy 136.54296 103.204432)
        (xy 136.58222 103.192574)
        (xy 136.62148 103.183716)
        (xy 136.66074 103.177858)
        (xy 136.7 103.175)
      )
    )
  )
  (zone (net 13) (net_name "/A9") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30077)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 156.613388 91.096967)
        (xy 156.560366 91.077842)
        (xy 156.507344 91.052717)
        (xy 156.454322 91.021593)
        (xy 156.4013 90.984468)
        (xy 156.348278 90.941344)
        (xy 155.611793 91.049293)
        (xy 156.25 91.25)
        (xy 156.294393 91.235677)
        (xy 156.338786 91.227355)
        (xy 156.38318 91.225032)
        (xy 156.427573 91.22871)
        (xy 156.471967 91.238388)
      )
    )
  )
  (zone (net 6) (net_name "/AD2") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30097)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 134.567157 102.999264)
        (xy 134.645376 102.929266)
        (xy 134.708764 102.88973)
        (xy 134.770895 102.865864)
        (xy 134.845339 102.842874)
        (xy 134.945671 102.80597)
        (xy 134.850707 102.574293)
        (xy 134.61903 102.479329)
        (xy 134.582124 102.579659)
        (xy 134.559135 102.654104)
        (xy 134.535268 102.716234)
        (xy 134.495732 102.779623)
        (xy 134.425736 102.857843)
      )
    )
  )
  (zone (net 47) (net_name "/A16") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30055)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.25 99.05)
        (xy 131.197653 99.043522)
        (xy 131.145307 99.031044)
        (xy 131.09296 99.012567)
        (xy 131.040614 98.988089)
        (xy 130.988268 98.957612)
        (xy 130.3115 99.15)
        (xy 130.988268 99.342388)
        (xy 131.040614 99.31191)
        (xy 131.09296 99.287432)
        (xy 131.145307 99.268955)
        (xy 131.197653 99.256477)
        (xy 131.25 99.25)
      )
    )
  )
  (zone (net 5) (net_name "/AD1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30081)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 134.378077 98.475)
        (xy 134.259138 98.4698)
        (xy 134.175184 98.4574)
        (xy 134.102892 98.4426)
        (xy 134.018938 98.4302)
        (xy 133.9 98.425)
        (xy 133.899 98.675)
        (xy 133.995671 98.90597)
        (xy 134.093243 98.849124)
        (xy 134.155097 98.78774)
        (xy 134.206407 98.731682)
        (xy 134.272342 98.690814)
        (xy 134.378077 98.675)
      )
    )
  )
  (zone (net 31) (net_name "/CARRY0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30104)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.7 93.35)
        (xy 135.595195 93.344186)
        (xy 135.522416 93.327319)
        (xy 135.461607 93.300262)
        (xy 135.39271 93.263878)
        (xy 135.295671 93.21903)
        (xy 135.199 93.45)
        (xy 135.295671 93.68097)
        (xy 135.39271 93.636121)
        (xy 135.461607 93.599737)
        (xy 135.522416 93.57268)
        (xy 135.595195 93.555813)
        (xy 135.7 93.55)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30101)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 149.15 100.975)
        (xy 149.045195 100.969186)
        (xy 148.972416 100.952319)
        (xy 148.911607 100.925262)
        (xy 148.84271 100.888878)
        (xy 148.745671 100.84403)
        (xy 148.649 101.075)
        (xy 148.745671 101.30597)
        (xy 148.84271 101.261121)
        (xy 148.911607 101.224737)
        (xy 148.972416 101.19768)
        (xy 149.045195 101.180813)
        (xy 149.15 101.175)
      )
    )
  )
  (zone (net 48) (net_name "/A17") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30138)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 156.4 99.425)
        (xy 156.278553 99.431)
        (xy 156.157106 99.434)
        (xy 156.035659 99.434)
        (xy 155.914212 99.431)
        (xy 155.792766 99.425)
        (xy 155.799 99.575)
        (xy 156.237377 99.689047)
        (xy 156.269901 99.670237)
        (xy 156.302426 99.654428)
        (xy 156.33495 99.641618)
        (xy 156.367475 99.631809)
        (xy 156.4 99.625)
      )
    )
  )
  (zone (net 53) (net_name "/A4") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30049)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.95 90.75)
        (xy 142.897653 90.743522)
        (xy 142.845307 90.731044)
        (xy 142.79296 90.712567)
        (xy 142.740614 90.688089)
        (xy 142.688268 90.657612)
        (xy 142.0115 90.85)
        (xy 142.688268 91.042388)
        (xy 142.740614 91.01191)
        (xy 142.79296 90.987432)
        (xy 142.845307 90.968955)
        (xy 142.897653 90.956477)
        (xy 142.95 90.95)
      )
    )
  )
  (zone (net 29) (net_name "/~{BLOCK}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30079)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.064918 104.45)
        (xy 131.186047 104.4578)
        (xy 131.271007 104.4764)
        (xy 131.343909 104.4986)
        (xy 131.428869 104.5172)
        (xy 131.55 104.525)
        (xy 131.551 104.275)
        (xy 131.454329 104.04403)
        (xy 131.356832 104.097818)
        (xy 131.29278 104.152945)
        (xy 131.238536 104.201774)
        (xy 131.170461 104.236671)
        (xy 131.064918 104.25)
      )
    )
  )
  (zone (net 51) (net_name "/A2") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30156)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.5 96.675)
        (xy 135.539259 96.677858)
        (xy 135.578519 96.683716)
        (xy 135.617779 96.692574)
        (xy 135.657039 96.704432)
        (xy 135.696299 96.719291)
        (xy 136.101 96.575)
        (xy 135.696299 96.430709)
        (xy 135.657039 96.445567)
        (xy 135.617779 96.457425)
        (xy 135.578519 96.466283)
        (xy 135.539259 96.472141)
        (xy 135.5 96.475)
      )
    )
  )
  (zone (net 29) (net_name "/~{BLOCK}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30111)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.809946 89.625)
        (xy 131.915031 89.63585)
        (xy 131.984767 89.664789)
        (xy 132.041397 89.7064)
        (xy 132.10717 89.755266)
        (xy 132.204329 89.80597)
        (xy 132.301 89.575)
        (xy 132.204329 89.34403)
        (xy 132.111221 89.382032)
        (xy 132.043137 89.40581)
        (xy 131.982169 89.418684)
        (xy 131.910408 89.423974)
        (xy 131.809946 89.425)
      )
    )
  )
  (zone (net 7) (net_name "/AD3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30069)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 125.525 102.3)
        (xy 125.472653 102.293522)
        (xy 125.420307 102.281044)
        (xy 125.36796 102.262567)
        (xy 125.315614 102.238089)
        (xy 125.263268 102.207612)
        (xy 124.5865 102.4)
        (xy 125.263268 102.592388)
        (xy 125.315614 102.56191)
        (xy 125.36796 102.537432)
        (xy 125.420307 102.518955)
        (xy 125.472653 102.506477)
        (xy 125.525 102.5)
      )
    )
  )
  (zone (net 15) (net_name "/A11") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30168)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 155.2 103.675)
        (xy 155.239259 103.677858)
        (xy 155.278519 103.683716)
        (xy 155.317779 103.692574)
        (xy 155.357039 103.704432)
        (xy 155.396299 103.719291)
        (xy 155.801 103.575)
        (xy 155.396299 103.430709)
        (xy 155.357039 103.445567)
        (xy 155.317779 103.457425)
        (xy 155.278519 103.466283)
        (xy 155.239259 103.472141)
        (xy 155.2 103.475)
      )
    )
  )
  (zone (net 22) (net_name "/~{Y0}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30036)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.95 108.125)
        (xy 142.897653 108.118522)
        (xy 142.845307 108.106044)
        (xy 142.79296 108.087567)
        (xy 142.740614 108.063089)
        (xy 142.688268 108.032612)
        (xy 142.0115 108.225)
        (xy 142.688268 108.417388)
        (xy 142.740614 108.38691)
        (xy 142.79296 108.362432)
        (xy 142.845307 108.343955)
        (xy 142.897653 108.331477)
        (xy 142.95 108.325)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30012)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 148.15 88.425)
        (xy 148.019134 88.412806)
        (xy 147.888268 88.388612)
        (xy 147.757402 88.352417)
        (xy 147.626536 88.304223)
        (xy 147.495671 88.24403)
        (xy 146.924 88.725)
        (xy 147.495671 89.20597)
        (xy 147.626536 89.145776)
        (xy 147.757402 89.097582)
        (xy 147.888268 89.061387)
        (xy 148.019134 89.037193)
        (xy 148.15 89.025)
      )
    )
  )
  (zone (net 9) (net_name "/AD5") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30171)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 136.7 100.975)
        (xy 136.66074 100.972141)
        (xy 136.62148 100.966283)
        (xy 136.58222 100.957425)
        (xy 136.54296 100.945567)
        (xy 136.503701 100.930709)
        (xy 136.099 101.075)
        (xy 136.503701 101.219291)
        (xy 136.54296 101.204432)
        (xy 136.58222 101.192574)
        (xy 136.62148 101.183716)
        (xy 136.66074 101.177858)
        (xy 136.7 101.175)
      )
    )
  )
  (zone (net 30) (net_name "/~{BYTE}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30031)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.35 90.3)
        (xy 135.402346 90.306477)
        (xy 135.454692 90.318955)
        (xy 135.507039 90.337432)
        (xy 135.559385 90.36191)
        (xy 135.611732 90.392388)
        (xy 136.2885 90.2)
        (xy 135.611732 90.007612)
        (xy 135.559385 90.038089)
        (xy 135.507039 90.062567)
        (xy 135.454692 90.081044)
        (xy 135.402346 90.093522)
        (xy 135.35 90.1)
      )
    )
  )
  (zone (net 5) (net_name "/AD1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30086)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 133.475736 98.392157)
        (xy 133.545732 98.470376)
        (xy 133.585268 98.533764)
        (xy 133.609135 98.595895)
        (xy 133.632124 98.670339)
        (xy 133.66903 98.770671)
        (xy 133.900707 98.675707)
        (xy 133.995671 98.44403)
        (xy 133.895339 98.407124)
        (xy 133.820895 98.384135)
        (xy 133.758764 98.360268)
        (xy 133.695376 98.320732)
        (xy 133.617157 98.250736)
      )
    )
  )
  (zone (net 4) (net_name "/AD0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30068)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 125.525 99.7)
        (xy 125.472653 99.693522)
        (xy 125.420307 99.681044)
        (xy 125.36796 99.662567)
        (xy 125.315614 99.638089)
        (xy 125.263268 99.607612)
        (xy 124.5865 99.8)
        (xy 125.263268 99.992388)
        (xy 125.315614 99.96191)
        (xy 125.36796 99.937432)
        (xy 125.420307 99.918955)
        (xy 125.472653 99.906477)
        (xy 125.525 99.9)
      )
    )
  )
  (zone (net 29) (net_name "/~{BLOCK}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30042)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 125.525 91.8825)
        (xy 125.472653 91.876022)
        (xy 125.420307 91.863544)
        (xy 125.36796 91.845067)
        (xy 125.315614 91.820589)
        (xy 125.263268 91.790112)
        (xy 124.5865 91.9825)
        (xy 125.263268 92.174888)
        (xy 125.315614 92.14441)
        (xy 125.36796 92.119932)
        (xy 125.420307 92.101455)
        (xy 125.472653 92.088977)
        (xy 125.525 92.0825)
      )
    )
  )
  (zone (net 29) (net_name "/~{BLOCK}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30073)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 148.95 89.775)
        (xy 148.992081 89.78649)
        (xy 149.034162 89.80398)
        (xy 149.076244 89.82747)
        (xy 149.118325 89.85696)
        (xy 149.160407 89.892451)
        (xy 149.8885 89.75)
        (xy 149.25 89.55)
        (xy 149.19 89.566999)
        (xy 149.13 89.577999)
        (xy 149.069999 89.583)
        (xy 149.01 89.582)
        (xy 148.95 89.575)
      )
    )
  )
  (zone (net 48) (net_name "/A17") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30116)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.838627 101.85)
        (xy 131.953144 101.8526)
        (xy 132.034297 101.8588)
        (xy 132.104328 101.8662)
        (xy 132.185481 101.8724)
        (xy 132.3 101.875)
        (xy 132.301 101.625)
        (xy 132.123223 101.448223)
        (xy 132.063006 101.516571)
        (xy 132.019997 101.572532)
        (xy 131.978636 101.614497)
        (xy 131.923366 101.640856)
        (xy 131.838627 101.65)
      )
    )
  )
  (zone (net 18) (net_name "/A14") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30037)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.25 103.6)
        (xy 131.197653 103.593522)
        (xy 131.145307 103.581044)
        (xy 131.09296 103.562567)
        (xy 131.040614 103.538089)
        (xy 130.988268 103.507612)
        (xy 130.3115 103.7)
        (xy 130.988268 103.892388)
        (xy 131.040614 103.86191)
        (xy 131.09296 103.837432)
        (xy 131.145307 103.818955)
        (xy 131.197653 103.806477)
        (xy 131.25 103.8)
      )
    )
  )
  (zone (net 47) (net_name "/A16") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30161)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 155.2 99.175)
        (xy 155.239259 99.177858)
        (xy 155.278519 99.183716)
        (xy 155.317779 99.192574)
        (xy 155.357039 99.204432)
        (xy 155.396299 99.219291)
        (xy 155.801 99.075)
        (xy 155.396299 98.930709)
        (xy 155.357039 98.945567)
        (xy 155.317779 98.957425)
        (xy 155.278519 98.966283)
        (xy 155.239259 98.972141)
        (xy 155.2 98.975)
      )
    )
  )
  (zone (net 11) (net_name "/AD7") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30165)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.5 102.175)
        (xy 141.539259 102.177858)
        (xy 141.578519 102.183716)
        (xy 141.617779 102.192574)
        (xy 141.657039 102.204432)
        (xy 141.696299 102.219291)
        (xy 142.101 102.075)
        (xy 141.696299 101.930709)
        (xy 141.657039 101.945567)
        (xy 141.617779 101.957425)
        (xy 141.578519 101.966283)
        (xy 141.539259 101.972141)
        (xy 141.5 101.975)
      )
    )
  )
  (zone (net 8) (net_name "/AD4") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30103)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.2 100.475)
        (xy 140.095195 100.469186)
        (xy 140.022416 100.452319)
        (xy 139.961607 100.425262)
        (xy 139.89271 100.388878)
        (xy 139.795671 100.34403)
        (xy 139.699 100.575)
        (xy 139.795671 100.80597)
        (xy 139.89271 100.761121)
        (xy 139.961607 100.724737)
        (xy 140.022416 100.69768)
        (xy 140.095195 100.680813)
        (xy 140.2 100.675)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30029)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.075 94.2)
        (xy 141.127346 94.206477)
        (xy 141.179692 94.218955)
        (xy 141.232039 94.237432)
        (xy 141.284385 94.26191)
        (xy 141.336732 94.292388)
        (xy 142.0135 94.1)
        (xy 141.336732 93.907612)
        (xy 141.284385 93.938089)
        (xy 141.232039 93.962567)
        (xy 141.179692 93.981044)
        (xy 141.127346 93.993522)
        (xy 141.075 94)
      )
    )
  )
  (zone (net 8) (net_name "/AD4") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30163)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.5 100.675)
        (xy 141.539259 100.677858)
        (xy 141.578519 100.683716)
        (xy 141.617779 100.692574)
        (xy 141.657039 100.704432)
        (xy 141.696299 100.719291)
        (xy 142.101 100.575)
        (xy 141.696299 100.430709)
        (xy 141.657039 100.445567)
        (xy 141.617779 100.457425)
        (xy 141.578519 100.466283)
        (xy 141.539259 100.472141)
        (xy 141.5 100.475)
      )
    )
  )
  (zone (net 48) (net_name "/A17") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30054)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.25 101.65)
        (xy 131.197653 101.643522)
        (xy 131.145307 101.631044)
        (xy 131.09296 101.612567)
        (xy 131.040614 101.588089)
        (xy 130.988268 101.557612)
        (xy 130.3115 101.75)
        (xy 130.988268 101.942388)
        (xy 131.040614 101.91191)
        (xy 131.09296 101.887432)
        (xy 131.145307 101.868955)
        (xy 131.197653 101.856477)
        (xy 131.25 101.85)
      )
    )
  )
  (zone (net 7) (net_name "/AD3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30100)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.8 99.975)
        (xy 135.695195 99.969186)
        (xy 135.622416 99.952319)
        (xy 135.561607 99.925262)
        (xy 135.49271 99.888878)
        (xy 135.395671 99.84403)
        (xy 135.299 100.075)
        (xy 135.395671 100.30597)
        (xy 135.49271 100.261121)
        (xy 135.561607 100.224737)
        (xy 135.622416 100.19768)
        (xy 135.695195 100.180813)
        (xy 135.8 100.175)
      )
    )
  )
  (zone (net 30) (net_name "/~{BYTE}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30121)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 129.594669 109.075)
        (xy 129.48439 109.075)
        (xy 129.406128 109.075)
        (xy 129.338539 109.075)
        (xy 129.260277 109.075)
        (xy 129.15 109.075)
        (xy 129.149 109.325)
        (xy 129.326777 109.501777)
        (xy 129.385441 109.43054)
        (xy 129.42414 109.368342)
        (xy 129.460295 109.319086)
        (xy 129.511331 109.286671)
        (xy 129.594669 109.275)
      )
    )
  )
  (zone (net 42) (net_name "/~{CE}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30126)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.5 102.725)
        (xy 141.621446 102.719)
        (xy 141.742893 102.716)
        (xy 141.86434 102.716)
        (xy 141.985787 102.719)
        (xy 142.107234 102.725)
        (xy 142.101 102.575)
        (xy 141.662622 102.460952)
        (xy 141.630097 102.479761)
        (xy 141.597573 102.495571)
        (xy 141.565048 102.50838)
        (xy 141.532524 102.51819)
        (xy 141.5 102.525)
      )
    )
  )
  (zone (net 46) (net_name "/BUS_A9") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30056)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.95 110.075)
        (xy 142.897653 110.068522)
        (xy 142.845307 110.056044)
        (xy 142.79296 110.037567)
        (xy 142.740614 110.013089)
        (xy 142.688268 109.982612)
        (xy 142.0115 110.175)
        (xy 142.688268 110.367388)
        (xy 142.740614 110.33691)
        (xy 142.79296 110.312432)
        (xy 142.845307 110.293955)
        (xy 142.897653 110.281477)
        (xy 142.95 110.275)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30099)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 128.85 95.7825)
        (xy 128.745195 95.776686)
        (xy 128.672416 95.759819)
        (xy 128.611607 95.732762)
        (xy 128.54271 95.696378)
        (xy 128.445671 95.65153)
        (xy 128.349 95.8825)
        (xy 128.445671 96.11347)
        (xy 128.54271 96.068621)
        (xy 128.611607 96.032237)
        (xy 128.672416 96.00518)
        (xy 128.745195 95.988313)
        (xy 128.85 95.9825)
      )
    )
  )
  (zone (net 42) (net_name "/~{CE}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30131)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 136.7 102.525)
        (xy 136.667475 102.51819)
        (xy 136.63495 102.50838)
        (xy 136.602426 102.495571)
        (xy 136.569901 102.479761)
        (xy 136.537377 102.460952)
        (xy 136.099 102.575)
        (xy 136.092766 102.725)
        (xy 136.214212 102.719)
        (xy 136.335659 102.716)
        (xy 136.457106 102.716)
        (xy 136.578553 102.719)
        (xy 136.7 102.725)
      )
    )
  )
  (zone (net 8) (net_name "/AD4") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30129)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.5 100.725)
        (xy 135.621446 100.719)
        (xy 135.742893 100.716)
        (xy 135.86434 100.716)
        (xy 135.985787 100.719)
        (xy 136.107234 100.725)
        (xy 136.101 100.575)
        (xy 135.662622 100.460952)
        (xy 135.630097 100.479761)
        (xy 135.597573 100.495571)
        (xy 135.565048 100.50838)
        (xy 135.532524 100.51819)
        (xy 135.5 100.525)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30034)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 154.675 94.4)
        (xy 154.727346 94.406477)
        (xy 154.779692 94.418955)
        (xy 154.832039 94.437432)
        (xy 154.884385 94.46191)
        (xy 154.936732 94.492388)
        (xy 155.6135 94.3)
        (xy 154.936732 94.107612)
        (xy 154.884385 94.138089)
        (xy 154.832039 94.162567)
        (xy 154.779692 94.181044)
        (xy 154.727346 94.193522)
        (xy 154.675 94.2)
      )
    )
  )
  (zone (net 22) (net_name "/~{Y0}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30006)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 162.107208 112.623629)
        (xy 162.338234 112.915544)
        (xy 162.428769 113.166624)
        (xy 162.45254 113.417412)
        (xy 162.483275 113.70845)
        (xy 162.594702 114.080281)
        (xy 163.380707 113.755707)
        (xy 163.705281 112.969702)
        (xy 163.33345 112.858275)
        (xy 163.042412 112.82754)
        (xy 162.791624 112.803769)
        (xy 162.540544 112.713234)
        (xy 162.248629 112.482208)
      )
    )
  )
  (zone (net 4) (net_name "/AD0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30185)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.5 98.175)
        (xy 141.539259 98.177858)
        (xy 141.578519 98.183716)
        (xy 141.617779 98.192574)
        (xy 141.657039 98.204432)
        (xy 141.696299 98.219291)
        (xy 142.100999 98.075)
        (xy 141.696299 97.930709)
        (xy 141.657039 97.945567)
        (xy 141.617779 97.957425)
        (xy 141.57852 97.966284)
        (xy 141.53926 97.972142)
        (xy 141.500001 97.975001)
      )
    )
  )
  (zone (net 9) (net_name "/AD5") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30045)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.25 100.35)
        (xy 131.197653 100.343522)
        (xy 131.145307 100.331044)
        (xy 131.09296 100.312567)
        (xy 131.040614 100.288089)
        (xy 130.988268 100.257612)
        (xy 130.3115 100.45)
        (xy 130.988268 100.642388)
        (xy 131.040614 100.61191)
        (xy 131.09296 100.587432)
        (xy 131.145307 100.568955)
        (xy 131.197653 100.556477)
        (xy 131.25 100.55)
      )
    )
  )
  (zone (net 39) (net_name "/A5") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30151)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 155.2 96.675)
        (xy 155.239259 96.677858)
        (xy 155.278519 96.683716)
        (xy 155.317779 96.692574)
        (xy 155.357039 96.704432)
        (xy 155.396299 96.719291)
        (xy 155.801 96.575)
        (xy 155.396299 96.430709)
        (xy 155.357039 96.445567)
        (xy 155.317779 96.457425)
        (xy 155.278519 96.466283)
        (xy 155.239259 96.472141)
        (xy 155.2 96.475)
      )
    )
  )
  (zone (net 19) (net_name "/A15") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30115)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 157.310044 96.343623)
        (xy 157.230844 96.260561)
        (xy 157.177963 96.198471)
        (xy 157.133856 96.143373)
        (xy 157.080976 96.081284)
        (xy 157.001777 95.998223)
        (xy 156.824293 96.174293)
        (xy 156.825 96.425)
        (xy 156.915872 96.419404)
        (xy 156.985783 96.410616)
        (xy 157.04462 96.410629)
        (xy 157.102271 96.43144)
        (xy 157.168623 96.485044)
      )
    )
  )
  (zone (net 11) (net_name "/AD7") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30135)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.5 102.125)
        (xy 135.532524 102.131809)
        (xy 135.565048 102.141618)
        (xy 135.597573 102.154428)
        (xy 135.630097 102.170237)
        (xy 135.662622 102.189047)
        (xy 136.101 102.075)
        (xy 136.107234 101.925)
        (xy 135.985787 101.931)
        (xy 135.86434 101.934)
        (xy 135.742893 101.934)
        (xy 135.621446 101.931)
        (xy 135.5 101.925)
      )
    )
  )
  (zone (net 30) (net_name "/~{BYTE}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30024)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 149.042677 90.623743)
        (xy 149.214273 90.606994)
        (xy 149.385869 90.596245)
        (xy 149.557465 90.591497)
        (xy 149.729061 90.592748)
        (xy 149.900658 90.6)
        (xy 149.888207 90.399293)
        (xy 149.15 90.320363)
        (xy 149.100251 90.364755)
        (xy 149.050502 90.403147)
        (xy 149.000754 90.435538)
        (xy 148.951005 90.46193)
        (xy 148.901257 90.482323)
      )
    )
  )
  (zone (net 11) (net_name "/AD7") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30094)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.02 102.175)
        (xy 140.124804 102.180813)
        (xy 140.197582 102.19768)
        (xy 140.258392 102.224737)
        (xy 140.327288 102.261121)
        (xy 140.424329 102.30597)
        (xy 140.521 102.075)
        (xy 140.424329 101.84403)
        (xy 140.327288 101.888878)
        (xy 140.258392 101.925262)
        (xy 140.197582 101.952319)
        (xy 140.124804 101.969186)
        (xy 140.02 101.975)
      )
    )
  )
  (zone (net 10) (net_name "/AD6") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30182)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.7 101.474999)
        (xy 142.66074 101.472141)
        (xy 142.62148 101.466283)
        (xy 142.58222 101.457424)
        (xy 142.54296 101.445566)
        (xy 142.503701 101.430709)
        (xy 142.099 101.575)
        (xy 142.503701 101.719291)
        (xy 142.54296 101.704432)
        (xy 142.58222 101.692574)
        (xy 142.62148 101.683715)
        (xy 142.66074 101.677857)
        (xy 142.7 101.674999)
      )
    )
  )
  (zone (net 15) (net_name "/A11") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30018)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 123.65 99.35)
        (xy 123.839824 99.338)
        (xy 124.029649 99.332)
        (xy 124.219473 99.332)
        (xy 124.409298 99.338)
        (xy 124.599123 99.35)
        (xy 124.5885 99.15)
        (xy 123.85456 99.027071)
        (xy 123.813647 99.063656)
        (xy 123.772735 99.094242)
        (xy 123.731824 99.118828)
        (xy 123.690912 99.137414)
        (xy 123.65 99.15)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30090)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 127.85 95.9825)
        (xy 127.954804 95.988313)
        (xy 128.027582 96.00518)
        (xy 128.088392 96.032237)
        (xy 128.157288 96.068621)
        (xy 128.254329 96.11347)
        (xy 128.351 95.8825)
        (xy 128.254329 95.65153)
        (xy 128.157288 95.696378)
        (xy 128.088392 95.732762)
        (xy 128.027582 95.759819)
        (xy 127.954804 95.776686)
        (xy 127.85 95.7825)
      )
    )
  )
  (zone (net 51) (net_name "/A2") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30051)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.25 93.8325)
        (xy 131.197653 93.826022)
        (xy 131.145307 93.813544)
        (xy 131.09296 93.795067)
        (xy 131.040614 93.770589)
        (xy 130.988268 93.740112)
        (xy 130.3115 93.9325)
        (xy 130.988268 94.124888)
        (xy 131.040614 94.09441)
        (xy 131.09296 94.069932)
        (xy 131.145307 94.051455)
        (xy 131.197653 94.038977)
        (xy 131.25 94.0325)
      )
    )
  )
  (zone (net 30) (net_name "/~{BYTE}") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30078)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 129.264918 90.3)
        (xy 129.386047 90.3078)
        (xy 129.471007 90.3264)
        (xy 129.543909 90.3486)
        (xy 129.628869 90.3672)
        (xy 129.75 90.375)
        (xy 129.751 90.125)
        (xy 129.654329 89.89403)
        (xy 129.556832 89.947818)
        (xy 129.49278 90.002945)
        (xy 129.438536 90.051774)
        (xy 129.370461 90.086671)
        (xy 129.264918 90.1)
      )
    )
  )
  (zone (net 43) (net_name "/A7") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30157)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 155.2 97.675)
        (xy 155.239259 97.677858)
        (xy 155.278519 97.683716)
        (xy 155.317779 97.692574)
        (xy 155.357039 97.704432)
        (xy 155.396299 97.719291)
        (xy 155.801 97.575)
        (xy 155.396299 97.430709)
        (xy 155.357039 97.445567)
        (xy 155.317779 97.457425)
        (xy 155.278519 97.466283)
        (xy 155.239259 97.472141)
        (xy 155.2 97.475)
      )
    )
  )
  (zone (net 31) (net_name "/CARRY0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30064)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 137.225 93.35)
        (xy 137.172653 93.343522)
        (xy 137.120307 93.331044)
        (xy 137.06796 93.312567)
        (xy 137.015614 93.288089)
        (xy 136.963268 93.257612)
        (xy 136.2865 93.45)
        (xy 136.963268 93.642388)
        (xy 137.015614 93.61191)
        (xy 137.06796 93.587432)
        (xy 137.120307 93.568955)
        (xy 137.172653 93.556477)
        (xy 137.225 93.55)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30020)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 128.562132 98.830025)
        (xy 128.470519 98.914283)
        (xy 128.399652 98.967613)
        (xy 128.335701 99.010634)
        (xy 128.264834 99.063964)
        (xy 128.173223 99.148223)
        (xy 128.349293 99.325707)
        (xy 128.526777 99.501777)
        (xy 128.611035 99.410164)
        (xy 128.664365 99.339297)
        (xy 128.707386 99.275346)
        (xy 128.760716 99.204479)
        (xy 128.844975 99.112868)
      )
    )
  )
  (zone (net 11) (net_name "/AD7") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30041)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.25 102.95)
        (xy 131.197653 102.943522)
        (xy 131.145307 102.931044)
        (xy 131.09296 102.912567)
        (xy 131.040614 102.888089)
        (xy 130.988268 102.857612)
        (xy 130.3115 103.05)
        (xy 130.988268 103.242388)
        (xy 131.040614 103.21191)
        (xy 131.09296 103.187432)
        (xy 131.145307 103.168955)
        (xy 131.197653 103.156477)
        (xy 131.25 103.15)
      )
    )
  )
  (zone (net 48) (net_name "/A17") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30105)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 156.925 97.425)
        (xy 156.930813 97.320195)
        (xy 156.94768 97.247416)
        (xy 156.974737 97.186607)
        (xy 157.011121 97.11771)
        (xy 157.05597 97.020671)
        (xy 156.825 96.924)
        (xy 156.59403 97.020671)
        (xy 156.638878 97.11771)
        (xy 156.675262 97.186607)
        (xy 156.702319 97.247416)
        (xy 156.719186 97.320195)
        (xy 156.725 97.425)
      )
    )
  )
  (zone (net 6) (net_name "/AD2") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30169)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.5 99.175)
        (xy 135.539259 99.177858)
        (xy 135.578519 99.183716)
        (xy 135.617779 99.192574)
        (xy 135.657039 99.204432)
        (xy 135.696299 99.219291)
        (xy 136.101 99.075)
        (xy 135.696299 98.930709)
        (xy 135.657039 98.945567)
        (xy 135.617779 98.957425)
        (xy 135.578519 98.966283)
        (xy 135.539259 98.972141)
        (xy 135.5 98.975)
      )
    )
  )
  (zone (net 7) (net_name "/AD3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30134)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.5 100.125)
        (xy 141.532524 100.131809)
        (xy 141.565048 100.141618)
        (xy 141.597573 100.154428)
        (xy 141.630097 100.170237)
        (xy 141.662622 100.189047)
        (xy 142.101 100.075)
        (xy 142.107234 99.925)
        (xy 141.985787 99.931)
        (xy 141.86434 99.934)
        (xy 141.742893 99.934)
        (xy 141.621446 99.931)
        (xy 141.5 99.925)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30026)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.340054 89.35)
        (xy 141.21852 89.35)
        (xy 141.132271 89.35)
        (xy 141.057782 89.35)
        (xy 140.971533 89.35)
        (xy 140.85 89.35)
        (xy 140.849 89.6)
        (xy 140.945671 89.83097)
        (xy 141.038778 89.792966)
        (xy 141.106861 89.769188)
        (xy 141.167829 89.756314)
        (xy 141.239591 89.751025)
        (xy 141.340054 89.75)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30003)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 127.52 114.595)
        (xy 127.496308 114.953229)
        (xy 127.429512 115.199846)
        (xy 127.326033 115.404821)
        (xy 127.192289 115.638122)
        (xy 127.034702 115.969719)
        (xy 127.82 116.296)
        (xy 128.605298 115.969719)
        (xy 128.447709 115.638122)
        (xy 128.313966 115.404821)
        (xy 128.210487 115.199846)
        (xy 128.143691 114.953229)
        (xy 128.12 114.595)
      )
    )
  )
  (zone (net 8) (net_name "/AD4") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30110)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 139.209946 100.625)
        (xy 139.315031 100.63585)
        (xy 139.384767 100.664789)
        (xy 139.441397 100.7064)
        (xy 139.50717 100.755266)
        (xy 139.604329 100.80597)
        (xy 139.701 100.575)
        (xy 139.604329 100.34403)
        (xy 139.511221 100.382032)
        (xy 139.443137 100.40581)
        (xy 139.382169 100.418684)
        (xy 139.310408 100.423974)
        (xy 139.209946 100.425)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30004)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 128.05 112.055)
        (xy 127.878637 112.292066)
        (xy 127.707275 112.496132)
        (xy 127.535913 112.667199)
        (xy 127.364551 112.805265)
        (xy 127.193189 112.910332)
        (xy 127.82 113.756)
        (xy 128.67 113.155)
        (xy 128.665999 113.000999)
        (xy 128.661999 112.813999)
        (xy 128.658 112.594)
        (xy 128.654 112.341)
        (xy 128.65 112.055)
      )
    )
  )
  (zone (net 44) (net_name "/BATT+") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30000)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 165.4 88.725)
        (xy 165.723463 88.765776)
        (xy 166.046926 88.848552)
        (xy 166.37039 88.973328)
        (xy 166.693853 89.140104)
        (xy 167.017317 89.34888)
        (xy 169.701 88.425)
        (xy 167.017317 87.50112)
        (xy 166.693853 87.709896)
        (xy 166.37039 87.876672)
        (xy 166.046926 88.001448)
        (xy 165.723463 88.084224)
        (xy 165.4 88.125)
      )
    )
  )
  (zone (net 6) (net_name "/AD2") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30140)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 136.7 98.925)
        (xy 136.578553 98.931)
        (xy 136.457106 98.934)
        (xy 136.335659 98.934)
        (xy 136.214212 98.931)
        (xy 136.092766 98.925)
        (xy 136.099 99.075)
        (xy 136.537377 99.189047)
        (xy 136.569901 99.170237)
        (xy 136.602426 99.154428)
        (xy 136.63495 99.141618)
        (xy 136.667475 99.131809)
        (xy 136.7 99.125)
      )
    )
  )
  (zone (net 51) (net_name "/A2") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30173)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 136.7 96.475)
        (xy 136.66074 96.472141)
        (xy 136.62148 96.466283)
        (xy 136.58222 96.457425)
        (xy 136.54296 96.445567)
        (xy 136.503701 96.430709)
        (xy 136.099 96.575)
        (xy 136.503701 96.719291)
        (xy 136.54296 96.704432)
        (xy 136.58222 96.692574)
        (xy 136.62148 96.683716)
        (xy 136.66074 96.677858)
        (xy 136.7 96.675)
      )
    )
  )
  (zone (net 50) (net_name "/A1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30159)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.5 97.175)
        (xy 141.539259 97.177858)
        (xy 141.578519 97.183716)
        (xy 141.617779 97.192574)
        (xy 141.657039 97.204432)
        (xy 141.696299 97.219291)
        (xy 142.101 97.075)
        (xy 141.696299 96.930709)
        (xy 141.657039 96.945567)
        (xy 141.617779 96.957425)
        (xy 141.578519 96.966283)
        (xy 141.539259 96.972141)
        (xy 141.5 96.975)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.3) (thermal_bridge_width 0.3) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 181.95 120.025)
        (xy 181.95 86.025)
        (xy 121.95 86.025)
        (xy 121.95 120.025)
      )
    )
  )
  (zone (net 29) (net_name "/~{BLOCK}") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30022)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.15 108.275)
        (xy 132.144186 108.379804)
        (xy 132.127319 108.452582)
        (xy 132.100262 108.513392)
        (xy 132.063878 108.582288)
        (xy 132.01903 108.679329)
        (xy 132.25 108.776)
        (xy 132.48097 108.679329)
        (xy 132.436121 108.582288)
        (xy 132.399737 108.513392)
        (xy 132.37268 108.452582)
        (xy 132.355813 108.379804)
        (xy 132.35 108.275)
      )
    )
  )
  (zone (net 20) (net_name "/~{RD}") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30042)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 153.774264 103.257843)
        (xy 153.704266 103.179623)
        (xy 153.66473 103.116234)
        (xy 153.640864 103.054104)
        (xy 153.617874 102.979659)
        (xy 153.58097 102.879329)
        (xy 153.349293 102.974293)
        (xy 153.254329 103.20597)
        (xy 153.354659 103.242874)
        (xy 153.429104 103.265864)
        (xy 153.491234 103.28973)
        (xy 153.554623 103.329266)
        (xy 153.632843 103.399264)
      )
    )
  )
  (zone (net 5) (net_name "/AD1") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30008)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.8 112.055)
        (xy 132.756944 112.424775)
        (xy 132.643421 112.666334)
        (xy 132.482896 112.860476)
        (xy 132.298835 113.088004)
        (xy 132.114702 113.429719)
        (xy 132.9 113.756)
        (xy 133.685298 113.429719)
        (xy 133.501164 113.088004)
        (xy 133.317102 112.860476)
        (xy 133.156577 112.666334)
        (xy 133.043055 112.424775)
        (xy 133 112.055)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30018)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 148.55 107.825)
        (xy 148.544186 107.929804)
        (xy 148.527319 108.002582)
        (xy 148.500262 108.063392)
        (xy 148.463878 108.132288)
        (xy 148.41903 108.229329)
        (xy 148.65 108.326)
        (xy 148.88097 108.229329)
        (xy 148.836121 108.132288)
        (xy 148.799737 108.063392)
        (xy 148.77268 108.002582)
        (xy 148.755813 107.929804)
        (xy 148.75 107.825)
      )
    )
  )
  (zone (net 6) (net_name "/AD2") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30053)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 134.6 102.130331)
        (xy 134.6 102.240608)
        (xy 134.6 102.31887)
        (xy 134.6 102.386459)
        (xy 134.6 102.464721)
        (xy 134.6 102.575)
        (xy 134.85 102.576)
        (xy 135.026777 102.398223)
        (xy 134.95554 102.339557)
        (xy 134.893342 102.300858)
        (xy 134.844086 102.264703)
        (xy 134.811671 102.213668)
        (xy 134.8 102.130331)
      )
    )
  )
  (zone (net 4) (net_name "/AD0") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30028)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.217157 97.449264)
        (xy 131.295376 97.379266)
        (xy 131.358764 97.33973)
        (xy 131.420895 97.315864)
        (xy 131.495339 97.292874)
        (xy 131.595671 97.25597)
        (xy 131.500707 97.024293)
        (xy 131.26903 96.929329)
        (xy 131.232124 97.029659)
        (xy 131.209135 97.104104)
        (xy 131.185268 97.166234)
        (xy 131.145732 97.229623)
        (xy 131.075736 97.307843)
      )
    )
  )
  (zone (net 7) (net_name "/AD3") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30006)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.34 112.055)
        (xy 135.296944 112.424775)
        (xy 135.183421 112.666334)
        (xy 135.022896 112.860476)
        (xy 134.838835 113.088004)
        (xy 134.654702 113.429719)
        (xy 135.44 113.756)
        (xy 136.225298 113.429719)
        (xy 136.041164 113.088004)
        (xy 135.857102 112.860476)
        (xy 135.696577 112.666334)
        (xy 135.583055 112.424775)
        (xy 135.54 112.055)
      )
    )
  )
  (zone (net 29) (net_name "/~{BLOCK}") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30041)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.974264 104.557843)
        (xy 131.904266 104.479623)
        (xy 131.86473 104.416234)
        (xy 131.840864 104.354104)
        (xy 131.817874 104.279659)
        (xy 131.78097 104.179329)
        (xy 131.549293 104.274293)
        (xy 131.454329 104.50597)
        (xy 131.554659 104.542874)
        (xy 131.629104 104.565864)
        (xy 131.691234 104.58973)
        (xy 131.754623 104.629266)
        (xy 131.832843 104.699264)
      )
    )
  )
  (zone (net 11) (net_name "/AD7") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30004)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.42 112.055)
        (xy 140.376944 112.424775)
        (xy 140.263421 112.666334)
        (xy 140.102896 112.860476)
        (xy 139.918835 113.088004)
        (xy 139.734702 113.429719)
        (xy 140.52 113.756)
        (xy 141.305298 113.429719)
        (xy 141.121164 113.088004)
        (xy 140.937102 112.860476)
        (xy 140.776577 112.666334)
        (xy 140.663055 112.424775)
        (xy 140.62 112.055)
      )
    )
  )
  (zone (net 20) (net_name "/~{RD}") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30009)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 154.487208 115.163629)
        (xy 154.718234 115.455544)
        (xy 154.808769 115.706624)
        (xy 154.83254 115.957412)
        (xy 154.863275 116.24845)
        (xy 154.974702 116.620281)
        (xy 155.760707 116.295707)
        (xy 156.085281 115.509702)
        (xy 155.71345 115.398275)
        (xy 155.422412 115.36754)
        (xy 155.171624 115.343769)
        (xy 154.920544 115.253234)
        (xy 154.628629 115.022208)
      )
    )
  )
  (zone (net 48) (net_name "/A17") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30020)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.2 101.125)
        (xy 132.194186 101.229804)
        (xy 132.177319 101.302582)
        (xy 132.150262 101.363392)
        (xy 132.113878 101.432288)
        (xy 132.06903 101.529329)
        (xy 132.3 101.626)
        (xy 132.53097 101.529329)
        (xy 132.486121 101.432288)
        (xy 132.449737 101.363392)
        (xy 132.42268 101.302582)
        (xy 132.405813 101.229804)
        (xy 132.4 101.125)
      )
    )
  )
  (zone (net 47) (net_name "/A16") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30016)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.446967 98.586612)
        (xy 132.369714 98.681001)
        (xy 132.335477 98.761104)
        (xy 132.322073 98.840783)
        (xy 132.307318 98.933903)
        (xy 132.26903 99.054329)
        (xy 132.499293 99.150707)
        (xy 132.73097 99.054329)
        (xy 132.677891 98.969315)
        (xy 132.615088 98.90467)
        (xy 132.564566 98.849902)
        (xy 132.548331 98.79452)
        (xy 132.588388 98.728033)
      )
    )
  )
  (zone (net 31) (net_name "/CARRY0") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30021)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 134.7 93.55)
        (xy 134.804804 93.555813)
        (xy 134.877582 93.57268)
        (xy 134.938392 93.599737)
        (xy 135.007288 93.636121)
        (xy 135.104329 93.68097)
        (xy 135.201 93.45)
        (xy 135.104329 93.21903)
        (xy 135.007288 93.263878)
        (xy 134.938392 93.300262)
        (xy 134.877582 93.327319)
        (xy 134.804804 93.344186)
        (xy 134.7 93.35)
      )
    )
  )
  (zone (net 19) (net_name "/A15") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30052)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.45 100.655331)
        (xy 131.45 100.765608)
        (xy 131.45 100.84387)
        (xy 131.45 100.911459)
        (xy 131.45 100.989721)
        (xy 131.45 101.1)
        (xy 131.7 101.101)
        (xy 131.876777 100.923223)
        (xy 131.80554 100.864557)
        (xy 131.743342 100.825858)
        (xy 131.694086 100.789703)
        (xy 131.661671 100.738668)
        (xy 131.65 100.655331)
      )
    )
  )
  (zone (net 16) (net_name "/A12") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30025)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 126.35 100.375)
        (xy 126.344186 100.479804)
        (xy 126.327319 100.552582)
        (xy 126.300262 100.613392)
        (xy 126.263878 100.682288)
        (xy 126.21903 100.779329)
        (xy 126.45 100.876)
        (xy 126.68097 100.779329)
        (xy 126.636121 100.682288)
        (xy 126.599737 100.613392)
        (xy 126.57268 100.552582)
        (xy 126.555813 100.479804)
        (xy 126.55 100.375)
      )
    )
  )
  (zone (net 69) (net_name "/~{WR}") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30043)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 155.074264 101.957843)
        (xy 155.004266 101.879623)
        (xy 154.96473 101.816234)
        (xy 154.940864 101.754104)
        (xy 154.917874 101.679659)
        (xy 154.88097 101.579329)
        (xy 154.649293 101.674293)
        (xy 154.554329 101.90597)
        (xy 154.654659 101.942874)
        (xy 154.729104 101.965864)
        (xy 154.791234 101.98973)
        (xy 154.854623 102.029266)
        (xy 154.932843 102.099264)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30001)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 127.52 114.595)
        (xy 127.496308 114.953229)
        (xy 127.429512 115.199846)
        (xy 127.326033 115.404821)
        (xy 127.192289 115.638122)
        (xy 127.034702 115.969719)
        (xy 127.82 116.296)
        (xy 128.605298 115.969719)
        (xy 128.447709 115.638122)
        (xy 128.313966 115.404821)
        (xy 128.210487 115.199846)
        (xy 128.143691 114.953229)
        (xy 128.12 114.595)
      )
    )
  )
  (zone (net 6) (net_name "/AD2") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30010)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 134.167208 115.163629)
        (xy 134.398234 115.455544)
        (xy 134.488769 115.706624)
        (xy 134.51254 115.957412)
        (xy 134.543275 116.24845)
        (xy 134.654702 116.620281)
        (xy 135.440707 116.295707)
        (xy 135.765281 115.509702)
        (xy 135.39345 115.398275)
        (xy 135.102412 115.36754)
        (xy 134.851624 115.343769)
        (xy 134.600544 115.253234)
        (xy 134.308629 115.022208)
      )
    )
  )
  (zone (net 18) (net_name "/A14") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30049)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 147.005331 98.375)
        (xy 147.115608 98.375)
        (xy 147.19387 98.375)
        (xy 147.261459 98.375)
        (xy 147.339721 98.375)
        (xy 147.45 98.375)
        (xy 147.451 98.125)
        (xy 147.273223 97.948223)
        (xy 147.214557 98.019459)
        (xy 147.175858 98.081656)
        (xy 147.139703 98.130913)
        (xy 147.088668 98.163328)
        (xy 147.005331 98.175)
      )
    )
  )
  (zone (net 10) (net_name "/AD6") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30030)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.650157 101.999263)
        (xy 142.728376 101.929265)
        (xy 142.791764 101.889729)
        (xy 142.853895 101.865863)
        (xy 142.928339 101.842873)
        (xy 143.028671 101.805969)
        (xy 142.933707 101.574292)
        (xy 142.70203 101.479328)
        (xy 142.665124 101.579658)
        (xy 142.642135 101.654103)
        (xy 142.618268 101.716233)
        (xy 142.578732 101.779622)
        (xy 142.508736 101.857842)
      )
    )
  )
  (zone (net 6) (net_name "/AD2") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30054)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.1 103.019669)
        (xy 135.1 102.90939)
        (xy 135.1 102.831128)
        (xy 135.1 102.763539)
        (xy 135.1 102.685277)
        (xy 135.1 102.575)
        (xy 134.85 102.574)
        (xy 134.673223 102.751777)
        (xy 134.744459 102.810441)
        (xy 134.806656 102.84914)
        (xy 134.855913 102.885295)
        (xy 134.888328 102.936331)
        (xy 134.9 103.019669)
      )
    )
  )
  (zone (net 47) (net_name "/A16") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30046)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 145.759946 97.725)
        (xy 145.865031 97.73585)
        (xy 145.934767 97.764789)
        (xy 145.991397 97.8064)
        (xy 146.05717 97.855266)
        (xy 146.154329 97.90597)
        (xy 146.251 97.675)
        (xy 146.154329 97.44403)
        (xy 146.061221 97.482032)
        (xy 145.993137 97.50581)
        (xy 145.932169 97.518684)
        (xy 145.860408 97.523974)
        (xy 145.759946 97.525)
      )
    )
  )
  (zone (net 6) (net_name "/AD2") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30026)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 134.867157 99.749264)
        (xy 134.945376 99.679266)
        (xy 135.008764 99.63973)
        (xy 135.070895 99.615864)
        (xy 135.145339 99.592874)
        (xy 135.245671 99.55597)
        (xy 135.150707 99.324293)
        (xy 134.91903 99.229329)
        (xy 134.882124 99.329659)
        (xy 134.859135 99.404104)
        (xy 134.835268 99.466234)
        (xy 134.795732 99.529623)
        (xy 134.725736 99.607843)
      )
    )
  )
  (zone (net 46) (net_name "/BUS_A9") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30015)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 143.16 110.657098)
        (xy 143.174804 110.551182)
        (xy 143.213251 110.484145)
        (xy 143.266392 110.431424)
        (xy 143.325281 110.368454)
        (xy 143.38097 110.270671)
        (xy 143.15 110.174)
        (xy 142.9 110.175)
        (xy 142.90624 110.295095)
        (xy 142.92112 110.379676)
        (xy 142.93888 110.45242)
        (xy 142.95376 110.537001)
        (xy 142.96 110.657098)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30002)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 128.05 112.055)
        (xy 127.878637 112.292066)
        (xy 127.707275 112.496132)
        (xy 127.535913 112.667199)
        (xy 127.364551 112.805265)
        (xy 127.193189 112.910332)
        (xy 127.82 113.756)
        (xy 128.67 113.155)
        (xy 128.665999 113.000999)
        (xy 128.661999 112.813999)
        (xy 128.658 112.594)
        (xy 128.654 112.341)
        (xy 128.65 112.055)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30038)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 148.75 101.575)
        (xy 148.755813 101.470195)
        (xy 148.77268 101.397416)
        (xy 148.799737 101.336607)
        (xy 148.836121 101.26771)
        (xy 148.88097 101.170671)
        (xy 148.65 101.074)
        (xy 148.41903 101.170671)
        (xy 148.463878 101.26771)
        (xy 148.500262 101.336607)
        (xy 148.527319 101.397416)
        (xy 148.544186 101.470195)
        (xy 148.55 101.575)
      )
    )
  )
  (zone (net 18) (net_name "/A14") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30027)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.582843 103.275736)
        (xy 132.504623 103.345732)
        (xy 132.441234 103.385268)
        (xy 132.379104 103.409135)
        (xy 132.304659 103.432124)
        (xy 132.204329 103.46903)
        (xy 132.299293 103.700707)
        (xy 132.53097 103.795671)
        (xy 132.567874 103.695339)
        (xy 132.590864 103.620895)
        (xy 132.61473 103.558764)
        (xy 132.654266 103.495376)
        (xy 132.724264 103.417157)
      )
    )
  )
  (zone (net 29) (net_name "/~{BLOCK}") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30032)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.4 90.075)
        (xy 132.405813 89.970195)
        (xy 132.42268 89.897416)
        (xy 132.449737 89.836607)
        (xy 132.486121 89.76771)
        (xy 132.53097 89.670671)
        (xy 132.3 89.574)
        (xy 132.06903 89.670671)
        (xy 132.113878 89.76771)
        (xy 132.150262 89.836607)
        (xy 132.177319 89.897416)
        (xy 132.194186 89.970195)
        (xy 132.2 90.075)
      )
    )
  )
  (zone (net 29) (net_name "/~{BLOCK}") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30017)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.125736 103.992157)
        (xy 131.195732 104.070376)
        (xy 131.235268 104.133764)
        (xy 131.259135 104.195895)
        (xy 131.282124 104.270339)
        (xy 131.31903 104.370671)
        (xy 131.550707 104.275707)
        (xy 131.645671 104.04403)
        (xy 131.545339 104.007124)
        (xy 131.470895 103.984135)
        (xy 131.408764 103.960268)
        (xy 131.345376 103.920732)
        (xy 131.267157 103.850736)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30000)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 128.12 115.455)
        (xy 128.226194 115.188134)
        (xy 128.332388 114.954268)
        (xy 128.438582 114.753402)
        (xy 128.544776 114.585536)
        (xy 128.65097 114.450671)
        (xy 127.82 113.754)
        (xy 126.98903 114.450671)
        (xy 127.095224 114.585536)
        (xy 127.201418 114.753402)
        (xy 127.307612 114.954268)
        (xy 127.413806 115.188134)
        (xy 127.52 115.455)
      )
    )
  )
  (zone (net 42) (net_name "/~{CE}") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30023)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 146.2 106.675)
        (xy 146.194186 106.779804)
        (xy 146.177319 106.852582)
        (xy 146.150262 106.913392)
        (xy 146.113878 106.982288)
        (xy 146.06903 107.079329)
        (xy 146.3 107.176)
        (xy 146.53097 107.079329)
        (xy 146.486121 106.982288)
        (xy 146.449737 106.913392)
        (xy 146.42268 106.852582)
        (xy 146.405813 106.779804)
        (xy 146.4 106.675)
      )
    )
  )
  (zone (net 30) (net_name "/~{BYTE}") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30045)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 129.44713 90.519291)
        (xy 129.527952 90.451742)
        (xy 129.595899 90.419752)
        (xy 129.663289 90.405204)
        (xy 129.74244 90.389982)
        (xy 129.845671 90.35597)
        (xy 129.750707 90.124293)
        (xy 129.51903 90.029329)
        (xy 129.480689 90.124194)
        (xy 129.451772 90.191953)
        (xy 129.420692 90.247134)
        (xy 129.375866 90.304264)
        (xy 129.305709 90.37787)
      )
    )
  )
  (zone (net 69) (net_name "/~{WR}") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30005)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 155.66 112.055)
        (xy 155.616944 112.424775)
        (xy 155.503421 112.666334)
        (xy 155.342896 112.860476)
        (xy 155.158835 113.088004)
        (xy 154.974702 113.429719)
        (xy 155.76 113.756)
        (xy 156.545298 113.429719)
        (xy 156.361164 113.088004)
        (xy 156.177102 112.860476)
        (xy 156.016577 112.666334)
        (xy 155.903055 112.424775)
        (xy 155.86 112.055)
      )
    )
  )
  (zone (net 8) (net_name "/AD4") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30040)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 139.8 101.075)
        (xy 139.805813 100.970195)
        (xy 139.82268 100.897416)
        (xy 139.849737 100.836607)
        (xy 139.886121 100.76771)
        (xy 139.93097 100.670671)
        (xy 139.7 100.574)
        (xy 139.46903 100.670671)
        (xy 139.513878 100.76771)
        (xy 139.550262 100.836607)
        (xy 139.577319 100.897416)
        (xy 139.594186 100.970195)
        (xy 139.6 101.075)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30019)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 154.25 93.8)
        (xy 154.244186 93.904804)
        (xy 154.227319 93.977582)
        (xy 154.200262 94.038392)
        (xy 154.163878 94.107288)
        (xy 154.11903 94.204329)
        (xy 154.35 94.301)
        (xy 154.58097 94.204329)
        (xy 154.536121 94.107288)
        (xy 154.499737 94.038392)
        (xy 154.47268 93.977582)
        (xy 154.455813 93.904804)
        (xy 154.45 93.8)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30035)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 154.45 90.25)
        (xy 154.455813 90.145195)
        (xy 154.47268 90.072416)
        (xy 154.499737 90.011607)
        (xy 154.536121 89.94271)
        (xy 154.58097 89.845671)
        (xy 154.35 89.749)
        (xy 154.11903 89.845671)
        (xy 154.163878 89.94271)
        (xy 154.200262 90.011607)
        (xy 154.227319 90.072416)
        (xy 154.244186 90.145195)
        (xy 154.25 90.25)
      )
    )
  )
  (zone (net 16) (net_name "/A12") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30031)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 126.55 94.525)
        (xy 126.555813 94.420195)
        (xy 126.57268 94.347416)
        (xy 126.599737 94.286607)
        (xy 126.636121 94.21771)
        (xy 126.68097 94.120671)
        (xy 126.45 94.024)
        (xy 126.21903 94.120671)
        (xy 126.263878 94.21771)
        (xy 126.300262 94.286607)
        (xy 126.327319 94.347416)
        (xy 126.344186 94.420195)
        (xy 126.35 94.525)
      )
    )
  )
  (zone (net 10) (net_name "/AD6") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30014)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 141.651371 115.022208)
        (xy 141.359455 115.253234)
        (xy 141.108374 115.343769)
        (xy 140.857586 115.36754)
        (xy 140.566549 115.398275)
        (xy 140.194719 115.509702)
        (xy 140.519293 116.295707)
        (xy 141.305298 116.620281)
        (xy 141.416723 116.24845)
        (xy 141.447458 115.957412)
        (xy 141.47123 115.706624)
        (xy 141.561765 115.455544)
        (xy 141.792792 115.163629)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30036)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.95 90.1)
        (xy 140.955813 89.995195)
        (xy 140.97268 89.922416)
        (xy 140.999737 89.861607)
        (xy 141.036121 89.79271)
        (xy 141.08097 89.695671)
        (xy 140.85 89.599)
        (xy 140.61903 89.695671)
        (xy 140.663878 89.79271)
        (xy 140.700262 89.861607)
        (xy 140.727319 89.922416)
        (xy 140.744186 89.995195)
        (xy 140.75 90.1)
      )
    )
  )
  (zone (net 8) (net_name "/AD4") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30012)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 139.111371 115.022208)
        (xy 138.819455 115.253234)
        (xy 138.568374 115.343769)
        (xy 138.317586 115.36754)
        (xy 138.026549 115.398275)
        (xy 137.654719 115.509702)
        (xy 137.979293 116.295707)
        (xy 138.765298 116.620281)
        (xy 138.876723 116.24845)
        (xy 138.907458 115.957412)
        (xy 138.93123 115.706624)
        (xy 139.021765 115.455544)
        (xy 139.252792 115.163629)
      )
    )
  )
  (zone (net 46) (net_name "/BUS_A9") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30007)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 142.96 112.055)
        (xy 142.916944 112.424775)
        (xy 142.803421 112.666334)
        (xy 142.642896 112.860476)
        (xy 142.458835 113.088004)
        (xy 142.274702 113.429719)
        (xy 143.06 113.756)
        (xy 143.845298 113.429719)
        (xy 143.661164 113.088004)
        (xy 143.477102 112.860476)
        (xy 143.316577 112.666334)
        (xy 143.203055 112.424775)
        (xy 143.16 112.055)
      )
    )
  )
  (zone (net 9) (net_name "/AD5") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30039)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 138.08 101.575)
        (xy 138.085813 101.470195)
        (xy 138.10268 101.397416)
        (xy 138.129737 101.336607)
        (xy 138.166121 101.26771)
        (xy 138.21097 101.170671)
        (xy 137.98 101.074)
        (xy 137.74903 101.170671)
        (xy 137.793878 101.26771)
        (xy 137.830262 101.336607)
        (xy 137.857319 101.397416)
        (xy 137.874186 101.470195)
        (xy 137.88 101.575)
      )
    )
  )
  (zone (net 31) (net_name "/CARRY0") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30044)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 133.345027 93.35)
        (xy 133.24019 93.341654)
        (xy 133.168885 93.318724)
        (xy 133.110063 93.28437)
        (xy 133.042675 93.241751)
        (xy 132.945671 93.19403)
        (xy 132.849 93.425)
        (xy 132.945671 93.65597)
        (xy 133.040662 93.61459)
        (xy 133.109199 93.584515)
        (xy 133.170175 93.564532)
        (xy 133.242486 93.553431)
        (xy 133.345027 93.55)
      )
    )
  )
  (zone (net 30) (net_name "/~{BYTE}") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30051)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 128.9 108.880331)
        (xy 128.9 108.990608)
        (xy 128.9 109.06887)
        (xy 128.9 109.136459)
        (xy 128.9 109.214721)
        (xy 128.9 109.325)
        (xy 129.15 109.326)
        (xy 129.326777 109.148223)
        (xy 129.25554 109.089557)
        (xy 129.193342 109.050858)
        (xy 129.144086 109.014703)
        (xy 129.111671 108.963668)
        (xy 129.1 108.880331)
      )
    )
  )
  (zone (net 11) (net_name "/AD7") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30033)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.62 102.575)
        (xy 140.625813 102.470195)
        (xy 140.64268 102.397416)
        (xy 140.669737 102.336607)
        (xy 140.706121 102.26771)
        (xy 140.75097 102.170671)
        (xy 140.52 102.074)
        (xy 140.28903 102.170671)
        (xy 140.333878 102.26771)
        (xy 140.370262 102.336607)
        (xy 140.397319 102.397416)
        (xy 140.414186 102.470195)
        (xy 140.42 102.575)
      )
    )
  )
  (zone (net 9) (net_name "/AD5") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30003)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 137.88 112.055)
        (xy 137.836944 112.424775)
        (xy 137.723421 112.666334)
        (xy 137.562896 112.860476)
        (xy 137.378835 113.088004)
        (xy 137.194702 113.429719)
        (xy 137.98 113.756)
        (xy 138.765298 113.429719)
        (xy 138.581164 113.088004)
        (xy 138.397102 112.860476)
        (xy 138.236577 112.666334)
        (xy 138.123055 112.424775)
        (xy 138.08 112.055)
      )
    )
  )
  (zone (net 45) (net_name "/BUS_A8") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30034)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 144.43 111.275)
        (xy 144.435813 111.170195)
        (xy 144.45268 111.097416)
        (xy 144.479737 111.036607)
        (xy 144.516121 110.96771)
        (xy 144.56097 110.870671)
        (xy 144.33 110.774)
        (xy 144.09903 110.870671)
        (xy 144.143878 110.96771)
        (xy 144.180262 111.036607)
        (xy 144.207319 111.097416)
        (xy 144.224186 111.170195)
        (xy 144.23 111.275)
      )
    )
  )
  (zone (net 19) (net_name "/A15") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30047)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 156.481377 96.485044)
        (xy 156.547728 96.43144)
        (xy 156.605378 96.410629)
        (xy 156.664216 96.410616)
        (xy 156.734127 96.419404)
        (xy 156.825 96.425)
        (xy 156.825707 96.174293)
        (xy 156.648223 95.998223)
        (xy 156.569023 96.081284)
        (xy 156.516142 96.143373)
        (xy 156.472035 96.198471)
        (xy 156.419155 96.260561)
        (xy 156.339956 96.343623)
      )
    )
  )
  (zone (net 4) (net_name "/AD0") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30011)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.627208 115.163629)
        (xy 131.858234 115.455544)
        (xy 131.948769 115.706624)
        (xy 131.97254 115.957412)
        (xy 132.003275 116.24845)
        (xy 132.114702 116.620281)
        (xy 132.900707 116.295707)
        (xy 133.225281 115.509702)
        (xy 132.85345 115.398275)
        (xy 132.562412 115.36754)
        (xy 132.311624 115.343769)
        (xy 132.060544 115.253234)
        (xy 131.768629 115.022208)
      )
    )
  )
  (zone (net 3) (net_name "VBUS") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30024)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 140.75 93.6)
        (xy 140.744186 93.704804)
        (xy 140.727319 93.777582)
        (xy 140.700262 93.838392)
        (xy 140.663878 93.907288)
        (xy 140.61903 94.004329)
        (xy 140.85 94.101)
        (xy 141.08097 94.004329)
        (xy 141.036121 93.907288)
        (xy 140.999737 93.838392)
        (xy 140.97268 93.777582)
        (xy 140.955813 93.704804)
        (xy 140.95 93.6)
      )
    )
  )
  (zone (net 48) (net_name "/A17") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30050)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 156.380331 97.175)
        (xy 156.490608 97.175)
        (xy 156.56887 97.175)
        (xy 156.636459 97.175)
        (xy 156.714721 97.175)
        (xy 156.825 97.175)
        (xy 156.826 96.925)
        (xy 156.648223 96.748223)
        (xy 156.589557 96.819459)
        (xy 156.550858 96.881656)
        (xy 156.514703 96.930913)
        (xy 156.463668 96.963328)
        (xy 156.380331 96.975)
      )
    )
  )
  (zone (net 45) (net_name "/BUS_A8") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30013)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 144.191371 115.022208)
        (xy 143.899455 115.253234)
        (xy 143.648374 115.343769)
        (xy 143.397586 115.36754)
        (xy 143.106549 115.398275)
        (xy 142.734719 115.509702)
        (xy 143.059293 116.295707)
        (xy 143.845298 116.620281)
        (xy 143.956723 116.24845)
        (xy 143.987458 115.957412)
        (xy 144.01123 115.706624)
        (xy 144.101765 115.455544)
        (xy 144.332792 115.163629)
      )
    )
  )
  (zone (net 5) (net_name "/AD1") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30029)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 133.617157 99.099264)
        (xy 133.695376 99.029266)
        (xy 133.758764 98.98973)
        (xy 133.820895 98.965864)
        (xy 133.895339 98.942874)
        (xy 133.995671 98.90597)
        (xy 133.900707 98.674293)
        (xy 133.66903 98.579329)
        (xy 133.632124 98.679659)
        (xy 133.609135 98.754104)
        (xy 133.585268 98.816234)
        (xy 133.545732 98.879623)
        (xy 133.475736 98.957843)
      )
    )
  )
  (zone (net 7) (net_name "/AD3") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30048)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.54 100.52635)
        (xy 135.54104 100.414399)
        (xy 135.54352 100.334969)
        (xy 135.54648 100.26638)
        (xy 135.54896 100.18695)
        (xy 135.55 100.075)
        (xy 135.3 100.074)
        (xy 135.123223 100.251777)
        (xy 135.193262 100.311035)
        (xy 135.252959 100.351482)
        (xy 135.299315 100.389757)
        (xy 135.329328 100.4425)
        (xy 135.34 100.52635)
      )
    )
  )
  (zone (net 42) (net_name "/~{CE}") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30037)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 146.4 103.025)
        (xy 146.405813 102.920195)
        (xy 146.42268 102.847416)
        (xy 146.449737 102.786607)
        (xy 146.486121 102.71771)
        (xy 146.53097 102.620671)
        (xy 146.3 102.524)
        (xy 146.06903 102.620671)
        (xy 146.113878 102.71771)
        (xy 146.150262 102.786607)
        (xy 146.177319 102.847416)
        (xy 146.194186 102.920195)
        (xy 146.2 103.025)
      )
    )
  )
)
