(kicad_pcb (version 20171130) (host pcbnew "(5.1.6-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 51)
    (zones 0)
    (modules 6)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.8)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 "Net-(D1-Pad1)")
  (net 3 "Net-(J2-Pad6)")
  (net 4 "Net-(J2-Pad4)")
  (net 5 "Net-(J2-Pad1)")
  (net 6 "Net-(D2-Pad2)")
  (net 7 "Net-(J1-Pad3)")
  (net 8 "Net-(J2-Pad5)")
  (net 9 "Net-(J2-Pad3)")
  (net 10 "Net-(J2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
  )
  (module Diode_SMD:D_1206_3216Metric (layer F.Cu) (tedit 5FB700BB)
    (at 146.6 104 270)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at 0 1.6 270) (layer F.SilkS))
    (fp_text value SD1206S0402R0 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "BJW_Libraries:Wuerth 691243310006" (layer F.Cu) (tedit 5FB6B9F7)
    (at 136.5 96.9)
    (descr "<b>WR-TBL Serie 2433 - 3.81 mm Horizontal Entry Modular w. Rising Cage Clamp <br></b>Max Height =9.1mm , Pitch 3.81mm , 6 Pins")
    (fp_text reference J1 (at 0 -5.135) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x06 (at 4.12 4.865) (layer F.Fab))
    (pad 6 thru_hole circle (at 9.525 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 5 thru_hole circle (at 5.715 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 4 thru_hole circle (at 1.905 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 3 thru_hole circle (at -1.905 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at -5.715 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 1 thru_hole circle (at -9.525 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad2)"))
  )
  (module BJW_Libraries:6_Pin_Header_.150 (layer F.Cu) (tedit 5FB6AFE4)
    (at 136.5 110)
    (fp_text reference J2 (at -0.05 -0.05) (layer F.SilkS))
    (fp_text value Conn_01x06_Male (at 0 -2.6) (layer F.Fab))
    (pad 6 thru_hole oval (at 9.525 0) (size 2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad6)"))
    (pad 5 thru_hole oval (at 5.715 0) (size 2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad5)"))
    (pad 4 thru_hole oval (at 1.905 0) (size 2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad4)"))
    (pad 3 thru_hole oval (at -1.905 0) (size 2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at -5.715 0) (size 2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad2)"))
    (pad 1 thru_hole oval (at -9.525 0) (size 2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)"))
  )
  (module Diode_SMD:D_1206_3216Metric (layer F.Cu) (tedit 5FB700BB)
    (at 135.2 103.9 270)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D2 (at 0 1.5 90) (layer F.SilkS))
    (fp_text value SD1206S0402R0 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module BJW_Libraries:SO-08 (layer F.Cu) (tedit 5DCEE3E9)
    (at 140.5 104 90)
    (descr "<B>Small Outline Narrow Plastic Gull Wing</B><p>\n150-mil body, package type SN")
    (fp_text reference Q2 (at -3.2 -1) (layer F.SilkS))
    (fp_text value NTMS4920 (at 3.81 -5.08) (layer F.Fab))
    (fp_text user 3d (at -1.905 0.635 90) (layer Cmts.User))
    (fp_text user "" (at -1.905 0.635 90) (layer Cmts.User))
    (fp_text user "" (at -1.905 0.635 90) (layer Cmts.User))
    (pad 5 smd rect (at 1.905 -2.6 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)") (solder_mask_margin 0.1016))
    (pad 6 smd rect (at 0.635 -2.6 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)") (solder_mask_margin 0.1016))
    (pad 8 smd rect (at -1.905 -2.6 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)") (solder_mask_margin 0.1016))
    (pad 4 smd rect (at 1.905 2.6 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-Pad4)") (solder_mask_margin 0.1016))
    (pad 3 smd rect (at 0.635 2.6 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad6)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -1.905 2.6 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad6)") (solder_mask_margin 0.1016))
    (pad 7 smd rect (at -0.635 -2.6 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)") (solder_mask_margin 0.1016))
    (pad 2 smd rect (at -0.635 2.6 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad6)") (solder_mask_margin 0.1016))
  )
  (module BJW_Libraries:SO-08 (layer F.Cu) (tedit 5DCEE3E9)
    (at 129.2 104 90)
    (descr "<B>Small Outline Narrow Plastic Gull Wing</B><p>\n150-mil body, package type SN")
    (fp_text reference Q1 (at -3.2 -0.9) (layer F.SilkS))
    (fp_text value NTMS4920 (at 3.81 -5.08) (layer F.Fab))
    (fp_text user 3d (at -1.905 0.635 90) (layer Cmts.User))
    (fp_text user "" (at -1.905 0.635 90) (layer Cmts.User))
    (fp_text user "" (at -1.905 0.635 90) (layer Cmts.User))
    (pad 5 smd rect (at 1.905 -2.6 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad2)") (solder_mask_margin 0.1016))
    (pad 6 smd rect (at 0.635 -2.6 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad2)") (solder_mask_margin 0.1016))
    (pad 8 smd rect (at -1.905 -2.6 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad2)") (solder_mask_margin 0.1016))
    (pad 4 smd rect (at 1.905 2.6 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad1)") (solder_mask_margin 0.1016))
    (pad 3 smd rect (at 0.635 2.6 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad6)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -1.905 2.6 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad6)") (solder_mask_margin 0.1016))
    (pad 7 smd rect (at -0.635 -2.6 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad2)") (solder_mask_margin 0.1016))
    (pad 2 smd rect (at -0.635 2.6 90) (size 0.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad6)") (solder_mask_margin 0.1016))
  )
  (gr_text "TinyG FET Board" (at 136.55 104.1) (layer B.SilkS))
  (gr_text +24 (at 145.85 94.5) (layer B.SilkS))
  (gr_text PUMP (at 140.05 94.5) (layer B.SilkS))
  (gr_text SOL (at 128.95 94.5) (layer B.SilkS))
  (gr_line (start 125 111.5) (end 125 93) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 148 111.5) (end 125 111.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 148 93) (end 148 111.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125 93) (end 148 93) (layer Edge.Cuts) (width 0.05))
  (zone (net 3) (net_name "Net-(J2-Pad6)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148 111.5) (xy 125 111.5) (xy 125 93.2) (xy 148 93.2)
      )
    )
  )
  (zone (net 3) (net_name "Net-(J2-Pad6)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148 111.5) (xy 125 111.5) (xy 125 93.2) (xy 148 93.2)
      )
    )
  )
)
