<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="40.7" y2="0" width="0" layer="20" locked="yes"/>
<wire x1="40.7" y1="0" x2="40.7" y2="22.9" width="0" layer="20" locked="yes"/>
<wire x1="40.7" y1="22.9" x2="0" y2="22.9" width="0" layer="20" locked="yes"/>
<wire x1="0" y1="22.9" x2="0" y2="0" width="0" layer="20" locked="yes"/>
<text>Peanut Labs
DWM1000 Breakout v1
July 2021</text>
<text>RST</text>
<text>3V3</text>
<text>AREF</text>
<text>GND</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>28</text>
<text>29</text>
<text>SCK</text>
<text>MOSI</text>
<text>MISO</text>
<text>Rx</text>
<text>Tx</text>
<text>DFU</text>
<text>VBAT</text>
<text>EN</text>
<text>VBUS</text>
<text>16</text>
<text>15</text>
<text>7</text>
<text>11</text>
<text>31</text>
<text>30</text>
<text>Designed for nRF52 Feather;
may not match other pinouts</text>
<text>Remove R2, R3, or R4
to reroute !RST, IRQ,
or !CS, respectively</text>
<text>!CS</text>
<text>IRQ</text>
<text>!RST</text>
</plain>
<libraries>
<library name="Connectors">
<packages>
<package name="PIN_HEADER_1X12_MALE_2.54MM_TH_VERT">
</package>
<package name="PIN_HEADER_1X16_MALE_2.54MM_TH_VERT">
</package>
<package name="PAD.03X.03">
</package>
</packages>
</library>
<library name="Passives">
<packages>
<package name="R0603">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 0603 Package for Resistors&lt;br/&gt;</description>
</package>
</packages>
</library>
<library name="Sensor">
<packages>
<package name="DWM1000">
<description>&lt;b&gt;DWM1000-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="Connectors" package="PIN_HEADER_1X12_MALE_2.54MM_TH_VERT" value="PIN_HEADER_1X12_MALE_2.54MM_TH_VERT">
<attribute name="MPN" value="61301211121"/>
<attribute name="NAME"/>
</element>
<element name="J2" library="Connectors" package="PIN_HEADER_1X16_MALE_2.54MM_TH_VERT" value="PIN_HEADER_1X16">
<attribute name="MPN" value="61301611121"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="Passives" package="R0603" value="100K">
<attribute name="MPN" value="ERA-3AEB104V"/>
<attribute name="MPN2" value="AT0603BRD07100KL"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
<attribute name="TOLERANCE" value="0.1%"/>
<attribute name="WATTAGE" value="1/10W"/>
</element>
<element name="U1" library="Sensor" package="DWM1000" value="DWM1000">
<attribute name="HEIGHT" value="3.15mm"/>
<attribute name="MANUFACTURER" value="Qorvo"/>
<attribute name="MPN" value="DWM1000"/>
<attribute name="NAME"/>
</element>
<element name="R4" library="Passives" package="R0603" value="0">
<attribute name="MPN" value="RC0603JR-070RL"/>
<attribute name="MPN2" value="ERJ-3GEY0R00V"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
<attribute name="TOLERANCE" value="N/A"/>
<attribute name="WATTAGE" value="1/10W"/>
</element>
<element name="R3" library="Passives" package="R0603" value="0">
<attribute name="MPN" value="RC0603JR-070RL"/>
<attribute name="MPN2" value="ERJ-3GEY0R00V"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
<attribute name="TOLERANCE" value="N/A"/>
<attribute name="WATTAGE" value="1/10W"/>
</element>
<element name="R2" library="Passives" package="R0603" value="0">
<attribute name="MPN" value="RC0603JR-070RL"/>
<attribute name="MPN2" value="ERJ-3GEY0R00V"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
<attribute name="TOLERANCE" value="N/A"/>
<attribute name="WATTAGE" value="1/10W"/>
</element>
<element name="EXTON" library="Connectors" package="PAD.03X.03" value="TEST-POINT3">
<attribute name="NAME"/>
<attribute name="POPULATE" value="0"/>
</element>
<element name="WKP" library="Connectors" package="PAD.03X.03" value="TEST-POINT3">
<attribute name="NAME"/>
<attribute name="POPULATE" value="0"/>
</element>
<element name="GPIO0" library="Connectors" package="PAD.03X.03" value="TEST-POINT3">
<attribute name="NAME"/>
<attribute name="POPULATE" value="0"/>
</element>
<element name="GPIO1" library="Connectors" package="PAD.03X.03" value="TEST-POINT3">
<attribute name="NAME"/>
<attribute name="POPULATE" value="0"/>
</element>
<element name="GPIO2" library="Connectors" package="PAD.03X.03" value="TEST-POINT3">
<attribute name="NAME"/>
<attribute name="POPULATE" value="0"/>
</element>
<element name="GPIO3" library="Connectors" package="PAD.03X.03" value="TEST-POINT3">
<attribute name="NAME"/>
<attribute name="POPULATE" value="0"/>
</element>
<element name="GPIO4" library="Connectors" package="PAD.03X.03" value="TEST-POINT3">
<attribute name="NAME"/>
<attribute name="POPULATE" value="0"/>
</element>
<element name="GPIO5" library="Connectors" package="PAD.03X.03" value="TEST-POINT3">
<attribute name="NAME"/>
<attribute name="POPULATE" value="0"/>
</element>
<element name="GPIO6" library="Connectors" package="PAD.03X.03" value="TEST-POINT3">
<attribute name="NAME"/>
<attribute name="POPULATE" value="0"/>
</element>
<element name="GPIO7" library="Connectors" package="PAD.03X.03" value="TEST-POINT3">
<attribute name="NAME"/>
<attribute name="POPULATE" value="0"/>
</element>
</elements>
<signals>
<signal name="3V3">
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="7"/>
<contactref element="J2" pad="15"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="16"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="23"/>
<contactref element="U1" pad="24"/>
<contactref element="R1" pad="P$2"/>
<contactref element="J2" pad="13"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="20"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="19"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="18"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="RESET">
<contactref element="J2" pad="16"/>
</signal>
<signal name="AREF">
<contactref element="J2" pad="14"/>
</signal>
<signal name="D2/A0">
<contactref element="J2" pad="12"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="D3/A1">
<contactref element="J2" pad="11"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="D4/A2">
<contactref element="J2" pad="10"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="D5/A3">
<contactref element="J2" pad="9"/>
</signal>
<signal name="D28/A4">
<contactref element="J2" pad="8"/>
</signal>
<signal name="D29/A5">
<contactref element="J2" pad="7"/>
</signal>
<signal name="RX">
<contactref element="J2" pad="3"/>
</signal>
<signal name="TX">
<contactref element="J2" pad="2"/>
</signal>
<signal name="VBAT">
<contactref element="J1" pad="12"/>
</signal>
<signal name="EN">
<contactref element="J1" pad="11"/>
</signal>
<signal name="D16">
<contactref element="J1" pad="9"/>
</signal>
<signal name="D15">
<contactref element="J1" pad="8"/>
</signal>
<signal name="D7">
<contactref element="J1" pad="7"/>
</signal>
<signal name="D11">
<contactref element="J1" pad="6"/>
</signal>
<signal name="D31/A7">
<contactref element="J1" pad="5"/>
</signal>
<signal name="D30/A6">
<contactref element="J1" pad="4"/>
</signal>
<signal name="D27">
<contactref element="J1" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="J1" pad="2"/>
</signal>
<signal name="SDA">
<contactref element="J1" pad="1"/>
</signal>
<signal name="VBUS">
<contactref element="J1" pad="10"/>
</signal>
<signal name="DFU">
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="1"/>
<contactref element="EXTON" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="WKP" pad="P$1"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="GPIO0" pad="P$1"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="14"/>
<contactref element="GPIO1" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="GPIO2" pad="P$1"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="12"/>
<contactref element="GPIO3" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="GPIO4" pad="P$1"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="10"/>
<contactref element="GPIO5" pad="P$1"/>
</signal>
<signal name="N$9">
<contactref element="GPIO6" pad="P$1"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="4"/>
<contactref element="GPIO7" pad="P$1"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="17"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="3"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$13">
<contactref element="U1" pad="22"/>
<contactref element="R1" pad="P$1"/>
<contactref element="R3" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
