<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<text>CoinKit Prototype</text>
<wire x1="0" y1="0" x2="245" y2="0" width="0.254" layer="20"/>
<wire x1="245" y1="0" x2="245" y2="210" width="0.254" layer="20"/>
<wire x1="0" y1="210" x2="0" y2="0" width="0.254" layer="20"/>
<wire x1="5.75" y1="44.75" x2="14.75" y2="44.75" width="0.5" layer="46"/>
<wire x1="14.75" y1="31.25" x2="5.75" y2="31.25" width="0.5" layer="46"/>
<wire x1="59.25" y1="31.25" x2="43.25" y2="31.25" width="0.5" layer="46"/>
<wire x1="43.25" y1="44.75" x2="59.25" y2="44.75" width="0.5" layer="46"/>
<wire x1="14.75" y1="44.75" x2="14.75" y2="42.625" width="0.5" layer="46"/>
<wire x1="14.75" y1="42" x2="14.75" y2="38.3125" width="0.5" layer="46"/>
<wire x1="14.75" y1="37.6875" x2="14.75" y2="34.25" width="0.5" layer="46"/>
<wire x1="14.75" y1="33.5" x2="14.75" y2="31.25" width="0.5" layer="46"/>
<wire x1="43.25" y1="44.75" x2="43.25" y2="42.625" width="0.5" layer="46"/>
<wire x1="43.25" y1="42" x2="43.25" y2="38.3125" width="0.5" layer="46"/>
<wire x1="43.25" y1="37.6875" x2="43.25" y2="34.125" width="0.5" layer="46"/>
<wire x1="43.25" y1="33.5" x2="43.25" y2="31.25" width="0.5" layer="46"/>
<wire x1="32.500025" y1="9.499996875" x2="4.95475" y2="30.68498125" width="0.5" layer="46" curve="-75.127654"/>
<wire x1="60.04524375" y1="30.68498125" x2="33.499821875" y2="9.5175375" width="0.5" layer="46" curve="-73.117158"/>
<wire x1="32.499975" y1="66.499996875" x2="60.04524375" y2="45.3150125" width="0.5" layer="46" curve="-75.127656"/>
<wire x1="4.95475625" y1="45.31501875" x2="31.500178125" y2="66.482453125" width="0.5" layer="46" curve="-73.117163"/>
<text>CoinKit Prototype</text>
<wire x1="65.25" y1="44.75" x2="74.25" y2="44.75" width="0.5" layer="46"/>
<wire x1="74.25" y1="31.25" x2="65.25" y2="31.25" width="0.5" layer="46"/>
<wire x1="118.75" y1="31.25" x2="102.75" y2="31.25" width="0.5" layer="46"/>
<wire x1="102.75" y1="44.75" x2="118.75" y2="44.75" width="0.5" layer="46"/>
<wire x1="74.25" y1="44.75" x2="74.25" y2="42.625" width="0.5" layer="46"/>
<wire x1="74.25" y1="42" x2="74.25" y2="38.3125" width="0.5" layer="46"/>
<wire x1="74.25" y1="37.6875" x2="74.25" y2="34.25" width="0.5" layer="46"/>
<wire x1="74.25" y1="33.5" x2="74.25" y2="31.25" width="0.5" layer="46"/>
<wire x1="102.75" y1="44.75" x2="102.75" y2="42.625" width="0.5" layer="46"/>
<wire x1="102.75" y1="42" x2="102.75" y2="38.3125" width="0.5" layer="46"/>
<wire x1="102.75" y1="37.6875" x2="102.75" y2="34.125" width="0.5" layer="46"/>
<wire x1="102.75" y1="33.5" x2="102.75" y2="31.25" width="0.5" layer="46"/>
<wire x1="92.000025" y1="9.499996875" x2="64.45475" y2="30.68498125" width="0.5" layer="46" curve="-75.127654"/>
<wire x1="119.54524375" y1="30.68498125" x2="92.999821875" y2="9.5175375" width="0.5" layer="46" curve="-73.117158"/>
<wire x1="91.999975" y1="66.499996875" x2="119.54524375" y2="45.3150125" width="0.5" layer="46" curve="-75.127656"/>
<wire x1="64.45475625" y1="45.31501875" x2="91.000178125" y2="66.482453125" width="0.5" layer="46" curve="-73.117163"/>
<text>CoinKit Prototype</text>
<wire x1="5.75" y1="111.75" x2="14.75" y2="111.75" width="0.5" layer="46"/>
<wire x1="14.75" y1="98.25" x2="5.75" y2="98.25" width="0.5" layer="46"/>
<wire x1="59.25" y1="98.25" x2="43.25" y2="98.25" width="0.5" layer="46"/>
<wire x1="43.25" y1="111.75" x2="59.25" y2="111.75" width="0.5" layer="46"/>
<wire x1="14.75" y1="111.75" x2="14.75" y2="109.625" width="0.5" layer="46"/>
<wire x1="14.75" y1="109" x2="14.75" y2="105.3125" width="0.5" layer="46"/>
<wire x1="14.75" y1="104.6875" x2="14.75" y2="101.25" width="0.5" layer="46"/>
<wire x1="14.75" y1="100.5" x2="14.75" y2="98.25" width="0.5" layer="46"/>
<wire x1="43.25" y1="111.75" x2="43.25" y2="109.625" width="0.5" layer="46"/>
<wire x1="43.25" y1="109" x2="43.25" y2="105.3125" width="0.5" layer="46"/>
<wire x1="43.25" y1="104.6875" x2="43.25" y2="101.125" width="0.5" layer="46"/>
<wire x1="43.25" y1="100.5" x2="43.25" y2="98.25" width="0.5" layer="46"/>
<wire x1="32.500025" y1="76.499996875" x2="4.95475" y2="97.68498125" width="0.5" layer="46" curve="-75.127654"/>
<wire x1="60.04524375" y1="97.68498125" x2="33.499821875" y2="76.5175375" width="0.5" layer="46" curve="-73.117158"/>
<wire x1="32.499975" y1="133.499996875" x2="60.04524375" y2="112.3150125" width="0.5" layer="46" curve="-75.127656"/>
<wire x1="4.95475625" y1="112.31501875" x2="31.500178125" y2="133.482453125" width="0.5" layer="46" curve="-73.117163"/>
<text>CoinKit Prototype</text>
<wire x1="65.25" y1="111.75" x2="74.25" y2="111.75" width="0.5" layer="46"/>
<wire x1="74.25" y1="98.25" x2="65.25" y2="98.25" width="0.5" layer="46"/>
<wire x1="118.75" y1="98.25" x2="102.75" y2="98.25" width="0.5" layer="46"/>
<wire x1="102.75" y1="111.75" x2="118.75" y2="111.75" width="0.5" layer="46"/>
<wire x1="74.25" y1="111.75" x2="74.25" y2="109.625" width="0.5" layer="46"/>
<wire x1="74.25" y1="109" x2="74.25" y2="105.3125" width="0.5" layer="46"/>
<wire x1="74.25" y1="104.6875" x2="74.25" y2="101.25" width="0.5" layer="46"/>
<wire x1="74.25" y1="100.5" x2="74.25" y2="98.25" width="0.5" layer="46"/>
<wire x1="102.75" y1="111.75" x2="102.75" y2="109.625" width="0.5" layer="46"/>
<wire x1="102.75" y1="109" x2="102.75" y2="105.3125" width="0.5" layer="46"/>
<wire x1="102.75" y1="104.6875" x2="102.75" y2="101.125" width="0.5" layer="46"/>
<wire x1="102.75" y1="100.5" x2="102.75" y2="98.25" width="0.5" layer="46"/>
<wire x1="92.000025" y1="76.499996875" x2="64.45475" y2="97.68498125" width="0.5" layer="46" curve="-75.127654"/>
<wire x1="119.54524375" y1="97.68498125" x2="92.999821875" y2="76.5175375" width="0.5" layer="46" curve="-73.117158"/>
<wire x1="91.999975" y1="133.499996875" x2="119.54524375" y2="112.3150125" width="0.5" layer="46" curve="-75.127656"/>
<wire x1="64.45475625" y1="112.31501875" x2="91.000178125" y2="133.482453125" width="0.5" layer="46" curve="-73.117163"/>
<text>CoinKit Prototype</text>
<wire x1="124.75" y1="44.75" x2="133.75" y2="44.75" width="0.5" layer="46"/>
<wire x1="133.75" y1="31.25" x2="124.75" y2="31.25" width="0.5" layer="46"/>
<wire x1="178.25" y1="31.25" x2="162.25" y2="31.25" width="0.5" layer="46"/>
<wire x1="162.25" y1="44.75" x2="178.25" y2="44.75" width="0.5" layer="46"/>
<wire x1="133.75" y1="44.75" x2="133.75" y2="42.625" width="0.5" layer="46"/>
<wire x1="133.75" y1="42" x2="133.75" y2="38.3125" width="0.5" layer="46"/>
<wire x1="133.75" y1="37.6875" x2="133.75" y2="34.25" width="0.5" layer="46"/>
<wire x1="133.75" y1="33.5" x2="133.75" y2="31.25" width="0.5" layer="46"/>
<wire x1="162.25" y1="44.75" x2="162.25" y2="42.625" width="0.5" layer="46"/>
<wire x1="162.25" y1="42" x2="162.25" y2="38.3125" width="0.5" layer="46"/>
<wire x1="162.25" y1="37.6875" x2="162.25" y2="34.125" width="0.5" layer="46"/>
<wire x1="162.25" y1="33.5" x2="162.25" y2="31.25" width="0.5" layer="46"/>
<wire x1="151.500025" y1="9.499996875" x2="123.95475" y2="30.68498125" width="0.5" layer="46" curve="-75.127654"/>
<wire x1="179.04524375" y1="30.68498125" x2="152.499821875" y2="9.5175375" width="0.5" layer="46" curve="-73.117158"/>
<wire x1="151.499975" y1="66.499996875" x2="179.04524375" y2="45.3150125" width="0.5" layer="46" curve="-75.127656"/>
<wire x1="123.95475625" y1="45.31501875" x2="150.500178125" y2="66.482453125" width="0.5" layer="46" curve="-73.117163"/>
<text>CoinKit Prototype</text>
<wire x1="124.75" y1="111.75" x2="133.75" y2="111.75" width="0.5" layer="46"/>
<wire x1="133.75" y1="98.25" x2="124.75" y2="98.25" width="0.5" layer="46"/>
<wire x1="178.25" y1="98.25" x2="162.25" y2="98.25" width="0.5" layer="46"/>
<wire x1="162.25" y1="111.75" x2="178.25" y2="111.75" width="0.5" layer="46"/>
<wire x1="133.75" y1="111.75" x2="133.75" y2="109.625" width="0.5" layer="46"/>
<wire x1="133.75" y1="109" x2="133.75" y2="105.3125" width="0.5" layer="46"/>
<wire x1="133.75" y1="104.6875" x2="133.75" y2="101.25" width="0.5" layer="46"/>
<wire x1="133.75" y1="100.5" x2="133.75" y2="98.25" width="0.5" layer="46"/>
<wire x1="162.25" y1="111.75" x2="162.25" y2="109.625" width="0.5" layer="46"/>
<wire x1="162.25" y1="109" x2="162.25" y2="105.3125" width="0.5" layer="46"/>
<wire x1="162.25" y1="104.6875" x2="162.25" y2="101.125" width="0.5" layer="46"/>
<wire x1="162.25" y1="100.5" x2="162.25" y2="98.25" width="0.5" layer="46"/>
<wire x1="151.500025" y1="76.499996875" x2="123.95475" y2="97.68498125" width="0.5" layer="46" curve="-75.127654"/>
<wire x1="179.04524375" y1="97.68498125" x2="152.499821875" y2="76.5175375" width="0.5" layer="46" curve="-73.117158"/>
<wire x1="151.499975" y1="133.499996875" x2="179.04524375" y2="112.3150125" width="0.5" layer="46" curve="-75.127656"/>
<wire x1="123.95475625" y1="112.31501875" x2="150.500178125" y2="133.482453125" width="0.5" layer="46" curve="-73.117163"/>
<text>CoinKit Prototype</text>
<wire x1="5.75" y1="178.75" x2="14.75" y2="178.75" width="0.5" layer="46"/>
<wire x1="14.75" y1="165.25" x2="5.75" y2="165.25" width="0.5" layer="46"/>
<wire x1="59.25" y1="165.25" x2="43.25" y2="165.25" width="0.5" layer="46"/>
<wire x1="43.25" y1="178.75" x2="59.25" y2="178.75" width="0.5" layer="46"/>
<wire x1="14.75" y1="178.75" x2="14.75" y2="176.625" width="0.5" layer="46"/>
<wire x1="14.75" y1="176" x2="14.75" y2="172.3125" width="0.5" layer="46"/>
<wire x1="14.75" y1="171.6875" x2="14.75" y2="168.25" width="0.5" layer="46"/>
<wire x1="14.75" y1="167.5" x2="14.75" y2="165.25" width="0.5" layer="46"/>
<wire x1="43.25" y1="178.75" x2="43.25" y2="176.625" width="0.5" layer="46"/>
<wire x1="43.25" y1="176" x2="43.25" y2="172.3125" width="0.5" layer="46"/>
<wire x1="43.25" y1="171.6875" x2="43.25" y2="168.125" width="0.5" layer="46"/>
<wire x1="43.25" y1="167.5" x2="43.25" y2="165.25" width="0.5" layer="46"/>
<wire x1="32.500025" y1="143.499996875" x2="4.95475" y2="164.68498125" width="0.5" layer="46" curve="-75.127654"/>
<wire x1="60.04524375" y1="164.68498125" x2="33.499821875" y2="143.5175375" width="0.5" layer="46" curve="-73.117158"/>
<wire x1="32.499975" y1="200.499996875" x2="60.04524375" y2="179.3150125" width="0.5" layer="46" curve="-75.127656"/>
<wire x1="4.95475625" y1="179.31501875" x2="31.500178125" y2="200.482453125" width="0.5" layer="46" curve="-73.117163"/>
<text>CoinKit Prototype</text>
<wire x1="65.25" y1="178.75" x2="74.25" y2="178.75" width="0.5" layer="46"/>
<wire x1="74.25" y1="165.25" x2="65.25" y2="165.25" width="0.5" layer="46"/>
<wire x1="118.75" y1="165.25" x2="102.75" y2="165.25" width="0.5" layer="46"/>
<wire x1="102.75" y1="178.75" x2="118.75" y2="178.75" width="0.5" layer="46"/>
<wire x1="74.25" y1="178.75" x2="74.25" y2="176.625" width="0.5" layer="46"/>
<wire x1="74.25" y1="176" x2="74.25" y2="172.3125" width="0.5" layer="46"/>
<wire x1="74.25" y1="171.6875" x2="74.25" y2="168.25" width="0.5" layer="46"/>
<wire x1="74.25" y1="167.5" x2="74.25" y2="165.25" width="0.5" layer="46"/>
<wire x1="102.75" y1="178.75" x2="102.75" y2="176.625" width="0.5" layer="46"/>
<wire x1="102.75" y1="176" x2="102.75" y2="172.3125" width="0.5" layer="46"/>
<wire x1="102.75" y1="171.6875" x2="102.75" y2="168.125" width="0.5" layer="46"/>
<wire x1="102.75" y1="167.5" x2="102.75" y2="165.25" width="0.5" layer="46"/>
<wire x1="92.000025" y1="143.499996875" x2="64.45475" y2="164.68498125" width="0.5" layer="46" curve="-75.127654"/>
<wire x1="119.54524375" y1="164.68498125" x2="92.999821875" y2="143.5175375" width="0.5" layer="46" curve="-73.117158"/>
<wire x1="91.999975" y1="200.499996875" x2="119.54524375" y2="179.3150125" width="0.5" layer="46" curve="-75.127656"/>
<wire x1="64.45475625" y1="179.31501875" x2="91.000178125" y2="200.482453125" width="0.5" layer="46" curve="-73.117163"/>
<text>CoinKit Prototype</text>
<wire x1="124.75" y1="178.75" x2="133.75" y2="178.75" width="0.5" layer="46"/>
<wire x1="133.75" y1="165.25" x2="124.75" y2="165.25" width="0.5" layer="46"/>
<wire x1="178.25" y1="165.25" x2="162.25" y2="165.25" width="0.5" layer="46"/>
<wire x1="162.25" y1="178.75" x2="178.25" y2="178.75" width="0.5" layer="46"/>
<wire x1="133.75" y1="178.75" x2="133.75" y2="176.625" width="0.5" layer="46"/>
<wire x1="133.75" y1="176" x2="133.75" y2="172.3125" width="0.5" layer="46"/>
<wire x1="133.75" y1="171.6875" x2="133.75" y2="168.25" width="0.5" layer="46"/>
<wire x1="133.75" y1="167.5" x2="133.75" y2="165.25" width="0.5" layer="46"/>
<wire x1="162.25" y1="178.75" x2="162.25" y2="176.625" width="0.5" layer="46"/>
<wire x1="162.25" y1="176" x2="162.25" y2="172.3125" width="0.5" layer="46"/>
<wire x1="162.25" y1="171.6875" x2="162.25" y2="168.125" width="0.5" layer="46"/>
<wire x1="162.25" y1="167.5" x2="162.25" y2="165.25" width="0.5" layer="46"/>
<wire x1="151.500025" y1="143.499996875" x2="123.95475" y2="164.68498125" width="0.5" layer="46" curve="-75.127654"/>
<wire x1="179.04524375" y1="164.68498125" x2="152.499821875" y2="143.5175375" width="0.5" layer="46" curve="-73.117158"/>
<wire x1="151.499975" y1="200.499996875" x2="179.04524375" y2="179.3150125" width="0.5" layer="46" curve="-75.127656"/>
<wire x1="123.95475625" y1="179.31501875" x2="150.500178125" y2="200.482453125" width="0.5" layer="46" curve="-73.117163"/>
<text>CoinKit Prototype</text>
<wire x1="184.75" y1="44.75" x2="193.75" y2="44.75" width="0.5" layer="46"/>
<wire x1="193.75" y1="31.25" x2="184.75" y2="31.25" width="0.5" layer="46"/>
<wire x1="238.25" y1="31.25" x2="222.25" y2="31.25" width="0.5" layer="46"/>
<wire x1="222.25" y1="44.75" x2="238.25" y2="44.75" width="0.5" layer="46"/>
<wire x1="193.75" y1="44.75" x2="193.75" y2="42.625" width="0.5" layer="46"/>
<wire x1="193.75" y1="42" x2="193.75" y2="38.3125" width="0.5" layer="46"/>
<wire x1="193.75" y1="37.6875" x2="193.75" y2="34.25" width="0.5" layer="46"/>
<wire x1="193.75" y1="33.5" x2="193.75" y2="31.25" width="0.5" layer="46"/>
<wire x1="222.25" y1="44.75" x2="222.25" y2="42.625" width="0.5" layer="46"/>
<wire x1="222.25" y1="42" x2="222.25" y2="38.3125" width="0.5" layer="46"/>
<wire x1="222.25" y1="37.6875" x2="222.25" y2="34.125" width="0.5" layer="46"/>
<wire x1="222.25" y1="33.5" x2="222.25" y2="31.25" width="0.5" layer="46"/>
<wire x1="211.500025" y1="9.499996875" x2="183.95475" y2="30.68498125" width="0.5" layer="46" curve="-75.127654"/>
<wire x1="239.04524375" y1="30.68498125" x2="212.499821875" y2="9.5175375" width="0.5" layer="46" curve="-73.117158"/>
<wire x1="211.499975" y1="66.499996875" x2="239.04524375" y2="45.3150125" width="0.5" layer="46" curve="-75.127656"/>
<wire x1="183.95475625" y1="45.31501875" x2="210.500178125" y2="66.482453125" width="0.5" layer="46" curve="-73.117163"/>
<text>CoinKit Prototype</text>
<wire x1="184.75" y1="111.75" x2="193.75" y2="111.75" width="0.5" layer="46"/>
<wire x1="193.75" y1="98.25" x2="184.75" y2="98.25" width="0.5" layer="46"/>
<wire x1="238.25" y1="98.25" x2="222.25" y2="98.25" width="0.5" layer="46"/>
<wire x1="222.25" y1="111.75" x2="238.25" y2="111.75" width="0.5" layer="46"/>
<wire x1="193.75" y1="111.75" x2="193.75" y2="109.625" width="0.5" layer="46"/>
<wire x1="193.75" y1="109" x2="193.75" y2="105.3125" width="0.5" layer="46"/>
<wire x1="193.75" y1="104.6875" x2="193.75" y2="101.25" width="0.5" layer="46"/>
<wire x1="193.75" y1="100.5" x2="193.75" y2="98.25" width="0.5" layer="46"/>
<wire x1="222.25" y1="111.75" x2="222.25" y2="109.625" width="0.5" layer="46"/>
<wire x1="222.25" y1="109" x2="222.25" y2="105.3125" width="0.5" layer="46"/>
<wire x1="222.25" y1="104.6875" x2="222.25" y2="101.125" width="0.5" layer="46"/>
<wire x1="222.25" y1="100.5" x2="222.25" y2="98.25" width="0.5" layer="46"/>
<wire x1="211.500025" y1="76.499996875" x2="183.95475" y2="97.68498125" width="0.5" layer="46" curve="-75.127654"/>
<wire x1="239.04524375" y1="97.68498125" x2="212.499821875" y2="76.5175375" width="0.5" layer="46" curve="-73.117158"/>
<wire x1="211.499975" y1="133.499996875" x2="239.04524375" y2="112.3150125" width="0.5" layer="46" curve="-75.127656"/>
<wire x1="183.95475625" y1="112.31501875" x2="210.500178125" y2="133.482453125" width="0.5" layer="46" curve="-73.117163"/>
<text>CoinKit Prototype</text>
<wire x1="184.75" y1="178.75" x2="193.75" y2="178.75" width="0.5" layer="46"/>
<wire x1="193.75" y1="165.25" x2="184.75" y2="165.25" width="0.5" layer="46"/>
<wire x1="238.25" y1="165.25" x2="222.25" y2="165.25" width="0.5" layer="46"/>
<wire x1="222.25" y1="178.75" x2="238.25" y2="178.75" width="0.5" layer="46"/>
<wire x1="193.75" y1="178.75" x2="193.75" y2="176.625" width="0.5" layer="46"/>
<wire x1="193.75" y1="176" x2="193.75" y2="172.3125" width="0.5" layer="46"/>
<wire x1="193.75" y1="171.6875" x2="193.75" y2="168.25" width="0.5" layer="46"/>
<wire x1="193.75" y1="167.5" x2="193.75" y2="165.25" width="0.5" layer="46"/>
<wire x1="222.25" y1="178.75" x2="222.25" y2="176.625" width="0.5" layer="46"/>
<wire x1="222.25" y1="176" x2="222.25" y2="172.3125" width="0.5" layer="46"/>
<wire x1="222.25" y1="171.6875" x2="222.25" y2="168.125" width="0.5" layer="46"/>
<wire x1="222.25" y1="167.5" x2="222.25" y2="165.25" width="0.5" layer="46"/>
<wire x1="211.500025" y1="143.499996875" x2="183.95475" y2="164.68498125" width="0.5" layer="46" curve="-75.127654"/>
<wire x1="239.04524375" y1="164.68498125" x2="212.499821875" y2="143.5175375" width="0.5" layer="46" curve="-73.117158"/>
<wire x1="211.499975" y1="200.499996875" x2="239.04524375" y2="179.3150125" width="0.5" layer="46" curve="-75.127656"/>
<wire x1="183.95475625" y1="179.31501875" x2="210.500178125" y2="200.482453125" width="0.5" layer="46" curve="-73.117163"/>
<text>GND</text>
<text>+34V</text>
<wire x1="0" y1="210" x2="245" y2="210" width="0.254" layer="20"/>
<text>CoinKit Prototype (x12)</text>
</plain>
<libraries>
<library name="CoinKit">
<packages>
<package name="8-SMD">
</package>
<package name="MDB">
</package>
<package name="TL3315NF100Q">
<description>http://spec_sheets.e-switch.com/specs/P010336.pdf</description>
</package>
<package name="CL503">
<description>http://ce.citizen.co.jp/up_img/product/KF9Gun57LXzH/CL-503_e.pdf</description>
</package>
<package name="0402">
</package>
<package name="ESP38-SMD-1.25-18X25MM">
</package>
<package name="CAP_6.3MMX6.3MM">
</package>
<package name="7443551111">
</package>
<package name="QFN10">
</package>
<package name="SOD-128">
</package>
<package name="FIDUCIAL">
</package>
</packages>
</library>
<library name="resistor">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;map name="nav_main"&gt;
&lt;area shape="rect" coords="0,1,140,23" href="../military_specs.asp" title=""&gt;
&lt;area shape="rect" coords="0,24,140,51" href="../about.asp" title=""&gt;
&lt;area shape="rect" coords="1,52,140,77" href="../rfq.asp" title=""&gt;
&lt;area shape="rect" coords="0,78,139,103" href="../products.asp" title=""&gt;
&lt;area shape="rect" coords="1,102,138,128" href="../excess_inventory.asp" title=""&gt;
&lt;area shape="rect" coords="1,129,138,150" href="../edge.asp" title=""&gt;
&lt;area shape="rect" coords="1,151,139,178" href="../industry_links.asp" title=""&gt;
&lt;area shape="rect" coords="0,179,139,201" href="../comments.asp" title=""&gt;
&lt;area shape="rect" coords="1,203,138,231" href="../directory.asp" title=""&gt;
&lt;area shape="default" nohref&gt;
&lt;/map&gt;

&lt;html&gt;

&lt;title&gt;&lt;/title&gt;

 &lt;LINK REL="StyleSheet" TYPE="text/css" HREF="style-sheet.css"&gt;

&lt;body bgcolor="#ffffff" text="#000000" marginwidth="0" marginheight="0" topmargin="0" leftmargin="0"&gt;
&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0 height="55%"&gt;
&lt;tr valign="top"&gt;

&lt;/td&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;/BODY&gt;&lt;/HTML&gt;</description>
<packages>
<package name="C1206K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1206 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3216</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="S1" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="S2" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="D2" library="CoinKit" package="CL503" value="CL503"/>
<element name="R7" library="CoinKit" package="0402" value="10k"/>
<element name="R14" library="CoinKit" package="0402" value="250R"/>
<element name="R12" library="CoinKit" package="0402" value="155R"/>
<element name="R13" library="CoinKit" package="0402" value="325R"/>
<element name="C6" library="CoinKit" package="0402" value="22uF"/>
<element name="C7" library="CoinKit" package="0402" value="0.1uF"/>
<element name="R10" library="CoinKit" package="0402" value="50R"/>
<element name="R11" library="CoinKit" package="0402" value="180R"/>
<element name="R9" library="CoinKit" package="0402" value="50R"/>
<element name="IC3" library="CoinKit" package="8-SMD" value="HCPL2731S"/>
<element name="U$5" library="CoinKit" package="MDB" value="MDB"/>
<element name="U$6" library="CoinKit" package="MDB" value="MDB"/>
<element name="R8" library="CoinKit" package="0402" value="10K"/>
<element name="SMPS1:IC1" library="CoinKit" package="QFN10" value="MP2562"/>
<element name="SMPS1:R5" library="CoinKit" package="0402" value="100k"/>
<element name="SMPS1:R6" library="CoinKit" package="0402" value="90.21k"/>
<element name="SMPS1:R4" library="CoinKit" package="0402" value="24.9k"/>
<element name="SMPS1:C3" library="CoinKit" package="0402" value="220pF"/>
<element name="SMPS1:R3" library="CoinKit" package="0402" value="120k"/>
<element name="SMPS1:R1" library="CoinKit" package="0402" value="127k"/>
<element name="SMPS1:R2" library="CoinKit" package="0402" value="40.2k"/>
<element name="SMPS1:C2" library="CoinKit" package="0402" value="22uF"/>
<element name="SMPS1:L1" library="CoinKit" package="7443551111" value="11.3uH"/>
<element name="IC2" library="CoinKit" package="ESP38-SMD-1.25-18X25MM" value="MODULE-WIFI-ESP-WROOM-32"/>
<element name="SMPS1:C5" library="CoinKit" package="CAP_6.3MMX6.3MM" value="22uF"/>
<element name="SMPS1:C1" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:C4" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:U$1" library="CoinKit" package="SOD-128" value="RB058LAM150TR"/>
<element name="S3" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="S4" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="D1" library="CoinKit" package="CL503" value="CL503"/>
<element name="R1" library="CoinKit" package="0402" value="10k"/>
<element name="R2" library="CoinKit" package="0402" value="250R"/>
<element name="R3" library="CoinKit" package="0402" value="155R"/>
<element name="R4" library="CoinKit" package="0402" value="325R"/>
<element name="C1" library="CoinKit" package="0402" value="22uF"/>
<element name="C2" library="CoinKit" package="0402" value="0.1uF"/>
<element name="R5" library="CoinKit" package="0402" value="50R"/>
<element name="R6" library="CoinKit" package="0402" value="180R"/>
<element name="R15" library="CoinKit" package="0402" value="50R"/>
<element name="IC1" library="CoinKit" package="8-SMD" value="HCPL2731S"/>
<element name="U$1" library="CoinKit" package="MDB" value="MDB"/>
<element name="U$2" library="CoinKit" package="MDB" value="MDB"/>
<element name="R16" library="CoinKit" package="0402" value="10K"/>
<element name="SMPS1:IC2" library="CoinKit" package="QFN10" value="MP2562"/>
<element name="SMPS1:R7" library="CoinKit" package="0402" value="100k"/>
<element name="SMPS1:R8" library="CoinKit" package="0402" value="90.21k"/>
<element name="SMPS1:R9" library="CoinKit" package="0402" value="24.9k"/>
<element name="SMPS1:C6" library="CoinKit" package="0402" value="220pF"/>
<element name="SMPS1:R10" library="CoinKit" package="0402" value="120k"/>
<element name="SMPS1:R11" library="CoinKit" package="0402" value="127k"/>
<element name="SMPS1:R12" library="CoinKit" package="0402" value="40.2k"/>
<element name="SMPS1:C7" library="CoinKit" package="0402" value="22uF"/>
<element name="SMPS1:L2" library="CoinKit" package="7443551111" value="11.3uH"/>
<element name="IC4" library="CoinKit" package="ESP38-SMD-1.25-18X25MM" value="MODULE-WIFI-ESP-WROOM-32"/>
<element name="SMPS1:C8" library="CoinKit" package="CAP_6.3MMX6.3MM" value="22uF"/>
<element name="SMPS1:C9" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:C10" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:U$2" library="CoinKit" package="SOD-128" value="RB058LAM150TR"/>
<element name="S5" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="S6" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="D3" library="CoinKit" package="CL503" value="CL503"/>
<element name="R17" library="CoinKit" package="0402" value="10k"/>
<element name="R18" library="CoinKit" package="0402" value="250R"/>
<element name="R19" library="CoinKit" package="0402" value="155R"/>
<element name="R20" library="CoinKit" package="0402" value="325R"/>
<element name="C3" library="CoinKit" package="0402" value="22uF"/>
<element name="C4" library="CoinKit" package="0402" value="0.1uF"/>
<element name="R21" library="CoinKit" package="0402" value="50R"/>
<element name="R22" library="CoinKit" package="0402" value="180R"/>
<element name="R23" library="CoinKit" package="0402" value="50R"/>
<element name="IC5" library="CoinKit" package="8-SMD" value="HCPL2731S"/>
<element name="U$3" library="CoinKit" package="MDB" value="MDB"/>
<element name="U$4" library="CoinKit" package="MDB" value="MDB"/>
<element name="R24" library="CoinKit" package="0402" value="10K"/>
<element name="SMPS1:IC3" library="CoinKit" package="QFN10" value="MP2562"/>
<element name="SMPS1:R13" library="CoinKit" package="0402" value="100k"/>
<element name="SMPS1:R14" library="CoinKit" package="0402" value="90.21k"/>
<element name="SMPS1:R15" library="CoinKit" package="0402" value="24.9k"/>
<element name="SMPS1:C11" library="CoinKit" package="0402" value="220pF"/>
<element name="SMPS1:R16" library="CoinKit" package="0402" value="120k"/>
<element name="SMPS1:R17" library="CoinKit" package="0402" value="127k"/>
<element name="SMPS1:R18" library="CoinKit" package="0402" value="40.2k"/>
<element name="SMPS1:C12" library="CoinKit" package="0402" value="22uF"/>
<element name="SMPS1:L3" library="CoinKit" package="7443551111" value="11.3uH"/>
<element name="IC6" library="CoinKit" package="ESP38-SMD-1.25-18X25MM" value="MODULE-WIFI-ESP-WROOM-32"/>
<element name="SMPS1:C13" library="CoinKit" package="CAP_6.3MMX6.3MM" value="22uF"/>
<element name="SMPS1:C14" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:C15" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:U$3" library="CoinKit" package="SOD-128" value="RB058LAM150TR"/>
<element name="S7" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="S8" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="D4" library="CoinKit" package="CL503" value="CL503"/>
<element name="R25" library="CoinKit" package="0402" value="10k"/>
<element name="R26" library="CoinKit" package="0402" value="250R"/>
<element name="R27" library="CoinKit" package="0402" value="155R"/>
<element name="R28" library="CoinKit" package="0402" value="325R"/>
<element name="C5" library="CoinKit" package="0402" value="22uF"/>
<element name="C8" library="CoinKit" package="0402" value="0.1uF"/>
<element name="R29" library="CoinKit" package="0402" value="50R"/>
<element name="R30" library="CoinKit" package="0402" value="180R"/>
<element name="R31" library="CoinKit" package="0402" value="50R"/>
<element name="IC7" library="CoinKit" package="8-SMD" value="HCPL2731S"/>
<element name="U$7" library="CoinKit" package="MDB" value="MDB"/>
<element name="U$8" library="CoinKit" package="MDB" value="MDB"/>
<element name="R32" library="CoinKit" package="0402" value="10K"/>
<element name="SMPS1:IC4" library="CoinKit" package="QFN10" value="MP2562"/>
<element name="SMPS1:R19" library="CoinKit" package="0402" value="100k"/>
<element name="SMPS1:R20" library="CoinKit" package="0402" value="90.21k"/>
<element name="SMPS1:R21" library="CoinKit" package="0402" value="24.9k"/>
<element name="SMPS1:C16" library="CoinKit" package="0402" value="220pF"/>
<element name="SMPS1:R22" library="CoinKit" package="0402" value="120k"/>
<element name="SMPS1:R23" library="CoinKit" package="0402" value="127k"/>
<element name="SMPS1:R24" library="CoinKit" package="0402" value="40.2k"/>
<element name="SMPS1:C17" library="CoinKit" package="0402" value="22uF"/>
<element name="SMPS1:L4" library="CoinKit" package="7443551111" value="11.3uH"/>
<element name="IC8" library="CoinKit" package="ESP38-SMD-1.25-18X25MM" value="MODULE-WIFI-ESP-WROOM-32"/>
<element name="SMPS1:C18" library="CoinKit" package="CAP_6.3MMX6.3MM" value="22uF"/>
<element name="SMPS1:C19" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:C20" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:U$4" library="CoinKit" package="SOD-128" value="RB058LAM150TR"/>
<element name="S9" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="S10" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="D5" library="CoinKit" package="CL503" value="CL503"/>
<element name="R33" library="CoinKit" package="0402" value="10k"/>
<element name="R34" library="CoinKit" package="0402" value="250R"/>
<element name="R35" library="CoinKit" package="0402" value="155R"/>
<element name="R36" library="CoinKit" package="0402" value="325R"/>
<element name="C9" library="CoinKit" package="0402" value="22uF"/>
<element name="C10" library="CoinKit" package="0402" value="0.1uF"/>
<element name="R37" library="CoinKit" package="0402" value="50R"/>
<element name="R38" library="CoinKit" package="0402" value="180R"/>
<element name="R39" library="CoinKit" package="0402" value="50R"/>
<element name="IC9" library="CoinKit" package="8-SMD" value="HCPL2731S"/>
<element name="U$9" library="CoinKit" package="MDB" value="MDB"/>
<element name="U$10" library="CoinKit" package="MDB" value="MDB"/>
<element name="R40" library="CoinKit" package="0402" value="10K"/>
<element name="SMPS1:IC5" library="CoinKit" package="QFN10" value="MP2562"/>
<element name="SMPS1:R25" library="CoinKit" package="0402" value="100k"/>
<element name="SMPS1:R26" library="CoinKit" package="0402" value="90.21k"/>
<element name="SMPS1:R27" library="CoinKit" package="0402" value="24.9k"/>
<element name="SMPS1:C21" library="CoinKit" package="0402" value="220pF"/>
<element name="SMPS1:R28" library="CoinKit" package="0402" value="120k"/>
<element name="SMPS1:R29" library="CoinKit" package="0402" value="127k"/>
<element name="SMPS1:R30" library="CoinKit" package="0402" value="40.2k"/>
<element name="SMPS1:C22" library="CoinKit" package="0402" value="22uF"/>
<element name="SMPS1:L5" library="CoinKit" package="7443551111" value="11.3uH"/>
<element name="IC10" library="CoinKit" package="ESP38-SMD-1.25-18X25MM" value="MODULE-WIFI-ESP-WROOM-32"/>
<element name="SMPS1:C23" library="CoinKit" package="CAP_6.3MMX6.3MM" value="22uF"/>
<element name="SMPS1:C24" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:C25" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:U$5" library="CoinKit" package="SOD-128" value="RB058LAM150TR"/>
<element name="S11" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="S12" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="D6" library="CoinKit" package="CL503" value="CL503"/>
<element name="R41" library="CoinKit" package="0402" value="10k"/>
<element name="R42" library="CoinKit" package="0402" value="250R"/>
<element name="R43" library="CoinKit" package="0402" value="155R"/>
<element name="R44" library="CoinKit" package="0402" value="325R"/>
<element name="C11" library="CoinKit" package="0402" value="22uF"/>
<element name="C12" library="CoinKit" package="0402" value="0.1uF"/>
<element name="R45" library="CoinKit" package="0402" value="50R"/>
<element name="R46" library="CoinKit" package="0402" value="180R"/>
<element name="R47" library="CoinKit" package="0402" value="50R"/>
<element name="IC11" library="CoinKit" package="8-SMD" value="HCPL2731S"/>
<element name="U$11" library="CoinKit" package="MDB" value="MDB"/>
<element name="U$12" library="CoinKit" package="MDB" value="MDB"/>
<element name="R48" library="CoinKit" package="0402" value="10K"/>
<element name="SMPS1:IC6" library="CoinKit" package="QFN10" value="MP2562"/>
<element name="SMPS1:R31" library="CoinKit" package="0402" value="100k"/>
<element name="SMPS1:R32" library="CoinKit" package="0402" value="90.21k"/>
<element name="SMPS1:R33" library="CoinKit" package="0402" value="24.9k"/>
<element name="SMPS1:C26" library="CoinKit" package="0402" value="220pF"/>
<element name="SMPS1:R34" library="CoinKit" package="0402" value="120k"/>
<element name="SMPS1:R35" library="CoinKit" package="0402" value="127k"/>
<element name="SMPS1:R36" library="CoinKit" package="0402" value="40.2k"/>
<element name="SMPS1:C27" library="CoinKit" package="0402" value="22uF"/>
<element name="SMPS1:L6" library="CoinKit" package="7443551111" value="11.3uH"/>
<element name="IC12" library="CoinKit" package="ESP38-SMD-1.25-18X25MM" value="MODULE-WIFI-ESP-WROOM-32"/>
<element name="SMPS1:C28" library="CoinKit" package="CAP_6.3MMX6.3MM" value="22uF"/>
<element name="SMPS1:C29" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:C30" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:U$6" library="CoinKit" package="SOD-128" value="RB058LAM150TR"/>
<element name="S13" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="S14" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="D7" library="CoinKit" package="CL503" value="CL503"/>
<element name="R49" library="CoinKit" package="0402" value="10k"/>
<element name="R50" library="CoinKit" package="0402" value="250R"/>
<element name="R51" library="CoinKit" package="0402" value="155R"/>
<element name="R52" library="CoinKit" package="0402" value="325R"/>
<element name="C13" library="CoinKit" package="0402" value="22uF"/>
<element name="C14" library="CoinKit" package="0402" value="0.1uF"/>
<element name="R53" library="CoinKit" package="0402" value="50R"/>
<element name="R54" library="CoinKit" package="0402" value="180R"/>
<element name="R55" library="CoinKit" package="0402" value="50R"/>
<element name="IC13" library="CoinKit" package="8-SMD" value="HCPL2731S"/>
<element name="U$13" library="CoinKit" package="MDB" value="MDB"/>
<element name="U$14" library="CoinKit" package="MDB" value="MDB"/>
<element name="R56" library="CoinKit" package="0402" value="10K"/>
<element name="SMPS1:IC7" library="CoinKit" package="QFN10" value="MP2562"/>
<element name="SMPS1:R37" library="CoinKit" package="0402" value="100k"/>
<element name="SMPS1:R38" library="CoinKit" package="0402" value="90.21k"/>
<element name="SMPS1:R39" library="CoinKit" package="0402" value="24.9k"/>
<element name="SMPS1:C31" library="CoinKit" package="0402" value="220pF"/>
<element name="SMPS1:R40" library="CoinKit" package="0402" value="120k"/>
<element name="SMPS1:R41" library="CoinKit" package="0402" value="127k"/>
<element name="SMPS1:R42" library="CoinKit" package="0402" value="40.2k"/>
<element name="SMPS1:C32" library="CoinKit" package="0402" value="22uF"/>
<element name="SMPS1:L7" library="CoinKit" package="7443551111" value="11.3uH"/>
<element name="IC14" library="CoinKit" package="ESP38-SMD-1.25-18X25MM" value="MODULE-WIFI-ESP-WROOM-32"/>
<element name="SMPS1:C33" library="CoinKit" package="CAP_6.3MMX6.3MM" value="22uF"/>
<element name="SMPS1:C34" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:C35" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:U$7" library="CoinKit" package="SOD-128" value="RB058LAM150TR"/>
<element name="S15" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="S16" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="D8" library="CoinKit" package="CL503" value="CL503"/>
<element name="R57" library="CoinKit" package="0402" value="10k"/>
<element name="R58" library="CoinKit" package="0402" value="250R"/>
<element name="R59" library="CoinKit" package="0402" value="155R"/>
<element name="R60" library="CoinKit" package="0402" value="325R"/>
<element name="C15" library="CoinKit" package="0402" value="22uF"/>
<element name="C16" library="CoinKit" package="0402" value="0.1uF"/>
<element name="R61" library="CoinKit" package="0402" value="50R"/>
<element name="R62" library="CoinKit" package="0402" value="180R"/>
<element name="R63" library="CoinKit" package="0402" value="50R"/>
<element name="IC15" library="CoinKit" package="8-SMD" value="HCPL2731S"/>
<element name="U$15" library="CoinKit" package="MDB" value="MDB"/>
<element name="U$16" library="CoinKit" package="MDB" value="MDB"/>
<element name="R64" library="CoinKit" package="0402" value="10K"/>
<element name="SMPS1:IC8" library="CoinKit" package="QFN10" value="MP2562"/>
<element name="SMPS1:R43" library="CoinKit" package="0402" value="100k"/>
<element name="SMPS1:R44" library="CoinKit" package="0402" value="90.21k"/>
<element name="SMPS1:R45" library="CoinKit" package="0402" value="24.9k"/>
<element name="SMPS1:C36" library="CoinKit" package="0402" value="220pF"/>
<element name="SMPS1:R46" library="CoinKit" package="0402" value="120k"/>
<element name="SMPS1:R47" library="CoinKit" package="0402" value="127k"/>
<element name="SMPS1:R48" library="CoinKit" package="0402" value="40.2k"/>
<element name="SMPS1:C37" library="CoinKit" package="0402" value="22uF"/>
<element name="SMPS1:L8" library="CoinKit" package="7443551111" value="11.3uH"/>
<element name="IC16" library="CoinKit" package="ESP38-SMD-1.25-18X25MM" value="MODULE-WIFI-ESP-WROOM-32"/>
<element name="SMPS1:C38" library="CoinKit" package="CAP_6.3MMX6.3MM" value="22uF"/>
<element name="SMPS1:C39" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:C40" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:U$8" library="CoinKit" package="SOD-128" value="RB058LAM150TR"/>
<element name="S17" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="S18" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="D9" library="CoinKit" package="CL503" value="CL503"/>
<element name="R65" library="CoinKit" package="0402" value="10k"/>
<element name="R66" library="CoinKit" package="0402" value="250R"/>
<element name="R67" library="CoinKit" package="0402" value="155R"/>
<element name="R68" library="CoinKit" package="0402" value="325R"/>
<element name="C17" library="CoinKit" package="0402" value="22uF"/>
<element name="C18" library="CoinKit" package="0402" value="0.1uF"/>
<element name="R69" library="CoinKit" package="0402" value="50R"/>
<element name="R70" library="CoinKit" package="0402" value="180R"/>
<element name="R71" library="CoinKit" package="0402" value="50R"/>
<element name="IC17" library="CoinKit" package="8-SMD" value="HCPL2731S"/>
<element name="U$17" library="CoinKit" package="MDB" value="MDB"/>
<element name="U$18" library="CoinKit" package="MDB" value="MDB"/>
<element name="R72" library="CoinKit" package="0402" value="10K"/>
<element name="SMPS1:IC9" library="CoinKit" package="QFN10" value="MP2562"/>
<element name="SMPS1:R49" library="CoinKit" package="0402" value="100k"/>
<element name="SMPS1:R50" library="CoinKit" package="0402" value="90.21k"/>
<element name="SMPS1:R51" library="CoinKit" package="0402" value="24.9k"/>
<element name="SMPS1:C41" library="CoinKit" package="0402" value="220pF"/>
<element name="SMPS1:R52" library="CoinKit" package="0402" value="120k"/>
<element name="SMPS1:R53" library="CoinKit" package="0402" value="127k"/>
<element name="SMPS1:R54" library="CoinKit" package="0402" value="40.2k"/>
<element name="SMPS1:C42" library="CoinKit" package="0402" value="22uF"/>
<element name="SMPS1:L9" library="CoinKit" package="7443551111" value="11.3uH"/>
<element name="IC18" library="CoinKit" package="ESP38-SMD-1.25-18X25MM" value="MODULE-WIFI-ESP-WROOM-32"/>
<element name="SMPS1:C43" library="CoinKit" package="CAP_6.3MMX6.3MM" value="22uF"/>
<element name="SMPS1:C44" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:C45" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:U$9" library="CoinKit" package="SOD-128" value="RB058LAM150TR"/>
<element name="S19" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="S20" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="D10" library="CoinKit" package="CL503" value="CL503"/>
<element name="R73" library="CoinKit" package="0402" value="10k"/>
<element name="R74" library="CoinKit" package="0402" value="250R"/>
<element name="R75" library="CoinKit" package="0402" value="155R"/>
<element name="R76" library="CoinKit" package="0402" value="325R"/>
<element name="C19" library="CoinKit" package="0402" value="22uF"/>
<element name="C20" library="CoinKit" package="0402" value="0.1uF"/>
<element name="R77" library="CoinKit" package="0402" value="50R"/>
<element name="R78" library="CoinKit" package="0402" value="180R"/>
<element name="R79" library="CoinKit" package="0402" value="50R"/>
<element name="IC19" library="CoinKit" package="8-SMD" value="HCPL2731S"/>
<element name="U$19" library="CoinKit" package="MDB" value="MDB"/>
<element name="U$20" library="CoinKit" package="MDB" value="MDB"/>
<element name="R80" library="CoinKit" package="0402" value="10K"/>
<element name="SMPS1:IC10" library="CoinKit" package="QFN10" value="MP2562"/>
<element name="SMPS1:R55" library="CoinKit" package="0402" value="100k"/>
<element name="SMPS1:R56" library="CoinKit" package="0402" value="90.21k"/>
<element name="SMPS1:R57" library="CoinKit" package="0402" value="24.9k"/>
<element name="SMPS1:C46" library="CoinKit" package="0402" value="220pF"/>
<element name="SMPS1:R58" library="CoinKit" package="0402" value="120k"/>
<element name="SMPS1:R59" library="CoinKit" package="0402" value="127k"/>
<element name="SMPS1:R60" library="CoinKit" package="0402" value="40.2k"/>
<element name="SMPS1:C47" library="CoinKit" package="0402" value="22uF"/>
<element name="SMPS1:L10" library="CoinKit" package="7443551111" value="11.3uH"/>
<element name="IC20" library="CoinKit" package="ESP38-SMD-1.25-18X25MM" value="MODULE-WIFI-ESP-WROOM-32"/>
<element name="SMPS1:C48" library="CoinKit" package="CAP_6.3MMX6.3MM" value="22uF"/>
<element name="SMPS1:C49" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:C50" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:U$10" library="CoinKit" package="SOD-128" value="RB058LAM150TR"/>
<element name="S21" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="S22" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="D11" library="CoinKit" package="CL503" value="CL503"/>
<element name="R81" library="CoinKit" package="0402" value="10k"/>
<element name="R82" library="CoinKit" package="0402" value="250R"/>
<element name="R83" library="CoinKit" package="0402" value="155R"/>
<element name="R84" library="CoinKit" package="0402" value="325R"/>
<element name="C21" library="CoinKit" package="0402" value="22uF"/>
<element name="C22" library="CoinKit" package="0402" value="0.1uF"/>
<element name="R85" library="CoinKit" package="0402" value="50R"/>
<element name="R86" library="CoinKit" package="0402" value="180R"/>
<element name="R87" library="CoinKit" package="0402" value="50R"/>
<element name="IC21" library="CoinKit" package="8-SMD" value="HCPL2731S"/>
<element name="U$21" library="CoinKit" package="MDB" value="MDB"/>
<element name="U$22" library="CoinKit" package="MDB" value="MDB"/>
<element name="R88" library="CoinKit" package="0402" value="10K"/>
<element name="SMPS1:IC11" library="CoinKit" package="QFN10" value="MP2562"/>
<element name="SMPS1:R61" library="CoinKit" package="0402" value="100k"/>
<element name="SMPS1:R62" library="CoinKit" package="0402" value="90.21k"/>
<element name="SMPS1:R63" library="CoinKit" package="0402" value="24.9k"/>
<element name="SMPS1:C51" library="CoinKit" package="0402" value="220pF"/>
<element name="SMPS1:R64" library="CoinKit" package="0402" value="120k"/>
<element name="SMPS1:R65" library="CoinKit" package="0402" value="127k"/>
<element name="SMPS1:R66" library="CoinKit" package="0402" value="40.2k"/>
<element name="SMPS1:C52" library="CoinKit" package="0402" value="22uF"/>
<element name="SMPS1:L11" library="CoinKit" package="7443551111" value="11.3uH"/>
<element name="IC22" library="CoinKit" package="ESP38-SMD-1.25-18X25MM" value="MODULE-WIFI-ESP-WROOM-32"/>
<element name="SMPS1:C53" library="CoinKit" package="CAP_6.3MMX6.3MM" value="22uF"/>
<element name="SMPS1:C54" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:C55" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:U$11" library="CoinKit" package="SOD-128" value="RB058LAM150TR"/>
<element name="S23" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="S24" library="CoinKit" package="TL3315NF100Q" value="TL3315"/>
<element name="D12" library="CoinKit" package="CL503" value="CL503"/>
<element name="R89" library="CoinKit" package="0402" value="10k"/>
<element name="R90" library="CoinKit" package="0402" value="250R"/>
<element name="R91" library="CoinKit" package="0402" value="155R"/>
<element name="R92" library="CoinKit" package="0402" value="325R"/>
<element name="C23" library="CoinKit" package="0402" value="22uF"/>
<element name="C24" library="CoinKit" package="0402" value="0.1uF"/>
<element name="R93" library="CoinKit" package="0402" value="50R"/>
<element name="R94" library="CoinKit" package="0402" value="180R"/>
<element name="R95" library="CoinKit" package="0402" value="50R"/>
<element name="IC23" library="CoinKit" package="8-SMD" value="HCPL2731S"/>
<element name="U$23" library="CoinKit" package="MDB" value="MDB"/>
<element name="U$24" library="CoinKit" package="MDB" value="MDB"/>
<element name="R96" library="CoinKit" package="0402" value="10K"/>
<element name="SMPS1:IC12" library="CoinKit" package="QFN10" value="MP2562"/>
<element name="SMPS1:R67" library="CoinKit" package="0402" value="100k"/>
<element name="SMPS1:R68" library="CoinKit" package="0402" value="90.21k"/>
<element name="SMPS1:R69" library="CoinKit" package="0402" value="24.9k"/>
<element name="SMPS1:C56" library="CoinKit" package="0402" value="220pF"/>
<element name="SMPS1:R70" library="CoinKit" package="0402" value="120k"/>
<element name="SMPS1:R71" library="CoinKit" package="0402" value="127k"/>
<element name="SMPS1:R72" library="CoinKit" package="0402" value="40.2k"/>
<element name="SMPS1:C57" library="CoinKit" package="0402" value="22uF"/>
<element name="SMPS1:L12" library="CoinKit" package="7443551111" value="11.3uH"/>
<element name="IC24" library="CoinKit" package="ESP38-SMD-1.25-18X25MM" value="MODULE-WIFI-ESP-WROOM-32"/>
<element name="SMPS1:C58" library="CoinKit" package="CAP_6.3MMX6.3MM" value="22uF"/>
<element name="SMPS1:C59" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:C60" library="resistor" package="C1206K" value="0.1uF"/>
<element name="SMPS1:U$12" library="CoinKit" package="SOD-128" value="RB058LAM150TR"/>
<element name="FID1" library="CoinKit" package="FIDUCIAL" value=""/>
<element name="FID2" library="CoinKit" package="FIDUCIAL" value=""/>
<element name="FID3" library="CoinKit" package="FIDUCIAL" value=""/>
<element name="FID4" library="CoinKit" package="FIDUCIAL" value=""/>
<element name="FID5" library="CoinKit" package="FIDUCIAL" value=""/>
<element name="FID6" library="CoinKit" package="FIDUCIAL" value=""/>
<element name="FID7" library="CoinKit" package="FIDUCIAL" value=""/>
<element name="FID8" library="CoinKit" package="FIDUCIAL" value=""/>
<element name="FID9" library="CoinKit" package="FIDUCIAL" value=""/>
<element name="FID10" library="CoinKit" package="FIDUCIAL" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="S1" pad="4R"/>
<contactref element="S1" pad="4S"/>
<contactref element="S1" pad="3R"/>
<contactref element="S1" pad="3S"/>
<contactref element="C6" pad="P$2"/>
<contactref element="C7" pad="P$1"/>
<contactref element="IC3" pad="5"/>
<contactref element="U$6" pad="0V"/>
<contactref element="U$5" pad="0V"/>
<contactref element="IC3" pad="3"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC2" pad="P$1"/>
<contactref element="IC2" pad="15"/>
<contactref element="IC2" pad="38"/>
<contactref element="IC2" pad="32"/>
<contactref element="SMPS1:IC1" pad="6"/>
<contactref element="SMPS1:IC1" pad="THERMAL"/>
<contactref element="SMPS1:R6" pad="P$1"/>
<contactref element="SMPS1:R4" pad="P$1"/>
<contactref element="SMPS1:R3" pad="P$1"/>
<contactref element="SMPS1:R2" pad="P$1"/>
<contactref element="SMPS1:C2" pad="P$2"/>
<contactref element="SMPS1:C5" pad="-"/>
<contactref element="SMPS1:C1" pad="2"/>
<contactref element="SMPS1:U$1" pad="P"/>
<contactref element="S5" pad="4R"/>
<contactref element="S5" pad="4S"/>
<contactref element="S5" pad="3R"/>
<contactref element="S5" pad="3S"/>
<contactref element="C3" pad="P$2"/>
<contactref element="C4" pad="P$1"/>
<contactref element="IC5" pad="5"/>
<contactref element="U$4" pad="0V"/>
<contactref element="U$3" pad="0V"/>
<contactref element="IC5" pad="3"/>
<contactref element="IC6" pad="1"/>
<contactref element="IC6" pad="P$1"/>
<contactref element="IC6" pad="15"/>
<contactref element="IC6" pad="38"/>
<contactref element="IC6" pad="32"/>
<contactref element="SMPS1:IC3" pad="6"/>
<contactref element="SMPS1:IC3" pad="THERMAL"/>
<contactref element="SMPS1:R14" pad="P$1"/>
<contactref element="SMPS1:R15" pad="P$1"/>
<contactref element="SMPS1:R16" pad="P$1"/>
<contactref element="SMPS1:R18" pad="P$1"/>
<contactref element="SMPS1:C12" pad="P$2"/>
<contactref element="SMPS1:C13" pad="-"/>
<contactref element="SMPS1:C14" pad="2"/>
<contactref element="SMPS1:U$3" pad="P"/>
<contactref element="S13" pad="4R"/>
<contactref element="S13" pad="4S"/>
<contactref element="S13" pad="3R"/>
<contactref element="S13" pad="3S"/>
<contactref element="C13" pad="P$2"/>
<contactref element="C14" pad="P$1"/>
<contactref element="IC13" pad="5"/>
<contactref element="U$14" pad="0V"/>
<contactref element="U$13" pad="0V"/>
<contactref element="IC13" pad="3"/>
<contactref element="IC14" pad="1"/>
<contactref element="IC14" pad="P$1"/>
<contactref element="IC14" pad="15"/>
<contactref element="IC14" pad="38"/>
<contactref element="IC14" pad="32"/>
<contactref element="SMPS1:IC7" pad="6"/>
<contactref element="SMPS1:IC7" pad="THERMAL"/>
<contactref element="SMPS1:R38" pad="P$1"/>
<contactref element="SMPS1:R39" pad="P$1"/>
<contactref element="SMPS1:R40" pad="P$1"/>
<contactref element="SMPS1:R42" pad="P$1"/>
<contactref element="SMPS1:C32" pad="P$2"/>
<contactref element="SMPS1:C33" pad="-"/>
<contactref element="SMPS1:C34" pad="2"/>
<contactref element="SMPS1:U$7" pad="P"/>
<contactref element="S15" pad="4R"/>
<contactref element="S15" pad="4S"/>
<contactref element="S15" pad="3R"/>
<contactref element="S15" pad="3S"/>
<contactref element="C15" pad="P$2"/>
<contactref element="C16" pad="P$1"/>
<contactref element="IC15" pad="5"/>
<contactref element="U$16" pad="0V"/>
<contactref element="U$15" pad="0V"/>
<contactref element="IC15" pad="3"/>
<contactref element="IC16" pad="1"/>
<contactref element="IC16" pad="P$1"/>
<contactref element="IC16" pad="15"/>
<contactref element="IC16" pad="38"/>
<contactref element="IC16" pad="32"/>
<contactref element="SMPS1:IC8" pad="6"/>
<contactref element="SMPS1:IC8" pad="THERMAL"/>
<contactref element="SMPS1:R44" pad="P$1"/>
<contactref element="SMPS1:R45" pad="P$1"/>
<contactref element="SMPS1:R46" pad="P$1"/>
<contactref element="SMPS1:R48" pad="P$1"/>
<contactref element="SMPS1:C37" pad="P$2"/>
<contactref element="SMPS1:C38" pad="-"/>
<contactref element="SMPS1:C39" pad="2"/>
<contactref element="SMPS1:U$8" pad="P"/>
<contactref element="S17" pad="4R"/>
<contactref element="S17" pad="4S"/>
<contactref element="S17" pad="3R"/>
<contactref element="S17" pad="3S"/>
<contactref element="C17" pad="P$2"/>
<contactref element="C18" pad="P$1"/>
<contactref element="IC17" pad="5"/>
<contactref element="U$18" pad="0V"/>
<contactref element="U$17" pad="0V"/>
<contactref element="IC17" pad="3"/>
<contactref element="IC18" pad="1"/>
<contactref element="IC18" pad="P$1"/>
<contactref element="IC18" pad="15"/>
<contactref element="IC18" pad="38"/>
<contactref element="IC18" pad="32"/>
<contactref element="SMPS1:IC9" pad="6"/>
<contactref element="SMPS1:IC9" pad="THERMAL"/>
<contactref element="SMPS1:R50" pad="P$1"/>
<contactref element="SMPS1:R51" pad="P$1"/>
<contactref element="SMPS1:R52" pad="P$1"/>
<contactref element="SMPS1:R54" pad="P$1"/>
<contactref element="SMPS1:C42" pad="P$2"/>
<contactref element="SMPS1:C43" pad="-"/>
<contactref element="SMPS1:C44" pad="2"/>
<contactref element="SMPS1:U$9" pad="P"/>
<contactref element="S23" pad="4R"/>
<contactref element="S23" pad="4S"/>
<contactref element="S23" pad="3R"/>
<contactref element="S23" pad="3S"/>
<contactref element="C23" pad="P$2"/>
<contactref element="C24" pad="P$1"/>
<contactref element="IC23" pad="5"/>
<contactref element="U$24" pad="0V"/>
<contactref element="U$23" pad="0V"/>
<contactref element="IC23" pad="3"/>
<contactref element="IC24" pad="1"/>
<contactref element="IC24" pad="P$1"/>
<contactref element="IC24" pad="15"/>
<contactref element="IC24" pad="38"/>
<contactref element="IC24" pad="32"/>
<contactref element="SMPS1:IC12" pad="6"/>
<contactref element="SMPS1:IC12" pad="THERMAL"/>
<contactref element="SMPS1:R68" pad="P$1"/>
<contactref element="SMPS1:R69" pad="P$1"/>
<contactref element="SMPS1:R70" pad="P$1"/>
<contactref element="SMPS1:R72" pad="P$1"/>
<contactref element="SMPS1:C57" pad="P$2"/>
<contactref element="SMPS1:C58" pad="-"/>
<contactref element="SMPS1:C59" pad="2"/>
<contactref element="SMPS1:U$12" pad="P"/>
<contactref element="S21" pad="4R"/>
<contactref element="S21" pad="4S"/>
<contactref element="S21" pad="3R"/>
<contactref element="S21" pad="3S"/>
<contactref element="C21" pad="P$2"/>
<contactref element="C22" pad="P$1"/>
<contactref element="IC21" pad="5"/>
<contactref element="U$22" pad="0V"/>
<contactref element="U$21" pad="0V"/>
<contactref element="IC21" pad="3"/>
<contactref element="IC22" pad="1"/>
<contactref element="IC22" pad="P$1"/>
<contactref element="IC22" pad="15"/>
<contactref element="IC22" pad="38"/>
<contactref element="IC22" pad="32"/>
<contactref element="SMPS1:IC11" pad="6"/>
<contactref element="SMPS1:IC11" pad="THERMAL"/>
<contactref element="SMPS1:R62" pad="P$1"/>
<contactref element="SMPS1:R63" pad="P$1"/>
<contactref element="SMPS1:R64" pad="P$1"/>
<contactref element="SMPS1:R66" pad="P$1"/>
<contactref element="SMPS1:C52" pad="P$2"/>
<contactref element="SMPS1:C53" pad="-"/>
<contactref element="SMPS1:C54" pad="2"/>
<contactref element="SMPS1:U$11" pad="P"/>
<contactref element="S19" pad="4R"/>
<contactref element="S19" pad="4S"/>
<contactref element="S19" pad="3R"/>
<contactref element="S19" pad="3S"/>
<contactref element="C19" pad="P$2"/>
<contactref element="C20" pad="P$1"/>
<contactref element="IC19" pad="5"/>
<contactref element="U$20" pad="0V"/>
<contactref element="U$19" pad="0V"/>
<contactref element="IC19" pad="3"/>
<contactref element="IC20" pad="1"/>
<contactref element="IC20" pad="P$1"/>
<contactref element="IC20" pad="15"/>
<contactref element="IC20" pad="38"/>
<contactref element="IC20" pad="32"/>
<contactref element="SMPS1:IC10" pad="6"/>
<contactref element="SMPS1:IC10" pad="THERMAL"/>
<contactref element="SMPS1:R56" pad="P$1"/>
<contactref element="SMPS1:R57" pad="P$1"/>
<contactref element="SMPS1:R58" pad="P$1"/>
<contactref element="SMPS1:R60" pad="P$1"/>
<contactref element="SMPS1:C47" pad="P$2"/>
<contactref element="SMPS1:C48" pad="-"/>
<contactref element="SMPS1:C49" pad="2"/>
<contactref element="SMPS1:U$10" pad="P"/>
<contactref element="S9" pad="4R"/>
<contactref element="S9" pad="4S"/>
<contactref element="S9" pad="3R"/>
<contactref element="S9" pad="3S"/>
<contactref element="C9" pad="P$2"/>
<contactref element="C10" pad="P$1"/>
<contactref element="IC9" pad="5"/>
<contactref element="U$10" pad="0V"/>
<contactref element="U$9" pad="0V"/>
<contactref element="IC9" pad="3"/>
<contactref element="IC10" pad="1"/>
<contactref element="IC10" pad="P$1"/>
<contactref element="IC10" pad="15"/>
<contactref element="IC10" pad="38"/>
<contactref element="IC10" pad="32"/>
<contactref element="SMPS1:IC5" pad="6"/>
<contactref element="SMPS1:IC5" pad="THERMAL"/>
<contactref element="SMPS1:R26" pad="P$1"/>
<contactref element="SMPS1:R27" pad="P$1"/>
<contactref element="SMPS1:R28" pad="P$1"/>
<contactref element="SMPS1:R30" pad="P$1"/>
<contactref element="SMPS1:C22" pad="P$2"/>
<contactref element="SMPS1:C23" pad="-"/>
<contactref element="SMPS1:C24" pad="2"/>
<contactref element="SMPS1:U$5" pad="P"/>
<contactref element="S11" pad="4R"/>
<contactref element="S11" pad="4S"/>
<contactref element="S11" pad="3R"/>
<contactref element="S11" pad="3S"/>
<contactref element="C11" pad="P$2"/>
<contactref element="C12" pad="P$1"/>
<contactref element="IC11" pad="5"/>
<contactref element="U$12" pad="0V"/>
<contactref element="U$11" pad="0V"/>
<contactref element="IC11" pad="3"/>
<contactref element="IC12" pad="1"/>
<contactref element="IC12" pad="P$1"/>
<contactref element="IC12" pad="15"/>
<contactref element="IC12" pad="38"/>
<contactref element="IC12" pad="32"/>
<contactref element="SMPS1:IC6" pad="6"/>
<contactref element="SMPS1:IC6" pad="THERMAL"/>
<contactref element="SMPS1:R32" pad="P$1"/>
<contactref element="SMPS1:R33" pad="P$1"/>
<contactref element="SMPS1:R34" pad="P$1"/>
<contactref element="SMPS1:R36" pad="P$1"/>
<contactref element="SMPS1:C27" pad="P$2"/>
<contactref element="SMPS1:C28" pad="-"/>
<contactref element="SMPS1:C29" pad="2"/>
<contactref element="SMPS1:U$6" pad="P"/>
<contactref element="S7" pad="4R"/>
<contactref element="S7" pad="4S"/>
<contactref element="S7" pad="3R"/>
<contactref element="S7" pad="3S"/>
<contactref element="C5" pad="P$2"/>
<contactref element="C8" pad="P$1"/>
<contactref element="IC7" pad="5"/>
<contactref element="U$8" pad="0V"/>
<contactref element="U$7" pad="0V"/>
<contactref element="IC7" pad="3"/>
<contactref element="IC8" pad="1"/>
<contactref element="IC8" pad="P$1"/>
<contactref element="IC8" pad="15"/>
<contactref element="IC8" pad="38"/>
<contactref element="IC8" pad="32"/>
<contactref element="SMPS1:IC4" pad="6"/>
<contactref element="SMPS1:IC4" pad="THERMAL"/>
<contactref element="SMPS1:R20" pad="P$1"/>
<contactref element="SMPS1:R21" pad="P$1"/>
<contactref element="SMPS1:R22" pad="P$1"/>
<contactref element="SMPS1:R24" pad="P$1"/>
<contactref element="SMPS1:C17" pad="P$2"/>
<contactref element="SMPS1:C18" pad="-"/>
<contactref element="SMPS1:C19" pad="2"/>
<contactref element="SMPS1:U$4" pad="P"/>
<contactref element="S3" pad="4R"/>
<contactref element="S3" pad="4S"/>
<contactref element="S3" pad="3R"/>
<contactref element="S3" pad="3S"/>
<contactref element="C1" pad="P$2"/>
<contactref element="C2" pad="P$1"/>
<contactref element="IC1" pad="5"/>
<contactref element="U$2" pad="0V"/>
<contactref element="U$1" pad="0V"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC4" pad="1"/>
<contactref element="IC4" pad="P$1"/>
<contactref element="IC4" pad="15"/>
<contactref element="IC4" pad="38"/>
<contactref element="IC4" pad="32"/>
<contactref element="SMPS1:IC2" pad="6"/>
<contactref element="SMPS1:IC2" pad="THERMAL"/>
<contactref element="SMPS1:R8" pad="P$1"/>
<contactref element="SMPS1:R9" pad="P$1"/>
<contactref element="SMPS1:R10" pad="P$1"/>
<contactref element="SMPS1:R12" pad="P$1"/>
<contactref element="SMPS1:C7" pad="P$2"/>
<contactref element="SMPS1:C8" pad="-"/>
<contactref element="SMPS1:C9" pad="2"/>
<contactref element="SMPS1:U$2" pad="P"/>
</signal>
<signal name="+3V3">
<contactref element="D2" pad="2"/>
<contactref element="R7" pad="P$1"/>
<contactref element="C6" pad="P$1"/>
<contactref element="IC3" pad="8"/>
<contactref element="R14" pad="P$1"/>
<contactref element="R8" pad="P$2"/>
<contactref element="IC2" pad="2"/>
<contactref element="SMPS1:R1" pad="P$1"/>
<contactref element="SMPS1:L1" pad="P$1"/>
<contactref element="SMPS1:C2" pad="P$1"/>
</signal>
<signal name="RESET">
<contactref element="S2" pad="1R"/>
<contactref element="S2" pad="1S"/>
<contactref element="S2" pad="2R"/>
<contactref element="S2" pad="2S"/>
<contactref element="IC2" pad="24"/>
</signal>
<signal name="RED1">
<contactref element="D2" pad="4"/>
<contactref element="R11" pad="P$2"/>
</signal>
<signal name="GREEN1">
<contactref element="D2" pad="3"/>
<contactref element="R10" pad="P$2"/>
</signal>
<signal name="BLUE1">
<contactref element="D2" pad="1"/>
<contactref element="R9" pad="P$2"/>
</signal>
<signal name="FUNCTION">
<contactref element="S1" pad="1R"/>
<contactref element="S1" pad="1S"/>
<contactref element="S1" pad="2R"/>
<contactref element="S1" pad="2S"/>
<contactref element="IC2" pad="25"/>
</signal>
<signal name="N$8">
<contactref element="IC2" pad="16"/>
</signal>
<signal name="C7">
<contactref element="R7" pad="P$2"/>
<contactref element="C7" pad="P$2"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="S2" pad="3R"/>
<contactref element="S2" pad="3S"/>
<contactref element="S2" pad="4R"/>
<contactref element="S2" pad="4S"/>
<contactref element="R8" pad="P$1"/>
</signal>
<signal name="GREEN">
<contactref element="R10" pad="P$1"/>
<contactref element="IC2" pad="28"/>
</signal>
<signal name="RED">
<contactref element="R11" pad="P$1"/>
<contactref element="IC2" pad="30"/>
</signal>
<signal name="MDB_TX2">
<contactref element="IC3" pad="1"/>
<contactref element="R13" pad="P$2"/>
</signal>
<signal name="MDB_DATA_GND">
<contactref element="IC3" pad="2"/>
<contactref element="U$5" pad="DGND"/>
<contactref element="U$6" pad="DGND"/>
</signal>
<signal name="MDB_TX">
<contactref element="R13" pad="P$1"/>
<contactref element="U$6" pad="TX"/>
<contactref element="U$5" pad="TX"/>
</signal>
<signal name="MDB_RX">
<contactref element="IC3" pad="6"/>
<contactref element="U$5" pad="RX"/>
<contactref element="U$6" pad="RX"/>
</signal>
<signal name="MDB_NC">
<contactref element="U$5" pad="NC"/>
<contactref element="U$6" pad="NC"/>
</signal>
<signal name="+34V">
<contactref element="U$5" pad="+34V"/>
<contactref element="U$6" pad="+34V"/>
<contactref element="SMPS1:IC1" pad="9"/>
<contactref element="SMPS1:IC1" pad="8"/>
<contactref element="SMPS1:R5" pad="P$2"/>
<contactref element="SMPS1:C5" pad="+"/>
<contactref element="SMPS1:C1" pad="1"/>
</signal>
<signal name="TX.">
<contactref element="R12" pad="P$2"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="SMPS1:FEEDBACK">
<contactref element="SMPS1:IC1" pad="5"/>
<contactref element="SMPS1:R2" pad="P$2"/>
<contactref element="SMPS1:R1" pad="P$2"/>
</signal>
<signal name="SMPS1:SWITCH">
<contactref element="SMPS1:IC1" pad="2"/>
<contactref element="SMPS1:IC1" pad="1"/>
<contactref element="SMPS1:L1" pad="P$2"/>
<contactref element="SMPS1:C4" pad="2"/>
<contactref element="SMPS1:U$1" pad="N"/>
</signal>
<signal name="SMPS1:N$1">
<contactref element="SMPS1:IC1" pad="4"/>
<contactref element="SMPS1:C3" pad="P$2"/>
</signal>
<signal name="SMPS1:N$2">
<contactref element="SMPS1:R3" pad="P$2"/>
<contactref element="SMPS1:C3" pad="P$1"/>
</signal>
<signal name="U1RX">
<contactref element="IC2" pad="17"/>
<contactref element="IC3" pad="7"/>
<contactref element="R14" pad="P$2"/>
</signal>
<signal name="U1TX">
<contactref element="IC2" pad="18"/>
<contactref element="R12" pad="P$1"/>
</signal>
<signal name="N$12">
<contactref element="IC2" pad="19"/>
</signal>
<signal name="N$13">
<contactref element="IC2" pad="20"/>
</signal>
<signal name="N$14">
<contactref element="IC2" pad="21"/>
</signal>
<signal name="N$15">
<contactref element="IC2" pad="22"/>
</signal>
<signal name="N$16">
<contactref element="IC2" pad="26"/>
</signal>
<signal name="N$17">
<contactref element="IC2" pad="27"/>
</signal>
<signal name="N$19">
<contactref element="IC2" pad="29"/>
</signal>
<signal name="N$22">
<contactref element="IC2" pad="33"/>
</signal>
<signal name="N$23">
<contactref element="IC2" pad="37"/>
</signal>
<signal name="N$24">
<contactref element="IC2" pad="36"/>
</signal>
<signal name="N$26">
<contactref element="IC2" pad="4"/>
</signal>
<signal name="N$27">
<contactref element="IC2" pad="5"/>
</signal>
<signal name="N$28">
<contactref element="IC2" pad="6"/>
</signal>
<signal name="N$29">
<contactref element="IC2" pad="7"/>
</signal>
<signal name="N$30">
<contactref element="IC2" pad="8"/>
</signal>
<signal name="N$31">
<contactref element="IC2" pad="9"/>
</signal>
<signal name="N$32">
<contactref element="IC2" pad="10"/>
</signal>
<signal name="N$33">
<contactref element="IC2" pad="11"/>
</signal>
<signal name="N$34">
<contactref element="IC2" pad="12"/>
</signal>
<signal name="SMPS1:N$4">
<contactref element="SMPS1:IC1" pad="7"/>
<contactref element="SMPS1:R6" pad="P$2"/>
</signal>
<signal name="SMPS1:N$6">
<contactref element="SMPS1:IC1" pad="3"/>
<contactref element="SMPS1:R4" pad="P$2"/>
<contactref element="SMPS1:R5" pad="P$1"/>
</signal>
<signal name="SMPS1:N$5">
<contactref element="SMPS1:IC1" pad="10"/>
<contactref element="SMPS1:C4" pad="1"/>
</signal>
<signal name="BLUE">
<contactref element="R9" pad="P$1"/>
<contactref element="IC2" pad="31"/>
</signal>
<signal name="N$1">
<contactref element="IC2" pad="13"/>
</signal>
<signal name="N$3">
<contactref element="IC2" pad="23"/>
</signal>
<signal name="N$4">
<contactref element="IC2" pad="14"/>
</signal>
<signal name="U0TX">
<contactref element="IC2" pad="35"/>
</signal>
<signal name="U0RX">
<contactref element="IC2" pad="34"/>
</signal>
<signal name="+3V1">
<contactref element="D1" pad="2"/>
<contactref element="R1" pad="P$1"/>
<contactref element="C1" pad="P$1"/>
<contactref element="IC1" pad="8"/>
<contactref element="R2" pad="P$1"/>
<contactref element="R16" pad="P$2"/>
<contactref element="IC4" pad="2"/>
<contactref element="SMPS1:R11" pad="P$1"/>
<contactref element="SMPS1:L2" pad="P$1"/>
<contactref element="SMPS1:C7" pad="P$1"/>
</signal>
<signal name="RESET1">
<contactref element="S4" pad="1R"/>
<contactref element="S4" pad="1S"/>
<contactref element="S4" pad="2R"/>
<contactref element="S4" pad="2S"/>
<contactref element="IC4" pad="24"/>
</signal>
<signal name="RED2">
<contactref element="D1" pad="4"/>
<contactref element="R6" pad="P$2"/>
</signal>
<signal name="GREEN2">
<contactref element="D1" pad="3"/>
<contactref element="R5" pad="P$2"/>
</signal>
<signal name="BLUE2">
<contactref element="D1" pad="1"/>
<contactref element="R15" pad="P$2"/>
</signal>
<signal name="FUNCTION1">
<contactref element="S3" pad="1R"/>
<contactref element="S3" pad="1S"/>
<contactref element="S3" pad="2R"/>
<contactref element="S3" pad="2S"/>
<contactref element="IC4" pad="25"/>
</signal>
<signal name="N$5">
<contactref element="IC4" pad="16"/>
</signal>
<signal name="C1">
<contactref element="R1" pad="P$2"/>
<contactref element="C2" pad="P$2"/>
<contactref element="IC4" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="S4" pad="3R"/>
<contactref element="S4" pad="3S"/>
<contactref element="S4" pad="4R"/>
<contactref element="S4" pad="4S"/>
<contactref element="R16" pad="P$1"/>
</signal>
<signal name="GREEN3">
<contactref element="R5" pad="P$1"/>
<contactref element="IC4" pad="28"/>
</signal>
<signal name="RED3">
<contactref element="R6" pad="P$1"/>
<contactref element="IC4" pad="30"/>
</signal>
<signal name="MDB_TX1">
<contactref element="IC1" pad="1"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="MDB_DATA_GND1">
<contactref element="IC1" pad="2"/>
<contactref element="U$1" pad="DGND"/>
<contactref element="U$2" pad="DGND"/>
</signal>
<signal name="MDB_TX3">
<contactref element="R4" pad="P$1"/>
<contactref element="U$2" pad="TX"/>
<contactref element="U$1" pad="TX"/>
</signal>
<signal name="MDB_RX1">
<contactref element="IC1" pad="6"/>
<contactref element="U$1" pad="RX"/>
<contactref element="U$2" pad="RX"/>
</signal>
<signal name="MDB_NC1">
<contactref element="U$1" pad="NC"/>
<contactref element="U$2" pad="NC"/>
</signal>
<signal name="+34V1">
<contactref element="U$1" pad="+34V"/>
<contactref element="U$2" pad="+34V"/>
<contactref element="SMPS1:IC2" pad="9"/>
<contactref element="SMPS1:IC2" pad="8"/>
<contactref element="SMPS1:R7" pad="P$2"/>
<contactref element="SMPS1:C8" pad="+"/>
<contactref element="SMPS1:C9" pad="1"/>
</signal>
<signal name="TX.1">
<contactref element="R3" pad="P$2"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="SMPS1:FEEDBACK1">
<contactref element="SMPS1:IC2" pad="5"/>
<contactref element="SMPS1:R12" pad="P$2"/>
<contactref element="SMPS1:R11" pad="P$2"/>
</signal>
<signal name="SMPS1:SWITCH1">
<contactref element="SMPS1:IC2" pad="2"/>
<contactref element="SMPS1:IC2" pad="1"/>
<contactref element="SMPS1:L2" pad="P$2"/>
<contactref element="SMPS1:C10" pad="2"/>
<contactref element="SMPS1:U$2" pad="N"/>
</signal>
<signal name="SMPS1:N$3">
<contactref element="SMPS1:IC2" pad="4"/>
<contactref element="SMPS1:C6" pad="P$2"/>
</signal>
<signal name="SMPS1:N$7">
<contactref element="SMPS1:R10" pad="P$2"/>
<contactref element="SMPS1:C6" pad="P$1"/>
</signal>
<signal name="U1RX1">
<contactref element="IC4" pad="17"/>
<contactref element="IC1" pad="7"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="U1TX1">
<contactref element="IC4" pad="18"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="IC4" pad="19"/>
</signal>
<signal name="N$9">
<contactref element="IC4" pad="20"/>
</signal>
<signal name="N$10">
<contactref element="IC4" pad="21"/>
</signal>
<signal name="N$11">
<contactref element="IC4" pad="22"/>
</signal>
<signal name="N$18">
<contactref element="IC4" pad="26"/>
</signal>
<signal name="N$20">
<contactref element="IC4" pad="27"/>
</signal>
<signal name="N$21">
<contactref element="IC4" pad="29"/>
</signal>
<signal name="N$25">
<contactref element="IC4" pad="33"/>
</signal>
<signal name="N$35">
<contactref element="IC4" pad="37"/>
</signal>
<signal name="N$36">
<contactref element="IC4" pad="36"/>
</signal>
<signal name="N$37">
<contactref element="IC4" pad="4"/>
</signal>
<signal name="N$38">
<contactref element="IC4" pad="5"/>
</signal>
<signal name="N$39">
<contactref element="IC4" pad="6"/>
</signal>
<signal name="N$40">
<contactref element="IC4" pad="7"/>
</signal>
<signal name="N$41">
<contactref element="IC4" pad="8"/>
</signal>
<signal name="N$42">
<contactref element="IC4" pad="9"/>
</signal>
<signal name="N$43">
<contactref element="IC4" pad="10"/>
</signal>
<signal name="N$44">
<contactref element="IC4" pad="11"/>
</signal>
<signal name="N$45">
<contactref element="IC4" pad="12"/>
</signal>
<signal name="SMPS1:N$8">
<contactref element="SMPS1:IC2" pad="7"/>
<contactref element="SMPS1:R8" pad="P$2"/>
</signal>
<signal name="SMPS1:N$9">
<contactref element="SMPS1:IC2" pad="3"/>
<contactref element="SMPS1:R9" pad="P$2"/>
<contactref element="SMPS1:R7" pad="P$1"/>
</signal>
<signal name="SMPS1:N$10">
<contactref element="SMPS1:IC2" pad="10"/>
<contactref element="SMPS1:C10" pad="1"/>
</signal>
<signal name="BLUE3">
<contactref element="R15" pad="P$1"/>
<contactref element="IC4" pad="31"/>
</signal>
<signal name="N$46">
<contactref element="IC4" pad="13"/>
</signal>
<signal name="N$47">
<contactref element="IC4" pad="23"/>
</signal>
<signal name="N$48">
<contactref element="IC4" pad="14"/>
</signal>
<signal name="U0TX1">
<contactref element="IC4" pad="35"/>
</signal>
<signal name="U0RX1">
<contactref element="IC4" pad="34"/>
</signal>
<signal name="+3V2">
<contactref element="D3" pad="2"/>
<contactref element="R17" pad="P$1"/>
<contactref element="C3" pad="P$1"/>
<contactref element="IC5" pad="8"/>
<contactref element="R18" pad="P$1"/>
<contactref element="R24" pad="P$2"/>
<contactref element="IC6" pad="2"/>
<contactref element="SMPS1:R17" pad="P$1"/>
<contactref element="SMPS1:L3" pad="P$1"/>
<contactref element="SMPS1:C12" pad="P$1"/>
</signal>
<signal name="RESET2">
<contactref element="S6" pad="1R"/>
<contactref element="S6" pad="1S"/>
<contactref element="S6" pad="2R"/>
<contactref element="S6" pad="2S"/>
<contactref element="IC6" pad="24"/>
</signal>
<signal name="RED4">
<contactref element="D3" pad="4"/>
<contactref element="R22" pad="P$2"/>
</signal>
<signal name="GREEN4">
<contactref element="D3" pad="3"/>
<contactref element="R21" pad="P$2"/>
</signal>
<signal name="BLUE4">
<contactref element="D3" pad="1"/>
<contactref element="R23" pad="P$2"/>
</signal>
<signal name="FUNCTION2">
<contactref element="S5" pad="1R"/>
<contactref element="S5" pad="1S"/>
<contactref element="S5" pad="2R"/>
<contactref element="S5" pad="2S"/>
<contactref element="IC6" pad="25"/>
</signal>
<signal name="N$49">
<contactref element="IC6" pad="16"/>
</signal>
<signal name="C2">
<contactref element="R17" pad="P$2"/>
<contactref element="C4" pad="P$2"/>
<contactref element="IC6" pad="3"/>
</signal>
<signal name="N$50">
<contactref element="S6" pad="3R"/>
<contactref element="S6" pad="3S"/>
<contactref element="S6" pad="4R"/>
<contactref element="S6" pad="4S"/>
<contactref element="R24" pad="P$1"/>
</signal>
<signal name="GREEN5">
<contactref element="R21" pad="P$1"/>
<contactref element="IC6" pad="28"/>
</signal>
<signal name="RED5">
<contactref element="R22" pad="P$1"/>
<contactref element="IC6" pad="30"/>
</signal>
<signal name="MDB_TX4">
<contactref element="IC5" pad="1"/>
<contactref element="R20" pad="P$2"/>
</signal>
<signal name="MDB_DATA_GND2">
<contactref element="IC5" pad="2"/>
<contactref element="U$3" pad="DGND"/>
<contactref element="U$4" pad="DGND"/>
</signal>
<signal name="MDB_TX5">
<contactref element="R20" pad="P$1"/>
<contactref element="U$4" pad="TX"/>
<contactref element="U$3" pad="TX"/>
</signal>
<signal name="MDB_RX2">
<contactref element="IC5" pad="6"/>
<contactref element="U$3" pad="RX"/>
<contactref element="U$4" pad="RX"/>
</signal>
<signal name="MDB_NC2">
<contactref element="U$3" pad="NC"/>
<contactref element="U$4" pad="NC"/>
</signal>
<signal name="+34V2">
<contactref element="U$3" pad="+34V"/>
<contactref element="U$4" pad="+34V"/>
<contactref element="SMPS1:IC3" pad="9"/>
<contactref element="SMPS1:IC3" pad="8"/>
<contactref element="SMPS1:R13" pad="P$2"/>
<contactref element="SMPS1:C13" pad="+"/>
<contactref element="SMPS1:C14" pad="1"/>
</signal>
<signal name="TX.2">
<contactref element="R19" pad="P$2"/>
<contactref element="IC5" pad="4"/>
</signal>
<signal name="SMPS1:FEEDBACK2">
<contactref element="SMPS1:IC3" pad="5"/>
<contactref element="SMPS1:R18" pad="P$2"/>
<contactref element="SMPS1:R17" pad="P$2"/>
</signal>
<signal name="SMPS1:SWITCH2">
<contactref element="SMPS1:IC3" pad="2"/>
<contactref element="SMPS1:IC3" pad="1"/>
<contactref element="SMPS1:L3" pad="P$2"/>
<contactref element="SMPS1:C15" pad="2"/>
<contactref element="SMPS1:U$3" pad="N"/>
</signal>
<signal name="SMPS1:N$11">
<contactref element="SMPS1:IC3" pad="4"/>
<contactref element="SMPS1:C11" pad="P$2"/>
</signal>
<signal name="SMPS1:N$12">
<contactref element="SMPS1:R16" pad="P$2"/>
<contactref element="SMPS1:C11" pad="P$1"/>
</signal>
<signal name="U1RX2">
<contactref element="IC6" pad="17"/>
<contactref element="IC5" pad="7"/>
<contactref element="R18" pad="P$2"/>
</signal>
<signal name="U1TX2">
<contactref element="IC6" pad="18"/>
<contactref element="R19" pad="P$1"/>
</signal>
<signal name="N$51">
<contactref element="IC6" pad="19"/>
</signal>
<signal name="N$52">
<contactref element="IC6" pad="20"/>
</signal>
<signal name="N$53">
<contactref element="IC6" pad="21"/>
</signal>
<signal name="N$54">
<contactref element="IC6" pad="22"/>
</signal>
<signal name="N$55">
<contactref element="IC6" pad="26"/>
</signal>
<signal name="N$56">
<contactref element="IC6" pad="27"/>
</signal>
<signal name="N$57">
<contactref element="IC6" pad="29"/>
</signal>
<signal name="N$58">
<contactref element="IC6" pad="33"/>
</signal>
<signal name="N$59">
<contactref element="IC6" pad="37"/>
</signal>
<signal name="N$60">
<contactref element="IC6" pad="36"/>
</signal>
<signal name="N$61">
<contactref element="IC6" pad="4"/>
</signal>
<signal name="N$62">
<contactref element="IC6" pad="5"/>
</signal>
<signal name="N$63">
<contactref element="IC6" pad="6"/>
</signal>
<signal name="N$64">
<contactref element="IC6" pad="7"/>
</signal>
<signal name="N$65">
<contactref element="IC6" pad="8"/>
</signal>
<signal name="N$66">
<contactref element="IC6" pad="9"/>
</signal>
<signal name="N$67">
<contactref element="IC6" pad="10"/>
</signal>
<signal name="N$68">
<contactref element="IC6" pad="11"/>
</signal>
<signal name="N$69">
<contactref element="IC6" pad="12"/>
</signal>
<signal name="SMPS1:N$13">
<contactref element="SMPS1:IC3" pad="7"/>
<contactref element="SMPS1:R14" pad="P$2"/>
</signal>
<signal name="SMPS1:N$14">
<contactref element="SMPS1:IC3" pad="3"/>
<contactref element="SMPS1:R15" pad="P$2"/>
<contactref element="SMPS1:R13" pad="P$1"/>
</signal>
<signal name="SMPS1:N$15">
<contactref element="SMPS1:IC3" pad="10"/>
<contactref element="SMPS1:C15" pad="1"/>
</signal>
<signal name="BLUE5">
<contactref element="R23" pad="P$1"/>
<contactref element="IC6" pad="31"/>
</signal>
<signal name="N$70">
<contactref element="IC6" pad="13"/>
</signal>
<signal name="N$71">
<contactref element="IC6" pad="23"/>
</signal>
<signal name="N$72">
<contactref element="IC6" pad="14"/>
</signal>
<signal name="U0TX2">
<contactref element="IC6" pad="35"/>
</signal>
<signal name="U0RX2">
<contactref element="IC6" pad="34"/>
</signal>
<signal name="+3V4">
<contactref element="D4" pad="2"/>
<contactref element="R25" pad="P$1"/>
<contactref element="C5" pad="P$1"/>
<contactref element="IC7" pad="8"/>
<contactref element="R26" pad="P$1"/>
<contactref element="R32" pad="P$2"/>
<contactref element="IC8" pad="2"/>
<contactref element="SMPS1:R23" pad="P$1"/>
<contactref element="SMPS1:L4" pad="P$1"/>
<contactref element="SMPS1:C17" pad="P$1"/>
</signal>
<signal name="RESET3">
<contactref element="S8" pad="1R"/>
<contactref element="S8" pad="1S"/>
<contactref element="S8" pad="2R"/>
<contactref element="S8" pad="2S"/>
<contactref element="IC8" pad="24"/>
</signal>
<signal name="RED6">
<contactref element="D4" pad="4"/>
<contactref element="R30" pad="P$2"/>
</signal>
<signal name="GREEN6">
<contactref element="D4" pad="3"/>
<contactref element="R29" pad="P$2"/>
</signal>
<signal name="BLUE6">
<contactref element="D4" pad="1"/>
<contactref element="R31" pad="P$2"/>
</signal>
<signal name="FUNCTION3">
<contactref element="S7" pad="1R"/>
<contactref element="S7" pad="1S"/>
<contactref element="S7" pad="2R"/>
<contactref element="S7" pad="2S"/>
<contactref element="IC8" pad="25"/>
</signal>
<signal name="N$73">
<contactref element="IC8" pad="16"/>
</signal>
<signal name="C3">
<contactref element="R25" pad="P$2"/>
<contactref element="C8" pad="P$2"/>
<contactref element="IC8" pad="3"/>
</signal>
<signal name="N$74">
<contactref element="S8" pad="3R"/>
<contactref element="S8" pad="3S"/>
<contactref element="S8" pad="4R"/>
<contactref element="S8" pad="4S"/>
<contactref element="R32" pad="P$1"/>
</signal>
<signal name="GREEN7">
<contactref element="R29" pad="P$1"/>
<contactref element="IC8" pad="28"/>
</signal>
<signal name="RED7">
<contactref element="R30" pad="P$1"/>
<contactref element="IC8" pad="30"/>
</signal>
<signal name="MDB_TX6">
<contactref element="IC7" pad="1"/>
<contactref element="R28" pad="P$2"/>
</signal>
<signal name="MDB_DATA_GND3">
<contactref element="IC7" pad="2"/>
<contactref element="U$7" pad="DGND"/>
<contactref element="U$8" pad="DGND"/>
</signal>
<signal name="MDB_TX7">
<contactref element="R28" pad="P$1"/>
<contactref element="U$8" pad="TX"/>
<contactref element="U$7" pad="TX"/>
</signal>
<signal name="MDB_RX3">
<contactref element="IC7" pad="6"/>
<contactref element="U$7" pad="RX"/>
<contactref element="U$8" pad="RX"/>
</signal>
<signal name="MDB_NC3">
<contactref element="U$7" pad="NC"/>
<contactref element="U$8" pad="NC"/>
</signal>
<signal name="+34V3">
<contactref element="U$7" pad="+34V"/>
<contactref element="U$8" pad="+34V"/>
<contactref element="SMPS1:IC4" pad="9"/>
<contactref element="SMPS1:IC4" pad="8"/>
<contactref element="SMPS1:R19" pad="P$2"/>
<contactref element="SMPS1:C18" pad="+"/>
<contactref element="SMPS1:C19" pad="1"/>
</signal>
<signal name="TX.3">
<contactref element="R27" pad="P$2"/>
<contactref element="IC7" pad="4"/>
</signal>
<signal name="SMPS1:FEEDBACK3">
<contactref element="SMPS1:IC4" pad="5"/>
<contactref element="SMPS1:R24" pad="P$2"/>
<contactref element="SMPS1:R23" pad="P$2"/>
</signal>
<signal name="SMPS1:SWITCH3">
<contactref element="SMPS1:IC4" pad="2"/>
<contactref element="SMPS1:IC4" pad="1"/>
<contactref element="SMPS1:L4" pad="P$2"/>
<contactref element="SMPS1:C20" pad="2"/>
<contactref element="SMPS1:U$4" pad="N"/>
</signal>
<signal name="SMPS1:N$16">
<contactref element="SMPS1:IC4" pad="4"/>
<contactref element="SMPS1:C16" pad="P$2"/>
</signal>
<signal name="SMPS1:N$17">
<contactref element="SMPS1:R22" pad="P$2"/>
<contactref element="SMPS1:C16" pad="P$1"/>
</signal>
<signal name="U1RX3">
<contactref element="IC8" pad="17"/>
<contactref element="IC7" pad="7"/>
<contactref element="R26" pad="P$2"/>
</signal>
<signal name="U1TX3">
<contactref element="IC8" pad="18"/>
<contactref element="R27" pad="P$1"/>
</signal>
<signal name="N$75">
<contactref element="IC8" pad="19"/>
</signal>
<signal name="N$76">
<contactref element="IC8" pad="20"/>
</signal>
<signal name="N$77">
<contactref element="IC8" pad="21"/>
</signal>
<signal name="N$78">
<contactref element="IC8" pad="22"/>
</signal>
<signal name="N$79">
<contactref element="IC8" pad="26"/>
</signal>
<signal name="N$80">
<contactref element="IC8" pad="27"/>
</signal>
<signal name="N$81">
<contactref element="IC8" pad="29"/>
</signal>
<signal name="N$82">
<contactref element="IC8" pad="33"/>
</signal>
<signal name="N$83">
<contactref element="IC8" pad="37"/>
</signal>
<signal name="N$84">
<contactref element="IC8" pad="36"/>
</signal>
<signal name="N$85">
<contactref element="IC8" pad="4"/>
</signal>
<signal name="N$86">
<contactref element="IC8" pad="5"/>
</signal>
<signal name="N$87">
<contactref element="IC8" pad="6"/>
</signal>
<signal name="N$88">
<contactref element="IC8" pad="7"/>
</signal>
<signal name="N$89">
<contactref element="IC8" pad="8"/>
</signal>
<signal name="N$90">
<contactref element="IC8" pad="9"/>
</signal>
<signal name="N$91">
<contactref element="IC8" pad="10"/>
</signal>
<signal name="N$92">
<contactref element="IC8" pad="11"/>
</signal>
<signal name="N$93">
<contactref element="IC8" pad="12"/>
</signal>
<signal name="SMPS1:N$18">
<contactref element="SMPS1:IC4" pad="7"/>
<contactref element="SMPS1:R20" pad="P$2"/>
</signal>
<signal name="SMPS1:N$19">
<contactref element="SMPS1:IC4" pad="3"/>
<contactref element="SMPS1:R21" pad="P$2"/>
<contactref element="SMPS1:R19" pad="P$1"/>
</signal>
<signal name="SMPS1:N$20">
<contactref element="SMPS1:IC4" pad="10"/>
<contactref element="SMPS1:C20" pad="1"/>
</signal>
<signal name="BLUE7">
<contactref element="R31" pad="P$1"/>
<contactref element="IC8" pad="31"/>
</signal>
<signal name="N$94">
<contactref element="IC8" pad="13"/>
</signal>
<signal name="N$95">
<contactref element="IC8" pad="23"/>
</signal>
<signal name="N$96">
<contactref element="IC8" pad="14"/>
</signal>
<signal name="U0TX3">
<contactref element="IC8" pad="35"/>
</signal>
<signal name="U0RX3">
<contactref element="IC8" pad="34"/>
</signal>
<signal name="+3V5">
<contactref element="D5" pad="2"/>
<contactref element="R33" pad="P$1"/>
<contactref element="C9" pad="P$1"/>
<contactref element="IC9" pad="8"/>
<contactref element="R34" pad="P$1"/>
<contactref element="R40" pad="P$2"/>
<contactref element="IC10" pad="2"/>
<contactref element="SMPS1:R29" pad="P$1"/>
<contactref element="SMPS1:L5" pad="P$1"/>
<contactref element="SMPS1:C22" pad="P$1"/>
</signal>
<signal name="RESET4">
<contactref element="S10" pad="1R"/>
<contactref element="S10" pad="1S"/>
<contactref element="S10" pad="2R"/>
<contactref element="S10" pad="2S"/>
<contactref element="IC10" pad="24"/>
</signal>
<signal name="RED8">
<contactref element="D5" pad="4"/>
<contactref element="R38" pad="P$2"/>
</signal>
<signal name="GREEN8">
<contactref element="D5" pad="3"/>
<contactref element="R37" pad="P$2"/>
</signal>
<signal name="BLUE8">
<contactref element="D5" pad="1"/>
<contactref element="R39" pad="P$2"/>
</signal>
<signal name="FUNCTION4">
<contactref element="S9" pad="1R"/>
<contactref element="S9" pad="1S"/>
<contactref element="S9" pad="2R"/>
<contactref element="S9" pad="2S"/>
<contactref element="IC10" pad="25"/>
</signal>
<signal name="N$97">
<contactref element="IC10" pad="16"/>
</signal>
<signal name="C4">
<contactref element="R33" pad="P$2"/>
<contactref element="C10" pad="P$2"/>
<contactref element="IC10" pad="3"/>
</signal>
<signal name="N$98">
<contactref element="S10" pad="3R"/>
<contactref element="S10" pad="3S"/>
<contactref element="S10" pad="4R"/>
<contactref element="S10" pad="4S"/>
<contactref element="R40" pad="P$1"/>
</signal>
<signal name="GREEN9">
<contactref element="R37" pad="P$1"/>
<contactref element="IC10" pad="28"/>
</signal>
<signal name="RED9">
<contactref element="R38" pad="P$1"/>
<contactref element="IC10" pad="30"/>
</signal>
<signal name="MDB_TX8">
<contactref element="IC9" pad="1"/>
<contactref element="R36" pad="P$2"/>
</signal>
<signal name="MDB_DATA_GND4">
<contactref element="IC9" pad="2"/>
<contactref element="U$9" pad="DGND"/>
<contactref element="U$10" pad="DGND"/>
</signal>
<signal name="MDB_TX9">
<contactref element="R36" pad="P$1"/>
<contactref element="U$10" pad="TX"/>
<contactref element="U$9" pad="TX"/>
</signal>
<signal name="MDB_RX4">
<contactref element="IC9" pad="6"/>
<contactref element="U$9" pad="RX"/>
<contactref element="U$10" pad="RX"/>
</signal>
<signal name="MDB_NC4">
<contactref element="U$9" pad="NC"/>
<contactref element="U$10" pad="NC"/>
</signal>
<signal name="+34V4">
<contactref element="U$9" pad="+34V"/>
<contactref element="U$10" pad="+34V"/>
<contactref element="SMPS1:IC5" pad="9"/>
<contactref element="SMPS1:IC5" pad="8"/>
<contactref element="SMPS1:R25" pad="P$2"/>
<contactref element="SMPS1:C23" pad="+"/>
<contactref element="SMPS1:C24" pad="1"/>
</signal>
<signal name="TX.4">
<contactref element="R35" pad="P$2"/>
<contactref element="IC9" pad="4"/>
</signal>
<signal name="SMPS1:FEEDBACK4">
<contactref element="SMPS1:IC5" pad="5"/>
<contactref element="SMPS1:R30" pad="P$2"/>
<contactref element="SMPS1:R29" pad="P$2"/>
</signal>
<signal name="SMPS1:SWITCH4">
<contactref element="SMPS1:IC5" pad="2"/>
<contactref element="SMPS1:IC5" pad="1"/>
<contactref element="SMPS1:L5" pad="P$2"/>
<contactref element="SMPS1:C25" pad="2"/>
<contactref element="SMPS1:U$5" pad="N"/>
</signal>
<signal name="SMPS1:N$21">
<contactref element="SMPS1:IC5" pad="4"/>
<contactref element="SMPS1:C21" pad="P$2"/>
</signal>
<signal name="SMPS1:N$22">
<contactref element="SMPS1:R28" pad="P$2"/>
<contactref element="SMPS1:C21" pad="P$1"/>
</signal>
<signal name="U1RX4">
<contactref element="IC10" pad="17"/>
<contactref element="IC9" pad="7"/>
<contactref element="R34" pad="P$2"/>
</signal>
<signal name="U1TX4">
<contactref element="IC10" pad="18"/>
<contactref element="R35" pad="P$1"/>
</signal>
<signal name="N$99">
<contactref element="IC10" pad="19"/>
</signal>
<signal name="N$100">
<contactref element="IC10" pad="20"/>
</signal>
<signal name="N$101">
<contactref element="IC10" pad="21"/>
</signal>
<signal name="N$102">
<contactref element="IC10" pad="22"/>
</signal>
<signal name="N$103">
<contactref element="IC10" pad="26"/>
</signal>
<signal name="N$104">
<contactref element="IC10" pad="27"/>
</signal>
<signal name="N$105">
<contactref element="IC10" pad="29"/>
</signal>
<signal name="N$106">
<contactref element="IC10" pad="33"/>
</signal>
<signal name="N$107">
<contactref element="IC10" pad="37"/>
</signal>
<signal name="N$108">
<contactref element="IC10" pad="36"/>
</signal>
<signal name="N$109">
<contactref element="IC10" pad="4"/>
</signal>
<signal name="N$110">
<contactref element="IC10" pad="5"/>
</signal>
<signal name="N$111">
<contactref element="IC10" pad="6"/>
</signal>
<signal name="N$112">
<contactref element="IC10" pad="7"/>
</signal>
<signal name="N$113">
<contactref element="IC10" pad="8"/>
</signal>
<signal name="N$114">
<contactref element="IC10" pad="9"/>
</signal>
<signal name="N$115">
<contactref element="IC10" pad="10"/>
</signal>
<signal name="N$116">
<contactref element="IC10" pad="11"/>
</signal>
<signal name="N$117">
<contactref element="IC10" pad="12"/>
</signal>
<signal name="SMPS1:N$23">
<contactref element="SMPS1:IC5" pad="7"/>
<contactref element="SMPS1:R26" pad="P$2"/>
</signal>
<signal name="SMPS1:N$24">
<contactref element="SMPS1:IC5" pad="3"/>
<contactref element="SMPS1:R27" pad="P$2"/>
<contactref element="SMPS1:R25" pad="P$1"/>
</signal>
<signal name="SMPS1:N$25">
<contactref element="SMPS1:IC5" pad="10"/>
<contactref element="SMPS1:C25" pad="1"/>
</signal>
<signal name="BLUE9">
<contactref element="R39" pad="P$1"/>
<contactref element="IC10" pad="31"/>
</signal>
<signal name="N$118">
<contactref element="IC10" pad="13"/>
</signal>
<signal name="N$119">
<contactref element="IC10" pad="23"/>
</signal>
<signal name="N$120">
<contactref element="IC10" pad="14"/>
</signal>
<signal name="U0TX4">
<contactref element="IC10" pad="35"/>
</signal>
<signal name="U0RX4">
<contactref element="IC10" pad="34"/>
</signal>
<signal name="+3V6">
<contactref element="D6" pad="2"/>
<contactref element="R41" pad="P$1"/>
<contactref element="C11" pad="P$1"/>
<contactref element="IC11" pad="8"/>
<contactref element="R42" pad="P$1"/>
<contactref element="R48" pad="P$2"/>
<contactref element="IC12" pad="2"/>
<contactref element="SMPS1:R35" pad="P$1"/>
<contactref element="SMPS1:L6" pad="P$1"/>
<contactref element="SMPS1:C27" pad="P$1"/>
</signal>
<signal name="RESET5">
<contactref element="S12" pad="1R"/>
<contactref element="S12" pad="1S"/>
<contactref element="S12" pad="2R"/>
<contactref element="S12" pad="2S"/>
<contactref element="IC12" pad="24"/>
</signal>
<signal name="RED10">
<contactref element="D6" pad="4"/>
<contactref element="R46" pad="P$2"/>
</signal>
<signal name="GREEN10">
<contactref element="D6" pad="3"/>
<contactref element="R45" pad="P$2"/>
</signal>
<signal name="BLUE10">
<contactref element="D6" pad="1"/>
<contactref element="R47" pad="P$2"/>
</signal>
<signal name="FUNCTION5">
<contactref element="S11" pad="1R"/>
<contactref element="S11" pad="1S"/>
<contactref element="S11" pad="2R"/>
<contactref element="S11" pad="2S"/>
<contactref element="IC12" pad="25"/>
</signal>
<signal name="N$121">
<contactref element="IC12" pad="16"/>
</signal>
<signal name="C5">
<contactref element="R41" pad="P$2"/>
<contactref element="C12" pad="P$2"/>
<contactref element="IC12" pad="3"/>
</signal>
<signal name="N$122">
<contactref element="S12" pad="3R"/>
<contactref element="S12" pad="3S"/>
<contactref element="S12" pad="4R"/>
<contactref element="S12" pad="4S"/>
<contactref element="R48" pad="P$1"/>
</signal>
<signal name="GREEN11">
<contactref element="R45" pad="P$1"/>
<contactref element="IC12" pad="28"/>
</signal>
<signal name="RED11">
<contactref element="R46" pad="P$1"/>
<contactref element="IC12" pad="30"/>
</signal>
<signal name="MDB_TX10">
<contactref element="IC11" pad="1"/>
<contactref element="R44" pad="P$2"/>
</signal>
<signal name="MDB_DATA_GND5">
<contactref element="IC11" pad="2"/>
<contactref element="U$11" pad="DGND"/>
<contactref element="U$12" pad="DGND"/>
</signal>
<signal name="MDB_TX11">
<contactref element="R44" pad="P$1"/>
<contactref element="U$12" pad="TX"/>
<contactref element="U$11" pad="TX"/>
</signal>
<signal name="MDB_RX5">
<contactref element="IC11" pad="6"/>
<contactref element="U$11" pad="RX"/>
<contactref element="U$12" pad="RX"/>
</signal>
<signal name="MDB_NC5">
<contactref element="U$11" pad="NC"/>
<contactref element="U$12" pad="NC"/>
</signal>
<signal name="+34V5">
<contactref element="U$11" pad="+34V"/>
<contactref element="U$12" pad="+34V"/>
<contactref element="SMPS1:IC6" pad="9"/>
<contactref element="SMPS1:IC6" pad="8"/>
<contactref element="SMPS1:R31" pad="P$2"/>
<contactref element="SMPS1:C28" pad="+"/>
<contactref element="SMPS1:C29" pad="1"/>
</signal>
<signal name="TX.5">
<contactref element="R43" pad="P$2"/>
<contactref element="IC11" pad="4"/>
</signal>
<signal name="SMPS1:FEEDBACK5">
<contactref element="SMPS1:IC6" pad="5"/>
<contactref element="SMPS1:R36" pad="P$2"/>
<contactref element="SMPS1:R35" pad="P$2"/>
</signal>
<signal name="SMPS1:SWITCH5">
<contactref element="SMPS1:IC6" pad="2"/>
<contactref element="SMPS1:IC6" pad="1"/>
<contactref element="SMPS1:L6" pad="P$2"/>
<contactref element="SMPS1:C30" pad="2"/>
<contactref element="SMPS1:U$6" pad="N"/>
</signal>
<signal name="SMPS1:N$26">
<contactref element="SMPS1:IC6" pad="4"/>
<contactref element="SMPS1:C26" pad="P$2"/>
</signal>
<signal name="SMPS1:N$27">
<contactref element="SMPS1:R34" pad="P$2"/>
<contactref element="SMPS1:C26" pad="P$1"/>
</signal>
<signal name="U1RX5">
<contactref element="IC12" pad="17"/>
<contactref element="IC11" pad="7"/>
<contactref element="R42" pad="P$2"/>
</signal>
<signal name="U1TX5">
<contactref element="IC12" pad="18"/>
<contactref element="R43" pad="P$1"/>
</signal>
<signal name="N$123">
<contactref element="IC12" pad="19"/>
</signal>
<signal name="N$124">
<contactref element="IC12" pad="20"/>
</signal>
<signal name="N$125">
<contactref element="IC12" pad="21"/>
</signal>
<signal name="N$126">
<contactref element="IC12" pad="22"/>
</signal>
<signal name="N$127">
<contactref element="IC12" pad="26"/>
</signal>
<signal name="N$128">
<contactref element="IC12" pad="27"/>
</signal>
<signal name="N$129">
<contactref element="IC12" pad="29"/>
</signal>
<signal name="N$130">
<contactref element="IC12" pad="33"/>
</signal>
<signal name="N$131">
<contactref element="IC12" pad="37"/>
</signal>
<signal name="N$132">
<contactref element="IC12" pad="36"/>
</signal>
<signal name="N$133">
<contactref element="IC12" pad="4"/>
</signal>
<signal name="N$134">
<contactref element="IC12" pad="5"/>
</signal>
<signal name="N$135">
<contactref element="IC12" pad="6"/>
</signal>
<signal name="N$136">
<contactref element="IC12" pad="7"/>
</signal>
<signal name="N$137">
<contactref element="IC12" pad="8"/>
</signal>
<signal name="N$138">
<contactref element="IC12" pad="9"/>
</signal>
<signal name="N$139">
<contactref element="IC12" pad="10"/>
</signal>
<signal name="N$140">
<contactref element="IC12" pad="11"/>
</signal>
<signal name="N$141">
<contactref element="IC12" pad="12"/>
</signal>
<signal name="SMPS1:N$28">
<contactref element="SMPS1:IC6" pad="7"/>
<contactref element="SMPS1:R32" pad="P$2"/>
</signal>
<signal name="SMPS1:N$29">
<contactref element="SMPS1:IC6" pad="3"/>
<contactref element="SMPS1:R33" pad="P$2"/>
<contactref element="SMPS1:R31" pad="P$1"/>
</signal>
<signal name="SMPS1:N$30">
<contactref element="SMPS1:IC6" pad="10"/>
<contactref element="SMPS1:C30" pad="1"/>
</signal>
<signal name="BLUE11">
<contactref element="R47" pad="P$1"/>
<contactref element="IC12" pad="31"/>
</signal>
<signal name="N$142">
<contactref element="IC12" pad="13"/>
</signal>
<signal name="N$143">
<contactref element="IC12" pad="23"/>
</signal>
<signal name="N$144">
<contactref element="IC12" pad="14"/>
</signal>
<signal name="U0TX5">
<contactref element="IC12" pad="35"/>
</signal>
<signal name="U0RX5">
<contactref element="IC12" pad="34"/>
</signal>
<signal name="+3V7">
<contactref element="D7" pad="2"/>
<contactref element="R49" pad="P$1"/>
<contactref element="C13" pad="P$1"/>
<contactref element="IC13" pad="8"/>
<contactref element="R50" pad="P$1"/>
<contactref element="R56" pad="P$2"/>
<contactref element="IC14" pad="2"/>
<contactref element="SMPS1:R41" pad="P$1"/>
<contactref element="SMPS1:L7" pad="P$1"/>
<contactref element="SMPS1:C32" pad="P$1"/>
</signal>
<signal name="RESET6">
<contactref element="S14" pad="1R"/>
<contactref element="S14" pad="1S"/>
<contactref element="S14" pad="2R"/>
<contactref element="S14" pad="2S"/>
<contactref element="IC14" pad="24"/>
</signal>
<signal name="RED12">
<contactref element="D7" pad="4"/>
<contactref element="R54" pad="P$2"/>
</signal>
<signal name="GREEN12">
<contactref element="D7" pad="3"/>
<contactref element="R53" pad="P$2"/>
</signal>
<signal name="BLUE12">
<contactref element="D7" pad="1"/>
<contactref element="R55" pad="P$2"/>
</signal>
<signal name="FUNCTION6">
<contactref element="S13" pad="1R"/>
<contactref element="S13" pad="1S"/>
<contactref element="S13" pad="2R"/>
<contactref element="S13" pad="2S"/>
<contactref element="IC14" pad="25"/>
</signal>
<signal name="N$145">
<contactref element="IC14" pad="16"/>
</signal>
<signal name="C6">
<contactref element="R49" pad="P$2"/>
<contactref element="C14" pad="P$2"/>
<contactref element="IC14" pad="3"/>
</signal>
<signal name="N$146">
<contactref element="S14" pad="3R"/>
<contactref element="S14" pad="3S"/>
<contactref element="S14" pad="4R"/>
<contactref element="S14" pad="4S"/>
<contactref element="R56" pad="P$1"/>
</signal>
<signal name="GREEN13">
<contactref element="R53" pad="P$1"/>
<contactref element="IC14" pad="28"/>
</signal>
<signal name="RED13">
<contactref element="R54" pad="P$1"/>
<contactref element="IC14" pad="30"/>
</signal>
<signal name="MDB_TX12">
<contactref element="IC13" pad="1"/>
<contactref element="R52" pad="P$2"/>
</signal>
<signal name="MDB_DATA_GND6">
<contactref element="IC13" pad="2"/>
<contactref element="U$13" pad="DGND"/>
<contactref element="U$14" pad="DGND"/>
</signal>
<signal name="MDB_TX13">
<contactref element="R52" pad="P$1"/>
<contactref element="U$14" pad="TX"/>
<contactref element="U$13" pad="TX"/>
</signal>
<signal name="MDB_RX6">
<contactref element="IC13" pad="6"/>
<contactref element="U$13" pad="RX"/>
<contactref element="U$14" pad="RX"/>
</signal>
<signal name="MDB_NC6">
<contactref element="U$13" pad="NC"/>
<contactref element="U$14" pad="NC"/>
</signal>
<signal name="+34V6">
<contactref element="U$13" pad="+34V"/>
<contactref element="U$14" pad="+34V"/>
<contactref element="SMPS1:IC7" pad="9"/>
<contactref element="SMPS1:IC7" pad="8"/>
<contactref element="SMPS1:R37" pad="P$2"/>
<contactref element="SMPS1:C33" pad="+"/>
<contactref element="SMPS1:C34" pad="1"/>
</signal>
<signal name="TX.6">
<contactref element="R51" pad="P$2"/>
<contactref element="IC13" pad="4"/>
</signal>
<signal name="SMPS1:FEEDBACK6">
<contactref element="SMPS1:IC7" pad="5"/>
<contactref element="SMPS1:R42" pad="P$2"/>
<contactref element="SMPS1:R41" pad="P$2"/>
</signal>
<signal name="SMPS1:SWITCH6">
<contactref element="SMPS1:IC7" pad="2"/>
<contactref element="SMPS1:IC7" pad="1"/>
<contactref element="SMPS1:L7" pad="P$2"/>
<contactref element="SMPS1:C35" pad="2"/>
<contactref element="SMPS1:U$7" pad="N"/>
</signal>
<signal name="SMPS1:N$31">
<contactref element="SMPS1:IC7" pad="4"/>
<contactref element="SMPS1:C31" pad="P$2"/>
</signal>
<signal name="SMPS1:N$32">
<contactref element="SMPS1:R40" pad="P$2"/>
<contactref element="SMPS1:C31" pad="P$1"/>
</signal>
<signal name="U1RX6">
<contactref element="IC14" pad="17"/>
<contactref element="IC13" pad="7"/>
<contactref element="R50" pad="P$2"/>
</signal>
<signal name="U1TX6">
<contactref element="IC14" pad="18"/>
<contactref element="R51" pad="P$1"/>
</signal>
<signal name="N$147">
<contactref element="IC14" pad="19"/>
</signal>
<signal name="N$148">
<contactref element="IC14" pad="20"/>
</signal>
<signal name="N$149">
<contactref element="IC14" pad="21"/>
</signal>
<signal name="N$150">
<contactref element="IC14" pad="22"/>
</signal>
<signal name="N$151">
<contactref element="IC14" pad="26"/>
</signal>
<signal name="N$152">
<contactref element="IC14" pad="27"/>
</signal>
<signal name="N$153">
<contactref element="IC14" pad="29"/>
</signal>
<signal name="N$154">
<contactref element="IC14" pad="33"/>
</signal>
<signal name="N$155">
<contactref element="IC14" pad="37"/>
</signal>
<signal name="N$156">
<contactref element="IC14" pad="36"/>
</signal>
<signal name="N$157">
<contactref element="IC14" pad="4"/>
</signal>
<signal name="N$158">
<contactref element="IC14" pad="5"/>
</signal>
<signal name="N$159">
<contactref element="IC14" pad="6"/>
</signal>
<signal name="N$160">
<contactref element="IC14" pad="7"/>
</signal>
<signal name="N$161">
<contactref element="IC14" pad="8"/>
</signal>
<signal name="N$162">
<contactref element="IC14" pad="9"/>
</signal>
<signal name="N$163">
<contactref element="IC14" pad="10"/>
</signal>
<signal name="N$164">
<contactref element="IC14" pad="11"/>
</signal>
<signal name="N$165">
<contactref element="IC14" pad="12"/>
</signal>
<signal name="SMPS1:N$33">
<contactref element="SMPS1:IC7" pad="7"/>
<contactref element="SMPS1:R38" pad="P$2"/>
</signal>
<signal name="SMPS1:N$34">
<contactref element="SMPS1:IC7" pad="3"/>
<contactref element="SMPS1:R39" pad="P$2"/>
<contactref element="SMPS1:R37" pad="P$1"/>
</signal>
<signal name="SMPS1:N$35">
<contactref element="SMPS1:IC7" pad="10"/>
<contactref element="SMPS1:C35" pad="1"/>
</signal>
<signal name="BLUE13">
<contactref element="R55" pad="P$1"/>
<contactref element="IC14" pad="31"/>
</signal>
<signal name="N$166">
<contactref element="IC14" pad="13"/>
</signal>
<signal name="N$167">
<contactref element="IC14" pad="23"/>
</signal>
<signal name="N$168">
<contactref element="IC14" pad="14"/>
</signal>
<signal name="U0TX6">
<contactref element="IC14" pad="35"/>
</signal>
<signal name="U0RX6">
<contactref element="IC14" pad="34"/>
</signal>
<signal name="+3V8">
<contactref element="D8" pad="2"/>
<contactref element="R57" pad="P$1"/>
<contactref element="C15" pad="P$1"/>
<contactref element="IC15" pad="8"/>
<contactref element="R58" pad="P$1"/>
<contactref element="R64" pad="P$2"/>
<contactref element="IC16" pad="2"/>
<contactref element="SMPS1:R47" pad="P$1"/>
<contactref element="SMPS1:L8" pad="P$1"/>
<contactref element="SMPS1:C37" pad="P$1"/>
</signal>
<signal name="RESET7">
<contactref element="S16" pad="1R"/>
<contactref element="S16" pad="1S"/>
<contactref element="S16" pad="2R"/>
<contactref element="S16" pad="2S"/>
<contactref element="IC16" pad="24"/>
</signal>
<signal name="RED14">
<contactref element="D8" pad="4"/>
<contactref element="R62" pad="P$2"/>
</signal>
<signal name="GREEN14">
<contactref element="D8" pad="3"/>
<contactref element="R61" pad="P$2"/>
</signal>
<signal name="BLUE14">
<contactref element="D8" pad="1"/>
<contactref element="R63" pad="P$2"/>
</signal>
<signal name="FUNCTION7">
<contactref element="S15" pad="1R"/>
<contactref element="S15" pad="1S"/>
<contactref element="S15" pad="2R"/>
<contactref element="S15" pad="2S"/>
<contactref element="IC16" pad="25"/>
</signal>
<signal name="N$169">
<contactref element="IC16" pad="16"/>
</signal>
<signal name="C8">
<contactref element="R57" pad="P$2"/>
<contactref element="C16" pad="P$2"/>
<contactref element="IC16" pad="3"/>
</signal>
<signal name="N$170">
<contactref element="S16" pad="3R"/>
<contactref element="S16" pad="3S"/>
<contactref element="S16" pad="4R"/>
<contactref element="S16" pad="4S"/>
<contactref element="R64" pad="P$1"/>
</signal>
<signal name="GREEN15">
<contactref element="R61" pad="P$1"/>
<contactref element="IC16" pad="28"/>
</signal>
<signal name="RED15">
<contactref element="R62" pad="P$1"/>
<contactref element="IC16" pad="30"/>
</signal>
<signal name="MDB_TX14">
<contactref element="IC15" pad="1"/>
<contactref element="R60" pad="P$2"/>
</signal>
<signal name="MDB_DATA_GND7">
<contactref element="IC15" pad="2"/>
<contactref element="U$15" pad="DGND"/>
<contactref element="U$16" pad="DGND"/>
</signal>
<signal name="MDB_TX15">
<contactref element="R60" pad="P$1"/>
<contactref element="U$16" pad="TX"/>
<contactref element="U$15" pad="TX"/>
</signal>
<signal name="MDB_RX7">
<contactref element="IC15" pad="6"/>
<contactref element="U$15" pad="RX"/>
<contactref element="U$16" pad="RX"/>
</signal>
<signal name="MDB_NC7">
<contactref element="U$15" pad="NC"/>
<contactref element="U$16" pad="NC"/>
</signal>
<signal name="+34V7">
<contactref element="U$15" pad="+34V"/>
<contactref element="U$16" pad="+34V"/>
<contactref element="SMPS1:IC8" pad="9"/>
<contactref element="SMPS1:IC8" pad="8"/>
<contactref element="SMPS1:R43" pad="P$2"/>
<contactref element="SMPS1:C38" pad="+"/>
<contactref element="SMPS1:C39" pad="1"/>
</signal>
<signal name="TX.7">
<contactref element="R59" pad="P$2"/>
<contactref element="IC15" pad="4"/>
</signal>
<signal name="SMPS1:FEEDBACK7">
<contactref element="SMPS1:IC8" pad="5"/>
<contactref element="SMPS1:R48" pad="P$2"/>
<contactref element="SMPS1:R47" pad="P$2"/>
</signal>
<signal name="SMPS1:SWITCH7">
<contactref element="SMPS1:IC8" pad="2"/>
<contactref element="SMPS1:IC8" pad="1"/>
<contactref element="SMPS1:L8" pad="P$2"/>
<contactref element="SMPS1:C40" pad="2"/>
<contactref element="SMPS1:U$8" pad="N"/>
</signal>
<signal name="SMPS1:N$36">
<contactref element="SMPS1:IC8" pad="4"/>
<contactref element="SMPS1:C36" pad="P$2"/>
</signal>
<signal name="SMPS1:N$37">
<contactref element="SMPS1:R46" pad="P$2"/>
<contactref element="SMPS1:C36" pad="P$1"/>
</signal>
<signal name="U1RX7">
<contactref element="IC16" pad="17"/>
<contactref element="IC15" pad="7"/>
<contactref element="R58" pad="P$2"/>
</signal>
<signal name="U1TX7">
<contactref element="IC16" pad="18"/>
<contactref element="R59" pad="P$1"/>
</signal>
<signal name="N$171">
<contactref element="IC16" pad="19"/>
</signal>
<signal name="N$172">
<contactref element="IC16" pad="20"/>
</signal>
<signal name="N$173">
<contactref element="IC16" pad="21"/>
</signal>
<signal name="N$174">
<contactref element="IC16" pad="22"/>
</signal>
<signal name="N$175">
<contactref element="IC16" pad="26"/>
</signal>
<signal name="N$176">
<contactref element="IC16" pad="27"/>
</signal>
<signal name="N$177">
<contactref element="IC16" pad="29"/>
</signal>
<signal name="N$178">
<contactref element="IC16" pad="33"/>
</signal>
<signal name="N$179">
<contactref element="IC16" pad="37"/>
</signal>
<signal name="N$180">
<contactref element="IC16" pad="36"/>
</signal>
<signal name="N$181">
<contactref element="IC16" pad="4"/>
</signal>
<signal name="N$182">
<contactref element="IC16" pad="5"/>
</signal>
<signal name="N$183">
<contactref element="IC16" pad="6"/>
</signal>
<signal name="N$184">
<contactref element="IC16" pad="7"/>
</signal>
<signal name="N$185">
<contactref element="IC16" pad="8"/>
</signal>
<signal name="N$186">
<contactref element="IC16" pad="9"/>
</signal>
<signal name="N$187">
<contactref element="IC16" pad="10"/>
</signal>
<signal name="N$188">
<contactref element="IC16" pad="11"/>
</signal>
<signal name="N$189">
<contactref element="IC16" pad="12"/>
</signal>
<signal name="SMPS1:N$38">
<contactref element="SMPS1:IC8" pad="7"/>
<contactref element="SMPS1:R44" pad="P$2"/>
</signal>
<signal name="SMPS1:N$39">
<contactref element="SMPS1:IC8" pad="3"/>
<contactref element="SMPS1:R45" pad="P$2"/>
<contactref element="SMPS1:R43" pad="P$1"/>
</signal>
<signal name="SMPS1:N$40">
<contactref element="SMPS1:IC8" pad="10"/>
<contactref element="SMPS1:C40" pad="1"/>
</signal>
<signal name="BLUE15">
<contactref element="R63" pad="P$1"/>
<contactref element="IC16" pad="31"/>
</signal>
<signal name="N$190">
<contactref element="IC16" pad="13"/>
</signal>
<signal name="N$191">
<contactref element="IC16" pad="23"/>
</signal>
<signal name="N$192">
<contactref element="IC16" pad="14"/>
</signal>
<signal name="U0TX7">
<contactref element="IC16" pad="35"/>
</signal>
<signal name="U0RX7">
<contactref element="IC16" pad="34"/>
</signal>
<signal name="+3V9">
<contactref element="D9" pad="2"/>
<contactref element="R65" pad="P$1"/>
<contactref element="C17" pad="P$1"/>
<contactref element="IC17" pad="8"/>
<contactref element="R66" pad="P$1"/>
<contactref element="R72" pad="P$2"/>
<contactref element="IC18" pad="2"/>
<contactref element="SMPS1:R53" pad="P$1"/>
<contactref element="SMPS1:L9" pad="P$1"/>
<contactref element="SMPS1:C42" pad="P$1"/>
</signal>
<signal name="RESET8">
<contactref element="S18" pad="1R"/>
<contactref element="S18" pad="1S"/>
<contactref element="S18" pad="2R"/>
<contactref element="S18" pad="2S"/>
<contactref element="IC18" pad="24"/>
</signal>
<signal name="RED16">
<contactref element="D9" pad="4"/>
<contactref element="R70" pad="P$2"/>
</signal>
<signal name="GREEN16">
<contactref element="D9" pad="3"/>
<contactref element="R69" pad="P$2"/>
</signal>
<signal name="BLUE16">
<contactref element="D9" pad="1"/>
<contactref element="R71" pad="P$2"/>
</signal>
<signal name="FUNCTION8">
<contactref element="S17" pad="1R"/>
<contactref element="S17" pad="1S"/>
<contactref element="S17" pad="2R"/>
<contactref element="S17" pad="2S"/>
<contactref element="IC18" pad="25"/>
</signal>
<signal name="N$193">
<contactref element="IC18" pad="16"/>
</signal>
<signal name="C9">
<contactref element="R65" pad="P$2"/>
<contactref element="C18" pad="P$2"/>
<contactref element="IC18" pad="3"/>
</signal>
<signal name="N$194">
<contactref element="S18" pad="3R"/>
<contactref element="S18" pad="3S"/>
<contactref element="S18" pad="4R"/>
<contactref element="S18" pad="4S"/>
<contactref element="R72" pad="P$1"/>
</signal>
<signal name="GREEN17">
<contactref element="R69" pad="P$1"/>
<contactref element="IC18" pad="28"/>
</signal>
<signal name="RED17">
<contactref element="R70" pad="P$1"/>
<contactref element="IC18" pad="30"/>
</signal>
<signal name="MDB_TX16">
<contactref element="IC17" pad="1"/>
<contactref element="R68" pad="P$2"/>
</signal>
<signal name="MDB_DATA_GND8">
<contactref element="IC17" pad="2"/>
<contactref element="U$17" pad="DGND"/>
<contactref element="U$18" pad="DGND"/>
</signal>
<signal name="MDB_TX17">
<contactref element="R68" pad="P$1"/>
<contactref element="U$18" pad="TX"/>
<contactref element="U$17" pad="TX"/>
</signal>
<signal name="MDB_RX8">
<contactref element="IC17" pad="6"/>
<contactref element="U$17" pad="RX"/>
<contactref element="U$18" pad="RX"/>
</signal>
<signal name="MDB_NC8">
<contactref element="U$17" pad="NC"/>
<contactref element="U$18" pad="NC"/>
</signal>
<signal name="+34V8">
<contactref element="U$17" pad="+34V"/>
<contactref element="U$18" pad="+34V"/>
<contactref element="SMPS1:IC9" pad="9"/>
<contactref element="SMPS1:IC9" pad="8"/>
<contactref element="SMPS1:R49" pad="P$2"/>
<contactref element="SMPS1:C43" pad="+"/>
<contactref element="SMPS1:C44" pad="1"/>
</signal>
<signal name="TX.8">
<contactref element="R67" pad="P$2"/>
<contactref element="IC17" pad="4"/>
</signal>
<signal name="SMPS1:FEEDBACK8">
<contactref element="SMPS1:IC9" pad="5"/>
<contactref element="SMPS1:R54" pad="P$2"/>
<contactref element="SMPS1:R53" pad="P$2"/>
</signal>
<signal name="SMPS1:SWITCH8">
<contactref element="SMPS1:IC9" pad="2"/>
<contactref element="SMPS1:IC9" pad="1"/>
<contactref element="SMPS1:L9" pad="P$2"/>
<contactref element="SMPS1:C45" pad="2"/>
<contactref element="SMPS1:U$9" pad="N"/>
</signal>
<signal name="SMPS1:N$41">
<contactref element="SMPS1:IC9" pad="4"/>
<contactref element="SMPS1:C41" pad="P$2"/>
</signal>
<signal name="SMPS1:N$42">
<contactref element="SMPS1:R52" pad="P$2"/>
<contactref element="SMPS1:C41" pad="P$1"/>
</signal>
<signal name="U1RX8">
<contactref element="IC18" pad="17"/>
<contactref element="IC17" pad="7"/>
<contactref element="R66" pad="P$2"/>
</signal>
<signal name="U1TX8">
<contactref element="IC18" pad="18"/>
<contactref element="R67" pad="P$1"/>
</signal>
<signal name="N$195">
<contactref element="IC18" pad="19"/>
</signal>
<signal name="N$196">
<contactref element="IC18" pad="20"/>
</signal>
<signal name="N$197">
<contactref element="IC18" pad="21"/>
</signal>
<signal name="N$198">
<contactref element="IC18" pad="22"/>
</signal>
<signal name="N$199">
<contactref element="IC18" pad="26"/>
</signal>
<signal name="N$200">
<contactref element="IC18" pad="27"/>
</signal>
<signal name="N$201">
<contactref element="IC18" pad="29"/>
</signal>
<signal name="N$202">
<contactref element="IC18" pad="33"/>
</signal>
<signal name="N$203">
<contactref element="IC18" pad="37"/>
</signal>
<signal name="N$204">
<contactref element="IC18" pad="36"/>
</signal>
<signal name="N$205">
<contactref element="IC18" pad="4"/>
</signal>
<signal name="N$206">
<contactref element="IC18" pad="5"/>
</signal>
<signal name="N$207">
<contactref element="IC18" pad="6"/>
</signal>
<signal name="N$208">
<contactref element="IC18" pad="7"/>
</signal>
<signal name="N$209">
<contactref element="IC18" pad="8"/>
</signal>
<signal name="N$210">
<contactref element="IC18" pad="9"/>
</signal>
<signal name="N$211">
<contactref element="IC18" pad="10"/>
</signal>
<signal name="N$212">
<contactref element="IC18" pad="11"/>
</signal>
<signal name="N$213">
<contactref element="IC18" pad="12"/>
</signal>
<signal name="SMPS1:N$43">
<contactref element="SMPS1:IC9" pad="7"/>
<contactref element="SMPS1:R50" pad="P$2"/>
</signal>
<signal name="SMPS1:N$44">
<contactref element="SMPS1:IC9" pad="3"/>
<contactref element="SMPS1:R51" pad="P$2"/>
<contactref element="SMPS1:R49" pad="P$1"/>
</signal>
<signal name="SMPS1:N$45">
<contactref element="SMPS1:IC9" pad="10"/>
<contactref element="SMPS1:C45" pad="1"/>
</signal>
<signal name="BLUE17">
<contactref element="R71" pad="P$1"/>
<contactref element="IC18" pad="31"/>
</signal>
<signal name="N$214">
<contactref element="IC18" pad="13"/>
</signal>
<signal name="N$215">
<contactref element="IC18" pad="23"/>
</signal>
<signal name="N$216">
<contactref element="IC18" pad="14"/>
</signal>
<signal name="U0TX8">
<contactref element="IC18" pad="35"/>
</signal>
<signal name="U0RX8">
<contactref element="IC18" pad="34"/>
</signal>
<signal name="+3V10">
<contactref element="D10" pad="2"/>
<contactref element="R73" pad="P$1"/>
<contactref element="C19" pad="P$1"/>
<contactref element="IC19" pad="8"/>
<contactref element="R74" pad="P$1"/>
<contactref element="R80" pad="P$2"/>
<contactref element="IC20" pad="2"/>
<contactref element="SMPS1:R59" pad="P$1"/>
<contactref element="SMPS1:L10" pad="P$1"/>
<contactref element="SMPS1:C47" pad="P$1"/>
</signal>
<signal name="RESET9">
<contactref element="S20" pad="1R"/>
<contactref element="S20" pad="1S"/>
<contactref element="S20" pad="2R"/>
<contactref element="S20" pad="2S"/>
<contactref element="IC20" pad="24"/>
</signal>
<signal name="RED18">
<contactref element="D10" pad="4"/>
<contactref element="R78" pad="P$2"/>
</signal>
<signal name="GREEN18">
<contactref element="D10" pad="3"/>
<contactref element="R77" pad="P$2"/>
</signal>
<signal name="BLUE18">
<contactref element="D10" pad="1"/>
<contactref element="R79" pad="P$2"/>
</signal>
<signal name="FUNCTION9">
<contactref element="S19" pad="1R"/>
<contactref element="S19" pad="1S"/>
<contactref element="S19" pad="2R"/>
<contactref element="S19" pad="2S"/>
<contactref element="IC20" pad="25"/>
</signal>
<signal name="N$217">
<contactref element="IC20" pad="16"/>
</signal>
<signal name="C10">
<contactref element="R73" pad="P$2"/>
<contactref element="C20" pad="P$2"/>
<contactref element="IC20" pad="3"/>
</signal>
<signal name="N$218">
<contactref element="S20" pad="3R"/>
<contactref element="S20" pad="3S"/>
<contactref element="S20" pad="4R"/>
<contactref element="S20" pad="4S"/>
<contactref element="R80" pad="P$1"/>
</signal>
<signal name="GREEN19">
<contactref element="R77" pad="P$1"/>
<contactref element="IC20" pad="28"/>
</signal>
<signal name="RED19">
<contactref element="R78" pad="P$1"/>
<contactref element="IC20" pad="30"/>
</signal>
<signal name="MDB_TX18">
<contactref element="IC19" pad="1"/>
<contactref element="R76" pad="P$2"/>
</signal>
<signal name="MDB_DATA_GND9">
<contactref element="IC19" pad="2"/>
<contactref element="U$19" pad="DGND"/>
<contactref element="U$20" pad="DGND"/>
</signal>
<signal name="MDB_TX19">
<contactref element="R76" pad="P$1"/>
<contactref element="U$20" pad="TX"/>
<contactref element="U$19" pad="TX"/>
</signal>
<signal name="MDB_RX9">
<contactref element="IC19" pad="6"/>
<contactref element="U$19" pad="RX"/>
<contactref element="U$20" pad="RX"/>
</signal>
<signal name="MDB_NC9">
<contactref element="U$19" pad="NC"/>
<contactref element="U$20" pad="NC"/>
</signal>
<signal name="+34V9">
<contactref element="U$19" pad="+34V"/>
<contactref element="U$20" pad="+34V"/>
<contactref element="SMPS1:IC10" pad="9"/>
<contactref element="SMPS1:IC10" pad="8"/>
<contactref element="SMPS1:R55" pad="P$2"/>
<contactref element="SMPS1:C48" pad="+"/>
<contactref element="SMPS1:C49" pad="1"/>
</signal>
<signal name="TX.9">
<contactref element="R75" pad="P$2"/>
<contactref element="IC19" pad="4"/>
</signal>
<signal name="SMPS1:FEEDBACK9">
<contactref element="SMPS1:IC10" pad="5"/>
<contactref element="SMPS1:R60" pad="P$2"/>
<contactref element="SMPS1:R59" pad="P$2"/>
</signal>
<signal name="SMPS1:SWITCH9">
<contactref element="SMPS1:IC10" pad="2"/>
<contactref element="SMPS1:IC10" pad="1"/>
<contactref element="SMPS1:L10" pad="P$2"/>
<contactref element="SMPS1:C50" pad="2"/>
<contactref element="SMPS1:U$10" pad="N"/>
</signal>
<signal name="SMPS1:N$46">
<contactref element="SMPS1:IC10" pad="4"/>
<contactref element="SMPS1:C46" pad="P$2"/>
</signal>
<signal name="SMPS1:N$47">
<contactref element="SMPS1:R58" pad="P$2"/>
<contactref element="SMPS1:C46" pad="P$1"/>
</signal>
<signal name="U1RX9">
<contactref element="IC20" pad="17"/>
<contactref element="IC19" pad="7"/>
<contactref element="R74" pad="P$2"/>
</signal>
<signal name="U1TX9">
<contactref element="IC20" pad="18"/>
<contactref element="R75" pad="P$1"/>
</signal>
<signal name="N$219">
<contactref element="IC20" pad="19"/>
</signal>
<signal name="N$220">
<contactref element="IC20" pad="20"/>
</signal>
<signal name="N$221">
<contactref element="IC20" pad="21"/>
</signal>
<signal name="N$222">
<contactref element="IC20" pad="22"/>
</signal>
<signal name="N$223">
<contactref element="IC20" pad="26"/>
</signal>
<signal name="N$224">
<contactref element="IC20" pad="27"/>
</signal>
<signal name="N$225">
<contactref element="IC20" pad="29"/>
</signal>
<signal name="N$226">
<contactref element="IC20" pad="33"/>
</signal>
<signal name="N$227">
<contactref element="IC20" pad="37"/>
</signal>
<signal name="N$228">
<contactref element="IC20" pad="36"/>
</signal>
<signal name="N$229">
<contactref element="IC20" pad="4"/>
</signal>
<signal name="N$230">
<contactref element="IC20" pad="5"/>
</signal>
<signal name="N$231">
<contactref element="IC20" pad="6"/>
</signal>
<signal name="N$232">
<contactref element="IC20" pad="7"/>
</signal>
<signal name="N$233">
<contactref element="IC20" pad="8"/>
</signal>
<signal name="N$234">
<contactref element="IC20" pad="9"/>
</signal>
<signal name="N$235">
<contactref element="IC20" pad="10"/>
</signal>
<signal name="N$236">
<contactref element="IC20" pad="11"/>
</signal>
<signal name="N$237">
<contactref element="IC20" pad="12"/>
</signal>
<signal name="SMPS1:N$48">
<contactref element="SMPS1:IC10" pad="7"/>
<contactref element="SMPS1:R56" pad="P$2"/>
</signal>
<signal name="SMPS1:N$49">
<contactref element="SMPS1:IC10" pad="3"/>
<contactref element="SMPS1:R57" pad="P$2"/>
<contactref element="SMPS1:R55" pad="P$1"/>
</signal>
<signal name="SMPS1:N$50">
<contactref element="SMPS1:IC10" pad="10"/>
<contactref element="SMPS1:C50" pad="1"/>
</signal>
<signal name="BLUE19">
<contactref element="R79" pad="P$1"/>
<contactref element="IC20" pad="31"/>
</signal>
<signal name="N$238">
<contactref element="IC20" pad="13"/>
</signal>
<signal name="N$239">
<contactref element="IC20" pad="23"/>
</signal>
<signal name="N$240">
<contactref element="IC20" pad="14"/>
</signal>
<signal name="U0TX9">
<contactref element="IC20" pad="35"/>
</signal>
<signal name="U0RX9">
<contactref element="IC20" pad="34"/>
</signal>
<signal name="+3V11">
<contactref element="D11" pad="2"/>
<contactref element="R81" pad="P$1"/>
<contactref element="C21" pad="P$1"/>
<contactref element="IC21" pad="8"/>
<contactref element="R82" pad="P$1"/>
<contactref element="R88" pad="P$2"/>
<contactref element="IC22" pad="2"/>
<contactref element="SMPS1:R65" pad="P$1"/>
<contactref element="SMPS1:L11" pad="P$1"/>
<contactref element="SMPS1:C52" pad="P$1"/>
</signal>
<signal name="RESET10">
<contactref element="S22" pad="1R"/>
<contactref element="S22" pad="1S"/>
<contactref element="S22" pad="2R"/>
<contactref element="S22" pad="2S"/>
<contactref element="IC22" pad="24"/>
</signal>
<signal name="RED20">
<contactref element="D11" pad="4"/>
<contactref element="R86" pad="P$2"/>
</signal>
<signal name="GREEN20">
<contactref element="D11" pad="3"/>
<contactref element="R85" pad="P$2"/>
</signal>
<signal name="BLUE20">
<contactref element="D11" pad="1"/>
<contactref element="R87" pad="P$2"/>
</signal>
<signal name="FUNCTION10">
<contactref element="S21" pad="1R"/>
<contactref element="S21" pad="1S"/>
<contactref element="S21" pad="2R"/>
<contactref element="S21" pad="2S"/>
<contactref element="IC22" pad="25"/>
</signal>
<signal name="N$241">
<contactref element="IC22" pad="16"/>
</signal>
<signal name="C11">
<contactref element="R81" pad="P$2"/>
<contactref element="C22" pad="P$2"/>
<contactref element="IC22" pad="3"/>
</signal>
<signal name="N$242">
<contactref element="S22" pad="3R"/>
<contactref element="S22" pad="3S"/>
<contactref element="S22" pad="4R"/>
<contactref element="S22" pad="4S"/>
<contactref element="R88" pad="P$1"/>
</signal>
<signal name="GREEN21">
<contactref element="R85" pad="P$1"/>
<contactref element="IC22" pad="28"/>
</signal>
<signal name="RED21">
<contactref element="R86" pad="P$1"/>
<contactref element="IC22" pad="30"/>
</signal>
<signal name="MDB_TX20">
<contactref element="IC21" pad="1"/>
<contactref element="R84" pad="P$2"/>
</signal>
<signal name="MDB_DATA_GND10">
<contactref element="IC21" pad="2"/>
<contactref element="U$21" pad="DGND"/>
<contactref element="U$22" pad="DGND"/>
</signal>
<signal name="MDB_TX21">
<contactref element="R84" pad="P$1"/>
<contactref element="U$22" pad="TX"/>
<contactref element="U$21" pad="TX"/>
</signal>
<signal name="MDB_RX10">
<contactref element="IC21" pad="6"/>
<contactref element="U$21" pad="RX"/>
<contactref element="U$22" pad="RX"/>
</signal>
<signal name="MDB_NC10">
<contactref element="U$21" pad="NC"/>
<contactref element="U$22" pad="NC"/>
</signal>
<signal name="+34V10">
<contactref element="U$21" pad="+34V"/>
<contactref element="U$22" pad="+34V"/>
<contactref element="SMPS1:IC11" pad="9"/>
<contactref element="SMPS1:IC11" pad="8"/>
<contactref element="SMPS1:R61" pad="P$2"/>
<contactref element="SMPS1:C53" pad="+"/>
<contactref element="SMPS1:C54" pad="1"/>
</signal>
<signal name="TX.10">
<contactref element="R83" pad="P$2"/>
<contactref element="IC21" pad="4"/>
</signal>
<signal name="SMPS1:FEEDBACK10">
<contactref element="SMPS1:IC11" pad="5"/>
<contactref element="SMPS1:R66" pad="P$2"/>
<contactref element="SMPS1:R65" pad="P$2"/>
</signal>
<signal name="SMPS1:SWITCH10">
<contactref element="SMPS1:IC11" pad="2"/>
<contactref element="SMPS1:IC11" pad="1"/>
<contactref element="SMPS1:L11" pad="P$2"/>
<contactref element="SMPS1:C55" pad="2"/>
<contactref element="SMPS1:U$11" pad="N"/>
</signal>
<signal name="SMPS1:N$51">
<contactref element="SMPS1:IC11" pad="4"/>
<contactref element="SMPS1:C51" pad="P$2"/>
</signal>
<signal name="SMPS1:N$52">
<contactref element="SMPS1:R64" pad="P$2"/>
<contactref element="SMPS1:C51" pad="P$1"/>
</signal>
<signal name="U1RX10">
<contactref element="IC22" pad="17"/>
<contactref element="IC21" pad="7"/>
<contactref element="R82" pad="P$2"/>
</signal>
<signal name="U1TX10">
<contactref element="IC22" pad="18"/>
<contactref element="R83" pad="P$1"/>
</signal>
<signal name="N$243">
<contactref element="IC22" pad="19"/>
</signal>
<signal name="N$244">
<contactref element="IC22" pad="20"/>
</signal>
<signal name="N$245">
<contactref element="IC22" pad="21"/>
</signal>
<signal name="N$246">
<contactref element="IC22" pad="22"/>
</signal>
<signal name="N$247">
<contactref element="IC22" pad="26"/>
</signal>
<signal name="N$248">
<contactref element="IC22" pad="27"/>
</signal>
<signal name="N$249">
<contactref element="IC22" pad="29"/>
</signal>
<signal name="N$250">
<contactref element="IC22" pad="33"/>
</signal>
<signal name="N$251">
<contactref element="IC22" pad="37"/>
</signal>
<signal name="N$252">
<contactref element="IC22" pad="36"/>
</signal>
<signal name="N$253">
<contactref element="IC22" pad="4"/>
</signal>
<signal name="N$254">
<contactref element="IC22" pad="5"/>
</signal>
<signal name="N$255">
<contactref element="IC22" pad="6"/>
</signal>
<signal name="N$256">
<contactref element="IC22" pad="7"/>
</signal>
<signal name="N$257">
<contactref element="IC22" pad="8"/>
</signal>
<signal name="N$258">
<contactref element="IC22" pad="9"/>
</signal>
<signal name="N$259">
<contactref element="IC22" pad="10"/>
</signal>
<signal name="N$260">
<contactref element="IC22" pad="11"/>
</signal>
<signal name="N$261">
<contactref element="IC22" pad="12"/>
</signal>
<signal name="SMPS1:N$53">
<contactref element="SMPS1:IC11" pad="7"/>
<contactref element="SMPS1:R62" pad="P$2"/>
</signal>
<signal name="SMPS1:N$54">
<contactref element="SMPS1:IC11" pad="3"/>
<contactref element="SMPS1:R63" pad="P$2"/>
<contactref element="SMPS1:R61" pad="P$1"/>
</signal>
<signal name="SMPS1:N$55">
<contactref element="SMPS1:IC11" pad="10"/>
<contactref element="SMPS1:C55" pad="1"/>
</signal>
<signal name="BLUE21">
<contactref element="R87" pad="P$1"/>
<contactref element="IC22" pad="31"/>
</signal>
<signal name="N$262">
<contactref element="IC22" pad="13"/>
</signal>
<signal name="N$263">
<contactref element="IC22" pad="23"/>
</signal>
<signal name="N$264">
<contactref element="IC22" pad="14"/>
</signal>
<signal name="U0TX10">
<contactref element="IC22" pad="35"/>
</signal>
<signal name="U0RX10">
<contactref element="IC22" pad="34"/>
</signal>
<signal name="+3V12">
<contactref element="D12" pad="2"/>
<contactref element="R89" pad="P$1"/>
<contactref element="C23" pad="P$1"/>
<contactref element="IC23" pad="8"/>
<contactref element="R90" pad="P$1"/>
<contactref element="R96" pad="P$2"/>
<contactref element="IC24" pad="2"/>
<contactref element="SMPS1:R71" pad="P$1"/>
<contactref element="SMPS1:L12" pad="P$1"/>
<contactref element="SMPS1:C57" pad="P$1"/>
</signal>
<signal name="RESET11">
<contactref element="S24" pad="1R"/>
<contactref element="S24" pad="1S"/>
<contactref element="S24" pad="2R"/>
<contactref element="S24" pad="2S"/>
<contactref element="IC24" pad="24"/>
</signal>
<signal name="RED22">
<contactref element="D12" pad="4"/>
<contactref element="R94" pad="P$2"/>
</signal>
<signal name="GREEN22">
<contactref element="D12" pad="3"/>
<contactref element="R93" pad="P$2"/>
</signal>
<signal name="BLUE22">
<contactref element="D12" pad="1"/>
<contactref element="R95" pad="P$2"/>
</signal>
<signal name="FUNCTION11">
<contactref element="S23" pad="1R"/>
<contactref element="S23" pad="1S"/>
<contactref element="S23" pad="2R"/>
<contactref element="S23" pad="2S"/>
<contactref element="IC24" pad="25"/>
</signal>
<signal name="N$265">
<contactref element="IC24" pad="16"/>
</signal>
<signal name="C12">
<contactref element="R89" pad="P$2"/>
<contactref element="C24" pad="P$2"/>
<contactref element="IC24" pad="3"/>
</signal>
<signal name="N$266">
<contactref element="S24" pad="3R"/>
<contactref element="S24" pad="3S"/>
<contactref element="S24" pad="4R"/>
<contactref element="S24" pad="4S"/>
<contactref element="R96" pad="P$1"/>
</signal>
<signal name="GREEN23">
<contactref element="R93" pad="P$1"/>
<contactref element="IC24" pad="28"/>
</signal>
<signal name="RED23">
<contactref element="R94" pad="P$1"/>
<contactref element="IC24" pad="30"/>
</signal>
<signal name="MDB_TX22">
<contactref element="IC23" pad="1"/>
<contactref element="R92" pad="P$2"/>
</signal>
<signal name="MDB_DATA_GND11">
<contactref element="IC23" pad="2"/>
<contactref element="U$23" pad="DGND"/>
<contactref element="U$24" pad="DGND"/>
</signal>
<signal name="MDB_TX23">
<contactref element="R92" pad="P$1"/>
<contactref element="U$24" pad="TX"/>
<contactref element="U$23" pad="TX"/>
</signal>
<signal name="MDB_RX11">
<contactref element="IC23" pad="6"/>
<contactref element="U$23" pad="RX"/>
<contactref element="U$24" pad="RX"/>
</signal>
<signal name="MDB_NC11">
<contactref element="U$23" pad="NC"/>
<contactref element="U$24" pad="NC"/>
</signal>
<signal name="+34V11">
<contactref element="U$23" pad="+34V"/>
<contactref element="U$24" pad="+34V"/>
<contactref element="SMPS1:IC12" pad="9"/>
<contactref element="SMPS1:IC12" pad="8"/>
<contactref element="SMPS1:R67" pad="P$2"/>
<contactref element="SMPS1:C58" pad="+"/>
<contactref element="SMPS1:C59" pad="1"/>
</signal>
<signal name="TX.11">
<contactref element="R91" pad="P$2"/>
<contactref element="IC23" pad="4"/>
</signal>
<signal name="SMPS1:FEEDBACK11">
<contactref element="SMPS1:IC12" pad="5"/>
<contactref element="SMPS1:R72" pad="P$2"/>
<contactref element="SMPS1:R71" pad="P$2"/>
</signal>
<signal name="SMPS1:SWITCH11">
<contactref element="SMPS1:IC12" pad="2"/>
<contactref element="SMPS1:IC12" pad="1"/>
<contactref element="SMPS1:L12" pad="P$2"/>
<contactref element="SMPS1:C60" pad="2"/>
<contactref element="SMPS1:U$12" pad="N"/>
</signal>
<signal name="SMPS1:N$56">
<contactref element="SMPS1:IC12" pad="4"/>
<contactref element="SMPS1:C56" pad="P$2"/>
</signal>
<signal name="SMPS1:N$57">
<contactref element="SMPS1:R70" pad="P$2"/>
<contactref element="SMPS1:C56" pad="P$1"/>
</signal>
<signal name="U1RX11">
<contactref element="IC24" pad="17"/>
<contactref element="IC23" pad="7"/>
<contactref element="R90" pad="P$2"/>
</signal>
<signal name="U1TX11">
<contactref element="IC24" pad="18"/>
<contactref element="R91" pad="P$1"/>
</signal>
<signal name="N$267">
<contactref element="IC24" pad="19"/>
</signal>
<signal name="N$268">
<contactref element="IC24" pad="20"/>
</signal>
<signal name="N$269">
<contactref element="IC24" pad="21"/>
</signal>
<signal name="N$270">
<contactref element="IC24" pad="22"/>
</signal>
<signal name="N$271">
<contactref element="IC24" pad="26"/>
</signal>
<signal name="N$272">
<contactref element="IC24" pad="27"/>
</signal>
<signal name="N$273">
<contactref element="IC24" pad="29"/>
</signal>
<signal name="N$274">
<contactref element="IC24" pad="33"/>
</signal>
<signal name="N$275">
<contactref element="IC24" pad="37"/>
</signal>
<signal name="N$276">
<contactref element="IC24" pad="36"/>
</signal>
<signal name="N$277">
<contactref element="IC24" pad="4"/>
</signal>
<signal name="N$278">
<contactref element="IC24" pad="5"/>
</signal>
<signal name="N$279">
<contactref element="IC24" pad="6"/>
</signal>
<signal name="N$280">
<contactref element="IC24" pad="7"/>
</signal>
<signal name="N$281">
<contactref element="IC24" pad="8"/>
</signal>
<signal name="N$282">
<contactref element="IC24" pad="9"/>
</signal>
<signal name="N$283">
<contactref element="IC24" pad="10"/>
</signal>
<signal name="N$284">
<contactref element="IC24" pad="11"/>
</signal>
<signal name="N$285">
<contactref element="IC24" pad="12"/>
</signal>
<signal name="SMPS1:N$58">
<contactref element="SMPS1:IC12" pad="7"/>
<contactref element="SMPS1:R68" pad="P$2"/>
</signal>
<signal name="SMPS1:N$59">
<contactref element="SMPS1:IC12" pad="3"/>
<contactref element="SMPS1:R69" pad="P$2"/>
<contactref element="SMPS1:R67" pad="P$1"/>
</signal>
<signal name="SMPS1:N$60">
<contactref element="SMPS1:IC12" pad="10"/>
<contactref element="SMPS1:C60" pad="1"/>
</signal>
<signal name="BLUE23">
<contactref element="R95" pad="P$1"/>
<contactref element="IC24" pad="31"/>
</signal>
<signal name="N$286">
<contactref element="IC24" pad="13"/>
</signal>
<signal name="N$287">
<contactref element="IC24" pad="23"/>
</signal>
<signal name="N$288">
<contactref element="IC24" pad="14"/>
</signal>
<signal name="U0TX11">
<contactref element="IC24" pad="35"/>
</signal>
<signal name="U0RX11">
<contactref element="IC24" pad="34"/>
</signal>
<signal name="S$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
