(kicad_pcb (version 4) (host pcbnew 4.0.4+e1-6308~48~ubuntu16.04.1-stable)
  (general
    (links 0)
    (no_connects 0)
    (area 78.425 62.485713 109.814287 89.775)
    (thickness 1.6)
    (drawings 18)
    (tracks 88)
    (zones 0)
    (modules 8)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.032 1.7272)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x01030_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory /home/donp/osh))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 583B886C)
    (at 94.9 75.4)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference "" (at 0 -1.9) (layer F.SilkS))
    (fp_text value R_0603 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5830FF80)
    (at 99.9 83.6 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value Pin_Header_Straight_1x02 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 583B74FF)
    (at 86.8 78.6 90)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference ATTINY (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value SOIC-8-N (at 0 1.27 90) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module ws2812:3535 (layer F.Cu) (tedit 583B7BBA)
    (at 94.7 78.9)
    (fp_text reference 3535 (at 0 2.4) (layer F.SilkS))
    (fp_text value 3535 (at 0.05 -2.2) (layer F.Fab))
    (pad IN smd rect (at 1.325 0.875) (size 1.05 0.85) (drill (offset 0.1 0)) (layers F.Cu F.Paste F.Mask))
    (pad VDD smd rect (at 1.325 -0.875) (size 1.05 0.85) (drill (offset 0.1 0)) (layers F.Cu F.Paste F.Mask))
    (pad GND smd rect (at -1.325 0.875) (size 1.05 0.85) (drill (offset -0.1 0)) (layers F.Cu F.Paste F.Mask))
    (pad OUT smd rect (at -1.325 -0.875) (size 1.05 0.85) (drill (offset -0.1 0)) (layers F.Cu F.Paste F.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 583B81A8)
    (at 84.5 72.4 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value Pin_Header_Straight_1x04 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5830FFE6)
    (at 99.9 71.9)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1) (layer F.SilkS))
    (fp_text value Pin_Header_Straight_1x03 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 583B8881)
    (at 94.6 84.1 180)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference "" (at 0 -2 180) (layer F.SilkS))
    (fp_text value LED_1206 (at 0 2 180) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 583B886C)
    (at 89.8 83.8)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference "" (at 0 -1.9) (layer F.SilkS))
    (fp_text value R_0603 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text D (at 101.6 74.5) (layer F.SilkS))
  (gr_text OUT (at 94.5 78.1) (layer F.SilkS))
  (gr_text IN (at 95.2 79.8) (layer F.SilkS))
  (gr_text "+\nV" (at 95.3 78.1) (layer F.SilkS))
  (gr_text "G\nN\nD" (at 94.2 79.6) (layer F.SilkS))
  (gr_text 1 (at 88.8 80.6) (layer F.SilkS))
  (gr_text +V (at 101.4 72.5) (layer F.SilkS))
  (gr_text "G\nN\nD" (at 101.4 77.2) (layer F.SilkS))
  (gr_text "G\nN\nD" (at 101.4 81) (layer F.SilkS))
  (gr_text +5.5 (at 101.5 83) (layer F.SilkS))
  (gr_text 2.7v-5.5v (at 82.8 81.4) (layer F.SilkS))
  (gr_text 3.7-5.5v (at 96.6 76.9) (layer F.SilkS))
  (gr_text donp.org (at 84.2 84.7) (layer B.SilkS))
  (gr_text "NeoTiny 2017 Jan" (at 86.6 85) (layer F.SilkS))
  (gr_line (start 102 69.8) (end 102 85.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81 85.6) (end 102 85.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81 69.8) (end 102 69.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81 69.8) (end 81 85.6) (angle 90) (layer Edge.Cuts) (width 0.15))
)
