(kicad_pcb (version 20171130) (host pcbnew 5.1.2)
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 39)
    (zones 0)
    (modules 9)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.0254)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J0-Pad3)")
  (net 2 "Net-(J0-Pad1)")
  (net 3 "Net-(A1-Pad1)")
  (net 4 "Net-(A2-Pad1)")
  (net 5 "Net-(B1-Pad1)")
  (net 6 "Net-(B2-Pad1)")
  (net 7 "Net-(H1-Pad1)")
  (net 8 "Net-(H2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(A2-Pad1)")
    (add_net "Net-(B1-Pad1)")
    (add_net "Net-(B2-Pad1)")
    (add_net "Net-(H1-Pad1)")
    (add_net "Net-(H2-Pad1)")
    (add_net "Net-(J0-Pad1)")
    (add_net "Net-(J0-Pad3)")
  )
  (module bottom:samtec-fte-105-03-g-dv (layer F.Cu) (tedit 5D1236BA)
    (at 0 -10.16 270)
    (fp_text reference J0 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text value Conn_02x05_Counter_Clockwise (at 0 6.35 90) (layer F.Fab) hide)
    (pad 10 smd rect (at -1.6002 1.9812 270) (size 0.508 1.3716) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(H2-Pad1)"))
    (pad 9 smd rect (at -0.8001 1.9812 270) (size 0.508 1.3716) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(H1-Pad1)"))
    (pad 8 smd rect (at 0 1.9812 270) (size 0.508 1.3716) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(A2-Pad1)"))
    (pad 7 smd rect (at 0.8001 1.9812 270) (size 0.508 1.3716) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(A1-Pad1)"))
    (pad 6 smd rect (at 1.6002 1.9812 270) (size 0.508 1.3716) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(B2-Pad1)"))
    (pad 5 smd rect (at 1.6002 -1.9812 270) (size 0.508 1.3716) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(B1-Pad1)"))
    (pad 4 smd rect (at 0.8001 -1.9812 270) (size 0.508 1.3716) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J0-Pad3)"))
    (pad 3 smd rect (at 0 -1.9812 270) (size 0.508 1.3716) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J0-Pad3)"))
    (pad 2 smd rect (at -0.8001 -1.9812 270) (size 0.508 1.3716) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J0-Pad1)"))
    (pad 1 smd rect (at -1.6002 -1.9812 270) (size 0.508 1.3716) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J0-Pad1)"))
    (model /home/zach/research/pcbs/3d/FTE-105-03-G-DV.stp
      (offset (xyz 0 0 0.3302))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module bottom:wire-pad (layer F.Cu) (tedit 5D095D0E)
    (at 7.10216 -8.464025 140)
    (fp_text reference T2 (at 0 1.397 320 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81 140) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 140) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(J0-Pad3)"))
  )
  (module bottom:wire-pad (layer F.Cu) (tedit 5D095D0E)
    (at 5.5245 -9.568715 150)
    (fp_text reference T1 (at 0 1.397 330 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81 150) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 150) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(J0-Pad1)"))
  )
  (module bottom:wire-pad (layer F.Cu) (tedit 5D095D0E)
    (at -5.5245 -9.568715 210)
    (fp_text reference H2 (at 0 1.397 30 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81 30) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 210) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(H2-Pad1)"))
  )
  (module bottom:wire-pad (layer F.Cu) (tedit 5D095D0E)
    (at -7.10216 -8.464025 220)
    (fp_text reference H1 (at 0 1.397 40 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81 40) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 220) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(H1-Pad1)"))
  )
  (module bottom:wire-pad (layer F.Cu) (tedit 5D095D0E)
    (at 10.013795 -4.669509 115)
    (fp_text reference B2 (at 0 1.397 295 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81 115) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 115) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(B2-Pad1)"))
  )
  (module bottom:wire-pad (layer F.Cu) (tedit 5D095D0E)
    (at 9.050811 -6.337446 125)
    (fp_text reference B1 (at 0 1.397 305 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81 125) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 125) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(B1-Pad1)"))
  )
  (module bottom:wire-pad (layer F.Cu) (tedit 5D095D0E)
    (at -9.05081 -6.337447 235)
    (fp_text reference A2 (at 0 1.397 55 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81 55) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 235) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(A2-Pad1)"))
  )
  (module bottom:wire-pad (layer F.Cu) (tedit 5D095D0E)
    (at -10.013795 -4.669509 245)
    (fp_text reference A1 (at 0 1.397 65 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81 65) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 245) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(A1-Pad1)"))
  )
  (gr_arc (start -9.525 0) (end -7.62 2.539998) (angle -106.260165) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 9.525 0) (end 7.62 -2.539998) (angle -106.260165) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 0 -1.27) (end -7.619999 2.539999) (angle -126.8698976) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 0 1.27) (end 7.619999 -2.539999) (angle -126.8698976) (layer Edge.Cuts) (width 0.05))
  (gr_text "The through holes are large enough for 2-56 screws, but normal (e.g. round-head) screws will likely touch the copper ring. Either turn the screw heads down or use e.g. \"Brass High-Profile Narrow Filister Head Slotted Screws\" from McMaster-Carr (PN: 90114A127)." (at -7.5 22.5) (layer Dwgs.User))
  (gr_circle (center 0 0) (end 13.589 0) (layer Edge.Cuts) (width 0.127))
  (gr_circle (center -8.255 0) (end -7.1247 0) (layer Edge.Cuts) (width 0.127))
  (gr_circle (center 8.255 0) (end 9.3853 0) (layer Edge.Cuts) (width 0.127))
)
