<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="96.19" x2="1.27" y2="10.16" width="0" layer="20"/>
<wire x1="1.27" y1="10.16" x2="5.08" y2="6.35" width="0" layer="20" curve="90"/>
<wire x1="5.08" y1="6.35" x2="76.19" y2="6.35" width="0" layer="20"/>
<wire x1="76.19" y1="6.35" x2="80" y2="10.16" width="0" layer="20" curve="90"/>
<wire x1="80" y1="10.16" x2="80" y2="96.19" width="0" layer="20"/>
<wire x1="80" y1="96.19" x2="76.19" y2="100" width="0" layer="20" curve="90"/>
<wire x1="76.19" y1="100" x2="5.08" y2="100" width="0" layer="20"/>
<wire x1="5.08" y1="100" x2="1.27" y2="96.19" width="0" layer="20" curve="90"/>
<text>AC N</text>
<text>AC L</text>
<text>NC</text>
<text>NO</text>
<text>NC</text>
<text>NO</text>
<text>HEAT AC L</text>
<text>COOL AC L</text>
<text>AC N</text>
<text>AC N</text>
<wire x1="24.765" y1="71.755" x2="25.4" y2="71.755" width="0.3048" layer="20"/>
<wire x1="25.4" y1="71.755" x2="25.4" y2="69.215" width="0.3048" layer="20"/>
<wire x1="25.4" y1="69.215" x2="26.67" y2="67.945" width="0.3048" layer="20"/>
<wire x1="26.67" y1="67.945" x2="32.385" y2="67.945" width="0.3048" layer="20"/>
<wire x1="32.385" y1="67.945" x2="33.655" y2="66.675" width="0.3048" layer="20"/>
<wire x1="33.655" y1="66.675" x2="33.655" y2="61.595" width="0.3048" layer="20"/>
<wire x1="33.655" y1="61.595" x2="32.385" y2="60.325" width="0.3048" layer="20"/>
<wire x1="32.385" y1="60.325" x2="24.765" y2="60.325" width="0.3048" layer="20"/>
<wire x1="24.765" y1="60.325" x2="24.765" y2="60.96" width="0.3048" layer="20"/>
<wire x1="24.765" y1="60.96" x2="31.75" y2="60.96" width="0.3048" layer="20"/>
<wire x1="31.75" y1="60.96" x2="33.02" y2="62.23" width="0.3048" layer="20"/>
<wire x1="33.02" y1="62.23" x2="33.02" y2="66.04" width="0.3048" layer="20"/>
<wire x1="33.02" y1="66.04" x2="31.75" y2="67.31" width="0.3048" layer="20"/>
<wire x1="31.75" y1="67.31" x2="26.67" y2="67.31" width="0.3048" layer="20"/>
<wire x1="26.67" y1="67.31" x2="24.765" y2="69.215" width="0.3048" layer="20"/>
<wire x1="24.765" y1="69.215" x2="24.765" y2="71.755" width="0.3048" layer="20"/>
<text>JLCJLCJLCJLC</text>
<text>AC L</text>
<text>AC N</text>
<text>GND</text>
<text>+5V</text>
<wire x1="24.765" y1="54.61" x2="25.4" y2="54.61" width="0.3048" layer="20"/>
<wire x1="25.4" y1="54.61" x2="25.4" y2="52.07" width="0.3048" layer="20"/>
<wire x1="25.4" y1="52.07" x2="26.67" y2="50.8" width="0.3048" layer="20"/>
<wire x1="26.67" y1="50.8" x2="32.385" y2="50.8" width="0.3048" layer="20"/>
<wire x1="32.385" y1="50.8" x2="33.655" y2="49.53" width="0.3048" layer="20"/>
<wire x1="33.655" y1="49.53" x2="33.655" y2="44.45" width="0.3048" layer="20"/>
<wire x1="33.655" y1="44.45" x2="32.385" y2="43.18" width="0.3048" layer="20"/>
<wire x1="32.385" y1="43.18" x2="24.765" y2="43.18" width="0.3048" layer="20"/>
<wire x1="24.765" y1="43.18" x2="24.765" y2="43.815" width="0.3048" layer="20"/>
<wire x1="24.765" y1="43.815" x2="31.75" y2="43.815" width="0.3048" layer="20"/>
<wire x1="31.75" y1="43.815" x2="33.02" y2="45.085" width="0.3048" layer="20"/>
<wire x1="33.02" y1="45.085" x2="33.02" y2="48.895" width="0.3048" layer="20"/>
<wire x1="33.02" y1="48.895" x2="31.75" y2="50.165" width="0.3048" layer="20"/>
<wire x1="31.75" y1="50.165" x2="26.67" y2="50.165" width="0.3048" layer="20"/>
<wire x1="26.67" y1="50.165" x2="24.765" y2="52.07" width="0.3048" layer="20"/>
<wire x1="24.765" y1="52.07" x2="24.765" y2="54.61" width="0.3048" layer="20"/>
<text>HEAT AC L</text>
<text>COOL AC L</text>
<text>AC N</text>
<text>AC N</text>
<text>BrewPi ESP32 AIO
v0.1
@thorrak says hi</text>
<text>+3v3</text>
<text>+5v</text>
<text>OW</text>
<text>AC L</text>
<text>AC N</text>
<text>2A</text>
<text>8A</text>
<text>+5v</text>
<text>OW</text>
<text>+3v3</text>
</plain>
<libraries>
<library name="Donnie">
<packages>
<package name="SMD-0805">
</package>
<package name="DIOM4325X250N">
</package>
<package name="FUSE_BK/PCE-5-R">
</package>
<package name="FUSRR508W60L835T400H810">
</package>
<package name="CONV_PSK-10D-5">
</package>
<package name="S10K350">
<description>&lt;b&gt;VARISTOR&lt;/b&gt;</description>
</package>
<package name="CAPPRD750W80D1600H2700">
</package>
<package name="1.152">
<description>&lt;b&gt;SMT Tooling Hole&lt;/b&gt; 1.152 mm with drill center</description>
</package>
<package name="D32_PRO_NO-KEEPOUT">
</package>
<package name="JP2-NOLABEL">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="LED_SMD_0603">
</package>
<package name="SOIC127P700X210-4N">
</package>
</packages>
</library>
<library name="con-wago-500">
<description>&lt;b&gt;Wago Screw Clamps&lt;/b&gt;&lt;p&gt;
Grid 5.00 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="W237-102">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO214AC">
<description>&lt;b&gt;DIODE&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SRD-05VDC-SL-C">
<packages>
<package name="SRD-05VDC-SL-C">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,0">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.0 mm with drill center</description>
</package>
</packages>
</library>
<library name="Box Header">
<packages>
<package name="MA05-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="RJ45-NO-SHIELD">
<description>&lt;b&gt;RJ45 Low Profile&lt;/b&gt; No Shield&lt;p&gt;
For all RJ45 N and Z Series Models&lt;br&gt;
Source: www.tycoelectronics.com .. ENG_DS_1654001_1099_RJ_L_0507.pdf</description>
</package>
</packages>
</library>
<library name="semicon-smd-ipc">
<description>&lt;b&gt;IPC Standard SMD Semiconductors&lt;/b&gt;&lt;p&gt;
A few devices defined according to the IPC standard.&lt;p&gt;
Based on:&lt;p&gt;
IPC-SM-782&lt;br&gt;
IRevision A, August 1993&lt;br&gt;
Includes Amendment 1, October 1996&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ_2">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="PS1" library="Donnie" package="CONV_PSK-10D-5" value="PSK-10D-5">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="CUI_PURCHASE_URL" value="https://www.cui.com/product/internal-ac-dc-power-supplies/board-mount/psk-10d-series?utm_source=snapeda.com&amp;utm_medium=referral&amp;utm_campaign=snapedaBOM"/>
<attribute name="DESCRIPTION" value=" 10 W, 85 ~ 305 Vac Input, Single Output, Encapsulated, Board Mount, Ac-Dc Power Supply "/>
<attribute name="MF" value="CUI"/>
<attribute name="MP" value="PSK-10D-5"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="DIP-6 CUI"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/PSK-10D-5/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="Donnie" package="SMD-0805" value="1uF">
<attribute name="LCSC_PART" value="C28323"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="Donnie" package="CAPPRD750W80D1600H2700" value="220uF">
<attribute name="LCSC_PART" value="C43349"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="Donnie" package="S10K350" value="S14K350">
<attribute name="DIGIKEY" value="495-76419-ND"/>
<attribute name="LCSC_PART" value="C78355"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="Donnie" package="DIOM4325X250N" value="SMAJ7.0A">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" 12V Clamp 33.3A Ipp Tvs Diode Surface Mount DO-214AC (SMA) "/>
<attribute name="LCSC_PART" value="C309904"/>
<attribute name="MF" value="Littelfuse"/>
<attribute name="MP" value="SMAJ7.0A"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="DO-214 Littelfuse"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/SMAJ7.0A/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="Donnie" package="SMD-0805" value="0.1uF">
<attribute name="LCSC_PART" value="C49678"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="con-wago-500" package="W237-102" value="">
<attribute name="LCSC_PART" value="C8269"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-102"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="POPULARITY" value="32"/>
<attribute name="VALUE"/>
</element>
<element name="F2" library="Donnie" package="FUSE_BK/PCE-5-R" value="2A_SLOW">
<attribute name="DIGIKEY" value="283-4166-1-ND"/>
<attribute name="MANUF" value="SS-5H-2A-APH"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HEAT" library="Donnie" package="LED_SMD_0603" value="LED_0603LED_SMD_0603">
<attribute name="DESCRIPTION" value=" Red 620nm LED Indication - Discrete 2.2V 0603 (1608 Metric) "/>
<attribute name="LCSC_PART" value="C2286"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0603 Rohm"/>
</element>
<element name="D3" library="diode" package="DO214AC" value="">
<attribute name="LCSC_PART" value="C95872"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="14"/>
<attribute name="VALUE"/>
</element>
<element name="HEAT_RELAY" library="SRD-05VDC-SL-C" package="SRD-05VDC-SL-C" value="RELAYPTH">
<attribute name="JLC_X" value="-0.3"/>
<attribute name="JLC_Y" value="-0.2"/>
<attribute name="LCSC_PART" value="C35449"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="COOL" library="Donnie" package="LED_SMD_0603" value="LED_0603LED_SMD_0603">
<attribute name="DESCRIPTION" value=" Red 620nm LED Indication - Discrete 2.2V 0603 (1608 Metric) "/>
<attribute name="LCSC_PART" value="C2286"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0603 Rohm"/>
</element>
<element name="D4" library="diode" package="DO214AC" value="">
<attribute name="LCSC_PART" value="C95872"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="14"/>
<attribute name="VALUE"/>
</element>
<element name="COOL_RELAY" library="SRD-05VDC-SL-C" package="SRD-05VDC-SL-C" value="RELAYPTH">
<attribute name="JLC_X" value="-0.3"/>
<attribute name="JLC_Y" value="-0.2"/>
<attribute name="LCSC_PART" value="C35449"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="holes" package="3,0" value=""/>
<element name="U$2" library="holes" package="3,0" value=""/>
<element name="U$3" library="holes" package="3,0" value=""/>
<element name="U$4" library="holes" package="3,0" value=""/>
<element name="X3" library="con-wago-500" package="W237-102" value="">
<attribute name="LCSC_PART" value="C8269"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-102"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="POPULARITY" value="32"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="con-wago-500" package="W237-102" value="">
<attribute name="LCSC_PART" value="C8269"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-102"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="POPULARITY" value="32"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="Donnie" package="FUSRR508W60L835T400H810" value="0697H8000-01">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" 2-Pin Radial Fuse | Rectangular | Slow Blow | UL | Bulk Pack | 8A "/>
<attribute name="DIGIKEY" value="507-1915-ND"/>
<attribute name="MF" value="Bel Fuse"/>
<attribute name="MP" value="0697H8000-01"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="Radial Box  Bel Fuse"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/0697H8000-01/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="U$5" library="Donnie" package="1.152" value=""/>
<element name="U$6" library="Donnie" package="1.152" value=""/>
<element name="R1" library="Donnie" package="SMD-0805" value="680R">
<attribute name="LCSC_PART" value="C17798"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PWR" library="Donnie" package="LED_SMD_0603" value="LED_0603LED_SMD_0603">
<attribute name="DESCRIPTION" value=" Red 620nm LED Indication - Discrete 2.2V 0603 (1608 Metric) "/>
<attribute name="LCSC_PART" value="C2286"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0603 Rohm"/>
</element>
<element name="U$7" library="Donnie" package="D32_PRO_NO-KEEPOUT" value="WEMOS-D32D32_PRO_NO-KEEPOUT"/>
<element name="X4" library="Box Header" package="RJ45-NO-SHIELD" value="RJ45-8X">
<attribute name="JLC_Y" value="7.55"/>
<attribute name="LCSC_PART" value="C3000197"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="RJ45-8X"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16R6101"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="Donnie" package="SMD-0805" value="4.7k">
<attribute name="LCSC_PART" value="C17673"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TFT" library="Box Header" package="MA05-2" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="14"/>
<attribute name="VALUE"/>
</element>
<element name="OW_VSEL" library="Donnie" package="JP2-NOLABEL" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="Donnie" package="SMD-0805" value="1uF">
<attribute name="LCSC_PART" value="C28323"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="Donnie" package="SMD-0805" value="0.1uF">
<attribute name="LCSC_PART" value="C49678"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="Donnie" package="SMD-0805" value="1uF">
<attribute name="LCSC_PART" value="C28323"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="Donnie" package="SMD-0805" value="0.1uF">
<attribute name="LCSC_PART" value="C49678"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="semicon-smd-ipc" package="SOT23" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="semicon-smd-ipc" package="SOT23" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="Donnie" package="SOIC127P700X210-4N" value="BPC-817S">
<attribute name="LCSC_PART" value="C106900"/>
<attribute name="NAME"/>
</element>
<element name="U2" library="Donnie" package="SOIC127P700X210-4N" value="BPC-817S">
<attribute name="LCSC_PART" value="C106900"/>
<attribute name="NAME"/>
</element>
<element name="R4" library="Donnie" package="SMD-0805" value="1k">
<attribute name="LCSC_PART" value="C17513"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="Donnie" package="SMD-0805" value="1k">
<attribute name="LCSC_PART" value="C17513"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="Donnie" package="SMD-0805" value="0R">
<attribute name="LCSC_PART" value="C17477"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="Donnie" package="SMD-0805" value="0R">
<attribute name="LCSC_PART" value="C17477"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ_OW" library="jumper" package="SJ_2" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="7"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="PS1" pad="6"/>
<contactref element="C5" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="C6" pad="2"/>
<contactref element="PWR" pad="C"/>
<contactref element="X4" pad="5"/>
<contactref element="TFT" pad="3"/>
<contactref element="U$7" pad="GND"/>
<contactref element="U$7" pad="GND2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="HEAT_RELAY" pad="COIL1"/>
<contactref element="D3" pad="C"/>
<contactref element="COOL_RELAY" pad="COIL1"/>
<contactref element="D4" pad="C"/>
<contactref element="TFT" pad="1"/>
<contactref element="U$7" pad="VBUS"/>
<contactref element="OW_VSEL" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="PS1" pad="4"/>
<contactref element="C5" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="C6" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="U2" pad="4"/>
<contactref element="SJ_OW" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="2"/>
<contactref element="PS1" pad="1"/>
<contactref element="F2" pad="2"/>
</signal>
<signal name="AC_N">
<contactref element="PS1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="X2" pad="2"/>
<contactref element="X3" pad="2"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="AC_L">
<contactref element="F2" pad="1"/>
<contactref element="X1" pad="1"/>
<contactref element="F1" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="HEAT" pad="A"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="HEAT_RELAY" pad="COIL0"/>
<contactref element="D3" pad="A"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$16">
<contactref element="COOL" pad="A"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="HEAT">
<contactref element="HEAT" pad="C"/>
<contactref element="U$7" pad="IO25"/>
</signal>
<signal name="COOL">
<contactref element="COOL" pad="C"/>
<contactref element="U$7" pad="IO26"/>
</signal>
<signal name="HEAT_AC">
<contactref element="HEAT_RELAY" pad="SWCLOSED"/>
<contactref element="X2" pad="1"/>
</signal>
<signal name="COOL_AC">
<contactref element="COOL_RELAY" pad="SWCLOSED"/>
<contactref element="X3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="PWR" pad="A"/>
</signal>
<signal name="VCC">
<contactref element="R3" pad="2"/>
<contactref element="U$7" pad="VCC"/>
<contactref element="OW_VSEL" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="SJ_OW" pad="1"/>
</signal>
<signal name="DOOR">
<contactref element="X4" pad="6"/>
<contactref element="U$7" pad="IO34"/>
</signal>
<signal name="VBUS">
<contactref element="X4" pad="3"/>
<contactref element="OW_VSEL" pad="2"/>
<contactref element="SJ_OW" pad="2"/>
</signal>
<signal name="DC">
<contactref element="U$7" pad="IO27"/>
<contactref element="TFT" pad="9"/>
</signal>
<signal name="CS">
<contactref element="U$7" pad="IO14"/>
<contactref element="TFT" pad="5"/>
</signal>
<signal name="T_CS">
<contactref element="U$7" pad="IO12"/>
<contactref element="TFT" pad="10"/>
</signal>
<signal name="RESET">
<contactref element="U$7" pad="IO33"/>
<contactref element="TFT" pad="7"/>
</signal>
<signal name="LED">
<contactref element="U$7" pad="IO32"/>
<contactref element="TFT" pad="6"/>
</signal>
<signal name="MOSI">
<contactref element="U$7" pad="IO23"/>
<contactref element="TFT" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="U$7" pad="IO19"/>
<contactref element="TFT" pad="8"/>
</signal>
<signal name="SCK">
<contactref element="U$7" pad="IO18"/>
<contactref element="TFT" pad="4"/>
</signal>
<signal name="1WIRE">
<contactref element="U$7" pad="IO13"/>
<contactref element="X4" pad="4"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="3"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R4" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="COOL_RELAY" pad="COIL0"/>
<contactref element="D4" pad="A"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="U2" pad="3"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R5" pad="2"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R6" pad="2"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R7" pad="2"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="FUSED_AC_L">
<contactref element="F1" pad="1"/>
<contactref element="HEAT_RELAY" pad="SWCOMMON"/>
<contactref element="COOL_RELAY" pad="SWCOMMON"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
