(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 39)
    (no_connects 0)
    (area 81.585999 91.872999 109.168001 113.613001)
    (thickness 1.6)
    (drawings 13)
    (tracks 103)
    (zones 0)
    (modules 19)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 "/CAN 1/CAN_H")
  (net 4 "/CAN 1/CAN_L")
  (net 5 "/CAN 2/CAN_H")
  (net 6 "/CAN 2/CAN_L")
  (net 7 "/CAN 3/CAN_H")
  (net 8 "/CAN 3/CAN_L")
  (net 9 "/CAN 1/TXD")
  (net 10 "/CAN 1/RXD")
  (net 11 "/CAN 2/TXD")
  (net 12 "/CAN 2/RXD")
  (net 13 "/CAN 3/TXD")
  (net 14 "/CAN 3/RXD")
  (net 15 "Net-(R1-Pad1)")
  (net 16 "Net-(R2-Pad1)")
  (net 17 "Net-(R3-Pad1)")
  (net 18 "Net-(R4-Pad1)")
  (net 19 "Net-(R5-Pad1)")
  (net 20 "Net-(R6-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net "/CAN 1/CAN_H")
    (add_net "/CAN 1/CAN_L")
    (add_net "/CAN 1/RXD")
    (add_net "/CAN 1/TXD")
    (add_net "/CAN 2/CAN_H")
    (add_net "/CAN 2/CAN_L")
    (add_net "/CAN 2/RXD")
    (add_net "/CAN 2/TXD")
    (add_net "/CAN 3/CAN_H")
    (add_net "/CAN 3/CAN_L")
    (add_net "/CAN 3/RXD")
    (add_net "/CAN 3/TXD")
    (add_net GND)
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5906AD23)
    (at 91.44 95.504 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0.254 1.778 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0.254 1.778 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5906AD17)
    (at 91.567 102.87 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -0.889 -2.159 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at -0.889 -2.159 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5906AD2E)
    (at 91.44 109.982 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0.127 -1.905 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0.127 -1.905 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 99.822 95.504)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D1 (at 0 -2.5) (layer F.SilkS))
    (fp_text value PESD2CAN (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "/CAN 1/CAN_H"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "/CAN 1/CAN_L"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 99.822 102.87)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D2 (at 0 -2.5) (layer F.SilkS))
    (fp_text value PESD2CAN (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "/CAN 2/CAN_H"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "/CAN 2/CAN_L"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 99.822 109.982)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D3 (at 0 -2.5) (layer F.SilkS))
    (fp_text value PESD2CAN (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "/CAN 3/CAN_H"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "/CAN 3/CAN_L"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 5906B1CD)
    (at 83.693 93.853)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J1 (at 2.413 -0.889) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/CAN 1/TXD"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/CAN 1/RXD"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/CAN 2/TXD"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "/CAN 2/RXD"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "/CAN 3/TXD"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "/CAN 3/RXD"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_2pol (layer F.Cu) (tedit 5906AB6D)
    (at 105.41 94.234 270)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J2 (at 3.048 -2.032 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.27 4.50088 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 4 "/CAN 1/CAN_L"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 3 "/CAN 1/CAN_H"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_2pol.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_2pol (layer F.Cu) (tedit 5906AB60)
    (at 105.41 108.712 270)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J3 (at 3.048 -2.032 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.27 4.50088 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 8 "/CAN 3/CAN_L"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 7 "/CAN 3/CAN_H"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_2pol.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_2pol (layer F.Cu) (tedit 5906AB65)
    (at 105.41 101.6 270)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J4 (at 3.048 -2.032 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.27 4.50088 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 6 "/CAN 2/CAN_L"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 5 "/CAN 2/CAN_H"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_2pol.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5906AD05)
    (at 87.63 96.393 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 1.778 180) (layer F.SilkS))
    (fp_text value 0R (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "/CAN 1/TXD"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5906A8B9)
    (at 87.63 98.933 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -2.794 0 180) (layer F.SilkS))
    (fp_text value 0R (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "/CAN 1/RXD"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5906ACFF)
    (at 87.63 101.473 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -2.794 0.381 180) (layer F.SilkS))
    (fp_text value 0R (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "/CAN 2/TXD"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5906ACF9)
    (at 87.63 104.013 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -2.794 -0.508 180) (layer F.SilkS))
    (fp_text value 0R (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "/CAN 2/RXD"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5906ACF4)
    (at 87.63 106.553 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -2.667 -0.381 180) (layer F.SilkS))
    (fp_text value 0R (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "/CAN 3/TXD"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5906ACEB)
    (at 87.63 109.093 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value 0R (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "/CAN 3/RXD"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-8 (layer F.Cu) (tedit 58CE4E7E)
    (at 95.25 95.504)
    (descr "8-pin SOT-23 package, http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/sot-23rj/rj_8.pdf")
    (tags SOT-23-8)
    (attr smd)
    (fp_text reference U1 (at 0 -2.5) (layer F.SilkS))
    (fp_text value TCAN33x (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.98) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at -1.1 -0.33) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.33) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 4 smd rect (at -1.1 0.98) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R2-Pad1)"))
    (pad 5 smd rect (at 1.1 0.98) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.1 0.33) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 "/CAN 1/CAN_L"))
    (pad 7 smd rect (at 1.1 -0.33) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "/CAN 1/CAN_H"))
    (pad 8 smd rect (at 1.1 -0.98) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-8 (layer F.Cu) (tedit 58CE4E7E)
    (at 95.377 102.87)
    (descr "8-pin SOT-23 package, http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/sot-23rj/rj_8.pdf")
    (tags SOT-23-8)
    (attr smd)
    (fp_text reference U2 (at 0 -2.5) (layer F.SilkS))
    (fp_text value TCAN33x (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.98) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at -1.1 -0.33) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.33) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 4 smd rect (at -1.1 0.98) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R4-Pad1)"))
    (pad 5 smd rect (at 1.1 0.98) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.1 0.33) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 "/CAN 2/CAN_L"))
    (pad 7 smd rect (at 1.1 -0.33) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 "/CAN 2/CAN_H"))
    (pad 8 smd rect (at 1.1 -0.98) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-8 (layer F.Cu) (tedit 58CE4E7E)
    (at 95.377 109.982)
    (descr "8-pin SOT-23 package, http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/sot-23rj/rj_8.pdf")
    (tags SOT-23-8)
    (attr smd)
    (fp_text reference U3 (at 0 -2.5) (layer F.SilkS))
    (fp_text value TCAN33x (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.98) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at -1.1 -0.33) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.33) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 4 smd rect (at -1.1 0.98) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R6-Pad1)"))
    (pad 5 smd rect (at 1.1 0.98) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.1 0.33) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 "/CAN 3/CAN_L"))
    (pad 7 smd rect (at 1.1 -0.33) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 "/CAN 3/CAN_H"))
    (pad 8 smd rect (at 1.1 -0.98) (size 1.06 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text FreECU.org (at 97.536 111.76) (layer B.SilkS))
  (gr_text "CAN 3 ->" (at 96.012 107.823) (layer B.SilkS))
  (gr_text "CAN 2 ->\n\n" (at 96.012 104.013) (layer B.SilkS))
  (gr_text "CAN 1 ->" (at 96.012 97.536) (layer B.SilkS))
  (gr_text "TX\nRX" (at 86.995 97.79) (layer B.SilkS))
  (gr_text "TX\nRX" (at 86.995 102.743) (layer B.SilkS))
  (gr_text "TX\nRX" (at 86.995 107.95) (layer B.SilkS))
  (gr_text "GND\n" (at 87.757 112.014) (layer B.SilkS))
  (gr_text 3V3 (at 87.503 93.472) (layer B.SilkS))
  (gr_line (start 81.661 91.948) (end 81.661 113.538) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.093 91.948) (end 81.661 91.948) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.093 113.538) (end 109.093 91.948) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.661 113.538) (end 109.093 113.538) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.661 113.538) (xy 81.661 91.948) (xy 109.093 91.948) (xy 109.093 113.538)
      )
    )
  )
)
