(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 451)
    (zones 0)
    (modules 34)
    (nets 28)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.254000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 BA)
  (net 2 BB)
  (net 3 BC)
  (net 4 BD)
  (net 5 BE)
  (net 6 BF)
  (net 7 BG)
  (net 8 BH)
  (net 9 10)
  (net 10 11)
  (net 11 GND)
  (net 12 5V)
  (net 13 "Net-(R1-Pad2)")
  (net 14 "Net-(R2-Pad2)")
  (net 15 "Net-(R3-Pad2)")
  (net 16 "Net-(R4-Pad2)")
  (net 17 "Net-(R5-Pad2)")
  (net 18 "Net-(R6-Pad2)")
  (net 19 "Net-(R7-Pad2)")
  (net 20 "Net-(R8-Pad2)")
  (net 21 VCC)
  (net 22 SRCLK)
  (net 23 RCLK)
  (net 24 OE)
  (net 25 SER)
  (net 26 12)
  (net 27 "Net-(U1-Pad9)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 10)
    (add_net 11)
    (add_net 12)
    (add_net 5V)
    (add_net BA)
    (add_net BB)
    (add_net BC)
    (add_net BD)
    (add_net BE)
    (add_net BF)
    (add_net BG)
    (add_net BH)
    (add_net GND)
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(U1-Pad9)")
    (add_net OE)
    (add_net RCLK)
    (add_net SER)
    (add_net SRCLK)
    (add_net VCC)
  )
  (module AOR_custom:AOR_LOGO (layer B.Cu) (tedit 5C26ADAA)
    (at 62.735 55.61 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value AOR_LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C9D86B5)
    (at 245.615 63.865)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C9D86B0)
    (at 245.615 44.815)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C9D86A4)
    (at 133.855 63.865)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C9D86A0)
    (at 133.855 44.815)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C9D8699)
    (at 22.73 63.865)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 12.57 64.5 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.82 180) (layer F.SilkS))
    (fp_text value R_US (at 0 1.82 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 13 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 30.35 63.23 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value R_US (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 5V))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 14 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 65.91 63.23 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value R_US (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 15 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 105.28 63.23 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value R_US (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 5V))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 16 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 141.475 63.23 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value R_US (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 5V))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 17 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 180.845 63.23 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value R_US (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 18 "Net-(R6-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 217.675 65.262 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value R_US (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 5V))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 19 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 255.14 63.23 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value R_US (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 20 "Net-(R8-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 2.41 46.72)
    (fp_text reference SW1 (at 5.08 5.715) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 1 BA) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(R1-Pad2)"))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 9 10) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 2.41 61.72)
    (fp_text reference SW2 (at -3.175 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 10 11) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(R1-Pad2)"))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 1 BA) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 40.088571 46.72)
    (fp_text reference SW3 (at 5.501429 5.715) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 2 BB) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 "Net-(R2-Pad2)"))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 9 10) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 40.088571 61.72)
    (fp_text reference SW4 (at -4.658571 -5.475) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 10 11) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 "Net-(R2-Pad2)"))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 2 BB) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 77.767142 46.72)
    (fp_text reference SW5 (at 5.287858 5.715) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 3 BC) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 "Net-(R3-Pad2)"))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 9 10) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 77.767142 61.72)
    (fp_text reference SW6 (at -5.507142 -5.475) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 10 11) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 "Net-(R3-Pad2)"))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 3 BC) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 115.445713 46.72)
    (fp_text reference SW7 (at 5.709287 5.08) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 9 10) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 "Net-(R4-Pad2)"))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 4 BD) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 115.445713 61.72)
    (fp_text reference SW8 (at -6.355713 -4.84) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 4 BD) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 "Net-(R4-Pad2)"))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 10 11) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 153.124284 46.72)
    (fp_text reference SW9 (at 6.130716 5.08) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 5 BE) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 "Net-(R5-Pad2)"))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 9 10) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 153.124284 61.72)
    (fp_text reference SW10 (at -6.569284 -4.84) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 10 11) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 "Net-(R5-Pad2)"))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 5 BE) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 190.802855 46.72)
    (fp_text reference SW11 (at 6.552145 5.08) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 9 10) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 "Net-(R6-Pad2)"))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 6 BF) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 190.802855 61.72)
    (fp_text reference SW12 (at -6.782855 -4.84) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 6 BF) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 "Net-(R6-Pad2)"))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 10 11) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 228.481426 46.72)
    (fp_text reference SW13 (at 6.973574 5.08) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 7 BG) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 "Net-(R7-Pad2)"))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 9 10) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 228.481426 61.72)
    (fp_text reference SW14 (at -6.996426 -4.84) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 10 11) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 "Net-(R7-Pad2)"))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 7 BG) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 266.16 46.72)
    (fp_text reference SW15 (at -7.845 4.445) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 9 10) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 "Net-(R8-Pad2)"))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 8 BH) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 266.16 61.72)
    (fp_text reference SW16 (at -7.21 -4.84) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 8 BH) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 "Net-(R8-Pad2)"))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 10 11) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C9D8694)
    (at 22.73 44.815)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module AOR_custom:AOR_LOGO (layer F.Cu) (tedit 5C26ADAA)
    (at 62.735 54.34 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value AOR_LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Connector_IDC:IDC-Header_2x05_P2.54mm_Vertical (layer B.Cu) (tedit 59DE0611)
    (at 216.024 59.674 90)
    (descr "Through hole straight IDC box header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x05 2.54mm double row")
    (fp_text reference J1 (at 1.27 6.604 90) (layer B.SilkS))
    (fp_text value Conn_01x10 (at 1.27 -16.764 90) (layer B.Fab))
    (fp_text user %R (at 1.27 -5.08 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 5V))
    (pad 3 thru_hole oval (at 0 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 VCC))
    (pad 4 thru_hole oval (at 2.54 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 SRCLK))
    (pad 5 thru_hole oval (at 0 -5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 RCLK))
    (pad 6 thru_hole oval (at 2.54 -5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 OE))
    (pad 7 thru_hole oval (at 0 -7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 SER))
    (pad 8 thru_hole oval (at 2.54 -7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 10))
    (pad 9 thru_hole oval (at 0 -10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 11))
    (pad 10 thru_hole oval (at 2.54 -10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 12))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 210.69 49.26 90)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -6 90) (layer F.SilkS))
    (fp_text value 74HC595 (at 0 6 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 BB))
    (pad 2 smd rect (at -2.7 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 BC))
    (pad 3 smd rect (at -2.7 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 BD))
    (pad 4 smd rect (at -2.7 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 BE))
    (pad 5 smd rect (at -2.7 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 BF))
    (pad 6 smd rect (at -2.7 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 BG))
    (pad 7 smd rect (at -2.7 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 BH))
    (pad 8 smd rect (at -2.7 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 9 smd rect (at 2.7 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U1-Pad9)"))
    (pad 10 smd rect (at 2.7 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 VCC))
    (pad 11 smd rect (at 2.7 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 SRCLK))
    (pad 12 smd rect (at 2.7 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 RCLK))
    (pad 13 smd rect (at 2.7 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 OE))
    (pad 14 smd rect (at 2.7 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 SER))
    (pad 15 smd rect (at 2.7 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 BA))
    (pad 16 smd rect (at 2.7 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 VCC))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "ACP3-E-BTN-PCB\nREV. E, 4-18-2019" (at 54.48 54.975 90) (layer B.SilkS))
  (gr_text "ACP3-E-BTN-PCB\nREV. E, 4-18-2019" (at 54.48 54.975 90) (layer F.SilkS))
  (gr_line (start 272.285 67.675) (end -3.305 67.675) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 272.285 41.005) (end 272.285 67.675) (layer Edge.Cuts) (width 0.2))
  (gr_line (start -3.305 41.005) (end 272.285 41.005) (layer Edge.Cuts) (width 0.2))
  (gr_line (start -3.305 67.675) (end -3.305 41.005) (layer Edge.Cuts) (width 0.2))
  (zone (net 11) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -3.305 41.005) (xy 272.285 41.005) (xy 272.285 67.675) (xy -3.305 67.675)
      )
    )
  )
  (zone (net 11) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -3.305 41.005) (xy 272.285 41.005) (xy 272.285 67.675) (xy -3.305 67.675)
      )
    )
  )
)
