(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "FreHD40GerberV1.1/")
		)
	)
	(net 0 "")
	(net 1 "Net-(BT1-+)")
	(net 2 "GND")
	(net 3 "VCC")
	(net 4 "Net-(U1-OSC1{slash}CLKI)")
	(net 5 "Net-(U1-OSC2{slash}CLK0)")
	(net 6 "+3.3V")
	(net 7 "Net-(D1-A)")
	(net 8 "Net-(D2-A)")
	(net 9 "MCLR")
	(net 10 "LED1")
	(net 11 "LED0")
	(net 12 "/SD_CS_3V3")
	(net 13 "/SD_CLK_3V3")
	(net 14 "/SPI_SDI_3V3")
	(net 15 "Net-(J2-DAT1)")
	(net 16 "/SD_IN_3V3")
	(net 17 "Net-(J2-DAT2)")
	(net 18 "SPI_SDI")
	(net 19 "Net-(JP1-B)")
	(net 20 "WR_N")
	(net 21 "RD_N")
	(net 22 "Net-(JP1-A)")
	(net 23 "SD_WRPROT")
	(net 24 "SD_CD")
	(net 25 "SPI_CLK")
	(net 26 "SPI_SDO")
	(net 27 "SD_CS_5V")
	(net 28 "SDA")
	(net 29 "SCL")
	(net 30 "RTC")
	(net 31 "DD6")
	(net 32 "A2")
	(net 33 "DD3")
	(net 34 "DD1")
	(net 35 "PIC_WAIT_N")
	(net 36 "RX")
	(net 37 "RTS")
	(net 38 "PIC_SEL_N")
	(net 39 "DD5")
	(net 40 "A0")
	(net 41 "DD0")
	(net 42 "DD4")
	(net 43 "DD2")
	(net 44 "CTS")
	(net 45 "unconnected-(J3-Pin_14-Pad14)")
	(net 46 "A1")
	(net 47 "A3")
	(net 48 "unconnected-(J3-Pin_2-Pad2)")
	(net 49 "DD7")
	(net 50 "TX")
	(net 51 "STAT_CS")
	(net 52 "Net-(U7-X1)")
	(net 53 "unconnected-(J3-Pin_7-Pad7)")
	(net 54 "BUS_WAIT_N")
	(net 55 "unconnected-(J3-Pin_13-Pad13)")
	(net 56 "D2")
	(net 57 "unconnected-(J3-Pin_3-Pad3)")
	(net 58 "unconnected-(J3-Pin_17-Pad17)")
	(net 59 "unconnected-(J3-Pin_23-Pad23)")
	(net 60 "D1")
	(net 61 "unconnected-(J3-Pin_15-Pad15)")
	(net 62 "D4")
	(net 63 "unconnected-(J3-Pin_21-Pad21)")
	(net 64 "A6")
	(net 65 "unconnected-(J3-Pin_6-Pad6)")
	(net 66 "unconnected-(J3-Pin_1-Pad1)")
	(net 67 "unconnected-(J3-Pin_9-Pad9)")
	(net 68 "D0")
	(net 69 "A5")
	(net 70 "A7")
	(net 71 "D6")
	(net 72 "unconnected-(U1-~{CS}{slash}AN7{slash}RE2-Pad10)")
	(net 73 "unconnected-(J3-Pin_11-Pad11)")
	(net 74 "D7")
	(net 75 "unconnected-(J3-Pin_4-Pad4)")
	(net 76 "unconnected-(J3-Pin_5-Pad5)")
	(net 77 "A4")
	(net 78 "unconnected-(J3-Pin_10-Pad10)")
	(net 79 "D5")
	(net 80 "unconnected-(U1-RB0{slash}INT0{slash}FLT0{slash}AN12-Pad33)")
	(net 81 "D3")
	(net 82 "unconnected-(J3-Pin_16-Pad16)")
	(net 83 "STAT_OE_N")
	(net 84 "unconnected-(U2-IO4-Pad16)")
	(net 85 "unconnected-(U6-QH'-Pad9)")
	(net 86 "unconnected-(U2-IO6-Pad14)")
	(net 87 "Net-(U7-X2)")
	(net 88 "Net-(D11-A)")
	(net 89 "Net-(D12-A)")
	(net 90 "unconnected-(J3-Pin_39-Pad39)")
	(net 91 "unconnected-(H1-Pad1)")
	(net 92 "unconnected-(H2-Pad1)")
	(net 93 "unconnected-(H3-Pad1)")
	(net 94 "unconnected-(H4-Pad1)")
	(footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm"
		(layer "F.Cu")
		(at 179.75 95 -90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
		(property "Reference" "C13"
			(at -0.5 2 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nf"
			(at 2.5 2.2 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm"
		(layer "F.Cu")
		(at 188.75 88.5)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
		(property "Reference" "C4"
			(at 6 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nf"
			(at 2.5 2.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "+3.3V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 147.56 97.5 180)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R1"
			(at 9.56 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 3.81 1.92 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0.75 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "SD_WRPROT")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 185.38 43.875 90)
		(descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x04 2.54mm single row")
		(property "Reference" "J4"
			(at 4.625 10.87 180)
			(layer "F.SilkS")
		)
		(property "Value" "CON2"
			(at 4.385 9.89 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.77 3.81 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pinfunction "Pin_4")
			(pintype "passive")
			(zone_connect 2)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-40_W15.24mm"
		(layer "F.Cu")
		(at 183.83 76.5 -90)
		(descr "40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
		(property "Reference" "U1"
			(at 10.25 -2.42 90)
			(layer "F.SilkS")
		)
		(property "Value" "PIC18F4620-IP"
			(at 7.62 50.59 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39682E.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "32K Flash, 1K SRAM, ADC, DIP40"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W15.24mm* PDIP*W15.24mm*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 24.13 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "MCLR")
			(pinfunction "~{MCLR}")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "A3")
			(pinfunction "RA0/AN0")
			(pintype "tri_state")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "A2")
			(pinfunction "RA1/AN1")
			(pintype "tri_state")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "A1")
			(pinfunction "RA2/AN2/Vref-/CVref")
			(pintype "tri_state")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "A0")
			(pinfunction "RA3/AN3/Vref+")
			(pintype "tri_state")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "RD_N")
			(pinfunction "VDDCORE/VCAP")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "SD_CS_5V")
			(pinfunction "RA5/AN4/~{SS1}/C2OUT")
			(pintype "tri_state")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "RTS")
			(pinfunction "~{RD}/AN5/RE0")
			(pintype "tri_state")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "CTS")
			(pinfunction "~{WR}/AN6/RE1")
			(pintype "tri_state")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "unconnected-(U1-~{CS}{slash}AN7{slash}RE2-Pad10)")
			(pinfunction "~{CS}/AN7/RE2")
			(pintype "tri_state+no_connect")
		)
		(pad "11" thru_hole oval
			(at 0 25.4 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pinfunction "VDD")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "12" thru_hole oval
			(at 0 27.94 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "13" thru_hole oval
			(at 0 30.48 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(U1-OSC1{slash}CLKI)")
			(pinfunction "OSC1/CLKI")
			(pintype "input")
		)
		(pad "14" thru_hole oval
			(at 0 33.02 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(U1-OSC2{slash}CLK0)")
			(pinfunction "OSC2/CLK0")
			(pintype "output")
		)
		(pad "15" thru_hole oval
			(at 0 35.56 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "STAT_CS")
			(pinfunction "T1OSO/T1CKI/RC0")
			(pintype "tri_state")
		)
		(pad "16" thru_hole oval
			(at 0 38.1 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "SDA")
			(pinfunction "T1OSI/CCP2/RC1")
			(pintype "tri_state")
		)
		(pad "17" thru_hole oval
			(at 0 40.64 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "SCL")
			(pinfunction "P1A/CCP1/RC2")
			(pintype "tri_state")
		)
		(pad "18" thru_hole oval
			(at 0 43.18 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "SPI_CLK")
			(pinfunction "SCK1/SCL1/RC3")
			(pintype "tri_state")
		)
		(pad "19" thru_hole oval
			(at 0 45.72 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "DD0")
			(pinfunction "PSP0/SCK2/SCL2/RD0")
			(pintype "tri_state")
		)
		(pad "20" thru_hole oval
			(at 0 48.26 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "DD1")
			(pinfunction "PSP1/SDI2/SDA2/RD1")
			(pintype "tri_state")
		)
		(pad "21" thru_hole oval
			(at 15.24 48.26 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "DD2")
			(pinfunction "PSP2/SDO2/RD2")
			(pintype "tri_state")
		)
		(pad "22" thru_hole oval
			(at 15.24 45.72 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "DD3")
			(pinfunction "PSP3/~{SS2}/RD3")
			(pintype "tri_state")
		)
		(pad "23" thru_hole oval
			(at 15.24 43.18 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "SPI_SDI")
			(pinfunction "SDI1/SDA1/RC4")
			(pintype "tri_state")
		)
		(pad "24" thru_hole oval
			(at 15.24 40.64 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "SPI_SDO")
			(pinfunction "SDO1/RC5")
			(pintype "tri_state")
		)
		(pad "25" thru_hole oval
			(at 15.24 38.1 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "TX")
			(pinfunction "TX/CK/RC6")
			(pintype "tri_state")
		)
		(pad "26" thru_hole oval
			(at 15.24 35.56 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "RX")
			(pinfunction "RX/DT/RC7")
			(pintype "tri_state")
		)
		(pad "27" thru_hole oval
			(at 15.24 33.02 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "DD4")
			(pinfunction "PSP4/RD4")
			(pintype "tri_state")
		)
		(pad "28" thru_hole oval
			(at 15.24 30.48 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "DD5")
			(pinfunction "PSP5/P1B/RD5")
			(pintype "tri_state")
		)
		(pad "29" thru_hole oval
			(at 15.24 27.94 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "DD6")
			(pinfunction "PSP6/P1C/RD6")
			(pintype "tri_state")
		)
		(pad "30" thru_hole oval
			(at 15.24 25.4 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "DD7")
			(pinfunction "PSP7/P1D/RD7")
			(pintype "tri_state")
		)
		(pad "31" thru_hole oval
			(at 15.24 22.86 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "32" thru_hole oval
			(at 15.24 20.32 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pinfunction "VDD")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "33" thru_hole oval
			(at 15.24 17.78 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "unconnected-(U1-RB0{slash}INT0{slash}FLT0{slash}AN12-Pad33)")
			(pinfunction "RB0/INT0/FLT0/AN12")
			(pintype "tri_state+no_connect")
		)
		(pad "34" thru_hole oval
			(at 15.24 15.24 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "PIC_SEL_N")
			(pinfunction "RB1/INT1/AN10")
			(pintype "tri_state")
		)
		(pad "35" thru_hole oval
			(at 15.24 12.7 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "RTC")
			(pinfunction "RB2/INT2/AN8")
			(pintype "tri_state")
		)
		(pad "36" thru_hole oval
			(at 15.24 10.16 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "PIC_WAIT_N")
			(pinfunction "RB3/CCP2/AN9")
			(pintype "tri_state")
		)
		(pad "37" thru_hole oval
			(at 15.24 7.62 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "SD_CD")
			(pinfunction "RB4/KBI0/AN11")
			(pintype "tri_state")
		)
		(pad "38" thru_hole oval
			(at 15.24 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "SD_WRPROT")
			(pinfunction "RB5/KBI1/T0CKI/C1OUT")
			(pintype "tri_state")
		)
		(pad "39" thru_hole oval
			(at 15.24 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "LED1")
			(pinfunction "RB6/KBI2/PGC")
			(pintype "tri_state")
		)
		(pad "40" thru_hole oval
			(at 15.24 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "LED0")
			(pinfunction "RB7/KBI3/PGD")
			(pintype "tri_state")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-40_W15.24mm.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-40_W15.24mm_Socket.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 119.5 59.25 90)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "J1"
			(at 0 -2.75 90)
			(layer "F.SilkS")
		)
		(property "Value" "CON5-External"
			(at 0.5 -6.925 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "MCLR")
			(pinfunction "Pin_1")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "LED0")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "LED1")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92_Inline"
		(layer "F.Cu")
		(at 191.23 78.36)
		(descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "U4"
			(at 3.52 -2.86 0)
			(layer "F.SilkS")
		)
		(property "Value" "TS2950-3.3"
			(at 1.27 2.79 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp2950.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Positive 100mA 30V Linear Micropower Voltage Regulator, Fixed Output 3.3V, TO-92"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?92*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "+3.3V")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "2" thru_hole oval
			(at 1.27 0)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" thru_hole oval
			(at 2.54 0)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pinfunction "VI")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Crystal:Crystal_DS15_D1.5mm_L5.0mm_Horizontal"
		(layer "F.Cu")
		(at 126 71.15 -90)
		(descr "Crystal THT DS15 5.0mm length 1.5mm diameter http://www.microcrystal.com/images/_Product-Documentation/03_TF_metal_Packages/01_Datasheet/DS-Series.pdf")
		(tags "['DS15']")
		(property "Reference" "Y2"
			(at 0.85 -3 90)
			(layer "F.SilkS")
		)
		(property "Value" "32.7kHz"
			(at 3.12 1.25 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Crystal:Crystal_DS15_D1.5mm_L5.0mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Two pin crystal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1 4 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1 1)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 87 "Net-(U7-X2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.7 0 270)
			(size 1 1)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "Net-(U7-X1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Crystal.3dshapes/Crystal_DS15_D1.5mm_L5.0mm_Horizontal.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Crystal.3dshapes/Crystal_C26-LF_D2.1mm_L6.5mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D4.0mm_P1.50mm"
		(layer "F.Cu")
		(at 191.25 72.5)
		(descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
		(property "Reference" "C12"
			(at 3 -2.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0.75 3.25 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D4.0mm_P1.50mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.75 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.5 0)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(thermal_bridge_angle 90)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 167.25 70)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
		(property "Reference" "C2"
			(at 6.75 0.25 90)
			(layer "F.SilkS")
		)
		(property "Value" "22pF"
			(at 2.5 2.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(U1-OSC1{slash}CLKI)")
			(pintype "passive")
			(thermal_bridge_angle 90)
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(thermal_bridge_angle 90)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_THT:LED_D3.0mm"
		(layer "F.Cu")
		(at 116.25 37.75)
		(descr "LED, diameter 3.0mm, 2 pins, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at -0.75 2.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 2.96 0)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_THT:LED_D3.0mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
			(hide yes)
			(offset
				(xyz 0 0 -2.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_THT:SW_PUSH_6mm"
		(layer "F.Cu")
		(at 119.5 63)
		(descr "Generic 6mm SW tactile push button")
		(tags "tact sw push 6mm")
		(property "Reference" "SW1"
			(at 8.75 2.25 90)
			(layer "F.SilkS")
		)
		(property "Value" "SW_Reset"
			(at 3.75 6.7 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Button_Switch_THT:SW_PUSH_6mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.25 2.25 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "MCLR")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 6.5 0 90)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "MCLR")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 4.5 90)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 6.5 4.5 90)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Crystal:Crystal_HC18-U_Vertical"
		(layer "F.Cu")
		(at 163 71.5 90)
		(descr "Crystal THT HC-18/U, http://5hertz.com/pdfs/04404_D.pdf")
		(tags "THT crystalHC-18/U")
		(property "Reference" "Y1"
			(at -2 -3.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "10MHz"
			(at 2.45 3.525 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Crystal:Crystal_HC18-U_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Two pin crystal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.45 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(U1-OSC1{slash}CLKI)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4.9 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(U1-OSC2{slash}CLK0)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Crystal.3dshapes/Crystal_HC18-U_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Crystal.3dshapes/Crystal_HC18-U_Vertical.wrl"
			(offset
				(xyz 0 0 1)
			)
			(scale
				(xyz 0.9 0.9 0.3)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-8_W7.62mm"
		(layer "F.Cu")
		(at 127.29 75.75 -90)
		(descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U7"
			(at 5.5 -2.46 90)
			(layer "F.SilkS")
		)
		(property "Value" "DS1307"
			(at 3.81 9.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DS1307.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "64 x 8, Serial, I2C Real-time clock, 4.5V to 5.5V VCC, 0°C to +70°C, DIP-8"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "Net-(U7-X1)")
			(pinfunction "X1")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 87 "Net-(U7-X2)")
			(pinfunction "X2")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(BT1-+)")
			(pinfunction "VBAT")
			(pintype "power_in")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "RTC")
			(pinfunction "SQW/OUT")
			(pintype "open_collector")
		)
		(pad "8" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
			(zone_connect 2)
			(thermal_bridge_angle 45)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad"
		(layer "F.Cu")
		(at 119 52.25)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "H1"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "unconnected-(H1-Pad1)")
			(pinfunction "1")
			(pintype "input+no_connect")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 119.69 91.75)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R18"
			(at -2.63 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4K7"
			(at 3.81 1.92 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "RTC")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_THT:LED_D3.0mm"
		(layer "F.Cu")
		(at 122.25 120.5)
		(descr "LED, diameter 3.0mm, 2 pins, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D12"
			(at -0.5 -2.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 2.96 0)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_THT:LED_D3.0mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "Net-(D12-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm_Green.wrl"
			(offset
				(xyz 0 0 -2.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:CONV_BOB-12009"
		(layer "F.Cu")
		(at 188.33 102.1)
		(property "Reference" "U8"
			(at 5.42 -8.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "BOB-12009"
			(at 2.39 9.135 0)
			(layer "F.Fab")
		)
		(property "Footprint" "footprints:CONV_BOB-12009"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "SparkFun"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "N/A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/BOB-12009/SparkFun/view-part/?ref=eda"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "01"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/BOB-12009/SparkFun/view-part/?ref=snap"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "BOB-12009"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "\n                        \n                            BSS138 - Logic-Level Translator Interface Evaluation Board\n                        \n"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "SparkFun Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(pad "GND_1" thru_hole circle
			(at 5.08 1.27)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "GND_2" thru_hole circle
			(at -5.08 1.27)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "HV" thru_hole circle
			(at 5.08 -1.27)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pinfunction "HV")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "HV1" thru_hole rect
			(at 5.08 -6.35)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "SPI_SDI")
			(pinfunction "HV1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "HV2" thru_hole circle
			(at 5.08 -3.81)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "SD_CS_5V")
			(pinfunction "HV2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "HV3" thru_hole circle
			(at 5.08 3.81)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "SPI_CLK")
			(pinfunction "HV3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "HV4" thru_hole circle
			(at 5.08 6.35)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "SPI_SDO")
			(pinfunction "HV4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "LV" thru_hole circle
			(at -5.08 -1.27)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "+3.3V")
			(pinfunction "LV")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "LV1" thru_hole rect
			(at -5.08 -6.35)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/SPI_SDI_3V3")
			(pinfunction "LV1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "LV2" thru_hole circle
			(at -5.08 -3.81)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/SD_CS_3V3")
			(pinfunction "LV2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "LV3" thru_hole circle
			(at -5.08 3.81)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/SD_CLK_3V3")
			(pinfunction "LV3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "LV4" thru_hole circle
			(at -5.08 6.35)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/SD_IN_3V3")
			(pinfunction "LV4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-12_W10.16mm.wrl"
			(hide yes)
			(offset
				(xyz -5 6.5 1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SON.3dshapes/Nexperia_HUSON-12_USON-12-1EP_1.35x2.5mm_P0.4mm_EP0.4x2mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 7.8 6.3 10)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-20_W7.62mm_Socket"
		(layer "F.Cu")
		(at 163 57.8 90)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
		(property "Reference" "U2"
			(at 3.81 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "GAL16V8D"
			(at 3.81 25.19 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm_Socket"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Programmable Logic Array, DIP-20/SOIC-20/PLCC-20"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* PDIP* SOIC* SO* PLCC*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "A0")
			(pinfunction "I1/CLK")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "A1")
			(pinfunction "I2")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "A2")
			(pinfunction "I3")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "A3")
			(pinfunction "I4")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "A4")
			(pinfunction "I5")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "A5")
			(pinfunction "I6")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "A6")
			(pinfunction "I7")
			(pintype "input")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "A7")
			(pinfunction "I8")
			(pintype "input")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "RD_N")
			(pinfunction "I9")
			(pintype "input")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "11" thru_hole oval
			(at 7.62 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "I10/~{OE}")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "12" thru_hole oval
			(at 7.62 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(JP1-A)")
			(pinfunction "IO8")
			(pintype "tri_state")
		)
		(pad "13" thru_hole oval
			(at 7.62 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "PIC_SEL_N")
			(pinfunction "IO7")
			(pintype "tri_state")
		)
		(pad "14" thru_hole oval
			(at 7.62 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 86 "unconnected-(U2-IO6-Pad14)")
			(pinfunction "IO6")
			(pintype "tri_state+no_connect")
		)
		(pad "15" thru_hole oval
			(at 7.62 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "BUS_WAIT_N")
			(pinfunction "IO5")
			(pintype "tri_state")
		)
		(pad "16" thru_hole oval
			(at 7.62 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "unconnected-(U2-IO4-Pad16)")
			(pinfunction "IO4")
			(pintype "tri_state+no_connect")
		)
		(pad "17" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(JP1-B)")
			(pinfunction "I03")
			(pintype "tri_state")
		)
		(pad "18" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "WR_N")
			(pinfunction "IO2")
			(pintype "tri_state")
		)
		(pad "19" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "STAT_OE_N")
			(pinfunction "IO1")
			(pintype "tri_state")
		)
		(pad "20" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
			(zone_connect 2)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm_Socket.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad"
		(layer "F.Cu")
		(at 192.75 119.25)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "H3"
			(at -4.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "unconnected-(H3-Pad1)")
			(pinfunction "1")
			(pintype "input+no_connect")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Even_Odd_Vertical"
		(layer "F.Cu")
		(at 130.86 44 90)
		(descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x20 2.54mm double row")
		(property "Reference" "J3"
			(at 5.25 -0.11 180)
			(layer "F.SilkS")
		)
		(property "Value" "TRS80-40Pin"
			(at 1.27 50.59 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Even_Odd_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 24.13 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "unconnected-(J3-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive+no_connect")
		)
		(pad "2" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "unconnected-(J3-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive+no_connect")
		)
		(pad "3" thru_hole oval
			(at 2.54 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "unconnected-(J3-Pin_3-Pad3)")
			(pinfunction "Pin_3")
			(pintype "passive+no_connect")
		)
		(pad "4" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "unconnected-(J3-Pin_4-Pad4)")
			(pinfunction "Pin_4")
			(pintype "passive+no_connect")
		)
		(pad "5" thru_hole oval
			(at 2.54 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "unconnected-(J3-Pin_5-Pad5)")
			(pinfunction "Pin_5")
			(pintype "passive+no_connect")
		)
		(pad "6" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "unconnected-(J3-Pin_6-Pad6)")
			(pinfunction "Pin_6")
			(pintype "passive+no_connect")
		)
		(pad "7" thru_hole oval
			(at 2.54 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "unconnected-(J3-Pin_7-Pad7)")
			(pinfunction "Pin_7")
			(pintype "passive+no_connect")
		)
		(pad "8" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_8")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "9" thru_hole oval
			(at 2.54 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "unconnected-(J3-Pin_9-Pad9)")
			(pinfunction "Pin_9")
			(pintype "passive+no_connect")
		)
		(pad "10" thru_hole oval
			(at 0 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "unconnected-(J3-Pin_10-Pad10)")
			(pinfunction "Pin_10")
			(pintype "passive+no_connect")
		)
		(pad "11" thru_hole oval
			(at 2.54 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "unconnected-(J3-Pin_11-Pad11)")
			(pinfunction "Pin_11")
			(pintype "passive+no_connect")
		)
		(pad "12" thru_hole oval
			(at 0 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "WR_N")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 2.54 15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "unconnected-(J3-Pin_13-Pad13)")
			(pinfunction "Pin_13")
			(pintype "passive+no_connect")
		)
		(pad "14" thru_hole oval
			(at 0 15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "unconnected-(J3-Pin_14-Pad14)")
			(pinfunction "Pin_14")
			(pintype "passive+no_connect")
		)
		(pad "15" thru_hole oval
			(at 2.54 17.78 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "unconnected-(J3-Pin_15-Pad15)")
			(pinfunction "Pin_15")
			(pintype "passive+no_connect")
		)
		(pad "16" thru_hole oval
			(at 0 17.78 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "unconnected-(J3-Pin_16-Pad16)")
			(pinfunction "Pin_16")
			(pintype "passive+no_connect")
		)
		(pad "17" thru_hole oval
			(at 2.54 20.32 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "unconnected-(J3-Pin_17-Pad17)")
			(pinfunction "Pin_17")
			(pintype "passive+no_connect")
		)
		(pad "18" thru_hole oval
			(at 0 20.32 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "D4")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole oval
			(at 2.54 22.86 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "RD_N")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" thru_hole oval
			(at 0 22.86 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "D7")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" thru_hole oval
			(at 2.54 25.4 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "unconnected-(J3-Pin_21-Pad21)")
			(pinfunction "Pin_21")
			(pintype "passive+no_connect")
		)
		(pad "22" thru_hole oval
			(at 0 25.4 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "D1")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" thru_hole oval
			(at 2.54 27.94 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "unconnected-(J3-Pin_23-Pad23)")
			(pinfunction "Pin_23")
			(pintype "passive+no_connect")
		)
		(pad "24" thru_hole oval
			(at 0 27.94 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "D6")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(pad "25" thru_hole oval
			(at 2.54 30.48 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "A0")
			(pinfunction "Pin_25")
			(pintype "passive")
		)
		(pad "26" thru_hole oval
			(at 0 30.48 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "D3")
			(pinfunction "Pin_26")
			(pintype "passive")
		)
		(pad "27" thru_hole oval
			(at 2.54 33.02 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "A1")
			(pinfunction "Pin_27")
			(pintype "passive")
		)
		(pad "28" thru_hole oval
			(at 0 33.02 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "D5")
			(pinfunction "Pin_28")
			(pintype "passive")
		)
		(pad "29" thru_hole oval
			(at 2.54 35.56 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_29")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "30" thru_hole oval
			(at 0 35.56 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "D0")
			(pinfunction "Pin_30")
			(pintype "passive")
		)
		(pad "31" thru_hole oval
			(at 2.54 38.1 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "A4")
			(pinfunction "Pin_31")
			(pintype "passive")
		)
		(pad "32" thru_hole oval
			(at 0 38.1 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "D2")
			(pinfunction "Pin_32")
			(pintype "passive")
		)
		(pad "33" thru_hole oval
			(at 2.54 40.64 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "BUS_WAIT_N")
			(pinfunction "Pin_33")
			(pintype "passive")
		)
		(pad "34" thru_hole oval
			(at 0 40.64 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "A3")
			(pinfunction "Pin_34")
			(pintype "passive")
		)
		(pad "35" thru_hole oval
			(at 2.54 43.18 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "A5")
			(pinfunction "Pin_35")
			(pintype "passive")
		)
		(pad "36" thru_hole oval
			(at 0 43.18 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "A7")
			(pinfunction "Pin_36")
			(pintype "passive")
		)
		(pad "37" thru_hole oval
			(at 2.54 45.72 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_37")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "38" thru_hole oval
			(at 0 45.72 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "A6")
			(pinfunction "Pin_38")
			(pintype "passive")
		)
		(pad "39" thru_hole oval
			(at 2.54 48.26 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "unconnected-(J3-Pin_39-Pad39)")
			(pinfunction "Pin_39")
			(pintype "passive+no_connect")
			(zone_connect 2)
		)
		(pad "40" thru_hole oval
			(at 0 48.26 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "A2")
			(pinfunction "Pin_40")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 2.5 0 -2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 180 0)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:BS-7_MPD_VCC_1"
		(layer "F.Cu")
		(at 119.2602 106 90)
		(tags "BS-7 ")
		(property "Reference" "BT1"
			(at 0 7.715 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "3.3V"
			(at 0 7.715 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "footprints:BS-7_MPD_VCC_1"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single-cell battery"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 7.715 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 19.9898 90)
			(size 2.0066 2.0066)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(BT1-+)")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 0 90)
			(size 1.6764 1.6764)
			(drill 1.1684)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "-")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_Keystone_105_1x2430.step"
			(offset
				(xyz 0 -19.5 -1.5)
			)
			(scale
				(xyz 0.8 0.8 0.8)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm_NumberLabels"
		(layer "F.Cu")
		(at 180.75 62 180)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip, labeled with numbers")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP1"
			(at 1.5 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "PicWait"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm_NumberLabels"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "3-pole Solder Jumper, pins 1+2 closed/bridged"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged12*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(net_tie_pad_groups "1, 2")
		(fp_text user "3"
			(at 2.6 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -2.6 0 0)
			(layer "F.SilkS")
		)
		(pad "1" smd custom
			(at -1.3 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 22 "Net-(JP1-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.55 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.55 -0.75)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd rect
			(at 0 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 35 "PIC_WAIT_N")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd custom
			(at 1.3 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 19 "Net-(JP1-B)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.55 0.75) (xy -0.55 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 119.69 86.75)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R16"
			(at -2.69 -0.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "4K7"
			(at 3.81 1.92 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "SDA")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad"
		(layer "F.Cu")
		(at 142.25 119.25)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "H4"
			(at -4 3.25 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "unconnected-(H4-Pad1)")
			(pinfunction "1")
			(pintype "input+no_connect")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 129.5 48.44 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R13"
			(at 4.31 -1.75 90)
			(layer "F.SilkS")
		)
		(property "Value" "330R"
			(at 3.81 1.92 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(D1-A)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "LED1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 123.24 44 90)
		(descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x02 2.54mm double row")
		(property "Reference" "J6"
			(at 5 -0.24 180)
			(layer "F.SilkS")
		)
		(property "Value" "PCB Connenctor"
			(at 1.27 4.87 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x02, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pinfunction "Pin_2")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "3" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pinfunction "Pin_3")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pinfunction "Pin_4")
			(pintype "passive")
			(zone_connect 2)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 2.5 0 -2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 180 0)
			)
		)
	)
	(footprint "LED_THT:LED_D3.0mm"
		(layer "F.Cu")
		(at 116.25 43.5)
		(descr "LED, diameter 3.0mm, 2 pins, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at -0.75 2.75 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 2.96 0)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_THT:LED_D3.0mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm_Green.step"
			(hide yes)
			(offset
				(xyz 0 0 -2.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D4.0mm_P1.50mm"
		(layer "F.Cu")
		(at 191.277401 84)
		(descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
		(property "Reference" "C5"
			(at 3.472599 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0.75 3.25 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D4.0mm_P1.50mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.75 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "+3.3V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.5 0)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(thermal_bridge_angle 90)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 167.25 66.5)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
		(property "Reference" "C3"
			(at 6.75 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "22pF"
			(at 2.75 2.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(U1-OSC2{slash}CLK0)")
			(pintype "passive")
			(thermal_bridge_angle 90)
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(thermal_bridge_angle 90)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 119.75 89.25)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R17"
			(at -2.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4K7"
			(at 3.81 1.92 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "SCL")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm"
		(layer "F.Cu")
		(at 136 47.25 -90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
		(property "Reference" "C1"
			(at 2.25 -2 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nf"
			(at 2.5 2.2 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-20_W7.62mm_Socket"
		(layer "F.Cu")
		(at 135.45 70.37 90)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
		(property "Reference" "U3"
			(at 3.87 -2.45 90)
			(layer "F.SilkS")
		)
		(property "Value" "74LS245"
			(at -19.25 51.05 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm_Socket"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74HC245"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Octal BUS Transceivers, 3-State outputs"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?20*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.54 10.555 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "RD_N")
			(pinfunction "A->B")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "D0")
			(pinfunction "A0")
			(pintype "tri_state")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "D1")
			(pinfunction "A1")
			(pintype "tri_state")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "D2")
			(pinfunction "A2")
			(pintype "tri_state")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "D3")
			(pinfunction "A3")
			(pintype "tri_state")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "D4")
			(pinfunction "A4")
			(pintype "tri_state")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "D5")
			(pinfunction "A5")
			(pintype "tri_state")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "D6")
			(pinfunction "A6")
			(pintype "tri_state")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "D7")
			(pinfunction "A7")
			(pintype "tri_state")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "11" thru_hole oval
			(at 7.62 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "DD7")
			(pinfunction "B7")
			(pintype "tri_state")
		)
		(pad "12" thru_hole oval
			(at 7.62 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "DD6")
			(pinfunction "B6")
			(pintype "tri_state")
		)
		(pad "13" thru_hole oval
			(at 7.62 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "DD5")
			(pinfunction "B5")
			(pintype "tri_state")
		)
		(pad "14" thru_hole oval
			(at 7.62 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "DD4")
			(pinfunction "B4")
			(pintype "tri_state")
		)
		(pad "15" thru_hole oval
			(at 7.62 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "DD3")
			(pinfunction "B3")
			(pintype "tri_state")
		)
		(pad "16" thru_hole oval
			(at 7.62 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "DD2")
			(pinfunction "B2")
			(pintype "tri_state")
		)
		(pad "17" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "DD1")
			(pinfunction "B1")
			(pintype "tri_state")
		)
		(pad "18" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "DD0")
			(pinfunction "B0")
			(pintype "tri_state")
		)
		(pad "19" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "PIC_SEL_N")
			(pinfunction "CE")
			(pintype "input")
		)
		(pad "20" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
			(zone_connect 2)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm_Socket.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm"
		(layer "F.Cu")
		(at 135 59.75 90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
		(property "Reference" "C15"
			(at 2.5 -2.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nf"
			(at 2.5 2.2 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Card:SD_Hirose_DM1AA_SF_PEJ82"
		(layer "F.Cu")
		(at 163.5 111.8)
		(descr "SD, SMD, top-mount, push-push (https://www.hirose.com/product/document?clcode=CL0609-0004-8-82&productname=DM1AA-SF-PEJ(82)&series=DM1&documenttype=2DDrawing&lang=en&documentid=0000915301)")
		(tags "SD card connector")
		(property "Reference" "J2"
			(at 16 7.95 0)
			(layer "F.SilkS")
		)
		(property "Value" "SD_Card"
			(at -0.6 10.45 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Card:SD_Hirose_DM1AA_SF_PEJ82"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://portal.fciconnect.com/Comergent//fci/drawing/10067847.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SD card receptacle"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SD*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -11.9 -12.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 10.5 -12.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at 6.075 -14.95)
			(size 1.1 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "/SD_CS_3V3")
			(pinfunction "CD/DAT3")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at 3.575 -14.95)
			(size 1.1 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "/SD_IN_3V3")
			(pinfunction "CMD")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at 1.075 -14.95)
			(size 1.1 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -1.425 -14.95)
			(size 1.1 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at -3.925 -14.95)
			(size 1.1 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "/SD_CLK_3V3")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "6" smd rect
			(at -6.425 -14.95)
			(size 1.1 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -8.85 -14.95)
			(size 1.1 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "/SPI_SDI_3V3")
			(pinfunction "DAT0")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at -10.55 -14.95)
			(size 1.1 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "Net-(J2-DAT1)")
			(pinfunction "DAT1")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at 8.575 -14.95)
			(size 1.1 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(J2-DAT2)")
			(pinfunction "DAT2")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at -13.6 -3.55)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "SD_CD")
			(pinfunction "CARD_DETECT")
			(pintype "output")
		)
		(pad "11" smd rect
			(at -13.6 5.4)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "SD_WRPROT")
			(pinfunction "WRITE_PROTECT")
			(pintype "output")
		)
		(pad "12" smd rect
			(at -13.6 8)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "SHELL1")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at -14.5 -8.2)
			(size 2 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "SHELL2")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at -14.5 10.45)
			(size 2 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "SHELL2")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 14.5 -8.2)
			(size 2 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "SHELL2")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 14.5 10.45)
			(size 2 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "SHELL2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Card.3dshapes/SD_Hirose_DM1AA_SF_PEJ82.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Card.3dshapes/microSD_HC_Hirose_DM3AT-SF-PEJM5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 2 2)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 127.75 120.5)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R34"
			(at 3.81 -1.92 0)
			(layer "F.SilkS")
		)
		(property "Value" "330R"
			(at 3.81 1.92 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "Net-(D12-A)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "LED0")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 179.88 114.75)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R4"
			(at 9.62 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 3.81 1.92 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -2.69 -1.75 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(J2-DAT1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm"
		(layer "F.Cu")
		(at 167.25 73.25)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
		(property "Reference" "C9"
			(at 6.75 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nf"
			(at 2.5 2.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
			(thermal_bridge_angle 90)
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm"
		(layer "F.Cu")
		(at 161.25 61)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
		(property "Reference" "C16"
			(at 6.75 0.75 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nf"
			(at 2.5 2.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-16_W7.62mm_Socket"
		(layer "F.Cu")
		(at 140.475 57.75 90)
		(descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
		(property "Reference" "U6"
			(at 3.81 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "74LS595"
			(at 3.81 20.11 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm_Socket"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT595.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "8-bit serial in/out Shift Register 3-State Outputs"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm* SOIC*5.3x10.2mm*P1.27mm* SOIC*7.5x10.3mm*P1.27mm*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 8.89 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "D1")
			(pinfunction "QB")
			(pintype "tri_state")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "D2")
			(pinfunction "QC")
			(pintype "tri_state")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "D3")
			(pinfunction "QD")
			(pintype "tri_state")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "D4")
			(pinfunction "QE")
			(pintype "tri_state")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "D5")
			(pinfunction "QF")
			(pintype "tri_state")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "D6")
			(pinfunction "QG")
			(pintype "tri_state")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "D7")
			(pinfunction "QH")
			(pintype "tri_state")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "9" thru_hole oval
			(at 7.62 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "unconnected-(U6-QH'-Pad9)")
			(pinfunction "QH'")
			(pintype "output+no_connect")
		)
		(pad "10" thru_hole oval
			(at 7.62 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pinfunction "~{SRCLR}")
			(pintype "input")
		)
		(pad "11" thru_hole oval
			(at 7.62 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "SPI_CLK")
			(pinfunction "SRCLK")
			(pintype "input")
		)
		(pad "12" thru_hole oval
			(at 7.62 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "STAT_CS")
			(pinfunction "RCLK")
			(pintype "input")
		)
		(pad "13" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "STAT_OE_N")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "14" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "SPI_SDO")
			(pinfunction "SER")
			(pintype "input")
		)
		(pad "15" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "D0")
			(pinfunction "QA")
			(pintype "tri_state")
		)
		(pad "16" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
			(zone_connect 2)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm_Socket.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm"
		(layer "F.Cu")
		(at 130.25 86.75 -90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
		(property "Reference" "C14"
			(at 2.5 -2.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nf"
			(at 2.5 2.2 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 187.25 84.06 90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R2"
			(at 3.56 1.75 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 3.81 1.92 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "MCLR")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 144.25 107.62 90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R33"
			(at 3.81 2 90)
			(layer "F.SilkS")
		)
		(property "Value" "330R"
			(at 3.81 1.92 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "Net-(D11-A)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "LED1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 147.56 95.25 180)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R3"
			(at 9.56 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 3.81 1.92 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "SD_CD")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VCC")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_THT:LED_D3.0mm"
		(layer "F.Cu")
		(at 116.5 120.5)
		(descr "LED, diameter 3.0mm, 2 pins, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D11"
			(at -0.5 -2.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 2.96 0)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_THT:LED_D3.0mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "Net-(D11-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
			(offset
				(xyz 0 0 -2.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 127 48.44 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R14"
			(at 4.56 1.75 90)
			(layer "F.SilkS")
		)
		(property "Value" "330R"
			(at 3.81 1.92 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(D2-A)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "LED0")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 179.88 112.25)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R12"
			(at 10.12 0.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 3.81 1.92 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J2-DAT2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad"
		(layer "F.Cu")
		(at 192.75 52.25)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "H2"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "FREHD.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "unconnected-(H2-Pad1)")
			(pinfunction "1")
			(pintype "input+no_connect")
		)
	)
	(gr_line
		(start 113.75 124.25)
		(end 198 124.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198 34)
		(end 113.75 34)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198 124.25)
		(end 198 34)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 113.75 34)
		(end 113.75 124.25)
		(layer "Edge.Cuts")
	)
	(image
		(at 120.25 83.5)
		(layer "Edge.Cuts")
		(scale 0.400152)
	)
	(gr_text "FreHD M1 (v1.1)\n@kiwisincebirth"
		(at 172.5 121.5 0)
		(layer "B.Cu" knockout)
	)
	(gr_text "FreHD M1 (v1.1)\n@kiwisincebirth"
		(at 172.5 121.5 0)
		(layer "B.SilkS")
	)
	(gr_text "Rd"
		(at 119 123.25 0)
		(layer "F.SilkS")
	)
	(gr_text "40"
		(at 179.25 46.25 0)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 125 57.75 90)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 130.75 46.25 0)
		(layer "F.SilkS")
	)
	(gr_text "BOB-12009"
		(at 187.75 97.5 -90)
		(layer "F.SilkS")
	)
	(gr_text "Gr"
		(at 124.75 123.25 0)
		(layer "F.SilkS")
	)
	(gr_text "GAL16V8D"
		(at 164.75 54.5 0)
		(layer "F.SilkS")
	)
	(gr_text "74x245"
		(at 137 66.75 0)
		(layer "F.SilkS")
	)
	(gr_text "LV4"
		(at 180.25 107.5 270)
		(layer "F.SilkS")
	)
	(gr_text "Gr"
		(at 128 62.5 90)
		(layer "F.SilkS")
	)
	(gr_text "HV4"
		(at 195 107.25 270)
		(layer "F.SilkS")
	)
	(gr_text "Rd"
		(at 130.5 62.5 90)
		(layer "F.SilkS")
	)
	(gr_text "Clr"
		(at 120 58.25 90)
		(layer "F.SilkS")
	)
	(gr_text "Gr"
		(at 118.75 46.25 0)
		(layer "F.SilkS")
	)
	(gr_text "74x595"
		(at 142 54.5 0)
		(layer "F.SilkS")
	)
	(gr_text "39"
		(at 179.135859 39.397765 0)
		(layer "F.SilkS")
	)
	(gr_text "HV1"
		(at 194.995 94.075 270)
		(layer "F.SilkS")
	)
	(gr_text "Rd"
		(at 118.75 40.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 122.5 57.75 90)
		(layer "F.SilkS")
	)
	(gr_text "DS1307"
		(at 126.5 79 180)
		(layer "F.SilkS")
	)
	(gr_text "PIC18F4620-IP"
		(at 182 83.5 180)
		(layer "F.SilkS")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 135.5 114.5) (xy 141.5 108) (xy 141.5 107) (xy 147 107) (xy 146.75 124.5) (xy 135.25 124.5)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 145.5 94.75) (xy 175.25 95) (xy 175.25 95.75) (xy 178.25 95.75) (xy 178.25 97.75) (xy 181 97.75)
				(xy 181 102.5) (xy 197.5 102.5) (xy 197.5 124) (xy 145.5 123.75)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 154.25 48.5) (xy 157 48.5) (xy 157 51.75) (xy 154.25 51.75)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 191.5 56.5) (xy 189.5 55.25) (xy 188.5 53.5) (xy 188.5 51) (xy 189.5 49.25) (xy 191.75 48) (xy 197.5 48)
				(xy 197.5 56.5)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 186.5 42.25) (xy 192 42.25) (xy 192 45.5) (xy 186.5 45.5)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 160.75 64.25) (xy 165.25 64.25) (xy 165.25 73.75) (xy 160.75 73.75)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 114.20122 34.5) (xy 197.5 34.5) (xy 197.5 124) (xy 114 123.75)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 113.75 34.25) (xy 121 34.25) (xy 121 46) (xy 123.75 48) (xy 123.75 53.75) (xy 121.5 56.75) (xy 113.75 56.75)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 117.75 69.75) (xy 117.75 74.25) (xy 127.75 74.25) (xy 127.75 69.75)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 183.5 42.25) (xy 183.5 45.5) (xy 187 45.5) (xy 187 42.25)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 114.25 34.5) (xy 197.5 34.5) (xy 197.5 124) (xy 114.25 123.75)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 191.5 42.25) (xy 191.5 45.5) (xy 194.75 45.5) (xy 194.75 42.25)
			)
		)
	)
)
