(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A5")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/D-")
  (net 2 "/D+")
  (net 3 "/Tx_{0}")
  (net 4 "/Rx_{0}")
  (net 5 "/Rx_{1}")
  (net 6 "unconnected-(J5-Pin_16-Pad16)")
  (net 7 "/Tx_{1}")
  (net 8 "unconnected-(J7-Pad2)")
  (net 9 "unconnected-(J7-Pad4)")
  (net 10 "unconnected-(J7-Pad5)")
  (net 11 "unconnected-(J7-Pad6)")
  (net 12 "unconnected-(J7-Pad7)")
  (net 13 "unconnected-(J4-Pad1)")
  (net 14 "/Rx_{2}")
  (net 15 "/Tx_{2}")
  (net 16 "unconnected-(J4-Pad4)")
  (net 17 "unconnected-(J4-Pad5)")
  (net 18 "unconnected-(J4-Pad6)")
  (net 19 "unconnected-(J4-Pad7)")
  (net 20 "unconnected-(J4-Pad8)")
  (net 21 "unconnected-(J4-Pad9)")
  (net 22 "VCC")
  (net 23 "GND")
  (net 24 "/Tx_{out}")
  (net 25 "/Rx_{out}")
  (net 26 "/DO+")
  (net 27 "/DO-")
  (net 28 "Net-(D3-K)")
  (net 29 "Net-(D4-K)")
  (net 30 "/RXI_{0}")
  (net 31 "/TXI_{0}")
  (net 32 "/RXI_{1}")
  (net 33 "/TXI_{1}")
  (net 34 "/TXI_{2}")
  (net 35 "/RXI_{2}")
  (net 36 "/S_{0}")
  (net 37 "/S_{1}")
  (net 38 "/S_{2}")
  (net 39 "/S_{3}")
  (net 40 "unconnected-(J7-Pad8)")
  (net 41 "Net-(J7-Pad9)")
  (net 42 "/U-")
  (net 43 "/U+")
  (net 44 "unconnected-(J6-ID-Pad4)")
  (net 45 "Net-(J7-Pad11)")
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (at 61.286 72.39 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at -2.032 -1.524) (layer "F.SilkS"))
    (fp_text value "Conn_01x04" (at 0 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "VCC") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "/D+") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "/D-") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 36 "/S_{0}") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 90.5495 58.889852 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "40k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "/Tx_{0}") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 23 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_RJ:RJ45_Amphenol_RJHSE538X" (layer "F.Cu")
    (at 77.038 73.911 180)
    (descr "Shielded, 2 LED, https://www.amphenolcanada.com/ProductSearch/drawings/AC/RJHSE538X.pdf")
    (tags "RJ45 8p8c ethernet cat5")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RJ connector, 8P8C (8 positions 8 connected), two LEDs")
    (property "ki_keywords" "8P8C RJ socket jack connector led")
    (attr through_hole)
    (fp_text reference "J7" (at 2.798 8.632) (layer "F.SilkS"))
    (fp_text value "RJ45_LED" (at -6.854 10.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.56 -6) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -2.79 -2.54 180) (size 3.25 3.25) (drill 3.25) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 9.91 -2.54 180) (size 3.25 3.25) (drill 3.25) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.5 1.5) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 32 "/RXI_{1}") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.016 1.78 180) (size 1.5 1.5) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 8 "unconnected-(J7-Pad2)") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle (at 2.032 0 180) (size 1.5 1.5) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 33 "/TXI_{1}") (pintype "passive"))
    (pad "4" thru_hole circle (at 3.048 1.78 180) (size 1.5 1.5) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 9 "unconnected-(J7-Pad4)") (pintype "passive+no_connect"))
    (pad "5" thru_hole circle (at 4.064 0 180) (size 1.5 1.5) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 10 "unconnected-(J7-Pad5)") (pintype "passive+no_connect"))
    (pad "6" thru_hole circle (at 5.08 1.78 180) (size 1.5 1.5) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 11 "unconnected-(J7-Pad6)") (pintype "passive+no_connect"))
    (pad "7" thru_hole circle (at 6.096 0 180) (size 1.5 1.5) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 12 "unconnected-(J7-Pad7)") (pintype "passive+no_connect"))
    (pad "8" thru_hole circle (at 7.112 1.78 180) (size 1.5 1.5) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 40 "unconnected-(J7-Pad8)") (pintype "passive+no_connect"))
    (pad "9" thru_hole circle (at -3.3 6.6 180) (size 1.5 1.5) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(J7-Pad9)") (pintype "passive"))
    (pad "10" thru_hole circle (at -1.01 6.6 180) (size 1.5 1.5) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 33 "/TXI_{1}") (pintype "passive"))
    (pad "11" thru_hole circle (at 8.13 6.6 180) (size 1.5 1.5) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 45 "Net-(J7-Pad11)") (pintype "passive"))
    (pad "12" thru_hole circle (at 10.42 6.6 180) (size 1.5 1.5) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 32 "/RXI_{1}") (pintype "passive"))
    (pad "SH" thru_hole circle (at -4.57 0.89 180) (size 2.3 2.3) (drill 1.57) (layers "*.Cu" "*.Mask"))
    (pad "SH" thru_hole circle (at 11.69 0.89 180) (size 2.3 2.3) (drill 1.57) (layers "*.Cu" "*.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ45_Amphenol_RJHSE538X.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6_Handsoldering" (layer "F.Cu")
    (at 82.368 55.118)
    (descr "SOT-363, SC-70-6, Handsoldering")
    (tags "SOT-363 SC-70-6 Handsoldering")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Dual PMOS transistor, 6 pin package")
    (property "ki_keywords" "transistor PMOS P-MOS P-MOSFET")
    (attr smd)
    (fp_text reference "Q3" (at -2.032 -2.032 90) (layer "F.SilkS"))
    (fp_text value "Q_Dual_PMOS_S1G1D2S2G2D1" (at 0 2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.33 -0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/TXI_{1}") (pinfunction "S") (pintype "passive"))
    (pad "2" smd rect (at -1.33 0) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "/S_{2}") (pinfunction "G") (pintype "input"))
    (pad "3" smd rect (at -1.33 0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/Rx_{1}") (pinfunction "D") (pintype "passive"))
    (pad "4" smd rect (at 1.33 0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/RXI_{1}") (pinfunction "S") (pintype "passive"))
    (pad "5" smd rect (at 1.33 0) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "/S_{2}") (pinfunction "G") (pintype "input"))
    (pad "6" smd rect (at 1.33 -0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/Tx_{1}") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (at 86.686 72.39 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 2.54 -1.016) (layer "F.SilkS"))
    (fp_text value "Conn_01x04" (at 0 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 37 "/S_{1}") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 31 "/TXI_{0}") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 30 "/RXI_{0}") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D1.8mm_W1.8mm_H2.4mm_Horizontal_O1.27mm_Z1.6mm" (layer "F.Cu")
    (at 59.762 75.692)
    (descr "LED, ,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins")
    (tags "LED   diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D3" (at -1.524 2.032) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 5.33) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(D3-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 22 "VCC") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D1.8mm_W1.8mm_H2.4mm_Horizontal_O1.27mm_Z1.6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 98.862 61.468 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R14" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "20k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 39 "/S_{3}") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 22 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Horizontal" (layer "F.Cu")
    (at 99.386 56.642 90)
    (descr "Through hole angled pin header, 2x05, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x05 2.54mm double row")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J8" (at 5.655 -2.27 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x10 Data Conn" (at 5.655 12.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.31 5.08 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 26 "/DO+") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 27 "/DO-") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 24 "/Tx_{out}") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "/Rx_{out}") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "VCC") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "VCC") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 43 "/U+") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 42 "/U-") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_ISO7380" (layer "F.Cu")
    (at 88 53)
    (descr "Mounting Hole 2.2mm, no annular, M2, ISO7380")
    (tags "mounting hole 2.2mm no annular m2 iso7380")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 2.032 -2.286) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 2.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x08_P2.54mm_Horizontal" (layer "F.Cu")
    (at 60.015999 60.96 90)
    (descr "Through hole angled pin header, 2x08, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x08 2.54mm double row")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x08, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J5" (at 2.794 -2.031999 90) (layer "F.SilkS"))
    (fp_text value "Conn_02x08_Top_Bottom Switch Conn" (at 5.655 20.05 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.31 8.89) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "/Rx_{0}") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "/Rx_{1}") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "/Rx_{2}") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "/Tx_{0}") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "/Tx_{1}") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "/Tx_{2}") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 39 "/S_{3}") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 38 "/S_{2}") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 37 "/S_{1}") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 36 "/S_{0}") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "/Rx_{out}") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 24 "/Tx_{out}") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "GND") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "unconnected-(J5-Pin_16-Pad16)") (pinfunction "Pin_16") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x08_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 93.3435 56.349852 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at 2.8475 -0.038148) (layer "F.SilkS"))
    (fp_text value "20k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 37 "/S_{1}") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 22 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 98.862 65.024 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R16" (at 3.794 0) (layer "F.SilkS"))
    (fp_text value "40k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 14 "/Rx_{2}") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 23 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 109.038 61.976)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R15" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "40k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 15 "/Tx_{2}") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 23 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_ISO7380" (layer "F.Cu")
    (at 57 67)
    (descr "Mounting Hole 2.2mm, no annular, M2, ISO7380")
    (tags "mounting hole 2.2mm no annular m2 iso7380")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0.658 -2.54) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 2.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6_Handsoldering" (layer "F.Cu")
    (at 104.152 62.596)
    (descr "SOT-363, SC-70-6, Handsoldering")
    (tags "SOT-363 SC-70-6 Handsoldering")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Dual PMOS transistor, 6 pin package")
    (property "ki_keywords" "transistor PMOS P-MOS P-MOSFET")
    (attr smd)
    (fp_text reference "Q4" (at 0 -2) (layer "F.SilkS"))
    (fp_text value "Q_Dual_PMOS_S1G1D2S2G2D1" (at 0 2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.33 -0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/TXI_{2}") (pinfunction "S") (pintype "passive"))
    (pad "2" smd rect (at -1.33 0) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/S_{3}") (pinfunction "G") (pintype "input"))
    (pad "3" smd rect (at -1.33 0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/Rx_{2}") (pinfunction "D") (pintype "passive"))
    (pad "4" smd rect (at 1.33 0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "/RXI_{2}") (pinfunction "S") (pintype "passive"))
    (pad "5" smd rect (at 1.33 0) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/S_{3}") (pinfunction "G") (pintype "input"))
    (pad "6" smd rect (at 1.33 -0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/Tx_{2}") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 80.844 58.404 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R12" (at 2.81 0.254 -180) (layer "F.SilkS"))
    (fp_text value "40k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 5 "/Rx_{1}") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 23 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_USB:USB_Micro-B_Molex-105017-0001" (layer "F.Cu")
    (at 124.3105 56.282 90)
    (descr "http://www.molex.com/pdm_docs/sd/1050170001_sd.pdf")
    (tags "Micro-USB SMD Typ-B")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "USB Micro Type B connector")
    (property "ki_keywords" "connector USB micro")
    (attr smd)
    (fp_text reference "J6" (at 0 -3.1125 90) (layer "F.SilkS"))
    (fp_text value "USB_B_Micro Debug" (at 0.3 4.3375 90) (layer "F.Fab"))
    (fp_text user "PCB Edge" (at 0 2.6875 90) (layer "Dwgs.User"))
    (fp_text user "${REFERENCE}" (at 0 0.8875 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.3 -1.4625 90) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "VCC") (pinfunction "VBUS") (pintype "power_out"))
    (pad "2" smd rect (at -0.65 -1.4625 90) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "/U-") (pinfunction "D-") (pintype "bidirectional"))
    (pad "3" smd rect (at 0 -1.4625 90) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "/U+") (pinfunction "D+") (pintype "bidirectional"))
    (pad "4" smd rect (at 0.65 -1.4625 90) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "unconnected-(J6-ID-Pad4)") (pinfunction "ID") (pintype "passive+no_connect"))
    (pad "5" smd rect (at 1.3 -1.4625 90) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "6" thru_hole oval (at -3.5 1.2375 270) (size 1.2 1.9) (drill oval 0.6 1.3) (layers "*.Cu" "*.Mask")
      (net 23 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at -2.9 1.2375 90) (size 1.2 1.9) (layers "F.Cu" "F.Mask")
      (net 23 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole circle (at -2.5 -1.4625 90) (size 1.45 1.45) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 23 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at -1 1.2375 90) (size 1.5 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at 1 1.2375 90) (size 1.5 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole circle (at 2.5 -1.4625 90) (size 1.45 1.45) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 23 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at 2.9 1.2375 90) (size 1.2 1.9) (layers "F.Cu" "F.Mask")
      (net 23 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole oval (at 3.5 1.2375 90) (size 1.2 1.9) (drill oval 0.6 1.3) (layers "*.Cu" "*.Mask")
      (net 23 "GND") (pinfunction "Shield") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_Micro-B_Molex-105017-0001.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 82.892 52.578)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R11" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "40k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 7 "/Tx_{1}") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 23 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Dsub:DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm" (layer "F.Cu")
    (at 110.169 69.349669)
    (descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 25mm mounting-hole-offset 25mm")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "9-pin female receptacle socket D-SUB connector")
    (property "ki_keywords" "connector receptacle female D-SUB DB9")
    (attr through_hole)
    (fp_text reference "J4" (at -5.54 -3.7) (layer "F.SilkS"))
    (fp_text value "DE9_Receptacle" (at -5.54 15.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.54 11.265) (layer "F.Fab"))
    (pad "0" thru_hole circle (at -18.04 0.3) (size 4 4) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "0" thru_hole circle (at 6.96 0.3) (size 4 4) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "unconnected-(J4-Pad1)") (pinfunction "1") (pintype "passive+no_connect"))
    (pad "2" thru_hole circle (at -2.77 0) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 34 "/TXI_{2}") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.54 0) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 35 "/RXI_{2}") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -8.31 0) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "unconnected-(J4-Pad4)") (pinfunction "4") (pintype "passive+no_connect"))
    (pad "5" thru_hole circle (at -11.08 0) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "unconnected-(J4-Pad5)") (pinfunction "5") (pintype "passive+no_connect"))
    (pad "6" thru_hole circle (at -1.385 2.84) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "unconnected-(J4-Pad6)") (pinfunction "6") (pintype "passive+no_connect"))
    (pad "7" thru_hole circle (at -4.155 2.84) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "unconnected-(J4-Pad7)") (pinfunction "7") (pintype "passive+no_connect"))
    (pad "8" thru_hole circle (at -6.925 2.84) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "unconnected-(J4-Pad8)") (pinfunction "8") (pintype "passive+no_connect"))
    (pad "9" thru_hole circle (at -9.695 2.84) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "unconnected-(J4-Pad9)") (pinfunction "9") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6_Handsoldering" (layer "F.Cu")
    (at 94.3435 60.159852 90)
    (descr "SOT-363, SC-70-6, Handsoldering")
    (tags "SOT-363 SC-70-6 Handsoldering")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Dual PMOS transistor, 6 pin package")
    (property "ki_keywords" "transistor PMOS P-MOS P-MOSFET")
    (attr smd)
    (fp_text reference "Q2" (at -2.324148 -2.0695 90) (layer "F.SilkS"))
    (fp_text value "Q_Dual_PMOS_S1G1D2S2G2D1" (at 0 2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.33 -0.65 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/TXI_{0}") (pinfunction "S") (pintype "passive"))
    (pad "2" smd rect (at -1.33 0 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "/S_{1}") (pinfunction "G") (pintype "input"))
    (pad "3" smd rect (at -1.33 0.65 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/Rx_{0}") (pinfunction "D") (pintype "passive"))
    (pad "4" smd rect (at 1.33 0.65 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/RXI_{0}") (pinfunction "S") (pintype "passive"))
    (pad "5" smd rect (at 1.33 0 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "/S_{1}") (pinfunction "G") (pintype "input"))
    (pad "6" smd rect (at 1.33 -0.65 90) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/Tx_{0}") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 58.238 71.866 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R19" (at 2.524 0.254 180) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 28 "Net-(D3-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 38 "/S_{2}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_ISO7380" (layer "F.Cu")
    (at 120 63)
    (descr "Mounting Hole 2.2mm, no annular, M2, ISO7380")
    (tags "mounting hole 2.2mm no annular m2 iso7380")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at -0.508 -2.75) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 2.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 83.384 58.42 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R9" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 38 "/S_{2}") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 22 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D1.8mm_W1.8mm_H2.4mm_Horizontal_O1.27mm_Z1.6mm" (layer "F.Cu")
    (at 84.654 75.692)
    (descr "LED, ,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins")
    (tags "LED   diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D4" (at -1.27 3.556) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 5.33) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(D4-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 22 "VCC") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D1.8mm_W1.8mm_H2.4mm_Horizontal_O1.27mm_Z1.6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (at 72.446 80.265)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 3.318 -0.001 -360) (layer "B.SilkS"))
    (fp_text value "20k" (at 0 -1.65 -360) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -360) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 36 "/S_{0}") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 22 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (at 81.098 69.342 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 3.048 0) (layer "B.SilkS"))
    (fp_text value "330" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 23 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 41 "Net-(J7-Pad9)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (at 70.922 77.979)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.778 -360) (layer "B.SilkS"))
    (fp_text value "300k" (at 0 -1.65 -360) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -360) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 27 "/DO-") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 23 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (at 62.81 78.486 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at -1.27 1.524) (layer "B.SilkS"))
    (fp_text value "300k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 26 "/DO+") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 23 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (at 91.782 73.914)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R20" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "1k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 29 "Net-(D4-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 39 "/S_{3}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (at 71.192 68.326 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "330" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 23 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 45 "Net-(J7-Pad11)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6_Handsoldering" (layer "B.Cu")
    (at 67.636 80.519)
    (descr "SOT-363, SC-70-6, Handsoldering")
    (tags "SOT-363 SC-70-6 Handsoldering")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Dual PMOS transistor, 6 pin package")
    (property "ki_keywords" "transistor PMOS P-MOS P-MOSFET")
    (attr smd)
    (fp_text reference "Q1" (at -1.778 -1.525) (layer "B.SilkS"))
    (fp_text value "Q_Dual_PMOS_S1G1D2S2G2D1" (at 0 -2 -360) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect (at -1.33 0.65) (size 1.5 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "/D+") (pinfunction "S") (pintype "passive"))
    (pad "2" smd rect (at -1.33 0) (size 1.5 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "/S_{0}") (pinfunction "G") (pintype "input"))
    (pad "3" smd rect (at -1.33 -0.65) (size 1.5 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "/DO-") (pinfunction "D") (pintype "passive"))
    (pad "4" smd rect (at 1.33 -0.65) (size 1.5 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "/D-") (pinfunction "S") (pintype "passive"))
    (pad "5" smd rect (at 1.33 0) (size 1.5 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "/S_{0}") (pinfunction "G") (pintype "input"))
    (pad "6" smd rect (at 1.33 0.65) (size 1.5 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "/DO+") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (at 98.624 60.198)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "vgaterm-io.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "40k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 4 "/Rx_{0}") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 23 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 57.222 50.8) (end 58.238 49.784)
    (layer "Edge.Cuts"))
  (gr_line (start 127.072 60.198) (end 126.564 60.706)
    (layer "Edge.Cuts"))
  (gr_line (start 127.072 60.198) (end 127.072 52.324)
    (layer "Edge.Cuts"))
  (gr_line (start 57.222 50.8) (end 57.222 63.246)
    (layer "Edge.Cuts"))
  (gr_line (start 55.19 65.278) (end 57.222 63.246)
    (layer "Edge.Cuts"))
  (gr_line (start 122.246 78.994) (end 122.246 61.722)
    (layer "Edge.Cuts"))
  (gr_line (start 55.19 68.326) (end 57.222 70.358)
    (layer "Edge.Cuts"))
  (gr_line (start 57.222 78.994) (end 57.222 70.358)
    (layer "Edge.Cuts"))
  (gr_line (start 55.19 68.326) (end 55.19 65.278)
    (layer "Edge.Cuts"))
  (gr_line (start 63.572 80.264) (end 58.492 80.264)
    (layer "Edge.Cuts"))
  (gr_line (start 58.492 80.264) (end 57.222 78.994)
    (layer "Edge.Cuts"))
  (gr_line (start 83.384 80.264) (end 82.876 82.296)
    (layer "Edge.Cuts"))
  (gr_line (start 121.23 49.784) (end 123.262 51.816)
    (layer "Edge.Cuts"))
  (gr_line (start 127.072 52.324) (end 126.564 51.816)
    (layer "Edge.Cuts"))
  (gr_line (start 126.564 60.706) (end 123.262 60.706)
    (layer "Edge.Cuts"))
  (gr_line (start 121.23 49.784) (end 58.238 49.784)
    (layer "Edge.Cuts"))
  (gr_line (start 64.08 82.296) (end 63.572 80.264)
    (layer "Edge.Cuts"))
  (gr_line (start 123.262 60.706) (end 122.246 61.722)
    (layer "Edge.Cuts"))
  (gr_line (start 83.384 80.264) (end 120.976 80.264)
    (layer "Edge.Cuts"))
  (gr_line (start 82.876 82.296) (end 64.08 82.296)
    (layer "Edge.Cuts"))
  (gr_line (start 126.564 51.816) (end 123.262 51.816)
    (layer "Edge.Cuts"))
  (gr_line (start 120.976 80.264) (end 122.246 78.994)
    (layer "Edge.Cuts"))
  (gr_text "Rx_{0}\nGND" (at 57.222 53.34) (layer "F.SilkS"))
  (gr_text "Rx_{2}\nRx_{1}" (at 60.27 53.34) (layer "F.SilkS"))
  (gr_text "S_{0}\nS_{1}" (at 70.938 53.34) (layer "F.SilkS"))
  (gr_text "Tx_{out}\nRx_{out}" (at 72.716 53.34) (layer "F.SilkS"))
  (gr_text "Tx_{2}\nTx_{1}" (at 65.604 53.34) (layer "F.SilkS"))
  (gr_text "S_{2}\nS_{3}" (at 68.398 53.34) (layer "F.SilkS"))
  (gr_text "A" (at 113.864 63.246) (layer "F.SilkS"))
  (gr_text "B" (at 111.07 58.039) (layer "F.SilkS"))
  (gr_text "Tx_{0}\nGND" (at 62.81 53.34) (layer "F.SilkS"))
  (gr_text "\nGND" (at 76.272 53.34) (layer "F.SilkS"))
  (gr_text "A1" (at 88.464 65.024) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 57.222 82.804) (xy 122.246 82.804))
    (height 4.064)
    (gr_text "65.0240 mm" (at 89.734 85.718) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 109.546 49.784) (xy 122.246 49.784))
    (height -10.414)
    (gr_text "12.7000 mm" (at 115.896 38.22) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 22) (net_name "VCC") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 52.07 99.568)
        (xy 132.334 99.568)
        (xy 133.096 22.606)
        (xy 51.308 22.606)
      )
    )
  )
  (zone (net 23) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 52.578 99.568)
        (xy 133.096 100.076)
        (xy 133.096 21.336)
        (xy 50.292 21.082)
      )
    )
  )
)
