(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 76)
    (no_connects 0)
    (area 135.134999 42.904999 172.205001 99.925)
    (thickness 1.6)
    (drawings 6)
    (tracks 76)
    (zones 0)
    (modules 8)
    (nets 39)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.635)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J1-Pad9)")
  (net 10 "Net-(J1-Pad10)")
  (net 11 "Net-(J1-Pad11)")
  (net 12 "Net-(J1-Pad12)")
  (net 13 "Net-(J1-Pad13)")
  (net 14 "Net-(J1-Pad14)")
  (net 15 "Net-(J1-Pad15)")
  (net 16 "Net-(J1-Pad16)")
  (net 17 "Net-(J1-Pad17)")
  (net 18 "Net-(J1-Pad18)")
  (net 19 "Net-(J1-Pad19)")
  (net 20 "Net-(J2-Pad1)")
  (net 21 "Net-(J2-Pad2)")
  (net 22 "Net-(J2-Pad3)")
  (net 23 "Net-(J2-Pad4)")
  (net 24 "Net-(J2-Pad5)")
  (net 25 "Net-(J2-Pad6)")
  (net 26 "Net-(J2-Pad7)")
  (net 27 "Net-(J2-Pad8)")
  (net 28 "Net-(J2-Pad9)")
  (net 29 "Net-(J2-Pad10)")
  (net 30 "Net-(J2-Pad11)")
  (net 31 "Net-(J2-Pad12)")
  (net 32 "Net-(J2-Pad13)")
  (net 33 "Net-(J2-Pad14)")
  (net 34 "Net-(J2-Pad15)")
  (net 35 "Net-(J2-Pad16)")
  (net 36 "Net-(J2-Pad17)")
  (net 37 "Net-(J2-Pad18)")
  (net 38 "Net-(J2-Pad19)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad19)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x19_Pitch2.54mm (layer F.Cu) (tedit 5AB9593E)
    (at 163.83 96.52 180)
    (descr "Through hole straight pin header, 1x19, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x19 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value "" (at 0 48.05 180) (layer F.Fab))
    (fp_text user %R (at 0 22.86 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad14)"))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad15)"))
    (pad 16 thru_hole oval (at 0 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad16)"))
    (pad 17 thru_hole oval (at 0 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad17)"))
    (pad 18 thru_hole oval (at 0 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad18)"))
    (pad 19 thru_hole oval (at 0 45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad19)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x19_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x19_Pitch2.54mm (layer F.Cu) (tedit 5AB95939)
    (at 143.51 96.52 180)
    (descr "Through hole straight pin header, 1x19, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x19 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value "" (at 0 48.05 180) (layer F.Fab))
    (fp_text user %R (at 0 22.86 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad14)"))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad15)"))
    (pad 16 thru_hole oval (at 0 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad16)"))
    (pad 17 thru_hole oval (at 0 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad17)"))
    (pad 18 thru_hole oval (at 0 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J2-Pad18)"))
    (pad 19 thru_hole oval (at 0 45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad19)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x19_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x19_Pitch2.54mm (layer F.Cu) (tedit 5AB9588D)
    (at 170.18 96.52 180)
    (descr "Through hole straight pin header, 1x19, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x19 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value "" (at 0 48.05 180) (layer F.Fab))
    (fp_text user %R (at 0 22.86 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad14)"))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad15)"))
    (pad 16 thru_hole oval (at 0 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad16)"))
    (pad 17 thru_hole oval (at 0 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad17)"))
    (pad 18 thru_hole oval (at 0 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad18)"))
    (pad 19 thru_hole oval (at 0 45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad19)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x19_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x19_Pitch2.54mm (layer F.Cu) (tedit 5AB95880)
    (at 137.16 96.52 180)
    (descr "Through hole straight pin header, 1x19, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x19 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value "" (at 0 48.05 180) (layer F.Fab))
    (fp_text user %R (at 0 22.86 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad14)"))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad15)"))
    (pad 16 thru_hole oval (at 0 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad16)"))
    (pad 17 thru_hole oval (at 0 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad17)"))
    (pad 18 thru_hole oval (at 0 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J2-Pad18)"))
    (pad 19 thru_hole oval (at 0 45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad19)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x19_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module modules:ESP32DevBoard (layer F.Cu) (tedit 5AB95E8B)
    (at 153.67 74.93)
    (fp_text reference U1 (at -7.62 -30.48) (layer F.SilkS) hide)
    (fp_text value ESP32DevBoard (at 0 -24.13) (layer F.Fab))
    (fp_text user ESP-WROOM-32 (at 0 -15.875 180) (layer F.SilkS))
    (pad 19 thru_hole circle (at 12.7 -24.13) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J1-Pad19)"))
    (pad 18 thru_hole circle (at 12.7 -21.59) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J1-Pad18)"))
    (pad 17 thru_hole circle (at 12.7 -19.05) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J1-Pad17)"))
    (pad 8 thru_hole circle (at 12.7 3.81) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-Pad8)"))
    (pad 7 thru_hole circle (at 12.7 6.35) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad7)"))
    (pad 6 thru_hole circle (at 12.7 8.89) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad6)"))
    (pad 5 thru_hole circle (at 12.7 11.43) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad5)"))
    (pad 4 thru_hole circle (at 12.7 13.97) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad4)"))
    (pad 3 thru_hole circle (at 12.7 16.51) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 12.7 19.05) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 12.7 21.59) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(J1-Pad1)"))
    (pad 16 thru_hole circle (at 12.7 -16.51) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J1-Pad16)"))
    (pad 15 thru_hole circle (at 12.7 -13.97) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J1-Pad15)"))
    (pad 14 thru_hole circle (at 12.7 -11.43) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J1-Pad14)"))
    (pad 13 thru_hole circle (at 12.7 -8.89) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J1-Pad13)"))
    (pad 12 thru_hole circle (at 12.7 -6.35) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J1-Pad12)"))
    (pad 11 thru_hole circle (at 12.7 -3.81) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-Pad11)"))
    (pad 10 thru_hole circle (at 12.7 -1.27) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J1-Pad10)"))
    (pad 9 thru_hole circle (at 12.7 1.27) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad9)"))
    (pad 30 thru_hole circle (at -12.7 1.27) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(J2-Pad9)"))
    (pad 29 thru_hole circle (at -12.7 -1.27) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(J2-Pad10)"))
    (pad 28 thru_hole circle (at -12.7 -3.81) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(J2-Pad11)"))
    (pad 27 thru_hole circle (at -12.7 -6.35) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(J2-Pad12)"))
    (pad 26 thru_hole circle (at -12.7 -8.89) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(J2-Pad13)"))
    (pad 25 thru_hole circle (at -12.7 -11.43) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(J2-Pad14)"))
    (pad 24 thru_hole circle (at -12.7 -13.97) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(J2-Pad15)"))
    (pad 23 thru_hole circle (at -12.7 -16.51) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(J2-Pad16)"))
    (pad 38 thru_hole circle (at -12.7 21.59) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J2-Pad1)"))
    (pad 37 thru_hole circle (at -12.7 19.05) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J2-Pad2)"))
    (pad 36 thru_hole circle (at -12.7 16.51) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(J2-Pad3)"))
    (pad 35 thru_hole circle (at -12.7 13.97) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J2-Pad4)"))
    (pad 34 thru_hole circle (at -12.7 11.43) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(J2-Pad5)"))
    (pad 33 thru_hole circle (at -12.7 8.89) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(J2-Pad6)"))
    (pad 32 thru_hole circle (at -12.7 6.35) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(J2-Pad7)"))
    (pad 31 thru_hole circle (at -12.7 3.81) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(J2-Pad8)"))
    (pad 22 thru_hole circle (at -12.7 -19.05) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(J2-Pad17)"))
    (pad 21 thru_hole circle (at -12.7 -21.59) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(J2-Pad18)"))
    (pad 20 thru_hole circle (at -12.7 -24.13) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(J2-Pad19)"))
  )
  (module modules:madcat10 (layer B.Cu) (tedit 5AB95EC9)
    (at 150.241 73.66 180)
    (fp_text reference "" (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0 180) (layer F.SilkS) hide)
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 153.67 64.77)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (attr virtual)
    (fp_text reference "" (at 0 -3.7) (layer F.SilkS))
    (fp_text value MountingHole_2.7mm (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 153.67 82.55)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (attr virtual)
    (fp_text reference "" (at 0 -3.7) (layer F.SilkS))
    (fp_text value MountingHole_2.7mm (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask))
  )
  (gr_text i326 (at 156.464 75.184) (layer F.SilkS))
  (gr_text RSP (at 156.464 72.517) (layer F.SilkS))
  (gr_line (start 135.89 97.79) (end 135.89 49.53) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.45 97.79) (end 135.89 97.79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.45 49.53) (end 171.45 97.79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.89 49.53) (end 171.45 49.53) (angle 90) (layer Edge.Cuts) (width 0.15))
)
