(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 79)
    (no_connects 0)
    (area 138.366499 97.726499 174.053501 118.173501)
    (thickness 1.6002)
    (drawings 35)
    (tracks 355)
    (zones 0)
    (modules 32)
    (nets 43)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 RTS)
  (net 2 DTR)
  (net 3 +5V)
  (net 4 GND)
  (net 5 "Net-(U2-Pad4)")
  (net 6 +3V3)
  (net 7 /D+)
  (net 8 /D-)
  (net 9 "Net-(R3-Pad2)")
  (net 10 CHREN)
  (net 11 CHR1)
  (net 12 CHR0)
  (net 13 RXD)
  (net 14 TXD)
  (net 15 "Net-(D2-PadA)")
  (net 16 "Net-(J3-PadID)")
  (net 17 GNDPWR)
  (net 18 /VBUS)
  (net 19 "Net-(D3-PadA)")
  (net 20 "Net-(D3-PadC)")
  (net 21 "Net-(D4-PadA)")
  (net 22 "Net-(D4-PadC)")
  (net 23 CTS)
  (net 24 VIO)
  (net 25 /SUSPENDb)
  (net 26 "Net-(U1-Pad1)")
  (net 27 "Net-(U1-Pad2)")
  (net 28 "Net-(U1-Pad10)")
  (net 29 "Net-(U1-Pad12)")
  (net 30 "Net-(U1-Pad16)")
  (net 31 "Net-(U1-Pad17)")
  (net 32 "Net-(U1-Pad20)")
  (net 33 "Net-(U1-Pad21)")
  (net 34 "Net-(U1-Pad22)")
  (net 35 "Net-(U1-Pad27)")
  (net 36 PIN6)
  (net 37 "Net-(J7-Pad3)")
  (net 38 "Net-(J7-Pad4)")
  (net 39 RST)
  (net 40 GPIO0)
  (net 41 "Net-(R8-Pad2)")
  (net 42 "Net-(R9-Pad1)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /SUSPENDb)
    (add_net /VBUS)
    (add_net CTS)
    (add_net GNDPWR)
    (add_net GPIO0)
    (add_net "Net-(D3-PadA)")
    (add_net "Net-(D3-PadC)")
    (add_net "Net-(D4-PadA)")
    (add_net "Net-(D4-PadC)")
    (add_net "Net-(J7-Pad3)")
    (add_net "Net-(J7-Pad4)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad27)")
    (add_net PIN6)
    (add_net RST)
    (add_net VIO)
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class 50ohm ""
    (clearance 0.15)
    (trace_width 0.8)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class "small clearance" ""
    (clearance 0.2)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +3V3)
    (add_net +5V)
    (add_net /D+)
    (add_net /D-)
    (add_net CHR0)
    (add_net CHR1)
    (add_net CHREN)
    (add_net DTR)
    (add_net GND)
    (add_net "Net-(D2-PadA)")
    (add_net "Net-(J3-PadID)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(U2-Pad4)")
    (add_net RTS)
    (add_net RXD)
    (add_net TXD)
  )
  (module SparkFun-Capacitors:SparkFun-Capacitors-0603 (layer F.Cu) (tedit 59DAA923)
    (at 161.798 103.251)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference C1 (at 0 1.143) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.0668) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module SparkFun-Capacitors:SparkFun-Capacitors-0603 (layer F.Cu) (tedit 59DAA89A)
    (at 156.21 100.965 180)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference C2 (at 2.032 0 270) (layer F.SilkS))
    (fp_text value 1uF (at 1.524 -1.143 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0 180) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 0.84836 0 180) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module SparkFun-Capacitors:SparkFun-Capacitors-0603 (layer F.Cu) (tedit 59DAA8AC)
    (at 152.654 107.315)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference C3 (at -2.032 0.127 90) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.0668) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module SparkFun-Capacitors:SparkFun-Capacitors-0603 (layer F.Cu) (tedit 59DAA8B2)
    (at 152.61336 109.22)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference C4 (at -1.99136 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.0668) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module SparkFun-Capacitors:SparkFun-Capacitors-0603 (layer F.Cu) (tedit 59DAA9D6)
    (at 172.212 100.965 270)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference C5 (at 0 1.016 270) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.0668 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0 270) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.84836 0 270) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 17 GNDPWR))
  )
  (module Diodes_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 59DAA3DE)
    (at 166.35 100.965)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at -2.393 0 90) (layer F.SilkS))
    (fp_text value D_Schottky_Small (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 1.25 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 18 /VBUS))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SparkFun-LED:SparkFun-LED-LED-0603 (layer F.Cu) (tedit 59DAA8E7)
    (at 164.831032 113.579446 90)
    (descr "LED 0603 SMT")
    (tags "LED 0603 SMT")
    (attr smd)
    (fp_text reference D2 (at 0 -0.9398 90) (layer F.SilkS) hide)
    (fp_text value SPND (at 0 0.9398 90) (layer F.SilkS))
    (pad A smd rect (at -0.8763 0) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D2-PadA)"))
    (pad C smd rect (at 0.8763 0) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module SparkFun-LED:SparkFun-LED-LED-0603 (layer F.Cu) (tedit 200000)
    (at 163.3093 106.2863 270)
    (descr "LED 0603 SMT")
    (tags "LED 0603 SMT")
    (attr smd)
    (fp_text reference D3 (at -1.8923 -0.0127 360) (layer F.SilkS))
    (fp_text value TX (at 0 0.9398 270) (layer F.SilkS))
    (pad A smd rect (at -0.8763 0 180) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D3-PadA)"))
    (pad C smd rect (at 0.8763 0 180) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D3-PadC)"))
  )
  (module SparkFun-LED:SparkFun-LED-LED-0603 (layer F.Cu) (tedit 200000)
    (at 163.3093 109.728 270)
    (descr "LED 0603 SMT")
    (tags "LED 0603 SMT")
    (attr smd)
    (fp_text reference D4 (at -1.651 -0.0127 360) (layer F.SilkS))
    (fp_text value RX (at 0 0.9398 270) (layer F.SilkS))
    (pad A smd rect (at -0.8763 0 180) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D4-PadA)"))
    (pad C smd rect (at 0.8763 0 180) (size 0.99822 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D4-PadC)"))
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X06_NO_SILK (layer F.Cu) (tedit 59DAA059)
    (at 139.7 101.6 270)
    (descr "PLATED THROUGH HOLE - 6 PIN NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - 6 PIN NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference J1 (at 0.254 -1.7018 270) (layer F.SilkS) hide)
    (fp_text value UART (at 0.5588 1.7272 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 23 CTS))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 24 VIO))
    (pad 4 thru_hole circle (at 7.62 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 14 TXD))
    (pad 5 thru_hole circle (at 10.16 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 13 RXD))
    (pad 6 thru_hole circle (at 12.7 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 36 PIN6))
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X04_NO_SILK (layer F.Cu) (tedit 59DAA465)
    (at 154.94 99.06)
    (descr "PLATED THROUGH HOLE - 4 PIN NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - 4 PIN NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference J2 (at 0.254 -1.7018) (layer F.SilkS) hide)
    (fp_text value Power (at 0.5588 1.7272) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 6 +3V3))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 3 +5V))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 18 /VBUS))
  )
  (module SparkFun-Connectors:SparkFun-Connectors-USB-B-MICRO-SMD (layer F.Cu) (tedit 59DAA3EA)
    (at 172.14088 107.8357 180)
    (descr "USB - MICROB SMD")
    (tags "USB - MICROB SMD")
    (attr smd)
    (fp_text reference J3 (at 0.254 -5.0038 180) (layer F.SilkS) hide)
    (fp_text value USB_MICRO-B_FEMALE-SMT (at 0.5588 5.0038 180) (layer F.SilkS) hide)
    (fp_text user "PCB Front" (at -3.28676 -6.11124 180) (layer Dwgs.User))
    (pad D+ smd rect (at 2.72288 0 270) (size 0.39878 1.4478) (layers F.Cu F.Paste F.Mask)
      (net 7 /D+))
    (pad D- smd rect (at 2.72288 -0.6477 270) (size 0.39878 1.4478) (layers F.Cu F.Paste F.Mask)
      (net 8 /D-))
    (pad GND smd rect (at 2.72288 1.29794 270) (size 0.39878 1.4478) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad ID smd rect (at 2.72288 0.6477 270) (size 0.39878 1.4478) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J3-PadID)"))
    (pad SHIE smd rect (at 0 -3.683 270) (size 1.79832 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 17 GNDPWR))
    (pad SHIE smd rect (at 0 3.683 270) (size 1.79832 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 17 GNDPWR))
    (pad SHIE smd rect (at 0 0 270) (size 2.49936 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 17 GNDPWR))
    (pad VBUS smd rect (at 2.72288 -1.29794 270) (size 0.39878 1.4478) (layers F.Cu F.Paste F.Mask)
      (net 18 /VBUS))
    (pad "" np_thru_hole circle (at 2.19964 -1.89992 180) (size 0.84836 0.84836) (drill 0.84836) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.19964 1.89992 180) (size 0.84836 0.84836) (drill 0.84836) (layers *.Cu *.Mask))
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X03_NO_SILK (layer F.Cu) (tedit 59DAA06E)
    (at 143.51 100.33)
    (descr "PLATED THROUGH HOLE - 3 PIN NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - 3 PIN NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference J5 (at 0.254 -1.7018) (layer F.SilkS) hide)
    (fp_text value JumperV (at 0.5588 1.7272) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 6 +3V3))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 24 VIO))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 3 +5V))
  )
  (module SparkFun-Resistors:SparkFun-Resistors-0603 (layer F.Cu) (tedit 59DAA92B)
    (at 161.75736 101.473)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference R1 (at 0 -1.0668) (layer F.SilkS))
    (fp_text value 100k (at 0 1.0668) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module SparkFun-Resistors:SparkFun-Resistors-0603 (layer F.Cu) (tedit 59DAA9DF)
    (at 169.926 100.965 270)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference R2 (at 0.127 1.016 270) (layer F.SilkS))
    (fp_text value 1M (at 0 1.0668 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0 270) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.84836 0 270) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 17 GNDPWR))
  )
  (module SparkFun-Resistors:SparkFun-Resistors-0603 (layer F.Cu) (tedit 59DAA8B6)
    (at 154.051 113.157)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference R3 (at -2.032 0 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.0668) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 0.84836 0) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R3-Pad2)"))
  )
  (module SparkFun-Resistors:SparkFun-Resistors-0603 (layer F.Cu) (tedit 59DAA8C8)
    (at 163.167332 113.579446 270)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference R4 (at 0 1.115332 270) (layer F.SilkS))
    (fp_text value 470 (at 0 1.0668 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0 270) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 25 /SUSPENDb))
    (pad 2 smd rect (at 0.84836 0 270) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D2-PadA)"))
  )
  (module SparkFun-Resistors:SparkFun-Resistors-0603 (layer F.Cu) (tedit 59DAA8C2)
    (at 157.48 114.173 180)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference R5 (at 0 0.762 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.0668 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0 180) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 25 /SUSPENDb))
    (pad 2 smd rect (at 0.84836 0 180) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module SparkFun-Resistors:SparkFun-Resistors-0603 (layer F.Cu) (tedit 59DAA8D5)
    (at 164.973 106.25836 90)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference R6 (at 0 1.143 90) (layer F.SilkS))
    (fp_text value 470 (at 0 1.0668 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0 90) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 0.84836 0 90) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D3-PadA)"))
  )
  (module SparkFun-Resistors:SparkFun-Resistors-0603 (layer F.Cu) (tedit 59DAA8D0)
    (at 164.973 109.728 90)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference R7 (at 0 1.143 90) (layer F.SilkS))
    (fp_text value 470 (at 0 1.0668 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0 90) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 0.84836 0 90) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D4-PadA)"))
  )
  (module nixiemisc:nixiemisc-QFN28G_0.5-5X5MM (layer F.Cu) (tedit 59DAA40F)
    (at 158.75 109.728)
    (attr smd)
    (fp_text reference U1 (at -0.97536 -3.80238) (layer F.SilkS))
    (fp_text value CP2102N (at -0.17018 3.69316) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.58826 -1.4986) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at -2.58826 -0.99822) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -2.58826 -0.49784) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 4 smd rect (at -2.58826 0) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 7 /D+))
    (pad 5 smd rect (at -2.58826 0.49784) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 8 /D-))
    (pad 6 smd rect (at -2.58826 0.99822) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 7 smd rect (at -2.58826 1.4986) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 8 smd rect (at -1.4986 2.58826 90) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 9 smd rect (at -0.99822 2.58826 90) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R3-Pad2)"))
    (pad 10 smd rect (at -0.49784 2.58826 90) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U1-Pad10)"))
    (pad 11 smd rect (at 0 2.58826 90) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 25 /SUSPENDb))
    (pad 12 smd rect (at 0.49784 2.58826 90) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U1-Pad12)"))
    (pad 13 smd rect (at 0.99822 2.58826 90) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 10 CHREN))
    (pad 14 smd rect (at 1.4986 2.58826 90) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 11 CHR1))
    (pad 15 smd rect (at 2.58826 1.4986 180) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 12 CHR0))
    (pad 16 smd rect (at 2.58826 0.99822 180) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U1-Pad16)"))
    (pad 17 smd rect (at 2.58826 0.49784 180) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U1-Pad17)"))
    (pad 18 smd rect (at 2.58826 0 180) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D4-PadC)"))
    (pad 19 smd rect (at 2.58826 -0.49784 180) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D3-PadC)"))
    (pad 20 smd rect (at 2.58826 -0.99822 180) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U1-Pad20)"))
    (pad 21 smd rect (at 2.58826 -1.4986 180) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U1-Pad21)"))
    (pad 22 smd rect (at 1.4986 -2.58826 270) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U1-Pad22)"))
    (pad 23 smd rect (at 0.99822 -2.58826 270) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 23 CTS))
    (pad 24 smd rect (at 0.49784 -2.58826 270) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 1 RTS))
    (pad 25 smd rect (at 0 -2.58826 270) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 14 TXD))
    (pad 26 smd rect (at -0.49784 -2.58826 270) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 13 RXD))
    (pad 27 smd rect (at -0.99822 -2.58826 270) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U1-Pad27)"))
    (pad 28 smd rect (at -1.4986 -2.58826 270) (size 0.89916 0.254) (layers F.Cu F.Paste F.Mask)
      (net 2 DTR))
    (pad 29 smd rect (at 0 0) (size 3.0988 3.0988) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module nixiemisc:nixiemisc-SOT25 (layer F.Cu) (tedit 59DAA3F5)
    (at 157.353 103.251 90)
    (descr "SMALL OUTLINE TRANSISTOR")
    (tags "SMALL OUTLINE TRANSISTOR")
    (attr smd)
    (fp_text reference U2 (at 1.27 -2.54 90) (layer F.SilkS) hide)
    (fp_text value AP2112 (at 1.905 2.794 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.94996 1.29794 90) (size 0.54864 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0 1.29794 90) (size 0.54864 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at 0.94996 1.29794 90) (size 0.54864 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 4 smd rect (at 0.94996 -1.29794 90) (size 0.54864 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at -0.94996 -1.29794 90) (size 0.54864 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
  )
  (module nixiemisc:nixiemisc-SOT143 (layer F.Cu) (tedit 59DAA3AD)
    (at 169.926 114.808 270)
    (descr SOT-143)
    (tags SOT-143)
    (attr smd)
    (fp_text reference U3 (at 1.27 -2.54 270) (layer F.SilkS) hide)
    (fp_text value ESD (at 1.905 2.54 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.7493 1.09982 270) (size 1.19888 1.43764) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.94996 1.09982 270) (size 0.99822 1.43764) (layers F.Cu F.Paste F.Mask)
      (net 18 /VBUS))
    (pad 3 smd rect (at 0.94996 -1.09982 270) (size 0.99822 1.43764) (layers F.Cu F.Paste F.Mask)
      (net 8 /D-))
    (pad 4 smd rect (at -0.94996 -1.09982 270) (size 0.99822 1.43764) (layers F.Cu F.Paste F.Mask)
      (net 7 /D+))
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X03_NO_SILK (layer F.Cu) (tedit 59DAA08B)
    (at 143.51 115.57)
    (descr "PLATED THROUGH HOLE - 3 PIN NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - 3 PIN NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference J6 (at 0.254 -1.7018) (layer F.SilkS) hide)
    (fp_text value JumperS (at 0.5588 1.7272) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 1 RTS))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 36 PIN6))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 2 DTR))
  )
  (module SparkFun-Resistors:SparkFun-Resistors-0603 (layer F.Cu) (tedit 59DAA88A)
    (at 154.051 104.21091 270)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference R8 (at 0 -1.0668 270) (layer F.SilkS))
    (fp_text value 12K (at 0 1.0668 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0 270) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 RTS))
    (pad 2 smd rect (at 0.84836 0 270) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R8-Pad2)"))
  )
  (module SparkFun-Resistors:SparkFun-Resistors-0603 (layer F.Cu) (tedit 59DAA87F)
    (at 149.225 104.08391 270)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference R9 (at -0.07091 1.143 270) (layer F.SilkS))
    (fp_text value 12K (at 0 1.0668 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0 270) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R9-Pad1)"))
    (pad 2 smd rect (at 0.84836 0 270) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 2 DTR))
  )
  (module SparkFun-Resistors:SparkFun-Resistors-0603 (layer F.Cu) (tedit 59DAA892)
    (at 152.03388 101.67091 180)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference R10 (at 2.04688 0.07091 270) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.0668 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0 180) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 0.84836 0 180) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 40 GPIO0))
  )
  (module SparkFun-Resistors:SparkFun-Resistors-0603 (layer F.Cu) (tedit 59DAA870)
    (at 148.082 108.54436 270)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference R11 (at 0.04064 -1.0668 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.0668 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.84836 0 270) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 0.84836 0 270) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J7-Pad3)"))
  )
  (module nixiemisc:nixiemisc-UMT6 (layer F.Cu) (tedit 59DAA401)
    (at 151.77988 104.21091 270)
    (descr "UMT6 PACKAGE EIAJ: SC-88")
    (tags "UMT6 PACKAGE EIAJ: SC-88")
    (attr smd)
    (fp_text reference U4 (at 1.905 -1.905 270) (layer F.SilkS) hide)
    (fp_text value UMH3NUMT6 (at 2.54 1.905 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.92456 -0.6477 270) (size 0.49784 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1 RTS))
    (pad 2 smd rect (at -0.92456 0 270) (size 0.49784 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R9-Pad1)"))
    (pad 3 smd rect (at -0.92456 0.6477 270) (size 0.49784 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 40 GPIO0))
    (pad 4 smd rect (at 0.92456 0.6477 90) (size 0.49784 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 2 DTR))
    (pad 5 smd rect (at 0.92456 0 90) (size 0.49784 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R8-Pad2)"))
    (pad 6 smd rect (at 0.92456 -0.6477 90) (size 0.49784 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 39 RST))
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X05_NO_SILK (layer F.Cu) (tedit 59DAA43A)
    (at 154.94 116.84)
    (descr "PLATED THROUGH HOLE - 5 PIN NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - 5 PIN NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference J4 (at 0.254 -1.7018) (layer F.SilkS) hide)
    (fp_text value Charge (at 0.5588 1.7272) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 10 CHREN))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 11 CHR1))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 12 CHR0))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 8 /D-))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 7 /D+))
  )
  (module Socket_Strips:Socket_Strip_Straight_2x04_Pitch2.54mm (layer B.Cu) (tedit 59DAA09B)
    (at 146.05 111.76)
    (descr "Through hole straight socket strip, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x04 2.54mm double row")
    (fp_text reference J7 (at -1.27 2.33) (layer B.SilkS) hide)
    (fp_text value ESP01 (at -1.27 -9.95) (layer B.Fab))
    (fp_text user %R (at -1.27 2.33) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 TXD))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J7-Pad3)"))
    (pad 4 thru_hole oval (at -2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J7-Pad4)"))
    (pad 5 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 RST))
    (pad 6 thru_hole oval (at -2.54 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 GPIO0))
    (pad 7 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 +3V3))
    (pad 8 thru_hole oval (at -2.54 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 RXD))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x04_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module logos:mermaid_l (layer B.Cu) (tedit 0)
    (at 170.942 102.362 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_text + (at 165.1 115.824 90) (layer F.SilkS))
  (gr_text - (at 162.56 115.824 90) (layer F.SilkS))
  (gr_text C0 (at 160.02 115.824 90) (layer F.SilkS))
  (gr_text C1 (at 157.48 115.824 90) (layer F.SilkS))
  (gr_text CH (at 154.94 115.824 90) (layer F.SilkS))
  (gr_text 3V3 (at 158.242 100.838 90) (layer F.SilkS))
  (gr_text 5V (at 159.766 100.584 90) (layer F.SilkS))
  (gr_text VBus (at 164.084 99.06 90) (layer F.SilkS))
  (gr_text GND (at 153.416 99.06 90) (layer F.SilkS))
  (gr_text CH_PD (at 148.082 109.22 90) (layer B.SilkS))
  (gr_text TXD (at 148.082 111.76 90) (layer B.SilkS))
  (gr_text RST (at 148.082 106.68 90) (layer B.SilkS))
  (gr_text 3V3 (at 148.082 104.14 90) (layer B.SilkS))
  (gr_text RXD (at 141.478 104.14 90) (layer B.SilkS))
  (gr_text GPIO0 (at 141.478 106.68 90) (layer B.SilkS))
  (gr_text GND (at 141.478 111.76 90) (layer B.SilkS))
  (gr_text GND (at 141.224 101.6 90) (layer F.SilkS))
  (gr_text CTS (at 141.224 104.14 90) (layer F.SilkS))
  (gr_text TXD (at 141.224 109.22 90) (layer F.SilkS))
  (gr_text RXD (at 141.224 111.76 90) (layer F.SilkS))
  (gr_text 5V (at 147.32 98.044 90) (layer F.SilkS))
  (gr_text 3V3 (at 144.78 98.044 90) (layer F.SilkS))
  (gr_text DTR (at 147.32 117.856 90) (layer F.SilkS))
  (gr_text RTS (at 144.78 117.856 90) (layer F.SilkS))
  (gr_text "nixies.us\nUART v0.1" (at 169.418 102.235) (layer B.Mask))
  (gr_line (start 173.99 97.79) (end 138.43 97.79) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 173.99 118.11) (end 173.99 97.79) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 138.43 118.11) (end 173.99 118.11) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 138.43 97.79) (end 138.43 118.11) (layer Edge.Cuts) (width 0.127))
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 173.736 98.044) (xy 138.684 98.044) (xy 138.684 117.856) (xy 173.736 117.856)
      )
    )
  )
  (zone (net 6) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.684 98.044) (xy 138.684 117.856) (xy 166.878 117.856) (xy 166.878 98.044)
      )
    )
  )
)
