(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "BITSv5.2")
    (date "2024-02-17")
    (rev "2")
    (company "UMDBPP")
  )
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" signal)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "prepreg") (thickness 0.1) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "core") (thickness 1.24) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "prepreg") (thickness 0.1) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 246.55 117.775)
    (grid_origin 105.2 44)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerbers/")
    )
  )
  (net 0 "")
  (net 1 "/QSPI_SS")
  (net 2 "/QSPI_SD1")
  (net 3 "/QSPI_SD2")
  (net 4 "GND")
  (net 5 "/QSPI_SD0")
  (net 6 "/QSPI_SCLK")
  (net 7 "/QSPI_SD3")
  (net 8 "+3V3")
  (net 9 "+BATT")
  (net 10 "Net-(U1-RUN)")
  (net 11 "Net-(J1-Pin_1)")
  (net 12 "unconnected-(U3-~{RESET}-Pad9)")
  (net 13 "Net-(J1-Pin_2)")
  (net 14 "unconnected-(U3-LNA_EN-Pad13)")
  (net 15 "unconnected-(U3-VCC_RF-Pad14)")
  (net 16 "unconnected-(U3-VIO_SEL-Pad15)")
  (net 17 "unconnected-(U3-~{SAFEBOOT}-Pad18)")
  (net 18 "+5V")
  (net 19 "Net-(D1-A)")
  (net 20 "Net-(C16-Pad1)")
  (net 21 "Net-(BT2-+)")
  (net 22 "Net-(U1-XIN)")
  (net 23 "Net-(C14-Pad1)")
  (net 24 "Net-(U5-VCC)")
  (net 25 "VBUS")
  (net 26 "/USB_D+")
  (net 27 "/USB_D-")
  (net 28 "Net-(D1-K)")
  (net 29 "/IRIDIUM_RXD")
  (net 30 "/IRIDIUM_CTS")
  (net 31 "/IRIDIUM_RTS")
  (net 32 "/IRIDIUM_NETAV")
  (net 33 "/IRIDIUM_RING")
  (net 34 "/IRIDIUM_TXD")
  (net 35 "Net-(U6-SS)")
  (net 36 "Net-(J2-CC1)")
  (net 37 "Net-(J2-D+-PadA6)")
  (net 38 "/LED")
  (net 39 "Net-(J6-In)")
  (net 40 "/TIMEPULSE")
  (net 41 "Net-(D2-K)")
  (net 42 "unconnected-(U1-GPIO14-Pad17)")
  (net 43 "unconnected-(U1-GPIO15-Pad18)")
  (net 44 "+1V1")
  (net 45 "Net-(J2-D--PadA7)")
  (net 46 "unconnected-(J2-SBU1-PadA8)")
  (net 47 "unconnected-(U1-GPIO7-Pad9)")
  (net 48 "unconnected-(U1-GPIO19-Pad30)")
  (net 49 "/EXTINT")
  (net 50 "/RDIO_RST")
  (net 51 "Net-(U1-XOUT)")
  (net 52 "/MISO")
  (net 53 "Net-(U1-USB_DM)")
  (net 54 "Net-(U1-USB_DP)")
  (net 55 "Net-(U6-OV1)")
  (net 56 "Net-(U6-ILM)")
  (net 57 "Net-(SW3-C)")
  (net 58 "Net-(U6-OV2)")
  (net 59 "unconnected-(J2-SBU2-PadB8)")
  (net 60 "/DRF_SW")
  (net 61 "/DRF_TXEN")
  (net 62 "/DRF_DIO1")
  (net 63 "/RP_SWCLK")
  (net 64 "/RP_SWD")
  (net 65 "/DRF_BUSY")
  (net 66 "unconnected-(U1-GPIO22-Pad34)")
  (net 67 "/SCK")
  (net 68 "/DRF_CS")
  (net 69 "/MOSI")
  (net 70 "/FRAM_CS")
  (net 71 "unconnected-(U1-GPIO28_ADC2-Pad40)")
  (net 72 "unconnected-(U1-GPIO23-Pad35)")
  (net 73 "Net-(SW2-B)")
  (net 74 "unconnected-(SW2-A-Pad1)")
  (net 75 "unconnected-(J4-Pin_7-Pad7)")
  (net 76 "Net-(J2-CC2)")
  (net 77 "/SCL")
  (net 78 "unconnected-(J4-Pin_9-Pad9)")
  (net 79 "unconnected-(U11-SDO-Pad6)")
  (net 80 "unconnected-(U1-GPIO16-Pad27)")
  (net 81 "unconnected-(U1-GPIO6-Pad8)")
  (net 82 "/SDA")
  (net 83 "unconnected-(U7-~{WP}-PadB2)")
  (net 84 "unconnected-(U7-~{HOLD}-PadD2)")
  (net 85 "/BATT_REG")
  (net 86 "Net-(U8-VCC)")
  (net 87 "Net-(U8-VOUT)")
  (net 88 "Net-(JP1-A)")
  (net 89 "Net-(J5-In)")
  (net 90 "Net-(SW3-B)")
  (net 91 "Net-(U8-FB)")
  (net 92 "Net-(U6-CP2)")
  (net 93 "Net-(U6-PR1)")
  (net 94 "Net-(U5-FB)")
  (net 95 "unconnected-(U5-PGOOD-Pad1)")
  (net 96 "unconnected-(U5-SW-Pad5)")
  (net 97 "unconnected-(U5-SW-Pad6)")
  (net 98 "unconnected-(U5-BOOT-Pad7)")
  (net 99 "unconnected-(U8-PGOOD-Pad1)")
  (net 100 "unconnected-(U8-SW-Pad5)")
  (net 101 "unconnected-(U8-SW-Pad6)")
  (net 102 "unconnected-(U8-BOOT-Pad7)")
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 145 68.8 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R9" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "DNF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "/SDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 115.325 48.9)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C17" (at 1.875 -0.1 90) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(U5-VCC)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 124.19 63.8256 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.16) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "+1V1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "BITSv5:CL-SB-12B-01_NDC" (layer "F.Cu")
    (at 110.1601 77.453102 180)
    (tags "CL-SB-12B-01T ")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Switch, single pole double throw")
    (property "ki_keywords" "switch single-pole double-throw spdt ON-ON")
    (attr smd)
    (fp_text reference "SW3" (at 0 2.198101 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "SLIDE" (at 0 2.198101 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.198101 180 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -3.399998 -0.0019 180) (size 0.889 0.889) (drill 0.889) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 3.399998 -0.0019 180) (size 0.889 0.889) (drill 0.889) (layers "*.Cu" "*.Mask"))
    (pad "1" smd rect (at -2.54 2.198101 180) (size 1.1938 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 0 -2.201898 180) (size 1.1938 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "Net-(SW3-B)") (pinfunction "B") (pintype "passive"))
    (pad "3" smd rect (at 2.54 2.198101 180) (size 1.1938 1.397) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "Net-(SW3-C)") (pinfunction "C") (pintype "passive"))
  )
  (footprint "BITSv5:RP2040-QFN-56" (layer "F.Cu")
    (at 130.38 66.8481 90)
    (descr "QFN, 56 Pin (http://www.cypress.com/file/416486/download#page=40), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -4.82 90) (layer "F.SilkS") hide)
    (fp_text value "MCU_RaspberryPi_RP2040_RP2040" (at 0 4.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" smd roundrect (at -0.6375 -0.6375 90) (size 1.084435 1.084435) (layers "F.Paste") (roundrect_rratio 0.2305347946))
    (pad "" smd roundrect (at -0.6375 0.6375 90) (size 1.084435 1.084435) (layers "F.Paste") (roundrect_rratio 0.2305347946))
    (pad "" smd roundrect (at 0.6375 -0.6375 90) (size 1.084435 1.084435) (layers "F.Paste") (roundrect_rratio 0.2305347946))
    (pad "" smd roundrect (at 0.6375 0.6375 90) (size 1.084435 1.084435) (layers "F.Paste") (roundrect_rratio 0.2305347946))
    (pad "1" smd roundrect (at -3.4375 -2.6 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -3.4375 -2.2 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/LED") (pinfunction "GPIO0") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -3.4375 -1.8 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/IRIDIUM_RXD") (pinfunction "GPIO1") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -3.4375 -1.4 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/IRIDIUM_CTS") (pinfunction "GPIO2") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -3.4375 -1 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/IRIDIUM_RTS") (pinfunction "GPIO3") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -3.4375 -0.6 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/IRIDIUM_NETAV") (pinfunction "GPIO4") (pintype "bidirectional"))
    (pad "7" smd roundrect (at -3.4375 -0.2 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/IRIDIUM_RING") (pinfunction "GPIO5") (pintype "bidirectional"))
    (pad "8" smd roundrect (at -3.4375 0.2 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "unconnected-(U1-GPIO6-Pad8)") (pinfunction "GPIO6") (pintype "bidirectional+no_connect"))
    (pad "9" smd roundrect (at -3.4375 0.6 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "unconnected-(U1-GPIO7-Pad9)") (pinfunction "GPIO7") (pintype "bidirectional+no_connect"))
    (pad "10" smd roundrect (at -3.4375 1 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "11" smd roundrect (at -3.4375 1.4 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/DRF_TXEN") (pinfunction "GPIO8") (pintype "bidirectional"))
    (pad "12" smd roundrect (at -3.4375 1.8 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "/DRF_SW") (pinfunction "GPIO9") (pintype "bidirectional"))
    (pad "13" smd roundrect (at -3.4375 2.2 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "/DRF_DIO1") (pinfunction "GPIO10") (pintype "bidirectional"))
    (pad "14" smd roundrect (at -3.4375 2.6 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "/DRF_BUSY") (pinfunction "GPIO11") (pintype "bidirectional"))
    (pad "15" smd roundrect (at -2.6 3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/IRIDIUM_TXD") (pinfunction "GPIO12") (pintype "bidirectional"))
    (pad "16" smd roundrect (at -2.2 3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "/RDIO_RST") (pinfunction "GPIO13") (pintype "bidirectional"))
    (pad "17" smd roundrect (at -1.8 3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "unconnected-(U1-GPIO14-Pad17)") (pinfunction "GPIO14") (pintype "bidirectional+no_connect"))
    (pad "18" smd roundrect (at -1.4 3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "unconnected-(U1-GPIO15-Pad18)") (pinfunction "GPIO15") (pintype "bidirectional+no_connect"))
    (pad "19" smd roundrect (at -1 3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "TESTEN") (pintype "passive"))
    (pad "20" smd roundrect (at -0.6 3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(U1-XIN)") (pinfunction "XIN") (pintype "input"))
    (pad "21" smd roundrect (at -0.2 3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(U1-XOUT)") (pinfunction "XOUT") (pintype "passive"))
    (pad "22" smd roundrect (at 0.2 3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "23" smd roundrect (at 0.6 3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "+1V1") (pinfunction "DVDD") (pintype "power_in"))
    (pad "24" smd roundrect (at 1 3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "/RP_SWCLK") (pinfunction "SWCLK") (pintype "output"))
    (pad "25" smd roundrect (at 1.4 3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/RP_SWD") (pinfunction "SWD") (pintype "bidirectional"))
    (pad "26" smd roundrect (at 1.8 3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(U1-RUN)") (pinfunction "RUN") (pintype "input"))
    (pad "27" smd roundrect (at 2.2 3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "unconnected-(U1-GPIO16-Pad27)") (pinfunction "GPIO16") (pintype "bidirectional+no_connect"))
    (pad "28" smd roundrect (at 2.6 3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/TIMEPULSE") (pinfunction "GPIO17") (pintype "bidirectional"))
    (pad "29" smd roundrect (at 3.4375 2.6 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "/EXTINT") (pinfunction "GPIO18") (pintype "bidirectional"))
    (pad "30" smd roundrect (at 3.4375 2.2 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "unconnected-(U1-GPIO19-Pad30)") (pinfunction "GPIO19") (pintype "bidirectional+no_connect"))
    (pad "31" smd roundrect (at 3.4375 1.8 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "/SDA") (pinfunction "GPIO20") (pintype "bidirectional"))
    (pad "32" smd roundrect (at 3.4375 1.4 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "/SCL") (pinfunction "GPIO21") (pintype "bidirectional"))
    (pad "33" smd roundrect (at 3.4375 1 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "34" smd roundrect (at 3.4375 0.6 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "unconnected-(U1-GPIO22-Pad34)") (pinfunction "GPIO22") (pintype "bidirectional+no_connect"))
    (pad "35" smd roundrect (at 3.4375 0.2 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "unconnected-(U1-GPIO23-Pad35)") (pinfunction "GPIO23") (pintype "bidirectional+no_connect"))
    (pad "36" smd roundrect (at 3.4375 -0.2 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "/MISO") (pinfunction "GPIO24") (pintype "bidirectional"))
    (pad "37" smd roundrect (at 3.4375 -0.6 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "/DRF_CS") (pinfunction "GPIO25") (pintype "bidirectional"))
    (pad "38" smd roundrect (at 3.4375 -1 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "/SCK") (pinfunction "GPIO26_ADC0") (pintype "bidirectional"))
    (pad "39" smd roundrect (at 3.4375 -1.4 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "/MOSI") (pinfunction "GPIO27_ADC1") (pintype "bidirectional"))
    (pad "40" smd roundrect (at 3.4375 -1.8 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "unconnected-(U1-GPIO28_ADC2-Pad40)") (pinfunction "GPIO28_ADC2") (pintype "bidirectional+no_connect"))
    (pad "41" smd roundrect (at 3.4375 -2.2 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "/FRAM_CS") (pinfunction "GPIO29_ADC3") (pintype "bidirectional"))
    (pad "42" smd roundrect (at 3.4375 -2.6 90) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "43" smd roundrect (at 2.6 -3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pinfunction "ADC_AVDD") (pintype "power_in"))
    (pad "44" smd roundrect (at 2.2 -3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pinfunction "VREG_IN") (pintype "power_in"))
    (pad "45" smd roundrect (at 1.8 -3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "+1V1") (pinfunction "VREG_VOUT") (pintype "power_out"))
    (pad "46" smd roundrect (at 1.4 -3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(U1-USB_DM)") (pinfunction "USB_DM") (pintype "bidirectional"))
    (pad "47" smd roundrect (at 1 -3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(U1-USB_DP)") (pinfunction "USB_DP") (pintype "bidirectional"))
    (pad "48" smd roundrect (at 0.6 -3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pinfunction "USB_VDD") (pintype "power_in"))
    (pad "49" smd roundrect (at 0.2 -3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "50" smd roundrect (at -0.2 -3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "+1V1") (pinfunction "DVDD") (pintype "power_in"))
    (pad "51" smd roundrect (at -0.6 -3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/QSPI_SD3") (pinfunction "QSPI_SD3") (pintype "bidirectional"))
    (pad "52" smd roundrect (at -1 -3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/QSPI_SCLK") (pinfunction "QSPI_SCLK") (pintype "output"))
    (pad "53" smd roundrect (at -1.4 -3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/QSPI_SD0") (pinfunction "QSPI_SD0") (pintype "bidirectional"))
    (pad "54" smd roundrect (at -1.8 -3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/QSPI_SD2") (pinfunction "QSPI_SD2") (pintype "bidirectional"))
    (pad "55" smd roundrect (at -2.2 -3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/QSPI_SD1") (pinfunction "QSPI_SD1") (pintype "bidirectional"))
    (pad "56" smd roundrect (at -2.6 -3.4375 90) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "/QSPI_SS") (pinfunction "QSPI_SS") (pintype "bidirectional"))
    (pad "57" thru_hole circle (at -1.275 -1.275 90) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at -1.275 0 90) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at -1.275 1.275 90) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 0 -1.275 90) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 0 0 90) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "57" smd roundrect (at 0 0 90) (size 3.2 3.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.045)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 0 1.275 90) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 1.275 -1.275 90) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 1.275 0 90) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "57" thru_hole circle (at 1.275 1.275 90) (size 0.6 0.6) (drill 0.35) (layers "*.Cu")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 119.8 62.4 45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R29" (at 0 -1.43 45) (layer "F.SilkS") hide)
    (fp_text value "15k" (at 0 1.43 45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 45) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "VBUS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 45) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "Net-(U6-PR1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "BITSv5:SOT23-6L_STM" (layer "F.Cu")
    (at 117.3451 68.548102 180)
    (tags "USBLC6-2SC6 ")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "USBLC6-2SC6")
    (attr smd)
    (fp_text reference "U10" (at -0.0549 2.348102 unlocked) (layer "F.SilkS"))
    (fp_text value "USBLC6-2SC6" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -0.4953 -1.4478 180 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -0.4953 -1.4478 180) (layer "F.Fab"))
    (pad "1" smd rect (at -1.362451 -0.950001 180) (size 0.972299 0.558) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/USB_D+") (pinfunction "1") (pintype "unspecified"))
    (pad "2" smd rect (at -1.362451 0 180) (size 0.972299 0.558) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "2") (pintype "unspecified"))
    (pad "3" smd rect (at -1.362451 0.950001 180) (size 0.972299 0.558) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/USB_D-") (pinfunction "3") (pintype "unspecified"))
    (pad "4" smd rect (at 1.362451 0.950001 180) (size 0.972299 0.558) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "Net-(J2-D--PadA7)") (pinfunction "4") (pintype "unspecified"))
    (pad "5" smd rect (at 1.362451 0 180) (size 0.972299 0.558) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "VBUS") (pinfunction "5") (pintype "unspecified"))
    (pad "6" smd rect (at 1.362451 -0.950001 180) (size 0.972299 0.558) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(J2-D+-PadA6)") (pinfunction "6") (pintype "unspecified"))
  )
  (footprint "BITSv5:SEIKO_ML414H_IV01E" (layer "F.Cu")
    (at 143.55 64.6)
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single-cell battery")
    (property "ki_keywords" "battery cell")
    (attr smd)
    (fp_text reference "BT2" (at 0.636025 -4.706525) (layer "F.SilkS") hide)
    (fp_text value "3V" (at 12.19213 4.19105) (layer "F.Fab"))
    (fp_text user "+" (at 3.15 -2.4) (layer "F.SilkS"))
    (pad "1" smd custom (at 2.1 -2.1) (size 1 1) (layers "F.Cu")
      (net 21 "Net-(BT2-+)") (pinfunction "+") (pintype "passive") (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly
          (pts
            (xy -1.8 -0.6)
            (xy 0.6 -0.6)
            (xy 0.6 1.8)
          )
          (width 0.0001) (fill yes))
      ))
    (pad "2" smd rect (at 0.65 1.85) (size 4.1 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "-") (pintype "passive") (solder_mask_margin 0.102))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 143 45.9 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R24" (at 0.9 1.1 -90) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "/SCL") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 111.7 58 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C21" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "4.7uF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "+BATT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 135.5 67.0656 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.17 180) (layer "F.SilkS") hide)
    (fp_text value "1K" (at 0 1.17 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(C14-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(U1-XOUT)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_Pad" (layer "F.Cu")
    (at 108.3 84.1)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "M2" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 119.2 44.2 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R33" (at -2.4 -0.4 90) (layer "F.SilkS"))
    (fp_text value "43.2k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "Net-(U8-FB)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (at 128.8 56.9)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at 1.5 -1.5) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 63 "/RP_SWCLK") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 123.7 60.4 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R17" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "44.2K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(U6-ILM)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 118.7 56.4 135)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R26" (at 0 -1.43 135) (layer "F.SilkS") hide)
    (fp_text value "5k" (at 0 1.43 135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 135) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "Net-(U6-CP2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 135) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_USB:USB_C_Receptacle_GCT_USB4105-xx-A_16P_TopMnt_Horizontal" (layer "F.Cu")
    (at 109.7951 68.598102 -90)
    (descr "USB 2.0 Type C Receptacle, GCT, 16P, top mounted, horizontal, 5A: https://gct.co/files/drawings/usb4105.pdf")
    (tags "USB C Type-C Receptacle SMD USB 2.0 16P 16C USB4105-15-A USB4105-15-A-060 USB4105-15-A-120 USB4105-GF-A USB4105-GF-A-060 USB4105-GF-A-120")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "USB 2.0-only Type-C Receptacle connector")
    (property "ki_keywords" "usb universal serial bus type-C USB2.0")
    (attr smd)
    (fp_text reference "J2" (at 0 -5.5 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "USB_C_Receptacle_USB2.0" (at 0 5 -90 unlocked) (layer "F.Fab"))
    (fp_text user "PCB Edge" (at 0 3.1 -90 unlocked) (layer "Dwgs.User") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -2.89 -2.605 270) (size 0.65 0.65) (drill 0.65) (layers "F&B.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 2.89 -2.605 270) (size 0.65 0.65) (drill 0.65) (layers "F&B.Cu" "*.Mask"))
    (pad "A1" smd rect (at -3.2 -3.68 270) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "A4" smd rect (at -2.4 -3.68 270) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "A5" smd rect (at -1.25 -3.68 270) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "Net-(J2-CC1)") (pinfunction "CC1") (pintype "bidirectional"))
    (pad "A6" smd rect (at -0.25 -3.68 270) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(J2-D+-PadA6)") (pinfunction "D+") (pintype "bidirectional"))
    (pad "A7" smd rect (at 0.25 -3.68 270) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "Net-(J2-D--PadA7)") (pinfunction "D-") (pintype "bidirectional"))
    (pad "A8" smd rect (at 1.25 -3.68 270) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "unconnected-(J2-SBU1-PadA8)") (pinfunction "SBU1") (pintype "bidirectional+no_connect"))
    (pad "A9" smd rect (at 2.4 -3.68 270) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "A12" smd rect (at 3.2 -3.68 270) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B1" smd rect (at 3.2 -3.68 270) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B4" smd rect (at 2.4 -3.68 270) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "B5" smd rect (at 1.75 -3.68 270) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "Net-(J2-CC2)") (pinfunction "CC2") (pintype "bidirectional"))
    (pad "B6" smd rect (at 0.75 -3.68 270) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(J2-D+-PadA6)") (pinfunction "D+") (pintype "bidirectional"))
    (pad "B7" smd rect (at -0.75 -3.68 270) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "Net-(J2-D--PadA7)") (pinfunction "D-") (pintype "bidirectional"))
    (pad "B8" smd rect (at -1.75 -3.68 270) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "unconnected-(J2-SBU2-PadB8)") (pinfunction "SBU2") (pintype "bidirectional+no_connect"))
    (pad "B9" smd rect (at -2.4 -3.68 270) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "B12" smd rect (at -3.2 -3.68 270) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "S1" thru_hole oval (at -4.32 -3.105 270) (size 1 2.1) (drill oval 0.6 1.7) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at -4.32 1.075 270) (size 1 1.8) (drill oval 0.6 1.4) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 4.32 -3.105 270) (size 1 2.1) (drill oval 0.6 1.7) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 4.32 1.075 270) (size 1 1.8) (drill oval 0.6 1.4) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_GCT_USB4105-xx-A_16P_TopMnt_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 111.4 49 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R32" (at 2.3 -0.4 90) (layer "F.SilkS"))
    (fp_text value "25.5k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "Net-(U5-FB)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 113.3 61.5 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R15" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "332k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "+BATT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "Net-(SW3-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_AMASS:AMASS_XT30PW-M_1x02_P2.50mm_Horizontal" (layer "F.Cu")
    (at 108.3 51.4 90)
    (descr "Connector XT30 Horizontal PCB Male, https://www.tme.eu/en/Document/ce4077e36b79046da520ca73227e15de/XT30PW%20SPEC.pdf")
    (tags "RC Connector XT30")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at -2.5 -14.5 90) (layer "F.SilkS"))
    (fp_text value "XT30" (at -2.5 3.5 90) (layer "F.Fab"))
    (fp_text user "+" (at -7.2 -2.2 90) (layer "F.SilkS"))
    (fp_text user "-" (at 3 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -2.5 -3 90) (layer "F.Fab"))
    (pad "" thru_hole circle (at -8 -10 90) (size 1.4 1.4) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "" thru_hole circle (at 3 -10 90) (size 1.4 1.4) (drill 1) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0 90) (size 3.5 3.5) (drill 1.9) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -5 0 90) (size 3.5 3.5) (drill 1.9) (layers "*.Cu" "*.Mask")
      (net 9 "+BATT") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_AMASS.3dshapes/AMASS_XT30PW-M_1x02_P2.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 131.13 61.7556 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C9" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-3" (layer "F.Cu")
    (at 118.1 73.3)
    (descr "SOT, 3 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178D.PDF inferred 3-pin variant), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "N-MOSFET transistor, gate/source/drain")
    (property "ki_keywords" "transistor NMOS N-MOS N-MOSFET")
    (attr smd)
    (fp_text reference "Q1" (at 0 -2.4) (layer "F.SilkS") hide)
    (fp_text value "Q_NMOS_GSD" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/LED") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(D1-K)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 130.96 52.725)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C28" (at 0 -1.85) (layer "F.SilkS") hide)
    (fp_text value "15uF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 8 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 129.6 44.7 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C25" (at 1.9 0 180) (layer "F.SilkS"))
    (fp_text value "22uF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "Net-(U8-VOUT)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Keystone_5000-5004_Miniature" (layer "F.Cu")
    (at 113.4 44.6)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr through_hole)
    (fp_text reference "TP6" (at 1.5 -1.8) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 85 "/BATT_REG") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Keystone_5000-5004_Miniature.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 150.075 60.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C39" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "BITSv5:TPS2121" (layer "F.Cu")
    (at 122.4 57 -90)
    (tags "TPS2121RUXR ")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "TPS2121RUXR")
    (attr smd)
    (fp_text reference "U6" (at 0 0 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "TPS2121RUXR" (at 0 0 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.675 -0.324998 270) (size 1.05 0.399999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(C16-Pad1)") (pinfunction "OUT") (pintype "power_in"))
    (pad "2" smd rect (at -0.675 0.375001 270) (size 1.05 0.399999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "/BATT_REG") (pinfunction "IN2") (pintype "power_in"))
    (pad "3" smd rect (at -0.750001 1.15) (size 0.599999 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "Net-(U6-CP2)") (pinfunction "CP2") (pintype "input"))
    (pad "4" smd rect (at -0.25 1.15) (size 0.599999 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "Net-(U6-OV2)") (pinfunction "OV2") (pintype "input"))
    (pad "5" smd rect (at 0.25 1.15) (size 0.599999 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "Net-(U6-OV1)") (pinfunction "OV1") (pintype "input"))
    (pad "6" smd rect (at 0.750001 1.15) (size 0.599999 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "Net-(U6-PR1)") (pinfunction "PR1") (pintype "input"))
    (pad "7" smd rect (at 0.675 0.375001 270) (size 1.05 0.399999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "VBUS") (pinfunction "IN1") (pintype "power_in"))
    (pad "8" smd rect (at 0.675 -0.324998 270) (size 1.05 0.399999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(C16-Pad1)") (pinfunction "OUT") (pintype "power_in"))
    (pad "9" smd rect (at 0.750001 -1.149998) (size 0.599999 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "ST") (pintype "output"))
    (pad "10" smd rect (at 0.25 -1.149998) (size 0.599999 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "Net-(U6-ILM)") (pinfunction "ILM") (pintype "bidirectional"))
    (pad "11" smd rect (at -0.25 -1.149998) (size 0.599999 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "Net-(U6-SS)") (pinfunction "SS") (pintype "bidirectional"))
    (pad "12" smd rect (at -0.750001 -1.149998) (size 0.599999 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
  )
  (footprint "BPP_Lib:RDN0011A-MFG-NO-VIA" (layer "F.Cu")
    (at 125.987501 45.1125 90)
    (tags "TPSM33625FRDNR ")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U8" (at -2.9875 2.312499 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "TPSM33625FRDNR" (at 0 4 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6 90 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -1.4 -1.962 90) (size 1.2 0.475) (layers "F.Cu")
      (net 99 "unconnected-(U8-PGOOD-Pad1)") (pinfunction "PGOOD") (pintype "open_collector+no_connect"))
    (pad "2" smd rect (at -1.4 -1.15 90) (size 1.2 0.349999) (layers "F.Cu")
      (net 18 "+5V") (pinfunction "EN") (pintype "input"))
    (pad "3" smd rect (at -1.4 -0.650001 90) (size 1.2 0.349999) (layers "F.Cu")
      (net 18 "+5V") (pinfunction "VIN") (pintype "power_in"))
    (pad "4" smd rect (at -1.2 1.000001 90) (size 1.599999 2.150001) (layers "F.Cu")
      (net 87 "Net-(U8-VOUT)") (pinfunction "VOUT") (pintype "power_out"))
    (pad "5" smd rect (at 1.2 1.000001 90) (size 1.599999 2.150001) (layers "F.Cu")
      (net 100 "unconnected-(U8-SW-Pad5)") (pinfunction "SW") (pintype "no_connect"))
    (pad "6" smd rect (at 1.4 -0.650001 90) (size 1.2 0.349999) (layers "F.Cu")
      (net 101 "unconnected-(U8-SW-Pad6)") (pinfunction "SW") (pintype "no_connect"))
    (pad "7" smd rect (at 1.4 -1.15 90) (size 1.2 0.349999) (layers "F.Cu")
      (net 102 "unconnected-(U8-BOOT-Pad7)") (pinfunction "BOOT") (pintype "no_connect"))
    (pad "8" smd rect (at 1.4 -1.962 90) (size 1.2 0.475) (layers "F.Cu")
      (net 86 "Net-(U8-VCC)") (pinfunction "VCC") (pintype "power_out"))
    (pad "9" smd rect (at 0.499999 -2.049998 90) (size 0.349999 0.900001) (layers "F.Cu")
      (net 91 "Net-(U8-FB)") (pinfunction "FB") (pintype "input"))
    (pad "10" smd rect (at 0 -1.75 90) (size 0.3 1.5) (layers "F.Cu")
      (net 4 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "10" thru_hole circle (at 0 -0.23 90) (size 0.499999 0.499999) (drill 0.2032) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "10" thru_hole circle (at 0 0.770001 90) (size 0.499999 0.499999) (drill 0.2032) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "10" thru_hole circle (at 0 1.769999 90) (size 0.499999 0.499999) (drill 0.2032) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "11" smd rect (at -0.499999 -2.049998 90) (size 0.349999 0.900001) (layers "F.Cu")
      (net 4 "GND") (pinfunction "MODE") (pintype "unspecified"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 135.97 68.5056 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C13" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "10pF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(U1-XIN)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 126 59.4)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C33" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(U6-SS)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 118.4 61.5 45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R23" (at 0 -1.43 45) (layer "F.SilkS") hide)
    (fp_text value "0" (at 0 1.43 45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 45) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(U6-OV1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 45) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_LGA:LGA-8_3x5mm_P1.25mm" (layer "F.Cu")
    (at 145.175 71.525 90)
    (descr "LGA-8")
    (tags "lga land grid array")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Barometric pressure sensor, 20cm resolution, 10 to 1200 mbar, I2C and SPI interface up to 20MHz, LGA-8")
    (property "ki_keywords" "pressure SPI I2C")
    (attr smd)
    (fp_text reference "U11" (at 0 -3.65 90) (layer "F.SilkS") hide)
    (fp_text value "MS5607-02BA" (at 0 3.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.075 -1.875 90) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "+3V3") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect (at -1.075 -0.625 90) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "+3V3") (pinfunction "PS") (pintype "input"))
    (pad "3" smd rect (at -1.075 0.625 90) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd rect (at -1.075 1.875 90) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "CSB") (pintype "input"))
    (pad "5" smd rect (at 1.075 1.875 90) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "CSB") (pintype "input"))
    (pad "6" smd rect (at 1.075 0.625 90) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "unconnected-(U11-SDO-Pad6)") (pinfunction "SDO") (pintype "output+no_connect"))
    (pad "7" smd rect (at 1.075 -0.625 90) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "/SDA") (pinfunction "SDI/SDA") (pintype "bidirectional"))
    (pad "8" smd rect (at 1.075 -1.875 90) (size 0.95 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "/SCL") (pinfunction "SCLK") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_LGA.3dshapes/LGA-8_3x5mm_P1.25mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 121.8 43.3 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C24" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "Net-(U8-VCC)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 147.3 65.2 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R14" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "3.3K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(D2-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(BT2-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 131.3 71.9456 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C10" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_Pad" (layer "F.Cu")
    (at 108.3 45.3)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "M2" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 129.31 48.275 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "100m" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "Net-(U8-VOUT)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 125.5 55.6)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C16" (at 0.8 1.5 90) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(C16-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_Push_1P1T_NO_CK_KMR2" (layer "F.Cu")
    (at 137.7 72.6)
    (descr "CK components KMR2 tactile switch http://www.ckswitches.com/media/1479/kmr2.pdf")
    (tags "tactile switch kmr2")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr smd)
    (fp_text reference "B1" (at -3.2 1.6 90) (layer "F.SilkS"))
    (fp_text value "KMR2" (at 0 2.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.45) (layer "F.Fab"))
    (pad "1" smd rect (at -2.05 -0.8) (size 0.9 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect (at 2.05 -0.8) (size 0.9 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at -2.05 0.8) (size 0.9 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(U1-RUN)") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect (at 2.05 0.8) (size 0.9 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(U1-RUN)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T_NO_CK_KMR2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 122.675 68.025 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C6" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "BITSv5:CAS-120TB_NDC-M" (layer "F.Cu")
    (at 133.275 80.125 180)
    (tags "CAS-120TB ")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Switch, single pole double throw")
    (property "ki_keywords" "switch single-pole double-throw spdt ON-ON")
    (attr smd)
    (fp_text reference "SW2" (at 0 0 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "~" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -1.750002 1.9423 180) (size 0.8112 1.406398) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "unconnected-(SW2-A-Pad1)") (pinfunction "A") (pintype "passive+no_connect"))
    (pad "2" smd rect (at 1.750002 1.9423 180) (size 0.8112 1.406398) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "Net-(SW2-B)") (pinfunction "B") (pintype "passive"))
    (pad "3" smd rect (at 0 -1.9423 180) (size 0.8112 1.406398) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "C") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 118.8 50.9 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C18" (at 0 -1.5 90) (layer "F.SilkS"))
    (fp_text value "47uF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 85 "/BATT_REG") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 124.825 48.9)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C38" (at 0 -1.85) (layer "F.SilkS") hide)
    (fp_text value "15uF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 18 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 137.43 64.6156)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.16) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "+1V1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 121.725 68.0156 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C12" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_SMD_2520-4Pin_2.5x2.0mm" (layer "F.Cu")
    (at 138.02 68.8306 -90)
    (descr "SMD Crystal SERIES SMD2520/4 http://www.newxtal.com/UploadFiles/Images/2012-11-12-09-29-09-776.pdf, 2.5x2.0mm^2 package")
    (tags "SMD SMT crystal")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Four pin crystal, GND on pins 2 and 4, small symbol")
    (property "ki_keywords" "quartz ceramic resonator oscillator")
    (attr smd)
    (fp_text reference "Y1" (at 0 -2.2 90) (layer "F.SilkS") hide)
    (fp_text value "12MHz" (at 0 2.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.875 0.7 270) (size 1.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(C14-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 0.875 0.7 270) (size 1.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 0.875 -0.7 270) (size 1.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(U1-XIN)") (pinfunction "3") (pintype "passive"))
    (pad "4" smd rect (at -0.875 -0.7 270) (size 1.15 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_2520-4Pin_2.5x2.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 143.7 75 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C29" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 114.9 61.5 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R16" (at 0 -1.43 -90) (layer "F.SilkS") hide)
    (fp_text value "100k" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(SW3-C)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 141.5 72.8 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R11" (at 1.3 -1 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(U1-RUN)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 122.4 46.2 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C23" (at -2.3 -0.3 270) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (at 132.3 56.8)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP2" (at 0 2) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 64 "/RP_SWD") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 120.8 45.6 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R20" (at -1.9 0 180) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "Net-(U8-VOUT)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "Net-(U8-FB)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "BITSv5:TVS1800" (layer "F.Cu")
    (at 108.7 59.8)
    (tags "TVS1800DRVR ")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "TVS1800DRVR")
    (attr smd)
    (fp_text reference "U9" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (fp_text value "TVS1800DRVR" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.974999 -0.650001 90) (size 0.299999 0.449999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "2" smd rect (at -0.974999 0 90) (size 0.299999 0.449999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "3" smd rect (at -0.974999 0.649999 90) (size 0.299999 0.449999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "4" smd rect (at 0.974999 0.649999 90) (size 0.299999 0.449999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "+BATT") (pinfunction "IN") (pintype "unspecified"))
    (pad "5" smd rect (at 0.974999 0 90) (size 0.299999 0.449999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "+BATT") (pinfunction "IN") (pintype "unspecified"))
    (pad "6" smd rect (at 0.974999 -0.650001 90) (size 0.299999 0.449999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "+BATT") (pinfunction "IN") (pintype "unspecified"))
    (pad "7" smd rect (at 0 0) (size 1 1.599999) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "PAD") (pintype "unspecified"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 137.43 65.5956)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C11" (at 0 -1.16) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 149.9 71.425 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Conn_01x03_Pin" (at 0 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(J1-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_1210_3225Metric" (layer "F.Cu")
    (at 125.5 52.5 -90)
    (descr "Inductor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Inductor, small symbol")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr smd)
    (fp_text reference "L4" (at 0 -2.28 -270) (layer "F.SilkS") hide)
    (fp_text value "3.3uH" (at 0 2.28 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4 0 270) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 18 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0 270) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 20 "Net-(C16-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 119.4 54.9 -45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R25" (at 0.290736 -1.139264 -45) (layer "F.SilkS"))
    (fp_text value "10.2k" (at 0 1.43 -45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 315) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "/BATT_REG") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 315) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "Net-(U6-CP2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 141.8 68.8)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R6" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "DNF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "/SCL") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 116.2 63.7 45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R22" (at 0 -1.43 45) (layer "F.SilkS") hide)
    (fp_text value "DNF" (at 0 1.43 45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 45) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "VBUS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 45) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(U6-OV1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 124.19 62.8156 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.16) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 124.19 65.8356)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.17) (layer "F.SilkS") hide)
    (fp_text value "27" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/USB_D+") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(U1-USB_DP)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 137.43 66.5956)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C14" (at 0 -1.16) (layer "F.SilkS") hide)
    (fp_text value "10pF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(C14-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 141.202389 75.827529 -25)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C30" (at 0.795282 1.474521 -115) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.43 155) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 155) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 335) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 335) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 131.425 76.125 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "1K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(SW2-B)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "/QSPI_SS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 122.2 62.6 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C15" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "VBUS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "BPP_Lib:RDN0011A-MFG-NO-VIA" (layer "F.Cu")
    (at 114.187501 52.8 90)
    (tags "TPSM33625FRDNR ")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U5" (at -1.6 -3.087501 90 unlocked) (layer "F.SilkS"))
    (fp_text value "TPSM33625FRDNR" (at 0 4 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6 90 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -1.4 -1.962 90) (size 1.2 0.475) (layers "F.Cu")
      (net 95 "unconnected-(U5-PGOOD-Pad1)") (pinfunction "PGOOD") (pintype "open_collector+no_connect"))
    (pad "2" smd rect (at -1.4 -1.15 90) (size 1.2 0.349999) (layers "F.Cu")
      (net 90 "Net-(SW3-B)") (pinfunction "EN") (pintype "input"))
    (pad "3" smd rect (at -1.4 -0.650001 90) (size 1.2 0.349999) (layers "F.Cu")
      (net 9 "+BATT") (pinfunction "VIN") (pintype "power_in"))
    (pad "4" smd rect (at -1.2 1.000001 90) (size 1.599999 2.150001) (layers "F.Cu")
      (net 85 "/BATT_REG") (pinfunction "VOUT") (pintype "power_out"))
    (pad "5" smd rect (at 1.2 1.000001 90) (size 1.599999 2.150001) (layers "F.Cu")
      (net 96 "unconnected-(U5-SW-Pad5)") (pinfunction "SW") (pintype "no_connect"))
    (pad "6" smd rect (at 1.4 -0.650001 90) (size 1.2 0.349999) (layers "F.Cu")
      (net 97 "unconnected-(U5-SW-Pad6)") (pinfunction "SW") (pintype "no_connect"))
    (pad "7" smd rect (at 1.4 -1.15 90) (size 1.2 0.349999) (layers "F.Cu")
      (net 98 "unconnected-(U5-BOOT-Pad7)") (pinfunction "BOOT") (pintype "no_connect"))
    (pad "8" smd rect (at 1.4 -1.962 90) (size 1.2 0.475) (layers "F.Cu")
      (net 24 "Net-(U5-VCC)") (pinfunction "VCC") (pintype "power_out"))
    (pad "9" smd rect (at 0.499999 -2.049998 90) (size 0.349999 0.900001) (layers "F.Cu")
      (net 94 "Net-(U5-FB)") (pinfunction "FB") (pintype "input"))
    (pad "10" smd rect (at 0 -1.75 90) (size 0.3 1.5) (layers "F.Cu")
      (net 4 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "10" thru_hole circle (at 0 -0.23 90) (size 0.499999 0.499999) (drill 0.2032) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "10" thru_hole circle (at 0 0.770001 90) (size 0.499999 0.499999) (drill 0.2032) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "10" thru_hole circle (at 0 1.769999 90) (size 0.499999 0.499999) (drill 0.2032) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "11" smd rect (at -0.499999 -2.049998 90) (size 0.349999 0.900001) (layers "F.Cu")
      (net 4 "GND") (pinfunction "MODE") (pintype "unspecified"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 126.98 71.9956 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 113 48.2 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R31" (at -1.1 -1.2 -90) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "/BATT_REG") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "Net-(U5-FB)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 144.6 45.9 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R21" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "/SDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 117.2 60.4 -135)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R28" (at 0 -1.43 -135) (layer "F.SilkS") hide)
    (fp_text value "0" (at 0 1.43 -135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 225) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(U6-OV2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 225) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 115.9175 76.79 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R12" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "470" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(D1-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 124.05 68.1256 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C4" (at 0 -1.16) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "+1V1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 124.19 64.8356)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.17) (layer "F.SilkS") hide)
    (fp_text value "27" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/USB_D-") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(U1-USB_DM)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 126.69 61.6956 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C32" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Molex:Molex_PicoBlade_53261-1071_1x10-1MP_P1.25mm_Horizontal" (layer "F.Cu")
    (at 122.43 83.9)
    (descr "Molex PicoBlade series connector, 53261-1071 (http://www.molex.com/pdm_docs/sd/532610271_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex PicoBlade top entry")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x10, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J4" (at 0 -4.4) (layer "F.SilkS"))
    (fp_text value "PicoBlade_53261-1071" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd roundrect (at -5.625 -2.4) (size 0.8 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/IRIDIUM_RXD") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at -4.375 -2.4) (size 0.8 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/IRIDIUM_CTS") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at -3.125 -2.4) (size 0.8 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/IRIDIUM_RTS") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at -1.875 -2.4) (size 0.8 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/IRIDIUM_NETAV") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd roundrect (at -0.625 -2.4) (size 0.8 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/IRIDIUM_RING") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd roundrect (at 0.625 -2.4) (size 0.8 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/IRIDIUM_TXD") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd roundrect (at 1.875 -2.4) (size 0.8 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "unconnected-(J4-Pin_7-Pad7)") (pinfunction "Pin_7") (pintype "passive+no_connect"))
    (pad "8" smd roundrect (at 3.125 -2.4) (size 0.8 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "+5V") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd roundrect (at 4.375 -2.4) (size 0.8 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "unconnected-(J4-Pin_9-Pad9)") (pinfunction "Pin_9") (pintype "passive+no_connect"))
    (pad "10" smd roundrect (at 5.625 -2.4) (size 0.8 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "Pin_10") (pintype "passive"))
    (pad "MP" smd roundrect (at -8.175 0.5) (size 2.1 3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1190480952))
    (pad "MP" smd roundrect (at 8.175 0.5) (size 2.1 3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1190480952))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_PicoBlade_53261-1071_1x10-1MP_P1.25mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (at 118.3675 75.95 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D1" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 120.8 51 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C34" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "/BATT_REG") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 123.1 53.3 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R13" (at 0 -1.43 -270) (layer "F.SilkS") hide)
    (fp_text value "100m" (at 0 1.43 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(C16-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 146.475 60.5 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C40" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(BT2-+)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 118.3 58.2 -45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R27" (at 0 -1.43 -45) (layer "F.SilkS") hide)
    (fp_text value "DNF" (at 0 1.43 -45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 315) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "/BATT_REG") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 315) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(U6-OV2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "BPP_Lib:BalloonArt" (layer "F.Cu")
    (at 145.1 84)
    (attr board_only exclude_from_bom)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "BalloonArt" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 119.035 71.035 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.16) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_Pad" (layer "F.Cu")
    (at 149.1 84.1)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "M2" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "TestPoint:TestPoint_Keystone_5000-5004_Miniature" (layer "F.Cu")
    (at 116.8 46.4)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr through_hole)
    (fp_text reference "TP4" (at 0 -2) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "+5V") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Keystone_5000-5004_Miniature.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 117.6 64.5 -135)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R30" (at 0 -1.43 -135) (layer "F.SilkS") hide)
    (fp_text value "47.5k" (at 0 1.43 -135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 225) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "Net-(U6-PR1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 225) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 131.7 44.7 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C31" (at -1.2 1.4 90) (layer "F.SilkS"))
    (fp_text value "22uF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "Net-(U8-VOUT)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_1210_3225Metric" (layer "F.Cu")
    (at 131.685 49.125 90)
    (descr "Inductor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Inductor, small symbol")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr smd)
    (fp_text reference "L3" (at 0 -2.28 90) (layer "F.SilkS") hide)
    (fp_text value "3.3uH" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4 0 90) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 8 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0 90) (size 1.25 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 87 "Net-(U8-VOUT)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123F" (layer "F.Cu")
    (at 149.5 62.5)
    (descr "D_SOD-123F")
    (tags "D_SOD-123F")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Schottky diode, small symbol")
    (property "ki_keywords" "diode Schottky")
    (attr smd)
    (fp_text reference "D2" (at -0.127 -1.905) (layer "F.SilkS") hide)
    (fp_text value "0.5A/40V/240mV" (at 0 2.1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.127 -1.905) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4 0) (size 1.1 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
      (net 41 "Net-(D2-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0) (size 1.1 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
      (net 8 "+3V3") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123F.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 113.5 57.2 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C19" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "+BATT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:U.FL_Molex_MCRF_73412-0110_Vertical" (layer "F.Cu")
    (at 149.1 44.95)
    (descr "Molex Microcoaxial RF Connectors (MCRF), mates Hirose U.FL, (http://www.molex.com/pdm_docs/sd/734120110_sd.pdf)")
    (tags "mcrf hirose ufl u.fl microcoaxial")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr smd)
    (fp_text reference "J5" (at 0 0.05) (layer "F.SilkS"))
    (fp_text value "U.FL" (at 0 -3.302) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.5) (layer "F.Fab"))
    (pad "1" smd rect (at 0 1.5) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "Net-(J5-In)") (pinfunction "In") (pintype "passive"))
    (pad "2" smd rect (at -1.475 0) (size 1.05 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 -1.5) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 1.475 0) (size 1.05 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/U.FL_Molex_MCRF_73412-0110_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 107.3 62.4)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "5.1K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(J2-CC2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 125.66 61.6956 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C8" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "BPP_Lib:BGA8CP30X40_5X3_309X228X35B25N" (layer "F.Cu")
    (at 138.1 76.4)
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "FRAM memory with SPI interface, SOIC-8 SON-8")
    (property "ki_keywords" "FRAM SPI 3.3V")
    (attr smd)
    (fp_text reference "U7" (at 0.6 2.2) (layer "F.SilkS"))
    (fp_text value "MB85RS1MT" (at 10.706375 2.096414) (layer "F.Fab"))
    (pad "A1" smd circle (at -0.4 -0.6) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "A3" smd circle (at 0.4 -0.6) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "/MOSI") (pinfunction "SI") (pintype "input") (solder_mask_margin 0.102))
    (pad "B2" smd circle (at 0 -0.3) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "unconnected-(U7-~{WP}-PadB2)") (pinfunction "~{WP}") (pintype "input+no_connect") (solder_mask_margin 0.102))
    (pad "C1" smd circle (at -0.4 0) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "/MISO") (pinfunction "SO") (pintype "output") (solder_mask_margin 0.102))
    (pad "C3" smd circle (at 0.4 0) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "/SCK") (pinfunction "SCK") (pintype "input") (solder_mask_margin 0.102))
    (pad "D2" smd circle (at 0 0.3) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "unconnected-(U7-~{HOLD}-PadD2)") (pinfunction "~{HOLD}") (pintype "input+no_connect") (solder_mask_margin 0.102))
    (pad "E1" smd circle (at -0.4 0.6) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/FRAM_CS") (pinfunction "~{CS}") (pintype "input") (solder_mask_margin 0.102))
    (pad "E3" smd circle (at 0.4 0.6) (size 0.2 0.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "+3V3") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.102))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 110.7 62.4 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R7" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "5.1K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(J2-CC1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 118.3575 77.59 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "DNF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "/QSPI_SS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "BITSv5:WSON_128JVPIQ_WIN" (layer "F.Cu")
    (at 123.085 72.7008 90)
    (tags "W25Q128JVPIQ ")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "128Mb Serial Flash Memory, Standard/Dual/Quad SPI, SOIC-8")
    (property "ki_keywords" "flash memory SPI QPI DTR")
    (attr smd)
    (fp_text reference "U2" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "W25Q128JVS" (at 0 0 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -2.8702 -1.905 90) (size 0.9652 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/QSPI_SS") (pinfunction "~{CS}") (pintype "input"))
    (pad "2" smd rect (at -2.8702 -0.635 90) (size 0.9652 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/QSPI_SD1") (pinfunction "DO(IO1)") (pintype "bidirectional"))
    (pad "3" smd rect (at -2.8702 0.635 90) (size 0.9652 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/QSPI_SD2") (pinfunction "IO2") (pintype "bidirectional"))
    (pad "4" smd rect (at -2.8702 1.905 90) (size 0.9652 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd rect (at 2.8702 1.905 90) (size 0.9652 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/QSPI_SD0") (pinfunction "DI(IO0)") (pintype "bidirectional"))
    (pad "6" smd rect (at 2.8702 0.635 90) (size 0.9652 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/QSPI_SCLK") (pinfunction "CLK") (pintype "input"))
    (pad "7" smd rect (at 2.8702 -0.635 90) (size 0.9652 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/QSPI_SD3") (pinfunction "IO3") (pintype "bidirectional"))
    (pad "8" smd rect (at 2.8702 -1.905 90) (size 0.9652 0.4318) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (pad "9" smd rect (at 0 0 90) (size 3.4544 4.3434) (layers "F.Cu" "F.Paste" "F.Mask"))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 115.5 57.4 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C20" (at 0 -1.85 90) (layer "F.SilkS") hide)
    (fp_text value "47uF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 85 "/BATT_REG") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "RF_GPS:ublox_MAX" (layer "F.Cu")
    (at 146.3 53.55 90)
    (descr "ublox MAX 6/7/8, (https://www.u-blox.com/sites/default/files/MAX-8-M8-FW3_HardwareIntegrationManual_%28UBX-15030059%29.pdf)")
    (tags "GPS ublox MAX 6/7/8")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "GNSS Module MAX M10, VCC 1.65V to 3.6V")
    (property "ki_keywords" "ublox GPS GNSS module")
    (attr smd)
    (fp_text reference "U3" (at 0 -6 90) (layer "F.SilkS") hide)
    (fp_text value "MAX-M10S" (at 0 1.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -4.75 -4.4 90) (size 1.8 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect (at -4.75 -3.3 90) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(J1-Pin_1)") (pinfunction "TXD") (pintype "output"))
    (pad "3" smd roundrect (at -4.75 -2.2 90) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(J1-Pin_2)") (pinfunction "RXD") (pintype "input"))
    (pad "4" smd roundrect (at -4.75 -1.1 90) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/TIMEPULSE") (pinfunction "TIMEPULSE") (pintype "output"))
    (pad "5" smd roundrect (at -4.75 0 90) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "/EXTINT") (pinfunction "EXTINT") (pintype "input"))
    (pad "6" smd roundrect (at -4.75 1.1 90) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(BT2-+)") (pinfunction "V_BCKP") (pintype "power_in"))
    (pad "7" smd roundrect (at -4.75 2.2 90) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pinfunction "VCC_IO") (pintype "power_in"))
    (pad "8" smd roundrect (at -4.75 3.3 90) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (pad "9" smd roundrect (at -4.75 4.4 90) (size 1.8 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "unconnected-(U3-~{RESET}-Pad9)") (pinfunction "~{RESET}") (pintype "input+no_connect"))
    (pad "10" smd roundrect (at 4.75 4.4 90) (size 1.8 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "11" smd roundrect (at 4.75 3.3 90) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "Net-(J5-In)") (pinfunction "RF_IN") (pintype "input"))
    (pad "12" smd roundrect (at 4.75 2.2 90) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "13" smd roundrect (at 4.75 1.1 90) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "unconnected-(U3-LNA_EN-Pad13)") (pinfunction "LNA_EN") (pintype "output+no_connect"))
    (pad "14" smd roundrect (at 4.75 0 90) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "unconnected-(U3-VCC_RF-Pad14)") (pinfunction "VCC_RF") (pintype "power_out+no_connect"))
    (pad "15" smd roundrect (at 4.75 -1.1 90) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "unconnected-(U3-VIO_SEL-Pad15)") (pinfunction "VIO_SEL") (pintype "input+no_connect"))
    (pad "16" smd roundrect (at 4.75 -2.2 90) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "17" smd roundrect (at 4.75 -3.3 90) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "18" smd roundrect (at 4.75 -4.4 90) (size 1.8 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "unconnected-(U3-~{SAFEBOOT}-Pad18)") (pinfunction "~{SAFEBOOT}") (pintype "input+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/RF_GPS.3dshapes/ublox_MAX.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Keystone_5000-5004_Miniature" (layer "F.Cu")
    (at 135.1 49.9)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr through_hole)
    (fp_text reference "TP5" (at 0.1 2.1) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "+3V3") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Keystone_5000-5004_Miniature.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "B.Cu")
    (at 118.85 50.4)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, open")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP1" (at 0 1.8) (layer "B.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 -1.9) (layer "B.Fab"))
    (pad "1" smd custom (at -0.65 0) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 88 "Net-(JP1-A)") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.5 -0.75)
            (xy 0 -0.75)
            (xy 0 0.75)
            (xy 0.5 0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 18 "+5V") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 -0.75)
            (xy -0.5 -0.75)
            (xy -0.5 0.75)
            (xy 0 0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 114.625 57.025 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C26" (at 0 1.43 90) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 88 "Net-(JP1-A)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "BITSv5:DRF1262TL" (layer "B.Cu")
    (at 127.6 67.2)
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U4" (at 0 17 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "DRF1262TL" (at 0 -16 180 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -17.5 180 unlocked) (layer "B.Fab"))
    (pad "1" smd roundrect (at -9.5 3.145) (size 3 1.29) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "/DRF_SW") (pinfunction "SW") (pintype "input") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at -9.5 0.6) (size 3 1.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "unspecified") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at -9.5 -1.94) (size 3 1.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 61 "/DRF_TXEN") (pinfunction "TXEN") (pintype "input") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at -9.5 -4.48) (size 3 1.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "unspecified") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at -9.5 -7.02) (size 3 1.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "unspecified") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at -9.5 -9.56) (size 3 1.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 88 "Net-(JP1-A)") (pinfunction "VDD") (pintype "power_in") (thermal_bridge_angle 45))
    (pad "7" smd roundrect (at -9.5 -12.1) (size 3 1.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 88 "Net-(JP1-A)") (pinfunction "VDD") (pintype "power_in") (thermal_bridge_angle 45))
    (pad "8" smd roundrect (at 9.5 -12.1) (size 3 1.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 62 "/DRF_DIO1") (pinfunction "DIO1") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "9" smd roundrect (at 9.5 -9.56) (size 3 1.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 65 "/DRF_BUSY") (pinfunction "BUSY") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "10" smd roundrect (at 9.5 -7.02) (size 3 1.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 50 "/RDIO_RST") (pinfunction "RST") (pintype "input") (thermal_bridge_angle 45))
    (pad "11" smd roundrect (at 9.5 -4.48) (size 3 1.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 52 "/MISO") (pinfunction "MISO") (pintype "output") (thermal_bridge_angle 45))
    (pad "12" smd roundrect (at 9.5 -1.94) (size 3 1.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 69 "/MOSI") (pinfunction "MOSI") (pintype "input") (thermal_bridge_angle 45))
    (pad "13" smd roundrect (at 9.5 0.6) (size 3 1.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 67 "/SCK") (pinfunction "SCK") (pintype "input") (thermal_bridge_angle 45))
    (pad "14" smd roundrect (at 9.5 3.145) (size 3 1.29) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 68 "/DRF_CS") (pinfunction "NSS") (pintype "input") (thermal_bridge_angle 45))
    (pad "15" smd roundrect (at 8.67 13.75 270) (size 3.5 1.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "unspecified") (thermal_bridge_angle 45))
    (pad "16" smd roundrect (at 6.13 13.75 270) (size 3.5 1.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(J6-In)") (pinfunction "ANT") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "17" smd roundrect (at 3.59 13.75 270) (size 3.5 1.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "unspecified") (thermal_bridge_angle 45))
  )
  (footprint "Connector_Coaxial:U.FL_Molex_MCRF_73412-0110_Vertical" (layer "B.Cu")
    (at 143.2 84 90)
    (descr "Molex Microcoaxial RF Connectors (MCRF), mates Hirose U.FL, (http://www.molex.com/pdm_docs/sd/734120110_sd.pdf)")
    (tags "mcrf hirose ufl u.fl microcoaxial")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr smd)
    (fp_text reference "J6" (at 0 -3.5 90) (layer "B.SilkS"))
    (fp_text value "U.FL" (at 0 3.302 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -3.5 90) (layer "B.Fab"))
    (pad "1" smd rect (at 0 -1.5 90) (size 1 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "Net-(J6-In)") (pinfunction "In") (pintype "passive"))
    (pad "2" smd rect (at -1.475 0 90) (size 1.05 2.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 1.5 90) (size 1 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 1.475 0 90) (size 1.05 2.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/U.FL_Molex_MCRF_73412-0110_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 113.1 57.025 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "BITSv5.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C27" (at 0 1.43 90) (layer "B.SilkS") hide)
    (fp_text value "1uF" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 88 "Net-(JP1-A)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 150.7 42.2) (mid 151.76066 42.63934) (end 152.2 43.7)
    (layer "Edge.Cuts"))
  (gr_line (start 107 42.2) (end 150.7 42.2)
    (layer "Edge.Cuts"))
  (gr_line (start 105.2 84.2) (end 105.2 44)
    (layer "Edge.Cuts"))
  (gr_arc (start 152.2 84.2) (mid 151.32132 86.32132) (end 149.2 87.2)
    (layer "Edge.Cuts"))
  (gr_line (start 152.2 84.2) (end 152.2 43.7)
    (layer "Edge.Cuts"))
  (gr_line (start 149.2 87.2) (end 108.2 87.2)
    (layer "Edge.Cuts"))
  (gr_arc (start 108.2 87.2) (mid 106.07868 86.32132) (end 105.2 84.2)
    (layer "Edge.Cuts"))
  (gr_arc (start 105.2 44) (mid 105.727208 42.727208) (end 107 42.2)
    (layer "Edge.Cuts"))
  (gr_text "BITSv5.2\n02/2024" (at 139.8 42.9 180) (layer "F.SilkS"))
  (gr_text "JLCJLCJLCJLC" (at 138.7 58.3 90) (layer "F.SilkS"))
  (gr_text "ON" (at 106.4 81.3) (layer "F.SilkS"))
  (gr_text "J. Bishop\nM. Shipman" (at 139.8 45.9 180) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 105.2 54.5) (xy 152.2 54.5))
    (height 0)
    (gr_text "47.0000 mm" (at 128.7 53.35) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 149.225 50.2) (xy 152.2 50.2))
    (height 0)
    (gr_text "2.9750 mm" (at 156.8 49.05) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 148.3 45.2) (xy 148.3 42.2))
    (height 0)
    (gr_text "3.0000 mm" (at 146.5 43.7 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 149.225 45.2) (xy 149.225 84.2))
    (height 0)
    (gr_text "39.0000 mm" (at 148.075 64.7 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 149.225 84.2) (xy 152.2 84.2))
    (height 0)
    (gr_text "2.9750 mm" (at 155.1 83.05) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 128.1 42.2) (xy 128.1 87.2))
    (height -7.6)
    (gr_text "45.0000 mm" (at 134.55 64.7 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 149.225 84.2) (xy 149.225 87.2))
    (height 0)
    (gr_text "3.0000 mm" (at 148.075 90.6 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 108.225 84.2) (xy 149.225 84.2))
    (height 0)
    (gr_text "41.0000 mm" (at 128.725 83.05) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 108.2 84.2) (xy 105.2 84.2))
    (height 0)
    (gr_text "3.0000 mm" (at 102.8 83.05) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 108.2 84.2) (xy 108.2 87.2))
    (height 0)
    (gr_text "3.0000 mm" (at 107.05 89.5 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.2")
    (pts (xy 149.225 45.2) (xy 149.225 84.2))
    (height 41.025)
    (gr_text "39.0000 mm" (at 107.05 64.7 90) (layer "User.2"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "GND") (hatch edge 0.5)
    (priority 5)
    (connect_pads yes (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 131.7 51.7)
        (xy 134.2 51.7)
        (xy 134.2 53.9)
        (xy 131.7 53.9)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (name "GND") (hatch edge 0.5)
    (priority 6)
    (connect_pads yes (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 1.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 125.8 47.7)
        (xy 126.9 47.7)
        (xy 127.8 48.6)
        (xy 127.8 50.2)
        (xy 127.1 50.2)
        (xy 126.9 50)
        (xy 125.8 50)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads yes (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 109.2 60.6)
        (xy 109.2 59)
        (xy 106.6 59)
        (xy 106.6 60.6)
      )
    )
  )
  (zone (net 87) (net_name "Net-(U8-VOUT)") (layer "F.Cu") (hatch edge 0.5)
    (priority 3)
    (connect_pads (clearance 0.127))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.1) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 132.7 48.5)
        (xy 132.7 44.7)
        (xy 126.6 44.7)
        (xy 125.8 45.5)
        (xy 125.8 46.5)
        (xy 127.8 48.5)
      )
    )
  )
  (zone (net 85) (net_name "/BATT_REG") (layer "F.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.127))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.1) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 116.9 56)
        (xy 116.9 56.9)
        (xy 114 56.9)
        (xy 114 53.1)
        (xy 116.2 53.1)
        (xy 116.8 52.5)
        (xy 116.8 51.3)
        (xy 122.3 51.3)
        (xy 122.3 57)
        (xy 121.7 57)
        (xy 121.7 56)
        (xy 120.8 55)
        (xy 117.9 55)
      )
    )
  )
  (zone (net 9) (net_name "+BATT") (layer "F.Cu") (name "BATT") (hatch edge 0.5)
    (connect_pads (clearance 0.127))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 113.9 53.4)
        (xy 105.2 53.4)
        (xy 105.2 56.8)
        (xy 109.3 60.9)
        (xy 110.1 60.9)
        (xy 113.9 57.1)
      )
    )
  )
  (zone (net 8) (net_name "+3V3") (layer "F.Cu") (hatch edge 0.5)
    (priority 7)
    (connect_pads yes (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 128.79 48.7)
        (xy 128.79 53.91)
        (xy 131.8 53.91)
        (xy 131.8 51.35)
        (xy 133 51.35)
        (xy 133 48.7)
        (xy 132.99 48.69)
        (xy 128.79 48.69)
      )
    )
  )
  (zone (net 20) (net_name "Net-(C16-Pad1)") (layer "F.Cu") (name "VCC") (hatch edge 0.5)
    (priority 2)
    (connect_pads (clearance 0.127))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.1) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 122.4 58.3)
        (xy 122.4 53.1)
        (xy 126.9 53.1)
        (xy 126.9 54.7)
        (xy 125.9 55.7)
        (xy 123.6 55.7)
        (xy 123.1 56.2)
        (xy 123.1 58.3)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (priority 8)
    (connect_pads yes (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 118.485 68.673102)
        (xy 118.16 68.998102)
        (xy 118.16 69.248102)
        (xy 117.56 69.248102)
        (xy 117.56 67.473102)
        (xy 118.16 67.473102)
        (xy 118.16 68.098102)
        (xy 118.485 68.423102)
      )
    )
  )
  (zone (net 25) (net_name "VBUS") (layer "F.Cu") (hatch edge 0.5)
    (priority 8)
    (connect_pads yes (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 115.46 68.95)
        (xy 116.6451 68.998102)
        (xy 116.6451 69.648102)
        (xy 117.3351 69.648102)
        (xy 117.3351 67.473102)
        (xy 116.6451 67.473102)
        (xy 116.6451 68.098102)
        (xy 115.46 68.15)
      )
    )
  )
  (zone (net 0) (net_name "") (layers "F.Cu" "In1.Cu") (name "SW_KEEPOUT") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.2) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias allowed) (pads allowed) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.25) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 124.6 44.5)
        (xy 124.6 42.4)
        (xy 128.4 42.4)
        (xy 128.4 44.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layers "F.Cu" "In1.Cu") (name "SW_KEEPOUT") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.2) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias allowed) (pads allowed) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.25) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 112.8 52.2)
        (xy 112.8 50.1)
        (xy 116.6 50.1)
        (xy 116.6 52.2)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layers "F.Cu" "In1.Cu" "In2.Cu" "B.Cu") (name "GND") (hatch edge 0.5)
    (priority 7)
    (connect_pads (clearance 0.127))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.1) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 140 42.2)
        (xy 140 64.2)
        (xy 152.2 64.2)
        (xy 152.2 42.2)
      )
    )
  )
  (zone (net 18) (net_name "+5V") (layers "F.Cu" "In2.Cu") (hatch edge 0.5)
    (priority 7)
    (connect_pads yes (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 122.615 52.905)
        (xy 122.615 47.695)
        (xy 125.625 47.695)
        (xy 125.625 50.255)
        (xy 126.825 50.255)
        (xy 126.825 52.905)
        (xy 126.815 52.915)
        (xy 122.615 52.915)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layers "F.Cu" "In2.Cu" "B.Cu") (hatch edge 0.5)
    (priority 15)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 129.46 87.37)
        (xy 152.318164 87.37)
        (xy 152.299847 75.4)
        (xy 133.969328 75.4)
        (xy 129.46 79.857326)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "In1.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads yes (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 152.475 41.6)
        (xy 104.275 41.6)
        (xy 104.275 88.025)
        (xy 152.475 88.025)
      )
    )
  )
  (zone (net 8) (net_name "+3V3") (layer "In2.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads yes (clearance 0))
    (min_thickness 1) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 147.5 79.1)
        (xy 147.5 63.3)
        (xy 137.9 63.3)
        (xy 137.9 47.8)
        (xy 122.810051 47.8)
        (xy 122.828906 79.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "In2.Cu") (hatch edge 0.5)
    (connect_pads yes (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 114.0701 71.423102)
        (xy 115.4201 71.423102)
        (xy 115.4201 65.673102)
        (xy 114.0701 65.673102)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "In2.Cu") (name "GND") (hatch edge 0.5)
    (connect_pads yes (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 1.5))
    (polygon
      (pts
        (xy 104.1 41.4)
        (xy 152.6 41.4)
        (xy 152.6 88.1)
        (xy 151.5 89.2)
        (xy 104.1 89.2)
      )
    )
  )
  (zone (net 88) (net_name "Net-(JP1-A)") (layer "B.Cu") (hatch edge 0.5)
    (priority 4)
    (connect_pads (clearance 0.127))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.1) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 119.3 49.1)
        (xy 119.3 59.3)
        (xy 115.5 59.3)
        (xy 115.5 50.6)
        (xy 117 49.1)
      )
    )
  )
  (zone (net 18) (net_name "+5V") (layer "B.Cu") (name "+5V") (hatch edge 0.5)
    (connect_pads (clearance 0.127))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.1) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 119.2 47.7)
        (xy 119.2 53.1)
        (xy 126.9 53.1)
        (xy 126.9 47.7)
      )
    )
  )
)
