(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "Boaretube Voltage Board")
    (date "10/11/2022")
    (rev "v01")
    (company "NHMFL")
    (comment 1 "Sujana Uppalapati")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "unconnected-(J1-Pad2)")
  (net 3 "unconnected-(J2-Pad2)")
  (net 4 "Net-(J2-Pad3)")
  (footprint "ap_Pad_Hole:125_Hole_Iso" (layer "F.Cu")
    (tedit 5F1621FD)
    (at 109.474 61.722)
    (property "Sheetfile" "BoreTube Voltage Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Pad2" (at 0.635 3.81) (layer "F.SilkS") hide)
    (fp_text value "125_hole_iso" (at 0.635 5.715) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (solder_mask_margin 4.445) (clearance 4.445))
  )
  (footprint "ap_PCB_Misc:Maglab_Logo" (layer "F.Cu")
    (tedit 5F3FD4DC)
    (at 157.575 62.135)
    (property "Sheetfile" "BoreTube Voltage Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "11" (at 2.0574 3.13436) (layer "F.SilkS") hide)
    (fp_text value "MAGLAB_LOGO_1_2" (at 2.62382 1.36652) (layer "F.Fab") hide)
    (fp_text user "AGLAB" (at 11.176 -1.5875) (layer "F.SilkS"))
    (fp_text user "NATIONAL" (at 9.144 -4.2545) (layer "F.SilkS"))
  )
  (footprint "ap_Pad_Hole:125_Hole_Iso" (layer "F.Cu")
    (tedit 5F1621FD)
    (at 199.39 61.722)
    (property "Sheetfile" "BoreTube Voltage Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Pad3" (at 0.635 3.81) (layer "F.SilkS") hide)
    (fp_text value "125_hole_iso" (at 0.635 5.715) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (solder_mask_margin 4.445) (clearance 4.445))
  )
  (footprint "ap_Pad_Hole:125_Hole_Iso" (layer "F.Cu")
    (tedit 5F1621FD)
    (at 109.474 96.52)
    (property "Sheetfile" "BoreTube Voltage Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Pad4" (at 0.635 3.81) (layer "F.SilkS") hide)
    (fp_text value "125_hole_iso" (at 0.635 5.715) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (solder_mask_margin 4.445) (clearance 4.445))
  )
  (footprint "KiCAD Library_SU:Wire wound resistor #NH05020R00FC02" (layer "F.Cu")
    (tedit 0)
    (at 124.826293 78.74)
    (property "Sheetfile" "BoreTube Voltage Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1 (Non Inductive)" (at 28.843707 -10.16 unlocked) (layer "F.SilkS"))
    (fp_text value "20 ohm" (at 30 17.5 unlocked) (layer "F.Fab") hide)
    (pad "" thru_hole circle (at 52.7939 -10.7188) (size 5.08 5.08) (drill 3.175) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 12.7635 10.7188) (size 5.08 5.08) (drill 3.175) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0) (size 5.08 5.08) (drill 1.4986) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 65.5574 0) (size 5.08 5.08) (drill 1.4986) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad3)") (pinfunction "2") (pintype "passive"))
  )
  (footprint "ap_Pad_Hole:125_Hole_Iso" (layer "F.Cu")
    (tedit 5F1621FD)
    (at 199.39 96.52)
    (property "Sheetfile" "BoreTube Voltage Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Pad1" (at 0.635 3.81) (layer "F.SilkS") hide)
    (fp_text value "125_hole_iso" (at 0.635 5.715) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (solder_mask_margin 4.445) (clearance 4.445))
  )
  (footprint "ap_Connector_Phoenix:MCV_3Pin_1803439" (layer "F.Cu")
    (tedit 5F3AFEB9)
    (at 199 81.62 90)
    (property "Sheetfile" "BoreTube Voltage Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -3.85 3.8 90) (layer "F.SilkS"))
    (fp_text value "MCV_3Pin_1803439" (at 3.81 6.35 90) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(J1-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole roundrect (at 3.81 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 3 "unconnected-(J2-Pad2)") (pinfunction "2") (pintype "passive+no_connect"))
    (pad "3" thru_hole roundrect (at 7.62 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J2-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_Phoenix_MC.3dshapes/MCV_3Pin_1803439.stp"
      (offset (xyz 7.62 3.048 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (footprint "ap_Connector_Phoenix:MCV_2Pin_1803426" (layer "F.Cu")
    (tedit 5F105FAF)
    (at 111.25 77.05 -90)
    (property "Sheetfile" "BoreTube Voltage Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -3.849994 3.850012 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "MCV_2Pin_1803426" (at 1.905 5.715 90) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect locked (at 0 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(J1-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole roundrect locked (at 3.81 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 "unconnected-(J1-Pad2)") (pinfunction "2") (pintype "passive+no_connect"))
  )
  (gr_rect (start 101.6 53.34) (end 208.28 104.14) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "To Boretube 'POGO' Pin" (at 104.648 78.74 270) (layer "F.SilkS"))
  (gr_text "To 5B Module" (at 205.232 77.47 -270) (layer "F.SilkS"))
  (gr_text "Boretube Voltage Board (v01)\nS Uppalapati 2022" (at 140.97 59.69) (layer "F.SilkS"))
  (gr_text "1" (at 204.216 83.82 90) (layer "F.SilkS"))
  (gr_text "1" (at 106.045 74.93 -90) (layer "F.SilkS"))
)
