<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<text>RX</text>
<text>TX</text>
<text>3V3</text>
<wire x1="0" y1="1.36783125" x2="0" y2="21.636971875" width="0.1524" layer="20"/>
<wire x1="0" y1="21.636971875" x2="1.350028125" y2="22.987" width="0.1524" layer="20" curve="-90"/>
<wire x1="1.350028125" y1="22.987" x2="48.5818375" y2="22.987" width="0.1524" layer="20"/>
<wire x1="48.5818375" y1="22.987" x2="49.9745" y2="21.5943375" width="0.1524" layer="20" curve="-90"/>
<wire x1="49.9745" y1="21.5943375" x2="49.9745" y2="1.302909375" width="0.1524" layer="20"/>
<wire x1="49.9745" y1="1.302909375" x2="48.671590625" y2="0" width="0.1524" layer="20" curve="-90"/>
<wire x1="48.671590625" y1="0" x2="1.36783125" y2="0" width="0.1524" layer="20"/>
<wire x1="1.36783125" y1="0" x2="0" y2="1.36783125" width="0.1524" layer="20" curve="-90"/>
<text>RX</text>
<text>TX</text>
<text>A3</text>
<text>A4</text>
<text>SDA</text>
<text>SCL</text>
<text>GND</text>
<text>D0</text>
<text>RX1</text>
<text>TX1</text>
<text>RX2</text>
<text>TX2</text>
<text>D9</text>
<text>D10</text>
<text>SCK</text>
<text>NSS</text>
<text>MISO</text>
<text>MOSI</text>
<text>GND</text>
<text>RST</text>
<text>CLK</text>
<text>DIO</text>
<text>3V3</text>
<text>Reset</text>
<text>-</text>
<text>Boot</text>
<text>LoRa-E5 Mini V1.0</text>
<text>-</text>
<text>U1</text>
<text>GND</text>
<text>3V3</text>
<text>RST</text>
<text>CLK</text>
<text>DIO</text>
<text>GND</text>
<text>JTAG</text>
<text>3V3</text>
<text>A4</text>
<text>D9</text>
<text>D10</text>
<text>SCK</text>
<text>NSS</text>
<text>MISO</text>
<text>MOSI</text>
<text>GND</text>
<text>RST</text>
<text>CLK</text>
<text>DIO</text>
<text>3V3</text>
<text>RX</text>
<text>TX</text>
<text>A3</text>
<text>SDA</text>
<text>SCL</text>
<text>GND</text>
<text>D0</text>
<text>RX1</text>
<text>TX1</text>
<text>RX2</text>
<text>TX2</text>
<text>3V3</text>
<text>3V3</text>
<text>RST</text>
<text>CLK</text>
<text>DIO</text>
<text>GND</text>
<text>RX</text>
<text>TX</text>
<text>3V3</text>
<text>GND</text>
<text>LoRa</text>
<text>E5</text>
<text>V1.0</text>
</plain>
<libraries>
<library name="Discrete-new">
<packages>
<package name="C0805">
<description>&lt;b&gt;0805&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="LED-0805">
</package>
<package name="R0603">
</package>
<package name="R0805">
</package>
</packages>
</library>
<library name="Connector-new">
<packages>
<package name="U-FL3P-SMD-2.6X2.6X1.0MM">
</package>
<package name="SMA5P-SMD-5.1-6.5X6.5X16.5MM">
</package>
<package name="H2X12-2.54-23MM">
</package>
</packages>
</library>
<library name="moudle-new">
<packages>
<package name="MOUDLE28P-1.25-12X12X2.5MM">
</package>
</packages>
</library>
<library name="Switch">
<packages>
<package name="SW4P-SMD-4.5X3.2X2.5MM">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06-SMD_RA_MALE">
<description>&lt;h3&gt;SMD - 6 Pin Right Angle Male Header&lt;/h3&gt;
tDocu layer shows pin locations.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X05_LOCK">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin with Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="_c2h">
<packages>
<package name="LOGO_C2I_015">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="moudle-new" package="MOUDLE28P-1.25-12X12X2.5MM" value="LoRa-E5-HF"/>
<element name="K2" library="Switch" package="SW4P-SMD-4.5X3.2X2.5MM" value="BUTTOM">
<attribute name="NAME"/>
</element>
<element name="K1" library="Switch" package="SW4P-SMD-4.5X3.2X2.5MM" value="BUTTOM">
<attribute name="NAME"/>
</element>
<element name="ANT2" library="Connector-new" package="U-FL3P-SMD-2.6X2.6X1.0MM" value="U-FL Connector">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="D2" library="Discrete-new" package="LED-0805" value="RED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="Discrete-new" package="C0805" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="ANT1" library="Connector-new" package="SMA5P-SMD-5.1-6.5X6.5X16.5MM" value="DIP SMA-K">
<attribute name="NAME"/>
</element>
<element name="C1" library="Discrete-new" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="Discrete-new" package="C0805" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="JH" library="Connector-new" package="H2X12-2.54-23MM" value="HEADER-2X12P-W23MM">
<attribute name="NAME"/>
</element>
<element name="RS" library="Discrete-new" package="R0603" value="0R">
<attribute name="NAME"/>
</element>
<element name="RU" library="Discrete-new" package="R0603" value="DNP">
<attribute name="NAME"/>
</element>
<element name="R3" library="Discrete-new" package="R0805" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="Discrete-new" package="R0805" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="Discrete-new" package="R0805" value="4K7">
<attribute name="NAME"/>
</element>
<element name="R5" library="Discrete-new" package="R0805" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X06-SMD_RA_MALE" value="FTDI">
<attribute name="PROD_ID" value="CONN-08971"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X05_LOCK" value="JTAG"/>
<element name="D1" library="Discrete-new" package="LED-0805" value="GREEN">
<attribute name="VALUE"/>
</element>
<element name="R1" library="Discrete-new" package="R0805" value="1K">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="_c2h" package="LOGO_C2I_015" value=""/>
<element name="U$2" library="_c2h" package="LOGO_C2I_015" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="14"/>
<contactref element="U1" pad="22"/>
<contactref element="U1" pad="16"/>
<contactref element="K2" pad="4"/>
<contactref element="K2" pad="3"/>
<contactref element="ANT2" pad="GND1"/>
<contactref element="ANT2" pad="GND2"/>
<contactref element="C3" pad="1"/>
<contactref element="ANT1" pad="GND4"/>
<contactref element="ANT1" pad="GND3"/>
<contactref element="ANT1" pad="GND2"/>
<contactref element="ANT1" pad="GND1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="JH" pad="C12"/>
<contactref element="JH" pad="D12"/>
<contactref element="JH" pad="E24"/>
<contactref element="JH" pad="F24"/>
<contactref element="JH" pad="E6"/>
<contactref element="JH" pad="F6"/>
<contactref element="JH" pad="B6"/>
<contactref element="JH" pad="A6"/>
<contactref element="R3" pad="2"/>
<contactref element="J1" pad="6"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="PA13/SWDIO">
<contactref element="U1" pad="3"/>
<contactref element="JH" pad="A3"/>
<contactref element="JH" pad="B3"/>
<contactref element="JH" pad="E3"/>
<contactref element="JH" pad="F3"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="PC0/RX1">
<contactref element="U1" pad="13"/>
<contactref element="JH" pad="C4"/>
<contactref element="JH" pad="F16"/>
<contactref element="JH" pad="D4"/>
<contactref element="JH" pad="E16"/>
</signal>
<signal name="PC1/TX1">
<contactref element="U1" pad="12"/>
<contactref element="JH" pad="D3"/>
<contactref element="JH" pad="C3"/>
<contactref element="JH" pad="F15"/>
<contactref element="JH" pad="E15"/>
</signal>
<signal name="PB5/LED">
<contactref element="U1" pad="11"/>
<contactref element="D2" pad="-"/>
</signal>
<signal name="RF">
<contactref element="U1" pad="15"/>
<contactref element="RS" pad="1"/>
<contactref element="RU" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="D2" pad="+"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="PA9/D9">
<contactref element="U1" pad="21"/>
<contactref element="JH" pad="F12"/>
<contactref element="JH" pad="E12"/>
<contactref element="JH" pad="B12"/>
<contactref element="JH" pad="A12"/>
</signal>
<signal name="N$29">
<contactref element="K1" pad="4"/>
<contactref element="K1" pad="3"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="ANT2" pad="D"/>
<contactref element="RU" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="ANT1" pad="ANT"/>
<contactref element="RS" pad="2"/>
</signal>
<signal name="PA15/SDA">
<contactref element="U1" pad="6"/>
<contactref element="R4" pad="2"/>
<contactref element="JH" pad="D9"/>
<contactref element="JH" pad="F21"/>
<contactref element="JH" pad="C9"/>
<contactref element="JH" pad="E21"/>
</signal>
<signal name="PB15/SCL">
<contactref element="U1" pad="5"/>
<contactref element="R5" pad="2"/>
<contactref element="JH" pad="C10"/>
<contactref element="JH" pad="E22"/>
<contactref element="JH" pad="F22"/>
<contactref element="JH" pad="D10"/>
</signal>
<signal name="RST">
<contactref element="U1" pad="17"/>
<contactref element="K2" pad="2"/>
<contactref element="K2" pad="1"/>
<contactref element="JH" pad="F5"/>
<contactref element="JH" pad="A5"/>
<contactref element="JH" pad="B5"/>
<contactref element="JH" pad="E5"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="PA10/MOSI">
<contactref element="U1" pad="27"/>
<contactref element="JH" pad="A7"/>
<contactref element="JH" pad="F7"/>
<contactref element="JH" pad="E7"/>
<contactref element="JH" pad="B7"/>
</signal>
<signal name="PB14/MISO">
<contactref element="U1" pad="26"/>
<contactref element="JH" pad="A8"/>
<contactref element="JH" pad="F8"/>
<contactref element="JH" pad="B8"/>
<contactref element="JH" pad="E8"/>
</signal>
<signal name="PB9/NSS">
<contactref element="U1" pad="25"/>
<contactref element="JH" pad="A9"/>
<contactref element="JH" pad="F9"/>
<contactref element="JH" pad="E9"/>
<contactref element="JH" pad="B9"/>
</signal>
<signal name="PA3/RX2">
<contactref element="U1" pad="18"/>
<contactref element="JH" pad="F14"/>
<contactref element="JH" pad="E14"/>
<contactref element="JH" pad="C2"/>
<contactref element="JH" pad="D2"/>
</signal>
<signal name="PA2/TX2">
<contactref element="U1" pad="19"/>
<contactref element="JH" pad="E13"/>
<contactref element="JH" pad="C1"/>
<contactref element="JH" pad="F13"/>
<contactref element="JH" pad="D1"/>
</signal>
<signal name="PB7/RX">
<contactref element="U1" pad="9"/>
<contactref element="JH" pad="F19"/>
<contactref element="JH" pad="D7"/>
<contactref element="JH" pad="C7"/>
<contactref element="JH" pad="E19"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="PB6/TX">
<contactref element="U1" pad="10"/>
<contactref element="JH" pad="F18"/>
<contactref element="JH" pad="C6"/>
<contactref element="JH" pad="E18"/>
<contactref element="JH" pad="D6"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="PB13/BOOT/SCK">
<contactref element="U1" pad="24"/>
<contactref element="K1" pad="1"/>
<contactref element="K1" pad="2"/>
<contactref element="JH" pad="B10"/>
<contactref element="JH" pad="A10"/>
<contactref element="JH" pad="E10"/>
<contactref element="JH" pad="F10"/>
</signal>
<signal name="PA14/SWCLK">
<contactref element="U1" pad="4"/>
<contactref element="JH" pad="B4"/>
<contactref element="JH" pad="A4"/>
<contactref element="JH" pad="E4"/>
<contactref element="JH" pad="F4"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="VDD_TCXO">
<contactref element="U1" pad="28"/>
</signal>
<signal name="3V3">
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="J3" pad="5"/>
<contactref element="J1" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="JH" pad="D11"/>
<contactref element="JH" pad="C11"/>
<contactref element="JH" pad="E23"/>
<contactref element="JH" pad="F23"/>
<contactref element="JH" pad="E1"/>
<contactref element="JH" pad="B1"/>
<contactref element="JH" pad="A1"/>
<contactref element="JH" pad="F1"/>
</signal>
<signal name="PB3/A3">
<contactref element="U1" pad="8"/>
<contactref element="JH" pad="F20"/>
<contactref element="JH" pad="C8"/>
<contactref element="JH" pad="E20"/>
<contactref element="JH" pad="D8"/>
</signal>
<signal name="PB4/A4">
<contactref element="U1" pad="7"/>
<contactref element="JH" pad="A2"/>
<contactref element="JH" pad="E2"/>
<contactref element="JH" pad="F2"/>
<contactref element="JH" pad="B2"/>
</signal>
<signal name="PA0/D0">
<contactref element="U1" pad="23"/>
<contactref element="JH" pad="F17"/>
<contactref element="JH" pad="D5"/>
<contactref element="JH" pad="E17"/>
<contactref element="JH" pad="C5"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
<contactref element="D1" pad="+"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="PB10/LED">
<contactref element="D1" pad="-"/>
<contactref element="U1" pad="20"/>
<contactref element="JH" pad="F11"/>
<contactref element="JH" pad="B11"/>
<contactref element="JH" pad="E11"/>
<contactref element="JH" pad="A11"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
