(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "MKR Shield")
		(date "2018-07-31")
		(rev "0.1")
		(company "Electronic Cats")
	)
	(layers
		(0 "F.Cu" signal "Top")
		(2 "B.Cu" signal "Bottom")
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "output")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "/A2")
	(net 3 "/CS")
	(net 4 "/D4")
	(net 5 "/A3")
	(net 6 "/AREF")
	(net 7 "/D2")
	(net 8 "/D3")
	(net 9 "/A1")
	(net 10 "/D5")
	(net 11 "/INT")
	(net 12 "/D0")
	(net 13 "/AN")
	(net 14 "/D1")
	(net 15 "/PWM")
	(net 16 "+5V")
	(net 17 "/MISO")
	(net 18 "/SCK")
	(net 19 "/SCL")
	(net 20 "/MOSI")
	(net 21 "/D7")
	(net 22 "/SDA")
	(net 23 "/D6")
	(net 24 "/RX")
	(net 25 "/VIN")
	(net 26 "+3V3")
	(net 27 "/TX")
	(net 28 "/RST")
	(footprint "custom:PinHeader_1x14_P2.54mm_Staggered"
		(layer "F.Cu")
		(at 129.54 97.79)
		(descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row, staggered")
		(tags "Through hole pin header THT 1x14 2.54mm single row staggered")
		(property "Reference" "J1"
			(at 0 -2.38 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x14"
			(at 0 35.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x14, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ziggybridge-mkr.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 16.51 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -0.254 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/AREF")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0.254 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/AN")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -0.254 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/A1")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0.254 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/A2")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -0.254 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/A3")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0.254 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/CS")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at -0.254 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/INT")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 0.254 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/PWM")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at -0.254 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/D0")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 0.254 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/D1")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at -0.254 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/D2")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 0.254 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/D3")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at -0.254 30.48)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/D4")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 0.254 33.02)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/D5")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x14_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "custom:PinHeader_1x14_P2.54mm_Staggered"
		(layer "F.Cu")
		(at 149.86 130.81 180)
		(descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row, staggered")
		(tags "Through hole pin header THT 1x14 2.54mm single row staggered")
		(property "Reference" "J2"
			(at 0 -2.38 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x14"
			(at 0 35.4 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x14, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ziggybridge-mkr.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 16.51 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -0.254 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/D6")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0.254 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/D7")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -0.254 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/MOSI")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0.254 7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/SCK")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -0.254 10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/MISO")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0.254 12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/SDA")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at -0.254 15.24 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/SCL")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 0.254 17.78 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/RX")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at -0.254 20.32 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/TX")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 0.254 22.86 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/RST")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at -0.254 25.4 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 0.254 27.94 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "+3V3")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at -0.254 30.48 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/VIN")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 0.254 33.02 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "+5V")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x14_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Symbol:KiCad-Logo2_6mm_SilkScreen"
		(locked yes)
		(layer "F.Cu")
		(at 139.065 92.075)
		(descr "KiCad Logo")
		(tags "Logo KiCad")
		(property "Reference" "REF**"
			(at 0 -5.08 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "KiCad-Logo2_6mm_SilkScreen"
			(at 0 6.35 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_missing_courtyard)
		(embedded_fonts no)
	)
	(footprint "custom:PinHeader_1x06_P2.54mm_Staggered"
		(layer "F.Cu")
		(at 173.99 96.52)
		(descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x14 2.54mm single row")
		(property "Reference" "J10"
			(at 0 -2.38 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x06"
			(at 0 15.24 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ziggybridge-mkr.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 16.51 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -0.254 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/RX")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0.254 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/TX")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -0.254 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0.254 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/SDA")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -0.254 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0.254 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "+3V3")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_SH_SM03B-SRSS-TB_1x03-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 179.07 97.79 90)
		(descr "JST SH series connector, SM03B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH horizontal")
		(property "Reference" "J5"
			(at 3.81 -0.635 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03"
			(at 0 3.98 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ziggybridge-mkr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "/TX")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "/RX")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.3 1.875 90)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
		)
		(pad "MP" smd roundrect
			(at 2.3 1.875 90)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM03B-SRSS-TB_1x03-1MP_P1.00mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "custom:mikrobus_logo"
		(locked yes)
		(layer "F.Cu")
		(at 160.02 102.87 -90)
		(property "Reference" "G***"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "custom:PinHeader_1x08_P2.54mm_Staggered"
		(layer "F.Cu")
		(at 176.53 91.44 -90)
		(descr "Through hole straight pin header, 1x8, 2.54mm pitch, single row, staggered")
		(tags "Through hole pin header THT 1x8 2.54mm single row staggered")
		(property "Reference" "J11"
			(at 0 -3.175 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x08"
			(at 0 20.32 270)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ziggybridge-mkr.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 16.51 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -0.254 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/AN")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0.254 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/RST")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -0.254 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/CS")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0.254 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/SCK")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -0.254 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/MISO")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0.254 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/MOSI")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at -0.254 15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "+3V3")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 0.254 17.78 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "custom:PinHeader_1x06_P2.54mm_Staggered"
		(layer "F.Cu")
		(at 173.99 119.38)
		(descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x14 2.54mm single row")
		(property "Reference" "J8"
			(at 0 -2.38 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x06"
			(at 0 15.24 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ziggybridge-mkr.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 16.51 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -0.254 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/D4")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0.254 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/D5")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -0.254 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/D6")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0.254 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/D7")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -0.254 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0.254 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "+3V3")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "custom:PinHeader_1x06_P2.54mm_Staggered"
		(layer "F.Cu")
		(at 171.45 119.38)
		(descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x14 2.54mm single row")
		(property "Reference" "J7"
			(at 0 -2.38 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x06"
			(at 0 15.24 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ziggybridge-mkr.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 16.51 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -0.254 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/D0")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0.254 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/D1")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -0.254 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/D2")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0.254 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/D3")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -0.254 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0.254 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "+3V3")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "custom:PinHeader_1x08_P2.54mm_Staggered"
		(layer "F.Cu")
		(at 176.53 114.3 -90)
		(descr "Through hole straight pin header, 1x8, 2.54mm pitch, single row, staggered")
		(tags "Through hole pin header THT 1x8 2.54mm single row staggered")
		(property "Reference" "J12"
			(at 0 -3.175 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x08"
			(at 0 20.32 270)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ziggybridge-mkr.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 16.51 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -0.254 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/PWM")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0.254 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/INT")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -0.254 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/RX")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0.254 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/TX")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -0.254 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/SCL")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0.254 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/SDA")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at -0.254 15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "+5V")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 0.254 17.78 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "custom:PinHeader_1x06_P2.54mm_Staggered"
		(layer "F.Cu")
		(at 171.45 96.52)
		(descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x14 2.54mm single row")
		(property "Reference" "J9"
			(at 0 -2.38 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x06"
			(at 0 15.24 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ziggybridge-mkr.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 16.51 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -0.254 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/CS")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0.254 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/MOSI")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -0.254 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/MISO")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0.254 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/SCK")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -0.254 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0.254 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "+3V3")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 179.07 107.315 90)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH horizontal")
		(property "Reference" "J6"
			(at 4.445 -0.535 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 0 3.98 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ziggybridge-mkr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "+3V3")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "/SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/SCL")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875 90)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875 90)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "custom:gs_logo_200mil"
		(locked yes)
		(layer "F.Cu")
		(at 139.7 114.3)
		(property "Reference" "GS1"
			(at 0 -3.175 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GS_logo"
			(at 0 -0.5 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at 0 0)
			(size 5.08 5.08)
			(layers "F.Cu")
			(zone_connect 0)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives)
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 129.54 88.9)
		(end 179.705 88.9)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 129.54 134.62)
		(mid 127.743949 133.876051)
		(end 127 132.08)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.705 134.62)
		(end 129.54 134.62)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 127 91.44)
		(mid 127.743949 89.643949)
		(end 129.54 88.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127 132.08)
		(end 127 91.44)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 182.245 91.44)
		(end 182.245 132.08)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 179.705 88.9)
		(mid 181.501051 89.643949)
		(end 182.245 91.44)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 182.245 132.08)
		(mid 181.501051 133.876051)
		(end 179.705 134.62)
		(layer "Edge.Cuts")
	)
	(gr_text "MOSI"
		(at 147.955 125.73 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 169.545 106.68 0)
		(layer "F.SilkS")
	)
	(gr_text "D0"
		(at 131.445 118.11 0)
		(layer "F.SilkS")
	)
	(gr_text "D1"
		(at 131.445 120.65 0)
		(layer "F.SilkS")
	)
	(gr_text "RST"
		(at 147.955 107.95 0)
		(layer "F.SilkS")
	)
	(gr_text "+3V3"
		(at 147.955 102.87 0)
		(layer "F.SilkS")
	)
	(gr_text "PWM"
		(at 131.445 115.57 0)
		(layer "F.SilkS")
	)
	(gr_text "AREF"
		(at 131.445 97.79 0)
		(layer "F.SilkS")
	)
	(gr_text "D7"
		(at 177.165 127 0)
		(layer "F.SilkS")
	)
	(gr_text "D2"
		(at 131.445 123.19 0)
		(layer "F.SilkS")
	)
	(gr_text "+5V"
		(at 147.955 97.79 0)
		(layer "F.SilkS")
	)
	(gr_text "D2"
		(at 168.275 124.46 0)
		(layer "F.SilkS")
	)
	(gr_text "A2"
		(at 131.445 105.41 0)
		(layer "F.SilkS")
	)
	(gr_text "MISO"
		(at 147.955 120.65 0)
		(layer "F.SilkS")
	)
	(gr_text "SCK"
		(at 169.545 104.14 0)
		(layer "F.SilkS")
	)
	(gr_text "SCL"
		(at 147.955 115.57 0)
		(layer "F.SilkS")
	)
	(gr_text "CS"
		(at 169.545 96.52 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 168.275 129.54 0)
		(layer "F.SilkS")
	)
	(gr_text "D6"
		(at 177.165 124.46 0)
		(layer "F.SilkS")
	)
	(gr_text "VIN"
		(at 147.955 100.33 0)
		(layer "F.SilkS")
	)
	(gr_text "PMOD"
		(at 180.34 125.73 -90)
		(layer "F.SilkS")
	)
	(gr_text "D0"
		(at 168.275 119.38 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 177.165 129.54 0)
		(layer "F.SilkS")
	)
	(gr_text "RX"
		(at 147.955 113.03 0)
		(layer "F.SilkS")
	)
	(gr_text "INT"
		(at 131.445 113.03 0)
		(layer "F.SilkS")
	)
	(gr_text "+3V3"
		(at 175.26 132.08 0)
		(layer "F.SilkS")
	)
	(gr_text "D5"
		(at 131.445 130.81 0)
		(layer "F.SilkS")
	)
	(gr_text "D5"
		(at 177.165 121.92 0)
		(layer "F.SilkS")
	)
	(gr_text "MOSI"
		(at 169.545 99.06 0)
		(layer "F.SilkS")
	)
	(gr_text "D4"
		(at 177.165 119.38 0)
		(layer "F.SilkS")
	)
	(gr_text "D4"
		(at 131.445 128.27 0)
		(layer "F.SilkS")
	)
	(gr_text "D6"
		(at 147.955 130.81 0)
		(layer "F.SilkS")
	)
	(gr_text "CS"
		(at 131.445 110.49 0)
		(layer "F.SilkS")
	)
	(gr_text "D3"
		(at 168.275 127 0)
		(layer "F.SilkS")
	)
	(gr_text "D7"
		(at 147.955 128.27 0)
		(layer "F.SilkS")
	)
	(gr_text "+3V3"
		(at 169.545 109.22 0)
		(layer "F.SilkS")
	)
	(gr_text "SDA"
		(at 147.955 118.11 0)
		(layer "F.SilkS")
	)
	(gr_text "A1"
		(at 131.445 102.87 0)
		(layer "F.SilkS")
	)
	(gr_text "MISO"
		(at 169.545 101.6 0)
		(layer "F.SilkS")
	)
	(gr_text "A3"
		(at 131.445 107.95 0)
		(layer "F.SilkS")
	)
	(gr_text "AN"
		(at 131.445 100.33 0)
		(layer "F.SilkS")
	)
	(gr_text "TX"
		(at 147.955 110.49 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 147.955 105.41 0)
		(layer "F.SilkS")
	)
	(gr_text "+3V3"
		(at 167.64 132.08 0)
		(layer "F.SilkS")
	)
	(gr_text "SCK"
		(at 147.955 123.19 0)
		(layer "F.SilkS")
	)
	(gr_text "D3"
		(at 131.445 125.73 0)
		(layer "F.SilkS")
	)
	(gr_text "D1"
		(at 168.275 121.92 0)
		(layer "F.SilkS")
	)
	(gr_text "RST"
		(at 173.99 92.71 270)
		(layer "B.SilkS")
	)
	(gr_text "SCL"
		(at 166.37 113.03 270)
		(layer "B.SilkS")
	)
	(gr_text "RX"
		(at 171.45 113.03 270)
		(layer "B.SilkS")
	)
	(gr_text "MISO"
		(at 148.59 120.65 0)
		(layer "B.SilkS")
	)
	(gr_text "+3V3"
		(at 177.8 109.22 0)
		(layer "B.SilkS")
	)
	(gr_text "PWM"
		(at 173.99 113.665 270)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 169.545 106.68 0)
		(layer "B.SilkS")
	)
	(gr_text "D5"
		(at 130.81 130.81 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 168.275 129.54 0)
		(layer "B.SilkS")
	)
	(gr_text "INT"
		(at 176.53 113.03 270)
		(layer "B.SilkS")
	)
	(gr_text "RX"
		(at 148.59 113.03 0)
		(layer "B.SilkS")
	)
	(gr_text "+5V"
		(at 148.59 97.79 0)
		(layer "B.SilkS")
	)
	(gr_text "MISO"
		(at 169.545 101.6 0)
		(layer "B.SilkS")
	)
	(gr_text "A2"
		(at 130.81 105.41 0)
		(layer "B.SilkS")
	)
	(gr_text "SCL"
		(at 148.59 115.57 0)
		(layer "B.SilkS")
	)
	(gr_text "RX"
		(at 175.895 96.52 0)
		(layer "B.SilkS")
	)
	(gr_text "VIN"
		(at 148.59 100.33 0)
		(layer "B.SilkS")
	)
	(gr_text "A1"
		(at 130.81 102.87 0)
		(layer "B.SilkS")
	)
	(gr_text "+5V"
		(at 161.29 113.03 270)
		(layer "B.SilkS")
	)
	(gr_text "MKR"
		(at 159.385 128.27 0)
		(layer "B.SilkS")
	)
	(gr_text "D7"
		(at 148.59 128.27 0)
		(layer "B.SilkS")
	)
	(gr_text "+3V3"
		(at 168.275 132.08 0)
		(layer "B.SilkS")
	)
	(gr_text "UART"
		(at 180.34 97.79 270)
		(layer "B.SilkS")
	)
	(gr_text "D4"
		(at 177.165 119.38 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 175.895 106.68 0)
		(layer "B.SilkS")
	)
	(gr_text "D3"
		(at 168.275 127 0)
		(layer "B.SilkS")
	)
	(gr_text "PMOD"
		(at 180.34 102.87 270)
		(layer "B.SilkS")
	)
	(gr_text "SCL"
		(at 175.895 101.6 0)
		(layer "B.SilkS")
	)
	(gr_text "AN"
		(at 176.53 92.71 270)
		(layer "B.SilkS")
	)
	(gr_text "TX"
		(at 168.91 113.03 270)
		(layer "B.SilkS")
	)
	(gr_text "D0"
		(at 130.81 118.11 0)
		(layer "B.SilkS")
	)
	(gr_text "CS"
		(at 171.45 92.71 270)
		(layer "B.SilkS")
	)
	(gr_text "D6"
		(at 177.165 124.46 0)
		(layer "B.SilkS")
	)
	(gr_text "A3"
		(at 130.81 107.95 0)
		(layer "B.SilkS")
	)
	(gr_text "D1"
		(at 168.275 121.92 0)
		(layer "B.SilkS")
	)
	(gr_text "CS"
		(at 130.81 110.49 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 177.165 129.54 0)
		(layer "B.SilkS")
	)
	(gr_text "+3V3"
		(at 177.8 132.08 0)
		(layer "B.SilkS")
	)
	(gr_text "D4"
		(at 130.81 128.27 0)
		(layer "B.SilkS")
	)
	(gr_text "PMOD"
		(at 180.34 125.73 270)
		(layer "B.SilkS")
	)
	(gr_text "D7"
		(at 177.165 127 0)
		(layer "B.SilkS")
	)
	(gr_text "PWM"
		(at 130.81 115.57 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 148.59 105.41 0)
		(layer "B.SilkS")
	)
	(gr_text "RST"
		(at 148.59 107.95 0)
		(layer "B.SilkS")
	)
	(gr_text "D2"
		(at 130.81 123.19 0)
		(layer "B.SilkS")
	)
	(gr_text "AREF"
		(at 130.81 97.79 0)
		(layer "B.SilkS")
	)
	(gr_text "MISO"
		(at 166.37 92.71 270)
		(layer "B.SilkS")
	)
	(gr_text "SDA"
		(at 148.59 118.11 0)
		(layer "B.SilkS")
	)
	(gr_text "SCK"
		(at 148.59 123.19 0)
		(layer "B.SilkS")
	)
	(gr_text "D0"
		(at 168.275 119.38 0)
		(layer "B.SilkS")
	)
	(gr_text "TX"
		(at 148.59 110.49 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 158.75 113.03 270)
		(layer "B.SilkS")
	)
	(gr_text "SCK"
		(at 169.545 104.14 0)
		(layer "B.SilkS")
	)
	(gr_text "D3"
		(at 130.81 125.73 0)
		(layer "B.SilkS")
	)
	(gr_text "D2"
		(at 168.275 124.46 0)
		(layer "B.SilkS")
	)
	(gr_text "+3V3"
		(at 148.59 102.87 0)
		(layer "B.SilkS")
	)
	(gr_text "MOSI"
		(at 169.545 99.06 0)
		(layer "B.SilkS")
	)
	(gr_text "INT"
		(at 130.81 113.03 0)
		(layer "B.SilkS")
	)
	(gr_text "+3V3"
		(at 169.545 109.22 0)
		(layer "B.SilkS")
	)
	(gr_text "CS"
		(at 169.545 96.52 0)
		(layer "B.SilkS")
	)
	(gr_text "SDA"
		(at 175.895 104.14 0)
		(layer "B.SilkS")
	)
	(gr_text "SDA"
		(at 163.83 113.03 270)
		(layer "B.SilkS")
	)
	(gr_text "Ziggy\nBridge"
		(at 159.385 121.92 0)
		(layer "B.SilkS")
	)
	(gr_text "AN"
		(at 130.81 100.33 0)
		(layer "B.SilkS")
	)
	(gr_text "TX"
		(at 175.895 99.06 0)
		(layer "B.SilkS")
	)
	(gr_text "MOSI"
		(at 163.83 92.71 270)
		(layer "B.SilkS")
	)
	(gr_text "+3V3"
		(at 161.29 92.71 270)
		(layer "B.SilkS")
	)
	(gr_text "D1"
		(at 130.81 120.65 0)
		(layer "B.SilkS")
	)
	(gr_text "D6"
		(at 148.59 130.81 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 158.75 92.71 270)
		(layer "B.SilkS")
	)
	(gr_text "QWIIC"
		(at 180.34 107.315 270)
		(layer "B.SilkS")
	)
	(gr_text "MOSI"
		(at 148.59 125.73 0)
		(layer "B.SilkS")
	)
	(gr_text "SCK"
		(at 168.91 92.71 270)
		(layer "B.SilkS")
	)
	(gr_text "D5"
		(at 177.165 121.92 0)
		(layer "B.SilkS")
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 149.96 134.97) (xy 129.46 134.97)
		)
		(height -11.65)
		(format
			(prefix "")
			(suffix "")
			(units 0)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0)
			(keep_text_aligned yes)
		)
		(gr_text "0.8071 in"
			(at 139.71 144.82 0)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 152.21 77.97) (xy 152.21 141.72)
		)
		(height 3.3)
		(format
			(prefix "")
			(suffix "")
			(units 0)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0)
			(keep_text_aligned yes)
		)
		(gr_text "2.5098 in"
			(at 147.11 109.845 90)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 129.46 75.72) (xy 149.96 75.72)
		)
		(height 4.2)
		(format
			(prefix "")
			(suffix "")
			(units 0)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0)
			(keep_text_aligned yes)
		)
		(gr_text "0.8071 in"
			(at 139.71 78.12 0)
			(layer "Dwgs.User")
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.254)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 127 88.9) (xy 127 134.62) (xy 182.245 134.62) (xy 182.245 88.9)
			)
		)
	)
	(embedded_fonts no)
)
