(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J1-Pad9)")
  (net 10 "Net-(J1-Pad10)")
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 128.05 83.4 90)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (property "Sheetfile" "arm-debug-flipper.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x10" (at 0 25.19 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 11.43) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical_SMD" (layer "F.Cu")
    (tedit 59FED6E3)
    (at 131.6 90.85)
    (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
    (property "Sheetfile" "arm-debug-flipper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at 0 -4.235) (layer "F.SilkS"))
    (fp_text value "Conn_02x05_Odd_Even" (at 0 4.235) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.95 -2.54) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at 1.95 -2.54) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at -1.95 -1.27) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 1.95 -1.27) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at -1.95 0) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at 1.95 0) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect (at -1.95 1.27) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(J1-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect (at 1.95 1.27) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(J1-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect (at -1.95 2.54) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(J1-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect (at 1.95 2.54) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(J1-Pad10)") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical_SMD" (layer "F.Cu")
    (tedit 59FED6E3)
    (at 147.4 90.85)
    (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
    (property "Sheetfile" "arm-debug-flipper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J2" (at 0 -4.235) (layer "F.SilkS"))
    (fp_text value "Conn_02x05_Odd_Even" (at 0 4.235) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.95 -2.54) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(J1-Pad2)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at 1.95 -2.54) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(J1-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at -1.95 -1.27) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(J1-Pad4)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 1.95 -1.27) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(J1-Pad3)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at -1.95 0) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(J1-Pad6)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at 1.95 0) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(J1-Pad5)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect (at -1.95 1.27) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(J1-Pad8)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect (at 1.95 1.27) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(J1-Pad7)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect (at -1.95 2.54) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(J1-Pad10)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect (at 1.95 2.54) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(J1-Pad9)") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:cross-eyed-10m" (layer "F.Cu")
    (tedit 0)
    (at 139.7 89.7)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (gr_rect (start 126.25 81.6) (end 152.7 94.55) (layer "Edge.Cuts") (width 0.1) (fill none))
)
