(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu16.04.1)
  (general
    (links 232)
    (no_connects 4)
    (area 97.490457 96.861885 179.3374 167.3674)
    (thickness 1.6)
    (drawings 26)
    (tracks 1054)
    (zones 0)
    (modules 126)
    (nets 79)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.5 2.5)
    (pad_drill 2.5)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 62.496 69.762)
    (grid_origin 62.506 69.752)
    (visible_elements FFFCCE0D)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 "Net-(D1-Pad3)")
  (net 3 "Net-(D2-Pad3)")
  (net 4 "Net-(D3-Pad3)")
  (net 5 "Net-(D4-Pad3)")
  (net 6 "Net-(D5-Pad3)")
  (net 7 "Net-(D6-Pad3)")
  (net 8 "Net-(D7-Pad3)")
  (net 9 "Net-(D8-Pad3)")
  (net 10 "Net-(D9-Pad3)")
  (net 11 "Net-(D10-Pad3)")
  (net 12 "Net-(D11-Pad3)")
  (net 13 "Net-(D12-Pad3)")
  (net 14 "Net-(D13-Pad3)")
  (net 15 "Net-(D14-Pad3)")
  (net 16 "Net-(D15-Pad3)")
  (net 17 "Net-(D16-Pad3)")
  (net 18 "Net-(D17-Pad3)")
  (net 19 "Net-(D18-Pad3)")
  (net 20 "Net-(D19-Pad1)")
  (net 21 /R)
  (net 22 /G)
  (net 23 /B)
  (net 24 /W)
  (net 25 "Net-(D20-Pad1)")
  (net 26 "Net-(D21-Pad1)")
  (net 27 "Net-(D22-Pad1)")
  (net 28 "Net-(D23-Pad1)")
  (net 29 "Net-(D24-Pad1)")
  (net 30 "Net-(D25-Pad1)")
  (net 31 "Net-(D26-Pad1)")
  (net 32 GND)
  (net 33 +3V3)
  (net 34 "Net-(R64-Pad2)")
  (net 35 "Net-(L1-Pad2)")
  (net 36 "Net-(D1-Pad1)")
  (net 37 "Net-(D2-Pad1)")
  (net 38 "Net-(D3-Pad1)")
  (net 39 "Net-(D4-Pad1)")
  (net 40 "Net-(D5-Pad1)")
  (net 41 "Net-(D6-Pad1)")
  (net 42 "Net-(D7-Pad1)")
  (net 43 "Net-(D8-Pad1)")
  (net 44 "Net-(D9-Pad1)")
  (net 45 "Net-(D10-Pad1)")
  (net 46 "Net-(D11-Pad1)")
  (net 47 "Net-(D12-Pad1)")
  (net 48 "Net-(D13-Pad1)")
  (net 49 "Net-(D14-Pad1)")
  (net 50 "Net-(D15-Pad1)")
  (net 51 "Net-(D16-Pad1)")
  (net 52 "Net-(D17-Pad1)")
  (net 53 "Net-(D18-Pad1)")
  (net 54 "Net-(D1-Pad5)")
  (net 55 "Net-(D2-Pad5)")
  (net 56 "Net-(D3-Pad5)")
  (net 57 "Net-(D4-Pad5)")
  (net 58 "Net-(D5-Pad5)")
  (net 59 "Net-(D6-Pad5)")
  (net 60 "Net-(D7-Pad5)")
  (net 61 "Net-(D8-Pad5)")
  (net 62 "Net-(D9-Pad5)")
  (net 63 "Net-(D10-Pad5)")
  (net 64 "Net-(D11-Pad5)")
  (net 65 "Net-(D12-Pad5)")
  (net 66 "Net-(D13-Pad5)")
  (net 67 "Net-(D14-Pad5)")
  (net 68 "Net-(D15-Pad5)")
  (net 69 "Net-(D16-Pad5)")
  (net 70 "Net-(D17-Pad5)")
  (net 71 "Net-(D18-Pad5)")
  (net 72 "Net-(Q1-Pad1)")
  (net 73 "Net-(Q2-Pad1)")
  (net 74 "Net-(Q3-Pad1)")
  (net 75 "Net-(Q4-Pad1)")
  (net 76 "Net-(J1-Pad2)")
  (net 77 "Net-(J1-Pad3)")
  (net 78 "Net-(J1-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +3V3)
    (add_net +5V)
    (add_net /B)
    (add_net /G)
    (add_net /R)
    (add_net /W)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D1-Pad5)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D10-Pad3)")
    (add_net "Net-(D10-Pad5)")
    (add_net "Net-(D11-Pad1)")
    (add_net "Net-(D11-Pad3)")
    (add_net "Net-(D11-Pad5)")
    (add_net "Net-(D12-Pad1)")
    (add_net "Net-(D12-Pad3)")
    (add_net "Net-(D12-Pad5)")
    (add_net "Net-(D13-Pad1)")
    (add_net "Net-(D13-Pad3)")
    (add_net "Net-(D13-Pad5)")
    (add_net "Net-(D14-Pad1)")
    (add_net "Net-(D14-Pad3)")
    (add_net "Net-(D14-Pad5)")
    (add_net "Net-(D15-Pad1)")
    (add_net "Net-(D15-Pad3)")
    (add_net "Net-(D15-Pad5)")
    (add_net "Net-(D16-Pad1)")
    (add_net "Net-(D16-Pad3)")
    (add_net "Net-(D16-Pad5)")
    (add_net "Net-(D17-Pad1)")
    (add_net "Net-(D17-Pad3)")
    (add_net "Net-(D17-Pad5)")
    (add_net "Net-(D18-Pad1)")
    (add_net "Net-(D18-Pad3)")
    (add_net "Net-(D18-Pad5)")
    (add_net "Net-(D19-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad3)")
    (add_net "Net-(D2-Pad5)")
    (add_net "Net-(D20-Pad1)")
    (add_net "Net-(D21-Pad1)")
    (add_net "Net-(D22-Pad1)")
    (add_net "Net-(D23-Pad1)")
    (add_net "Net-(D24-Pad1)")
    (add_net "Net-(D25-Pad1)")
    (add_net "Net-(D26-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad3)")
    (add_net "Net-(D3-Pad5)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad3)")
    (add_net "Net-(D4-Pad5)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad3)")
    (add_net "Net-(D5-Pad5)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D6-Pad3)")
    (add_net "Net-(D6-Pad5)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D7-Pad3)")
    (add_net "Net-(D7-Pad5)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D8-Pad3)")
    (add_net "Net-(D8-Pad5)")
    (add_net "Net-(D9-Pad1)")
    (add_net "Net-(D9-Pad3)")
    (add_net "Net-(D9-Pad5)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q4-Pad1)")
    (add_net "Net-(R64-Pad2)")
  )
  (module LEDs-components:MountingHole_0.5mm_M2 (layer F.Cu) (tedit 5838D4CA)
    (at 164.194 156.29)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_0.5mm_M2 (at 0 3.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module LEDs-components:MountingHole_0.5mm_M2 (layer F.Cu) (tedit 5838D4CA)
    (at 165.194 156.29)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_0.5mm_M2 (at 0 3.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module LEDs-components:MountingHole_0.5mm_M2 (layer F.Cu) (tedit 5838D4CA)
    (at 167.25 156.29)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_0.5mm_M2 (at 0 3.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module LEDs-components:MountingHole_0.5mm_M2 (layer F.Cu) (tedit 5838D4CA)
    (at 166.25 156.29)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_0.5mm_M2 (at 0 3.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module LEDs-components:MountingHole_0.5mm_M2 (layer F.Cu) (tedit 5838D4CA)
    (at 167.25 154.25)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_0.5mm_M2 (at 0 3.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module LEDs-components:MountingHole_0.5mm_M2 (layer F.Cu) (tedit 5838D4CA)
    (at 166.25 154.25)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_0.5mm_M2 (at 0 3.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module LEDs-components:MountingHole_0.5mm_M2 (layer F.Cu) (tedit 5838D4CA)
    (at 165.194 154.25)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_0.5mm_M2 (at 0 3.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module LEDs-components:MountingHole_0.5mm_M2 (layer F.Cu) (tedit 5838D4CA)
    (at 164.194 154.25)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_0.5mm_M2 (at 0 3.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module LEDs-components:MountingHole_0.5mm_M2 (layer F.Cu) (tedit 5838D4CA)
    (at 112.306 156.29)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_0.5mm_M2 (at 0 3.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module LEDs-components:MountingHole_0.5mm_M2 (layer F.Cu) (tedit 5838D4CA)
    (at 111.306 156.29)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_0.5mm_M2 (at 0 3.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module LEDs-components:MountingHole_0.5mm_M2 (layer F.Cu) (tedit 5838D4CA)
    (at 110.25 156.29)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_0.5mm_M2 (at 0 3.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module LEDs-components:MountingHole_0.5mm_M2 (layer F.Cu) (tedit 5838D4CA)
    (at 109.25 156.29)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_0.5mm_M2 (at 0 3.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module LEDs-components:MountingHole_0.5mm_M2 (layer F.Cu) (tedit 5838D4CA)
    (at 111.306 154.25)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_0.5mm_M2 (at 0 3.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module LEDs-components:MountingHole_0.5mm_M2 (layer F.Cu) (tedit 5838D4CA)
    (at 110.25 154.25)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_0.5mm_M2 (at 0 3.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module LEDs-components:MountingHole_0.5mm_M2 (layer F.Cu) (tedit 5838D4CA)
    (at 109.25 154.25)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_0.5mm_M2 (at 0 3.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 169.5 149.09)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module LEDs-components:LED_RGB_28x35-6 (layer F.Cu) (tedit 5B2C245F)
    (at 110.90625 163.54)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (attr smd)
    (fp_text reference D17 (at -1.1 -3.2 180) (layer F.SilkS))
    (fp_text value 150352M173300 (at 0.2 2.8) (layer F.Fab))
    (pad 1 smd rect (at -1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(D17-Pad1)"))
    (pad 2 smd rect (at 1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D17-Pad3)"))
    (pad 4 smd rect (at 1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(D17-Pad5)"))
    (pad 6 smd rect (at 1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_RGB_PLCC-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs-components:LED_RGB_28x35-6 (layer F.Cu) (tedit 5B2C245F)
    (at 105 103.5 90)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (attr smd)
    (fp_text reference D18 (at -1.1 -3.2 270) (layer F.SilkS))
    (fp_text value 150352M173300 (at 0.2 2.8 90) (layer F.Fab))
    (pad 1 smd rect (at -1.55 -0.85 180) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(D18-Pad1)"))
    (pad 2 smd rect (at 1.55 -0.85 180) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -1.55 0 180) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D18-Pad3)"))
    (pad 4 smd rect (at 1.55 0 180) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -1.55 0.85 180) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(D18-Pad5)"))
    (pad 6 smd rect (at 1.55 0.85 180) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_RGB_PLCC-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs-components:LED_RGB_28x35-6 (layer F.Cu) (tedit 5B2C245F)
    (at 118.71875 163.54)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (attr smd)
    (fp_text reference D16 (at -1.1 -3.2 180) (layer F.SilkS))
    (fp_text value 150352M173300 (at 0.2 2.8) (layer F.Fab))
    (pad 1 smd rect (at -1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(D16-Pad1)"))
    (pad 2 smd rect (at 1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D16-Pad3)"))
    (pad 4 smd rect (at 1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(D16-Pad5)"))
    (pad 6 smd rect (at 1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_RGB_PLCC-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs-components:LED_RGB_28x35-6 (layer F.Cu) (tedit 5B2C245F)
    (at 126.53125 163.54)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (attr smd)
    (fp_text reference D15 (at -1.1 -3.2 180) (layer F.SilkS))
    (fp_text value 150352M173300 (at 0.2 2.8) (layer F.Fab))
    (pad 1 smd rect (at -1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(D15-Pad1)"))
    (pad 2 smd rect (at 1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D15-Pad3)"))
    (pad 4 smd rect (at 1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(D15-Pad5)"))
    (pad 6 smd rect (at 1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_RGB_PLCC-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs-components:LED_RGB_28x35-6 (layer F.Cu) (tedit 5B2C245F)
    (at 134.34375 163.54)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (attr smd)
    (fp_text reference D14 (at -1.1 -3.2 180) (layer F.SilkS))
    (fp_text value 150352M173300 (at 0.2 2.8) (layer F.Fab))
    (pad 1 smd rect (at -1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(D14-Pad1)"))
    (pad 2 smd rect (at 1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D14-Pad3)"))
    (pad 4 smd rect (at 1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(D14-Pad5)"))
    (pad 6 smd rect (at 1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_RGB_PLCC-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs-components:LED_RGB_28x35-6 (layer F.Cu) (tedit 5B2C245F)
    (at 142.15625 163.54)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (attr smd)
    (fp_text reference D13 (at -1.1 -3.2 180) (layer F.SilkS))
    (fp_text value 150352M173300 (at 0.2 2.8) (layer F.Fab))
    (pad 1 smd rect (at -1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D13-Pad1)"))
    (pad 2 smd rect (at 1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D13-Pad3)"))
    (pad 4 smd rect (at 1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(D13-Pad5)"))
    (pad 6 smd rect (at 1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_RGB_PLCC-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs-components:LED_RGB_28x35-6 (layer F.Cu) (tedit 5B2C245F)
    (at 149.96875 163.54)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (attr smd)
    (fp_text reference D12 (at -1.1 -3.2 180) (layer F.SilkS))
    (fp_text value 150352M173300 (at 0.2 2.8) (layer F.Fab))
    (pad 1 smd rect (at -1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D12-Pad1)"))
    (pad 2 smd rect (at 1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D12-Pad3)"))
    (pad 4 smd rect (at 1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(D12-Pad5)"))
    (pad 6 smd rect (at 1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_RGB_PLCC-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs-components:LED_RGB_28x35-6 (layer F.Cu) (tedit 5B2C245F)
    (at 157.78125 163.54)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (attr smd)
    (fp_text reference D11 (at -1.1 -3.2 180) (layer F.SilkS))
    (fp_text value 150352M173300 (at 0.2 2.8) (layer F.Fab))
    (pad 1 smd rect (at -1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D11-Pad1)"))
    (pad 2 smd rect (at 1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D11-Pad3)"))
    (pad 4 smd rect (at 1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(D11-Pad5)"))
    (pad 6 smd rect (at 1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_RGB_PLCC-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs-components:LED_RGB_28x35-6 (layer F.Cu) (tedit 5B2C245F)
    (at 165.59375 163.54)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (attr smd)
    (fp_text reference D10 (at -1.1 -3.2 180) (layer F.SilkS))
    (fp_text value 150352M173300 (at 0.2 2.8) (layer F.Fab))
    (pad 1 smd rect (at -1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D10-Pad3)"))
    (pad 4 smd rect (at 1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(D10-Pad5)"))
    (pad 6 smd rect (at 1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_RGB_PLCC-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs-components:LED_RGB_28x35-6 (layer F.Cu) (tedit 5B2C245F)
    (at 171.5 103.5 90)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (attr smd)
    (fp_text reference D9 (at -1.1 -3.2 270) (layer F.SilkS))
    (fp_text value 150352M173300 (at 0.2 2.8 90) (layer F.Fab))
    (pad 1 smd rect (at -1.55 -0.85 180) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D9-Pad1)"))
    (pad 2 smd rect (at 1.55 -0.85 180) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -1.55 0 180) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D9-Pad3)"))
    (pad 4 smd rect (at 1.55 0 180) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -1.55 0.85 180) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(D9-Pad5)"))
    (pad 6 smd rect (at 1.55 0.85 180) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_RGB_PLCC-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs-components:LED_RGB_28x35-6 (layer F.Cu) (tedit 5B2C245F)
    (at 165.59375 109 180)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (attr smd)
    (fp_text reference D8 (at -1.1 -3.2 360) (layer F.SilkS))
    (fp_text value 150352M173300 (at 0.2 2.8 180) (layer F.Fab))
    (pad 1 smd rect (at -1.55 -0.85 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D8-Pad1)"))
    (pad 2 smd rect (at 1.55 -0.85 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -1.55 0 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D8-Pad3)"))
    (pad 4 smd rect (at 1.55 0 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -1.55 0.85 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(D8-Pad5)"))
    (pad 6 smd rect (at 1.55 0.85 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_RGB_PLCC-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs-components:LED_RGB_28x35-6 (layer F.Cu) (tedit 5B2C245F)
    (at 157.78125 109 180)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (attr smd)
    (fp_text reference D7 (at -1.1 -3.2 360) (layer F.SilkS))
    (fp_text value 150352M173300 (at 0.2 2.8 180) (layer F.Fab))
    (pad 1 smd rect (at -1.55 -0.85 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D7-Pad1)"))
    (pad 2 smd rect (at 1.55 -0.85 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -1.55 0 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D7-Pad3)"))
    (pad 4 smd rect (at 1.55 0 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -1.55 0.85 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(D7-Pad5)"))
    (pad 6 smd rect (at 1.55 0.85 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_RGB_PLCC-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs-components:LED_RGB_28x35-6 (layer F.Cu) (tedit 5B2C245F)
    (at 149.96875 109 180)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (attr smd)
    (fp_text reference D6 (at -1.1 -3.2 360) (layer F.SilkS))
    (fp_text value 150352M173300 (at 0.2 2.8 180) (layer F.Fab))
    (pad 1 smd rect (at -1.55 -0.85 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at 1.55 -0.85 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -1.55 0 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D6-Pad3)"))
    (pad 4 smd rect (at 1.55 0 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -1.55 0.85 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(D6-Pad5)"))
    (pad 6 smd rect (at 1.55 0.85 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_RGB_PLCC-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs-components:LED_RGB_28x35-6 (layer F.Cu) (tedit 5B2C245F)
    (at 142.15625 109 180)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (attr smd)
    (fp_text reference D5 (at -1.1 -3.2 360) (layer F.SilkS))
    (fp_text value 150352M173300 (at 0.2 2.8 180) (layer F.Fab))
    (pad 1 smd rect (at -1.55 -0.85 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 1.55 -0.85 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -1.55 0 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D5-Pad3)"))
    (pad 4 smd rect (at 1.55 0 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -1.55 0.85 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(D5-Pad5)"))
    (pad 6 smd rect (at 1.55 0.85 270) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_RGB_PLCC-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs-components:LED_RGB_28x35-6 (layer F.Cu) (tedit 5B2C245F)
    (at 134.34375 109)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (attr smd)
    (fp_text reference D4 (at -1.1 -3.2 180) (layer F.SilkS))
    (fp_text value 150352M173300 (at 0.2 2.8) (layer F.Fab))
    (pad 1 smd rect (at -1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D4-Pad3)"))
    (pad 4 smd rect (at 1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(D4-Pad5)"))
    (pad 6 smd rect (at 1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_RGB_PLCC-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs-components:LED_RGB_28x35-6 (layer F.Cu) (tedit 5B2C245F)
    (at 126.53125 109)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (attr smd)
    (fp_text reference D3 (at -1.1 -3.2 180) (layer F.SilkS))
    (fp_text value 150352M173300 (at 0.2 2.8) (layer F.Fab))
    (pad 1 smd rect (at -1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D3-Pad3)"))
    (pad 4 smd rect (at 1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(D3-Pad5)"))
    (pad 6 smd rect (at 1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_RGB_PLCC-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs-components:LED_RGB_28x35-6 (layer F.Cu) (tedit 5B2C245F)
    (at 118.71875 109)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (attr smd)
    (fp_text reference D2 (at -1.1 -3.2 180) (layer F.SilkS))
    (fp_text value 150352M173300 (at 0.2 2.8) (layer F.Fab))
    (pad 1 smd rect (at -1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad3)"))
    (pad 4 smd rect (at 1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(D2-Pad5)"))
    (pad 6 smd rect (at 1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_RGB_PLCC-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs-components:LED_RGB_28x35-6 (layer F.Cu) (tedit 5B2C245F)
    (at 110.90625 109)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (attr smd)
    (fp_text reference D1 (at -1.1 -3.2 180) (layer F.SilkS))
    (fp_text value 150352M173300 (at 0.2 2.8) (layer F.Fab))
    (pad 1 smd rect (at -1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.55 -0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad3)"))
    (pad 4 smd rect (at 1.55 0 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(D1-Pad5)"))
    (pad 6 smd rect (at 1.55 0.85 90) (size 0.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_RGB_PLCC-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs-components:LED_PLCC2 (layer F.Cu) (tedit 5AE39143)
    (at 160.10725 134.09)
    (fp_text reference D26 (at -2.032 3.197) (layer F.SilkS))
    (fp_text value CLM3C-WKW-CWBYA153 (at 0 -3.915) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.375) (size 2.4 1.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at 0 1.375) (size 2.4 1.75) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D26-Pad1)"))
  )
  (module LEDs-components:LED_PLCC2 (layer F.Cu) (tedit 5AE39143)
    (at 153.66975 134.09)
    (fp_text reference D25 (at -2.032 3.197) (layer F.SilkS))
    (fp_text value CLM3C-WKW-CWBYA153 (at 0 -3.915) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.375) (size 2.4 1.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at 0 1.375) (size 2.4 1.75) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D25-Pad1)"))
  )
  (module LEDs-components:LED_PLCC2 (layer F.Cu) (tedit 5AE39143)
    (at 140.79475 134.09)
    (fp_text reference D23 (at -2.032 3.197) (layer F.SilkS))
    (fp_text value CLM3C-WKW-CWBYA153 (at 0 -3.915) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.375) (size 2.4 1.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at 0 1.375) (size 2.4 1.75) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D23-Pad1)"))
  )
  (module LEDs-components:LED_PLCC2 (layer F.Cu) (tedit 5AE39143)
    (at 134.35725 134.09)
    (fp_text reference D22 (at -2.032 3.197) (layer F.SilkS))
    (fp_text value CLM3C-WKW-CWBYA153 (at 0 -3.915) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.375) (size 2.4 1.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at 0 1.375) (size 2.4 1.75) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D22-Pad1)"))
  )
  (module LEDs-components:LED_PLCC2 (layer F.Cu) (tedit 5AE39143)
    (at 127.91975 134.09)
    (fp_text reference D21 (at -2.032 3.197) (layer F.SilkS))
    (fp_text value CLM3C-WKW-CWBYA153 (at 0 -3.915) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.375) (size 2.4 1.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at 0 1.375) (size 2.4 1.75) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D21-Pad1)"))
  )
  (module LEDs-components:LED_PLCC2 (layer F.Cu) (tedit 5AE39143)
    (at 121.48225 134.09)
    (fp_text reference D20 (at -2.032 3.197) (layer F.SilkS))
    (fp_text value CLM3C-WKW-CWBYA153 (at 0 -3.915) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.375) (size 2.4 1.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at 0 1.375) (size 2.4 1.75) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D20-Pad1)"))
  )
  (module LEDs-components:LED_PLCC2 (layer F.Cu) (tedit 5AE39143)
    (at 115.04475 134.09)
    (fp_text reference D19 (at -2.032 3.197) (layer F.SilkS))
    (fp_text value CLM3C-WKW-CWBYA153 (at 0 -3.915) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.375) (size 2.4 1.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at 0 1.375) (size 2.4 1.75) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D19-Pad1)"))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 142.8462 147.362522 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L1 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 2.2u (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 +3V3))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(L1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 156.5622 148.886522 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 22u (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 32 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 159.0006 148.886522 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 10u (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 33 +3V3))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 32 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:MSOP-8_3x3mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 148.5866 147.260922)
    (descr "8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 -2.6) (layer F.SilkS))
    (fp_text value PAM2401 (at 0 2.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.2 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(L1-Pad2)"))
    (pad 2 smd rect (at -2.2 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 33 +3V3))
    (pad 3 smd rect (at -2.2 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 33 +3V3))
    (pad 4 smd rect (at -2.2 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 32 GND))
    (pad 5 smd rect (at 2.2 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R64-Pad2)"))
    (pad 6 smd rect (at 2.2 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 2.2 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 8 smd rect (at 2.2 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 32 GND))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/MSOP-8_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 153.819 148.378522)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R65 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 100k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R64-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 153.819 146.854522)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R64 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 750k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R64-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 153.819 145.330522 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R63 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs-components:2x2_horizontal_header (layer B.Cu) (tedit 5B6236D8)
    (at 173 161.54 270)
    (fp_text reference P4 (at -1.54 -2.81 270) (layer B.SilkS))
    (fp_text value M22-6550242R (at -5.655 -4.08 270) (layer B.Fab))
    (pad 1 smd rect (at -3.05 -1 270) (size 1.8 1) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -3.05 1 270) (size 1.8 1) (layers B.Cu B.Paste B.Mask)
      (net 21 /R))
    (pad 3 smd rect (at 0.45 -1 270) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 23 /B))
    (pad 4 smd rect (at 0.45 1 270) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 22 /G))
  )
  (module LEDs-components:2x2_horizontal_header (layer B.Cu) (tedit 5B6236D8)
    (at 103.5 161.54 270)
    (fp_text reference P3 (at -1.54 -2.81 270) (layer B.SilkS))
    (fp_text value M22-6550242R (at -5.655 -4.08 270) (layer B.Fab))
    (pad 1 smd rect (at -3.05 -1 270) (size 1.8 1) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -3.05 1 270) (size 1.8 1) (layers B.Cu B.Paste B.Mask)
      (net 21 /R))
    (pad 3 smd rect (at 0.45 -1 270) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 23 /B))
    (pad 4 smd rect (at 0.45 1 270) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 22 /G))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 106.067 118.647 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 610 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad3)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /R))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 108.734 118.647 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 610 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad3)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /R))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 114.08 117.123 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 610 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D3-Pad3)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /R))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 111.413 118.647 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 610 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D4-Pad3)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /R))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 162.432 118.647)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 610 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D5-Pad3)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /R))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 165.087 118.647)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 610 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D6-Pad3)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /R))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 106.055 117.123 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(D1-Pad5)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 /G))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 108.734 117.123 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(D2-Pad5)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 /G))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 114.068 118.647 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(D3-Pad5)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 /G))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 111.413 117.123 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(D4-Pad5)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 /G))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 162.432 117.123)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(D5-Pad5)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 /G))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 165.087 117.123)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(D6-Pad5)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 /G))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 106.067 115.599 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 108.734 115.599 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 114.068 115.599 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 111.413 115.599 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 162.432 115.599)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 165.087 115.599)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 167.742 118.647)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 610 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D7-Pad3)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /R))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 170.397 118.647)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R20 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 610 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D8-Pad3)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /R))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 173.052 118.647)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 610 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D9-Pad3)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /R))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 165.376 159.922 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R22 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 610 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D10-Pad3)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /R))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 157.502 159.922 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R23 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 610 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D11-Pad3)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /R))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 149.882 159.922 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R24 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 610 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D12-Pad3)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /R))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 167.742 117.123)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R25 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(D7-Pad5)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 /G))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 173.052 117.123)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R27 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(D9-Pad5)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 /G))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 167.154 159.922 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R28 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(D10-Pad5)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 /G))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 159.28 159.922 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R29 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(D11-Pad5)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 /G))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 151.66 159.922 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R30 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(D12-Pad5)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 /G))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 173.052 115.599)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R33 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D9-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 163.598 159.922 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R34 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 155.724 159.922 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R35 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D11-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 148.104 159.922 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R36 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D12-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 142.008 159.922 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R37 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 610 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D13-Pad3)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /R))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 134.134 159.934 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R38 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 610 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D14-Pad3)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /R))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 126.248 159.922 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R39 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 610 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D15-Pad3)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /R))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 118.64 159.922 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R40 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 610 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D16-Pad3)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /R))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 110.766 159.922 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R41 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 610 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D17-Pad3)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /R))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 143.786 159.922 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R43 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(D13-Pad5)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 /G))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 135.912 159.922 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R44 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(D14-Pad5)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 /G))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 128.038 159.922 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R45 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(D15-Pad5)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 /G))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 120.418 159.922 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R46 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(D16-Pad5)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 /G))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 112.544 159.922 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R47 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(D17-Pad5)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 /G))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 103.4 117.123 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R48 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(D18-Pad5)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 /G))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 140.23 159.922 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R49 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D13-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 132.356 159.922 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R50 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(D14-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 124.482 159.922 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R51 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(D15-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 108.988 159.922 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R53 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(D17-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 114.427 139.161922)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R55 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 360 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D19-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 /W))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 120.904 139.161922)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R56 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 360 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D20-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 /W))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 127.381 139.161922)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R57 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 360 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D21-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 /W))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 133.858 139.161922)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R58 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 360 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D22-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 /W))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 140.208 139.161922)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R59 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 360 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D23-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 /W))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 146.685 139.161922)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R60 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 360 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D24-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 /W))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 153.035 139.161922)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R61 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 360 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D25-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 /W))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 159.512 139.161922)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R62 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 360 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D26-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 /W))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 167.742 115.599)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R31 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D7-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 170.397 115.599)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R32 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D8-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 170.397 117.123)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R26 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(D8-Pad5)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 /G))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 103.412 118.647 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R42 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 610 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D18-Pad3)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /R))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs-components:2x2_horizontal_socket (layer B.Cu) (tedit 5AE1046F)
    (at 103.5 106.4 90)
    (fp_text reference P1 (at -7.745 -2.31 90) (layer B.SilkS))
    (fp_text value 10112690-G03-02LF (at -6.475 5.31 90) (layer B.Fab))
    (pad 1 smd rect (at -5.475 1 90) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -5.475 -1 90) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 21 /R))
    (pad 3 smd rect (at -2.175 1 90) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 23 /B))
    (pad 4 smd rect (at -2.175 -1 90) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 22 /G))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 103.4 115.599 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R54 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(D18-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 116.862 159.922 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R52 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 440 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(D16-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs-components:2x2_horizontal_socket (layer B.Cu) (tedit 5AE1046F)
    (at 173 106.4 90)
    (fp_text reference P2 (at -7.745 -2.31 90) (layer B.SilkS))
    (fp_text value 10112690-G03-02LF (at -6.475 5.31 90) (layer B.Fab))
    (pad 1 smd rect (at -5.475 1 90) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -5.475 -1 90) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 21 /R))
    (pad 3 smd rect (at -2.175 1 90) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 23 /B))
    (pad 4 smd rect (at -2.175 -1 90) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 22 /G))
  )
  (module LEDs-components:LED_PLCC2 (layer F.Cu) (tedit 5AE39143)
    (at 147.23225 134.09)
    (fp_text reference D24 (at -2.032 3.197) (layer F.SilkS))
    (fp_text value CLM3C-WKW-CWBYA153 (at 0 -3.915) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.375) (size 2.4 1.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at 0 1.375) (size 2.4 1.75) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D24-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 141.246 124.362 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value MMBT3904 (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 GND))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 21 /R))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 136.42 124.362 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value MMBT3904 (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 GND))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 /G))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 131.66 124.346 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value MMBT3904 (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 GND))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 /W))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 146.072 124.362 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value MMBT3904 (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(Q4-Pad1)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 GND))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 /B))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs-components:IDC_Header_SMD_10pins (layer B.Cu) (tedit 57A0F63C)
    (at 121.7 146.5 90)
    (descr "10 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference J1 (at 5.08 9.652 90) (layer B.SilkS))
    (fp_text value 3020-10-0300-00 (at 5.08 -3.191 90) (layer B.Fab))
    (pad 1 smd oval (at 0 0 90) (size 0.89 4.9) (layers B.Cu B.Paste B.Mask)
      (net 32 GND))
    (pad 2 smd rect (at 0 6.5 90) (size 0.89 4.8) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at 2.54 0 90) (size 0.89 4.8) (layers B.Cu B.Paste B.Mask)
      (net 77 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at 2.54 6.5 90) (size 0.89 4.8) (layers B.Cu B.Paste B.Mask)
      (net 33 +3V3))
    (pad 5 smd rect (at 5.08 0 90) (size 0.89 4.8) (layers B.Cu B.Paste B.Mask)
      (net 78 "Net-(J1-Pad5)"))
    (pad 6 connect rect (at 5.08 6.5 90) (size 0.89 4.8) (layers B.Cu B.Mask))
    (pad 7 smd rect (at 7.62 0 90) (size 0.89 4.8) (layers B.Cu B.Paste B.Mask)
      (net 32 GND))
    (pad 8 smd rect (at 7.62 6.5 90) (size 0.89 4.8) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at 10.16 0 90) (size 0.89 4.8) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at 10.16 6.5 90) (size 0.89 4.8) (layers B.Cu B.Paste B.Mask)
      (net 33 +3V3))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 136.928 129.696)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R66 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 1k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 133.88 129.696)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R67 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 1k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(J1-Pad5)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 130.844 129.696)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R68 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 1k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 140.738 129.696)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R69 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 1k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(Q4-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 107 149.09)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module LEDs-components:MountingHole_0.5mm_M2 (layer F.Cu) (tedit 5838D4CA)
    (at 112.306 154.25)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_0.5mm_M2 (at 0 3.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (gr_line (start 169.5 100) (end 176.5 100) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 100) (end 107 100) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176.5 156.54) (end 167.5 156.54) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109 156.54) (end 100 156.54) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.556 154) (end 112.556 156.54) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.944 154) (end 163.944 156.54) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.556 154) (end 163.944 154) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176.5 154) (end 167.5 154) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.5 154) (end 167.5 156.54) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109 154) (end 109 156.54) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.75 111) (end 159.75 113) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.75 111) (end 116.75 113) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.75 113) (end 159.75 113) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.944 156.54) (end 112.556 156.54) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176.5 165.54) (end 176.5 156.54) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 165.54) (end 100 156.54) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107 165.54) (end 169.5 165.54) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.75 111) (end 159.75 111) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 154) (end 100 100) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109 154) (end 100 154) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176.5 100) (end 176.5 154) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 169.5 165.54) (end 176.5 165.54) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 169.5 107) (end 169.5 100) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107 107) (end 169.5 107) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107 100) (end 107 107) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 165.54) (end 107 165.54) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name +5V) (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.1778))
    (polygon
      (pts
        (xy 100.352 100.232) (xy 106.702 100.232) (xy 106.702 107.344) (xy 169.694 107.344) (xy 169.694 100.232)
        (xy 176.298 100.232) (xy 176.298 153.572) (xy 100.352 153.572)
      )
    )
  )
  (zone (net 1) (net_name +5V) (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.1778))
    (polygon
      (pts
        (xy 100.352 100.232) (xy 106.702 100.232) (xy 106.702 107.344) (xy 169.694 107.344) (xy 169.694 100.232)
        (xy 176.298 100.232) (xy 176.298 153.572) (xy 100.352 153.572)
      )
    )
  )
  (zone (net 1) (net_name +5V) (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.1778))
    (polygon
      (pts
        (xy 176.298 156.755) (xy 176.298 165.264) (xy 100.352 165.264) (xy 100.352 156.755)
      )
    )
  )
  (zone (net 1) (net_name +5V) (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.1778))
    (polygon
      (pts
        (xy 176.298 156.755) (xy 176.298 165.264) (xy 100.352 165.264) (xy 100.352 156.755)
      )
    )
  )
)
