(kicad_pcb (version 4) (host pcbnew 4.0.6+dfsg1-1)
  (general
    (links 34)
    (no_connects 0)
    (area 94.116316 137.5 153.750001 188.750001)
    (thickness 1.6)
    (drawings 37)
    (tracks 55)
    (zones 0)
    (modules 14)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.15)
    (user_trace_width 0.6)
    (user_trace_width 2)
    (user_trace_width 2.54)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.15)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.33)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory output/))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 SDA)
  (net 4 SCL)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.15)
    (via_dia 0.6)
    (via_drill 0.33)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net SCL)
    (add_net SDA)
  )
  (module mrmeeseeks:Badgelife-Shitty-2x2 (layer F.Cu) (tedit 5AC7D7CF)
    (at 128.5 179.5)
    (descr "Through hole angled pin header, 2x02, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x02 2.54mm double row")
    (fp_text reference X1 (at 0 0) (layer F.Fab))
    (fp_text value Badgelife_shitty_connector (at 0 4.2) (layer F.Fab))
    (fp_text user sda (at 3.5 -1.5) (layer F.SilkS))
    (fp_text user scl (at 3.25 2.25) (layer F.SilkS))
    (fp_text user gnd (at -3.25 2.25) (layer F.SilkS))
    (fp_text user 3.3v (at -3.5 -1.5) (layer F.SilkS))
    (pad 4 thru_hole circle (at 1.27 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 SDA))
    (pad 3 thru_hole oval (at 1.27 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SCL))
    (pad 1 thru_hole oval (at -1.27 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at -1.27 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module mrmeeseeks:Pin_Header_Straight_2x09_Pitch2.54mm-NoSilk (layer F.Cu) (tedit 5AA33E7A)
    (at 118.364 171.2 90)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference REF** (at 1.27 -2.33 90) (layer F.Fab) hide)
    (fp_text value Pin_Header_Straight_2x09_Pitch2.54mm (at 1.27 22.65 90) (layer F.Fab))
    (fp_text user %R (at 1.27 10.16 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module mrmeeseeks:Pin_Header_Straight_2x09_Pitch2.54mm-NoSilk (layer F.Cu) (tedit 5AA33E7A)
    (at 118.364 166.1 90)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference REF** (at 1.27 -2.33 90) (layer F.Fab) hide)
    (fp_text value Pin_Header_Straight_2x09_Pitch2.54mm (at 1.27 22.65 90) (layer F.Fab))
    (fp_text user %R (at 1.27 10.16 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module mrmeeseeks:Pin_Header_Straight_2x09_Pitch2.54mm-NoSilk (layer F.Cu) (tedit 5AA33E7A)
    (at 118.364 161.036 90)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference REF** (at 1.27 -2.33 90) (layer F.Fab) hide)
    (fp_text value Pin_Header_Straight_2x09_Pitch2.54mm (at 1.27 22.65 90) (layer F.Fab))
    (fp_text user %R (at 1.27 10.16 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module mrmeeseeks:Pin_Header_Straight_2x09_Pitch2.54mm-NoSilk (layer F.Cu) (tedit 5AA33E7A)
    (at 118.364 155.956 90)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference REF** (at 1.27 -2.33 90) (layer F.Fab) hide)
    (fp_text value Pin_Header_Straight_2x09_Pitch2.54mm (at 1.27 22.65 90) (layer F.Fab))
    (fp_text user %R (at 1.27 10.16 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module mrmeeseeks:Power_Rail-01x08 (layer F.Cu) (tedit 5AC7D1EA)
    (at 115.7986 153.416)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.Fab) hide)
    (fp_text value Conn_01x08 (at 0 17.57) (layer F.Fab))
    (fp_text user %R (at 0 7.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3) (solder_mask_margin 0.1))
    (pad 2 thru_hole rect (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3) (solder_mask_margin 0.1))
    (pad 3 thru_hole rect (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3) (solder_mask_margin 0.1))
    (pad 4 thru_hole rect (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3) (solder_mask_margin 0.1))
    (pad 5 thru_hole rect (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3) (solder_mask_margin 0.1))
    (pad 6 thru_hole rect (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3) (solder_mask_margin 0.1))
    (pad 7 thru_hole rect (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3) (solder_mask_margin 0.1))
    (pad 8 thru_hole rect (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3) (solder_mask_margin 0.1))
  )
  (module mrmeeseeks:Power_Rail-01x08 (layer F.Cu) (tedit 5AC7D1EA)
    (at 141.224 153.416)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.Fab) hide)
    (fp_text value Conn_01x08 (at 0 17.57) (layer F.Fab))
    (fp_text user %R (at 0 7.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1))
    (pad 2 thru_hole rect (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1))
    (pad 3 thru_hole rect (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1))
    (pad 4 thru_hole rect (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1))
    (pad 5 thru_hole rect (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1))
    (pad 6 thru_hole rect (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1))
    (pad 7 thru_hole rect (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1))
    (pad 8 thru_hole rect (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1))
  )
  (module mrmeeseeks:Power_Rail-01x09 (layer F.Cu) (tedit 5AC7D21B)
    (at 118.364 150.876 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.Fab) hide)
    (fp_text value Conn_01x09 (at 0 17.57 90) (layer F.Fab))
    (fp_text user %R (at 0 7.62 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 SDA) (solder_mask_margin 0.1))
    (pad 2 thru_hole rect (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 SDA) (solder_mask_margin 0.1))
    (pad 3 thru_hole rect (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 SDA) (solder_mask_margin 0.1))
    (pad 4 thru_hole rect (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 SDA) (solder_mask_margin 0.1))
    (pad 5 thru_hole rect (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 SDA) (solder_mask_margin 0.1))
    (pad 6 thru_hole rect (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 SDA) (solder_mask_margin 0.1))
    (pad 7 thru_hole rect (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 SDA) (solder_mask_margin 0.1))
    (pad 8 thru_hole rect (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 SDA) (solder_mask_margin 0.1))
    (pad 9 thru_hole rect (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 SDA) (solder_mask_margin 0.1))
  )
  (module mrmeeseeks:Power_Rail-01x09 (layer F.Cu) (tedit 5AC7D21B)
    (at 118.364 173.736 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 90) (layer F.Fab) hide)
    (fp_text value Conn_01x09 (at 0 17.57 90) (layer F.Fab))
    (fp_text user %R (at 0 7.62 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SCL) (solder_mask_margin 0.1))
    (pad 2 thru_hole rect (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SCL) (solder_mask_margin 0.1))
    (pad 3 thru_hole rect (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SCL) (solder_mask_margin 0.1))
    (pad 4 thru_hole rect (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SCL) (solder_mask_margin 0.1))
    (pad 5 thru_hole rect (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SCL) (solder_mask_margin 0.1))
    (pad 6 thru_hole rect (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SCL) (solder_mask_margin 0.1))
    (pad 7 thru_hole rect (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SCL) (solder_mask_margin 0.1))
    (pad 8 thru_hole rect (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SCL) (solder_mask_margin 0.1))
    (pad 9 thru_hole rect (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SCL) (solder_mask_margin 0.1))
  )
  (module mrmeeseeks:badgelife-shitty-label-3.3v (layer F.Cu) (tedit 0)
    (at 113.4 162.2 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module mrmeeseeks:badgelife-shitty-label-sda (layer F.Cu) (tedit 0)
    (at 128.2 148.8)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module mrmeeseeks:badgelife-shitty-label-scl (layer F.Cu) (tedit 0)
    (at 128.4 175.7)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module mrmeeseeks:badgelife-shitty-label-gnd (layer F.Cu) (tedit 0)
    (at 143.7 162.3 270)
    (fp_text reference G*** (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer F.SilkS) hide)
  )
  (module mrmeeseeks:badgelife-shitty-devboard-silk (layer F.Cu) (tedit 0)
    (at 128.9 144.6)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_line (start 145.05 145.95) (end 145.05 144.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.8 141) (end 119.25 141) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.8 141) (end 118.1 141) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.9 145.45) (end 111.95 145.45) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.9 146) (end 111.9 145.45) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138 183.1) (end 118.15 183.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145 145.3) (end 145 144.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.95 145.7) (end 111.95 175.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145 144.95) (end 145 177.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 138.55 176.65) (end 145 177.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.9 175.65) (end 111.9 176.65) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 118.4 176.6) (end 118.1 183.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.6 141.05) (end 140 141.05) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 140.65 145.45) (end 139.95 141.05) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 117.05 146.15) (end 111.9 145.55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 6.500769 (width 0.3) (layer Dwgs.User)
    (gr_text "6.501 mm" (at 99.902029 145.192277 270.881404) (layer Dwgs.User))
    (feature1 (pts (xy 115.7 148.2) (xy 98.602189 148.463044)))
    (feature2 (pts (xy 115.6 141.7) (xy 98.502189 141.963044)))
    (crossbar (pts (xy 101.20187 141.92151) (xy 101.30187 148.42151)))
    (arrow1a (pts (xy 101.30187 148.42151) (xy 100.69819 147.30416)))
    (arrow1b (pts (xy 101.30187 148.42151) (xy 101.870893 147.286119)))
    (arrow2a (pts (xy 101.20187 141.92151) (xy 100.632847 143.056901)))
    (arrow2b (pts (xy 101.20187 141.92151) (xy 101.80555 143.03886)))
  )
  (dimension 27.2 (width 0.3) (layer Dwgs.User)
    (gr_text "27.200 mm" (at 128.5 138.85) (layer Dwgs.User))
    (feature1 (pts (xy 142.1 149) (xy 142.1 137.5)))
    (feature2 (pts (xy 114.9 149) (xy 114.9 137.5)))
    (crossbar (pts (xy 114.9 140.2) (xy 142.1 140.2)))
    (arrow1a (pts (xy 142.1 140.2) (xy 140.973496 140.786421)))
    (arrow1b (pts (xy 142.1 140.2) (xy 140.973496 139.613579)))
    (arrow2a (pts (xy 114.9 140.2) (xy 116.026504 140.786421)))
    (arrow2b (pts (xy 114.9 140.2) (xy 116.026504 139.613579)))
  )
  (dimension 2.54 (width 0.3) (layer Dwgs.User)
    (gr_text "2.540 mm" (at 145.876 152.146 90) (layer Dwgs.User))
    (feature1 (pts (xy 138.684 150.876) (xy 147.226 150.876)))
    (feature2 (pts (xy 138.684 153.416) (xy 147.226 153.416)))
    (crossbar (pts (xy 144.526 153.416) (xy 144.526 150.876)))
    (arrow1a (pts (xy 144.526 150.876) (xy 145.112421 152.002504)))
    (arrow1b (pts (xy 144.526 150.876) (xy 143.939579 152.002504)))
    (arrow2a (pts (xy 144.526 153.416) (xy 145.112421 152.289496)))
    (arrow2b (pts (xy 144.526 153.416) (xy 143.939579 152.289496)))
  )
  (dimension 2.54 (width 0.3) (layer Dwgs.User)
    (gr_text "2.540 mm" (at 145.622 172.466 270) (layer Dwgs.User))
    (feature1 (pts (xy 138.684 173.736) (xy 146.972 173.736)))
    (feature2 (pts (xy 138.684 171.196) (xy 146.972 171.196)))
    (crossbar (pts (xy 144.272 171.196) (xy 144.272 173.736)))
    (arrow1a (pts (xy 144.272 173.736) (xy 143.685579 172.609496)))
    (arrow1b (pts (xy 144.272 173.736) (xy 144.858421 172.609496)))
    (arrow2a (pts (xy 144.272 171.196) (xy 143.685579 172.322504)))
    (arrow2b (pts (xy 144.272 171.196) (xy 144.858421 172.322504)))
  )
)
