(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 0.7874)
    (drawings 25)
    (tracks 141)
    (zones 0)
    (modules 30)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu mixed)
    (1 In1.Cu mixed)
    (2 In2.Cu mixed)
    (31 B.Cu mixed)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.508)
    (user_trace_width 0.1016)
    (user_trace_width 0.127)
    (user_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (trace_clearance 0.1524)
    (zone_clearance 0.127)
    (zone_45_only yes)
    (trace_min 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.4572)
    (via_min_drill 0.2032)
    (user_via 0.4572 0.2032)
    (user_via 0.6858 0.3302)
    (user_via 0.8128 0.4064)
    (user_via 1.2192 0.6096)
    (user_via 1.4224 0.8128)
    (blind_buried_vias_allowed yes)
    (uvia_size 0.3302)
    (uvia_drill 0.2032)
    (uvias_allowed yes)
    (uvia_min_size 0.2032)
    (uvia_min_drill 0.1016)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.78 2.78)
    (pad_drill 1.78)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7EFFFE7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./gerbers"))
  )
  (net 0 "")
  (net 1 /BIAS_IN)
  (net 2 /3.3VA)
  (net 3 /BIAS)
  (net 4 /SHDNn)
  (net 5 /Vcm2V)
  (net 6 /Vsum)
  (net 7 /Vout-)
  (net 8 /Vout+)
  (net 9 /SDA)
  (net 10 /SCL)
  (net 11 /BIAS_R)
  (net 12 /GND)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3302)
    (uvia_drill 0.2032)
    (add_net /3.3VA)
    (add_net /BIAS)
    (add_net /BIAS_IN)
    (add_net /BIAS_R)
    (add_net /GND)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /SHDNn)
    (add_net /Vcm2V)
    (add_net /Vout+)
    (add_net /Vout-)
    (add_net /Vsum)
  )
  (net_class 10mil ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.8128)
    (via_drill 0.4064)
    (uvia_dia 0.3048)
    (uvia_drill 0.2032)
  )
  (net_class 15mil ""
    (clearance 0.1524)
    (trace_width 0.381)
    (via_dia 0.8128)
    (via_drill 0.4064)
    (uvia_dia 0.3048)
    (uvia_drill 0.2032)
  )
  (net_class 20mil ""
    (clearance 0.1524)
    (trace_width 0.508)
    (via_dia 1.2192)
    (via_drill 0.6096)
    (uvia_dia 0.3302)
    (uvia_drill 0.2032)
  )
  (net_class 25mil ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 1.4224)
    (via_drill 0.8128)
    (uvia_dia 0.3302)
    (uvia_drill 0.2032)
  )
  (net_class 6mil ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3302)
    (uvia_drill 0.2032)
  )
  (net_class 8mil ""
    (clearance 0.1524)
    (trace_width 0.2032)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3302)
    (uvia_drill 0.2032)
  )
  (module MSAG_Misc:R_0805 (layer F.Cu) (tedit 5BBB67CF)
    (at -17.3736 -7.2898 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference Rb2 (at 3.1242 0.0254) (layer F.SilkS))
    (fp_text value TBD (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /BIAS_IN))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /BIAS_R))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:msag_logo2_0.5in (layer F.Cu) (tedit 0)
    (at -1.524 18.288)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module MSAG_Misc:goddard_rocket_0.3inA (layer F.Cu) (tedit 0)
    (at -20.066 15.748)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module MSAG_Misc:nasa_logo_0.3inA (layer F.Cu) (tedit 0)
    (at -10.922 17.018)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module MSAG_Misc:BurstCube_bwA_0p5in (layer F.Cu) (tedit 0)
    (at 10.16 14.478)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module MSAG_Misc:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C52ECC1)
    (at -20.701 -12.7)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /BIAS))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /BIAS_R))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C52ECC1)
    (at 9.017 -12.7)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JVDDH1 (at -2.413 1.143 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /3.3VA))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:BurstCube_bwB_0p3in (layer F.Cu) (tedit 0)
    (at -22.098 -17.1958)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module MSAG_Misc:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C52ECC1)
    (at -7.4168 -1.016 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JBIASH1 (at 2.286 1.4224 180) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /BIAS_IN))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5C52ECD9)
    (at 2.921 8.763)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JEN1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /3.3VA))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /SHDNn))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805 (layer F.Cu) (tedit 5BBB67CF)
    (at -12.954 5.334 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference Rpd1 (at 0.127 1.8796) (layer F.SilkS))
    (fp_text value 2.7k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /SDA))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 /3.3VA))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805 (layer F.Cu) (tedit 5BBB67CF)
    (at -6.35 5.334 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference Rpc1 (at 0.0254 2.0066) (layer F.SilkS))
    (fp_text value 2.7k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /SCL))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 /3.3VA))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_1206_HandSoldering (layer F.Cu) (tedit 5BBB67FD)
    (at -17.272 -4.699 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference Rb1 (at 4.2164 0.1524 270) (layer F.SilkS))
    (fp_text value 10 (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 /BIAS_IN))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 /BIAS_R))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:SMA_TH (layer F.Cu) (tedit 5C81344B)
    (at 0.762 -11.684)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (fp_text reference JVDD1 (at 0 -4.572) (layer F.SilkS))
    (fp_text value SMA (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.55) (layer F.Fab))
    (pad 5 thru_hole circle (at 2.54 2.54) (size 2.2098 2.2098) (drill 1.4986) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 4 thru_hole circle (at -2.54 2.54) (size 2.2098 2.2098) (drill 1.4986) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 3 thru_hole circle (at -2.54 -2.54) (size 2.2098 2.2098) (drill 1.4986) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.2098 2.2098) (drill 1.4986) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.1082 2.1082) (drill 1.397) (layers *.Cu *.Mask)
      (net 2 /3.3VA))
    (model ${MSAG}/MSAG_KiCad3d/SMA_VERTICAL_TH.stp
      (offset (xyz 0 0 9.4742))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:SSMB_TH (layer F.Cu) (tedit 5D5FD4D3)
    (at 2.9718 -3.9624 90)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (fp_text reference JOUTP1 (at 0.4572 -3.175 270) (layer F.SilkS))
    (fp_text value SSMB (at 5.588 0.508 90) (layer F.Fab))
    (fp_text user %R (at 4.318 -1.27 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 8 /Vout+))
    (pad 2 thru_hole circle (at -1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 3 thru_hole circle (at -1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 4 thru_hole circle (at 1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 5 thru_hole circle (at 1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 12 /GND))
    (model ${MSAG}/MSAG_KiCad3d/ssmb_straight_7209-1511-050.STEP
      (offset (xyz 0 0 6.7))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module MSAG_Misc:SSMB_TH (layer F.Cu) (tedit 5D5FD4D3)
    (at 2.9972 1.4732 90)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (fp_text reference JOUTN1 (at -0.4318 -3.1242 90) (layer F.SilkS))
    (fp_text value SSMB (at 5.588 0.508 90) (layer F.Fab))
    (fp_text user %R (at 4.318 -1.27 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 7 /Vout-))
    (pad 2 thru_hole circle (at -1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 3 thru_hole circle (at -1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 4 thru_hole circle (at 1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 5 thru_hole circle (at 1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 12 /GND))
    (model ${MSAG}/MSAG_KiCad3d/ssmb_straight_7209-1511-050.STEP
      (offset (xyz 0 0 6.7))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5C52ECD9)
    (at 8.382 -3.556)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JOUT1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /Vout+))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /Vout-))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_2x02_Pitch2.54mm (layer F.Cu) (tedit 5E44A200)
    (at -18.161 8.636)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference JHK1 (at 1.016 -2.33) (layer F.SilkS))
    (fp_text value Conn_02x02_Odd_Even (at 1.27 4.87) (layer F.Fab))
    (fp_text user %R (at 1.27 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /Vcm2V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /Vsum))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /GND))
    (model ${MSAG}/MSAG_KiCad3d/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_2x02_Pitch2.54mm (layer F.Cu) (tedit 5E44A200)
    (at -11.4935 8.636)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference JD1 (at 1.27 -2.33) (layer F.SilkS))
    (fp_text value Conn_02x02_Odd_Even (at 1.27 4.87) (layer F.Fab))
    (fp_text user %R (at 1.27 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /SDA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /SDA))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /GND))
    (model ${MSAG}/MSAG_KiCad3d/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_2x02_Pitch2.54mm (layer F.Cu) (tedit 5E44A200)
    (at -4.826 8.636)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference JC1 (at 1.27 -2.33) (layer F.SilkS))
    (fp_text value Conn_02x02_Odd_Even (at 1.27 4.87) (layer F.Fab))
    (fp_text user %R (at 1.27 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /SCL))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /SCL))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /GND))
    (model ${MSAG}/MSAG_KiCad3d/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:BNC_TE-5-1634503-1 (layer F.Cu) (tedit 5C5B374F)
    (at -10.795 -14.351)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (fp_text reference JBIAS1 (at 0 -4.572) (layer F.SilkS))
    (fp_text value BNC (at 0 0.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.55) (layer F.Fab))
    (pad 5 thru_hole circle (at 3.23 3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 4 thru_hole circle (at -3.23 3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 3 thru_hole circle (at -3.23 -3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 2 thru_hole circle (at 3.23 -3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 /BIAS_IN))
    (model ${MSAG}/MSAG_KiCad3d/TE-5-1634503-1.stp
      (offset (xyz 0 0 13.33499979972839))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:NANO_25_FLYLEADS_MALE (layer F.Cu) (tedit 5E5ED198)
    (at 17.78 0 270)
    (fp_text reference JB1 (at -17.78 -2.54 270) (layer F.SilkS))
    (fp_text value NANO_25_MALE (at -0.1778 -3.8608 90) (layer F.Fab))
    (fp_text user 24 (at 11.43 0 90) (layer F.SilkS))
    (fp_text user 21 (at 3.81 0 90) (layer F.SilkS))
    (fp_text user 20 (at 1.27 0 90) (layer F.SilkS))
    (fp_text user 26 (at 13.97 0 90) (layer F.SilkS))
    (fp_text user 23 (at 8.89 0 90) (layer F.SilkS))
    (fp_text user 22 (at 6.35 0 90) (layer F.SilkS))
    (fp_text user 19 (at -1.27 0 90) (layer F.SilkS))
    (fp_text user 16 (at -8.89 0 90) (layer F.SilkS))
    (fp_text user 18 (at -3.81 0 90) (layer F.SilkS))
    (fp_text user 17 (at -6.35 0 90) (layer F.SilkS))
    (fp_text user 15 (at -11.43 0 90) (layer F.SilkS))
    (fp_text user 14 (at -13.97 0 90) (layer F.SilkS))
    (fp_text user 13 (at 15.24 -2.54 90) (layer F.SilkS))
    (fp_text user 12 (at 12.7 -2.54 90) (layer F.SilkS))
    (fp_text user 11 (at 10.16 -2.54 90) (layer F.SilkS))
    (fp_text user 10 (at 7.62 -2.54 90) (layer F.SilkS))
    (fp_text user 9 (at 5.08 -2.54 90) (layer F.SilkS))
    (fp_text user 8 (at 2.54 -2.54 90) (layer F.SilkS))
    (fp_text user 7 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text user 6 (at -2.54 -2.54 90) (layer F.SilkS))
    (fp_text user 5 (at -5.08 -2.54 90) (layer F.SilkS))
    (fp_text user 4 (at -7.62 -2.54 90) (layer F.SilkS))
    (fp_text user 3 (at -10.16 -2.54 90) (layer F.SilkS))
    (fp_text user 2 (at -12.7 -2.54 90) (layer F.SilkS))
    (fp_text user 1 (at -15.24 -2.54 90) (layer F.SilkS))
    (pad 25 thru_hole circle (at 13.97 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 4 /SHDNn))
    (pad 24 thru_hole circle (at 11.43 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 5 /Vcm2V))
    (pad 23 thru_hole circle (at 8.89 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 6 /Vsum))
    (pad 21 thru_hole circle (at 3.81 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 7 /Vout-))
    (pad 22 thru_hole circle (at 6.35 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 20 thru_hole circle (at 1.27 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 8 /Vout+))
    (pad 16 thru_hole circle (at -8.89 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 2 /3.3VA))
    (pad 18 thru_hole circle (at -3.81 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 15 thru_hole circle (at -11.43 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 2 /3.3VA))
    (pad 14 thru_hole circle (at -13.97 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 17 thru_hole circle (at -6.35 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 19 thru_hole circle (at -1.27 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 13 thru_hole circle (at 15.24 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 9 /SDA))
    (pad 12 thru_hole circle (at 12.7 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 10 /SCL))
    (pad 11 thru_hole circle (at 10.16 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 3 /BIAS))
    (pad 10 thru_hole circle (at 7.62 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 9 thru_hole circle (at 5.08 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 8 thru_hole circle (at 2.54 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 3 /BIAS))
    (pad 4 thru_hole circle (at -7.62 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 3 /BIAS))
    (pad 3 thru_hole circle (at -10.16 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 2 thru_hole circle (at -12.7 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 3 /BIAS))
    (pad 5 thru_hole circle (at -5.08 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 6 thru_hole circle (at -2.54 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 27 thru_hole circle (at 19.05 0 90) (size 3.656 3.656) (drill 2.64) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 26 thru_hole circle (at -19.05 0 90) (size 3.656 3.656) (drill 2.64) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 7 thru_hole circle (at 0 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 1 thru_hole rect (at -15.24 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
  )
  (module MSAG_Misc:NANO_25_FLYLEADS_MALE (layer F.Cu) (tedit 5E5ED198)
    (at -26.289 0 270)
    (fp_text reference JA1 (at -16.256 2.159 270) (layer F.SilkS))
    (fp_text value NANO_25_MALE (at -0.1778 -3.8608 90) (layer F.Fab))
    (fp_text user 24 (at 11.43 0 90) (layer F.SilkS))
    (fp_text user 21 (at 3.81 0 90) (layer F.SilkS))
    (fp_text user 20 (at 1.27 0 90) (layer F.SilkS))
    (fp_text user 26 (at 13.97 0 90) (layer F.SilkS))
    (fp_text user 23 (at 8.89 0 90) (layer F.SilkS))
    (fp_text user 22 (at 6.35 0 90) (layer F.SilkS))
    (fp_text user 19 (at -1.27 0 90) (layer F.SilkS))
    (fp_text user 16 (at -8.89 0 90) (layer F.SilkS))
    (fp_text user 18 (at -3.81 0 90) (layer F.SilkS))
    (fp_text user 17 (at -6.35 0 90) (layer F.SilkS))
    (fp_text user 15 (at -11.43 0 90) (layer F.SilkS))
    (fp_text user 14 (at -13.97 0 90) (layer F.SilkS))
    (fp_text user 13 (at 15.24 -2.54 90) (layer F.SilkS))
    (fp_text user 12 (at 12.7 -2.54 90) (layer F.SilkS))
    (fp_text user 11 (at 10.16 -2.54 90) (layer F.SilkS))
    (fp_text user 10 (at 7.62 -2.54 90) (layer F.SilkS))
    (fp_text user 9 (at 5.08 -2.54 90) (layer F.SilkS))
    (fp_text user 8 (at 2.54 -2.54 90) (layer F.SilkS))
    (fp_text user 7 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text user 6 (at -2.54 -2.54 90) (layer F.SilkS))
    (fp_text user 5 (at -5.08 -2.54 90) (layer F.SilkS))
    (fp_text user 4 (at -7.62 -2.54 90) (layer F.SilkS))
    (fp_text user 3 (at -10.16 -2.54 90) (layer F.SilkS))
    (fp_text user 2 (at -12.7 -2.54 90) (layer F.SilkS))
    (fp_text user 1 (at -15.24 -2.54 90) (layer F.SilkS))
    (pad 25 thru_hole circle (at 13.97 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 4 /SHDNn))
    (pad 24 thru_hole circle (at 11.43 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 5 /Vcm2V))
    (pad 23 thru_hole circle (at 8.89 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 6 /Vsum))
    (pad 21 thru_hole circle (at 3.81 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 7 /Vout-))
    (pad 22 thru_hole circle (at 6.35 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 20 thru_hole circle (at 1.27 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 8 /Vout+))
    (pad 16 thru_hole circle (at -8.89 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 2 /3.3VA))
    (pad 18 thru_hole circle (at -3.81 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 15 thru_hole circle (at -11.43 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 2 /3.3VA))
    (pad 14 thru_hole circle (at -13.97 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 17 thru_hole circle (at -6.35 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 19 thru_hole circle (at -1.27 1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 13 thru_hole circle (at 15.24 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 9 /SDA))
    (pad 12 thru_hole circle (at 12.7 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 10 /SCL))
    (pad 11 thru_hole circle (at 10.16 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 3 /BIAS))
    (pad 10 thru_hole circle (at 7.62 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 9 thru_hole circle (at 5.08 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 8 thru_hole circle (at 2.54 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 3 /BIAS))
    (pad 4 thru_hole circle (at -7.62 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 3 /BIAS))
    (pad 3 thru_hole circle (at -10.16 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 2 thru_hole circle (at -12.7 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 3 /BIAS))
    (pad 5 thru_hole circle (at -5.08 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 6 thru_hole circle (at -2.54 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 27 thru_hole circle (at 19.05 0 90) (size 3.656 3.656) (drill 2.64) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 26 thru_hole circle (at -19.05 0 90) (size 3.656 3.656) (drill 2.64) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 7 thru_hole circle (at 0 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
    (pad 1 thru_hole rect (at -15.24 -1.27 90) (size 1.218 1.218) (drill 0.71) (layers *.Cu *.Mask)
      (net 12 /GND))
  )
  (module MSAG_Misc:C_0805 (layer F.Cu) (tedit 5BB7E3B0)
    (at 13.1572 -3.8608 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4P1 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 0.1u_25V (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /3.3VA))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /GND))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0805 (layer F.Cu) (tedit 5BB7E3B0)
    (at 13.1318 -7.0104 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3P1 (at 0 -1.6256) (layer F.SilkS))
    (fp_text value 0.1u_25V (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /3.3VA))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /GND))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_1210 (layer F.Cu) (tedit 5BB7E40E)
    (at -19.304 -1.016 270)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C3B1 (at 0 2.2098 90) (layer F.SilkS))
    (fp_text value 4.7u_100V (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 11 /BIAS_R))
    (pad 2 smd rect (at 1.5 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 12 /GND))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0805 (layer F.Cu) (tedit 5BB7E3B0)
    (at 13.1064 -10.1346 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2P1 (at -0.0254 -1.6256) (layer F.SilkS))
    (fp_text value 1u_25V (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /3.3VA))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /GND))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0805 (layer F.Cu) (tedit 5BB7E3B0)
    (at -15.367 -1.524 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2B1 (at 0.1778 1.6002 90) (layer F.SilkS))
    (fp_text value 1u_100V (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /BIAS_R))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /GND))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0805 (layer F.Cu) (tedit 5BB7E3B0)
    (at 13.1064 -13.1572 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1P1 (at 0 -1.5494) (layer F.SilkS))
    (fp_text value 10u_25V (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /3.3VA))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /GND))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0805 (layer F.Cu) (tedit 5BB7E3B0)
    (at -12.192 -3.937 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1B1 (at -0.0254 -1.651 90) (layer F.SilkS))
    (fp_text value 1u_100V (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /BIAS_IN))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /GND))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text SCL (at -3.3782 2.6162) (layer F.SilkS))
  (gr_text SHDNn (at -5.969 13.97) (layer F.SilkS))
  (gr_text SDA (at -11.3284 2.2606) (layer F.SilkS))
  (gr_text GND (at -5.588 -6.604) (layer F.SilkS))
  (gr_text BIAS_IN (at -10.668 -6.604) (layer F.SilkS))
  (gr_text 3.3VA (at -18.288 2.54) (layer F.SilkS))
  (gr_text GND (at -21.082 2.54) (layer F.SilkS))
  (gr_text JUMPER (at -23.368 -18.542) (layer F.SilkS))
  (gr_text BIAS (at -22.098 -20.066) (layer F.SilkS))
  (gr_text "BurstCube IDAB Rev1 BoB\n03/2020" (at -4.572 -19.558) (layer F.SilkS))
  (gr_line (start -29.21 21.59) (end -29.21 -21.59) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 21.59 21.59) (end -29.21 21.59) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 21.59 -21.59) (end 21.59 21.59) (layer Edge.Cuts) (width 0.15))
  (gr_line (start -29.21 -21.59) (end 21.59 -21.59) (layer Edge.Cuts) (width 0.15))
  (zone (net 12) (net_name /GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -29.21 -21.59) (xy -29.21 21.59) (xy 21.59 21.59) (xy 21.59 -21.59)
      )
    )
  )
  (zone (net 3) (net_name /BIAS) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21.59 21.59) (xy -29.21 21.59) (xy -29.21 -21.59) (xy 21.59 -21.59)
      )
    )
    (polygon
      (pts
        (xy -19.304 -18.923) (xy -19.304 -11.303) (xy -21.59 -11.303) (xy -21.59 15.621) (xy 18.034 15.621)
        (xy 18.034 -13.843) (xy 18.034 -16.256) (xy 16.256 -16.256) (xy 14.859 -16.256) (xy 10.795 -18.923)
      )
    )
  )
  (zone (net 2) (net_name /3.3VA) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -29.21 -21.59) (xy -29.21 21.59) (xy 21.59 21.59) (xy 21.59 -21.59)
      )
    )
  )
  (zone (net 2) (net_name /3.3VA) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 13.208 -14.478) (xy 13.208 -2.54) (xy 17.526 -2.54) (xy 17.526 -14.478)
      )
    )
  )
  (zone (net 12) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.827 -15.113) (xy 12.827 -1.778) (xy 10.795 -1.778) (xy 10.795 -8.509) (xy 7.239 -8.509)
        (xy 7.239 -11.557) (xy 10.795 -11.557) (xy 10.795 -15.113)
      )
    )
  )
)
