<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="1.42875" y1="0.9525" x2="29.03125" y2="0.9525" width="0" layer="20"/>
<wire x1="29.03125" y1="0.9525" x2="29.03125" y2="19.355" width="0" layer="20"/>
<wire x1="29.03125" y1="19.355" x2="1.42875" y2="19.355" width="0" layer="20"/>
<wire x1="1.42875" y1="19.355" x2="1.42875" y2="0.9525" width="0" layer="20"/>
<text>SRAM2FRAM Converter</text>
<text>Designed in Thailand
By TinLethax</text>
<text>rev3</text>
<text>OSH</text>
<text>For TI-82</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP15R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="FM18W08">
<description>FM18W08</description>
<packages>
<package name="SOIC127P1032X267-28N">
<description>28-SOIC, 1.27 mm pitch, 10.32 mm span, 17.91 X 7.50 X 2.67 mm body
&lt;p&gt;28-pin SOIC package with 1.27 mm pitch, 10.32 mm span with body size 17.91 X 7.50 X 2.67 mm&lt;/p&gt;</description>
</package>
<package name="SOIC-28N-INVERTED">
<description>28-SOIC, 1.27 mm pitch, 10.32 mm span, 17.91 X 7.50 X 2.67 mm body
&lt;p&gt;28-pin SOIC package with 1.27 mm pitch, 10.32 mm span with body size 17.91 X 7.50 X 2.67 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="stm8s103k3">
<description>STM8S103K3</description>
<packages>
<package name="QFP80P900X900X160-32N">
<description>32-QFP, 0.80 mm pitch, 9.00 mm span, 7.00 X 7.00 X 1.60 mm body
&lt;p&gt;32-pin QFP package with 0.80 mm pitch, 9.00 mm lead span1 X 9.00 mm lead span2 with body size 7.00 X 7.00 X 1.60 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="oshw">
<description>&lt;p&gt;&lt;strong&gt;Open Source Hardware PCB Logos&lt;/strong&gt;
&lt;p&gt;A simple polygon based version of the OSHWA logos for use on Eagle PCB's
&lt;p&gt;For use please refer to the OSHWA definition at &lt;a href="http://www.oshwa.org/definition/"&gt;http://www.oshwa.org/definition/&lt;/a&gt;
&lt;p&gt;Based on the NBitWonder version (&lt;a href="http://nbitwonder.com"&gt;http://nbitwonder.com&lt;/a&gt;)
&lt;p&gt;&lt;strong&gt;Andrew Cooper&lt;/strong&gt;&lt;br&gt;28Nov2016&lt;br&gt;&lt;a href="http://www.darkerview.com"&gt;www.DarkerView.com&lt;/a&gt;</description>
<packages>
<package name="OSHW_5MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="adafruit" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="C0603" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SWIM" library="testpad" package="TP15R" value="TPSQTP15R">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="RST" library="testpad" package="TP15R" value="TPSQTP15R">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="FM18W08" package="SOIC127P1032X267-28N" value="FM18W08">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PAD" library="FM18W08" package="SOIC-28N-INVERTED" value="FM18W08-INVERTED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="stm8s103k3" package="QFP80P900X900X160-32N" value="STM8S103K3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GOLD_ORB_SM1" library="oshw" package="OSHW_5MM" value="OSHWLOGOLOGO5MM"/>
<element name="R1" library="adafruit" package="R0603" value="47k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="A0">
<contactref element="U1" pad="10"/>
<contactref element="PAD" pad="10"/>
<contactref element="U2" pad="9"/>
</signal>
<signal name="A1">
<contactref element="U1" pad="9"/>
<contactref element="PAD" pad="9"/>
<contactref element="U2" pad="10"/>
</signal>
<signal name="A2">
<contactref element="U1" pad="8"/>
<contactref element="PAD" pad="8"/>
<contactref element="U2" pad="11"/>
</signal>
<signal name="A3">
<contactref element="U1" pad="7"/>
<contactref element="PAD" pad="7"/>
<contactref element="U2" pad="12"/>
</signal>
<signal name="A4">
<contactref element="U1" pad="6"/>
<contactref element="PAD" pad="6"/>
<contactref element="U2" pad="13"/>
</signal>
<signal name="A5">
<contactref element="U1" pad="5"/>
<contactref element="PAD" pad="5"/>
<contactref element="U2" pad="14"/>
</signal>
<signal name="A6">
<contactref element="U1" pad="4"/>
<contactref element="PAD" pad="4"/>
<contactref element="U2" pad="15"/>
</signal>
<signal name="A7">
<contactref element="U1" pad="3"/>
<contactref element="PAD" pad="3"/>
<contactref element="U2" pad="16"/>
</signal>
<signal name="A8">
<contactref element="U2" pad="18"/>
<contactref element="U1" pad="25"/>
<contactref element="PAD" pad="25"/>
</signal>
<signal name="A9">
<contactref element="U2" pad="19"/>
<contactref element="U1" pad="24"/>
<contactref element="PAD" pad="24"/>
</signal>
<signal name="A10">
<contactref element="U2" pad="20"/>
<contactref element="U1" pad="21"/>
<contactref element="PAD" pad="21"/>
</signal>
<signal name="A11">
<contactref element="U2" pad="21"/>
<contactref element="U1" pad="23"/>
<contactref element="PAD" pad="23"/>
</signal>
<signal name="A12">
<contactref element="U2" pad="22"/>
<contactref element="U1" pad="2"/>
<contactref element="PAD" pad="2"/>
</signal>
<signal name="A13">
<contactref element="U2" pad="23"/>
<contactref element="U1" pad="26"/>
<contactref element="PAD" pad="26"/>
</signal>
<signal name="A14">
<contactref element="U2" pad="24"/>
<contactref element="U1" pad="1"/>
<contactref element="PAD" pad="1"/>
</signal>
<signal name="/CE_HOST">
<contactref element="U2" pad="3"/>
<contactref element="PAD" pad="20"/>
</signal>
<signal name="/CE_FRAM">
<contactref element="U2" pad="7"/>
<contactref element="U1" pad="20"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="C1" pad="1"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="+5V">
<contactref element="PAD" pad="28"/>
<contactref element="U1" pad="28"/>
<contactref element="U2" pad="6"/>
<contactref element="C2" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U2" pad="4"/>
<contactref element="PAD" pad="14"/>
<contactref element="U1" pad="14"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="D0">
<contactref element="U1" pad="11"/>
<contactref element="PAD" pad="11"/>
</signal>
<signal name="D1">
<contactref element="U1" pad="12"/>
<contactref element="PAD" pad="12"/>
</signal>
<signal name="D4">
<contactref element="U1" pad="16"/>
<contactref element="PAD" pad="16"/>
</signal>
<signal name="D5">
<contactref element="U1" pad="17"/>
<contactref element="PAD" pad="17"/>
</signal>
<signal name="D6">
<contactref element="U1" pad="18"/>
<contactref element="PAD" pad="18"/>
</signal>
<signal name="D7">
<contactref element="U1" pad="19"/>
<contactref element="PAD" pad="19"/>
</signal>
<signal name="D2">
<contactref element="PAD" pad="13"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="D3">
<contactref element="PAD" pad="15"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="/WE">
<contactref element="U1" pad="27"/>
<contactref element="PAD" pad="27"/>
</signal>
<signal name="/OE">
<contactref element="PAD" pad="22"/>
<contactref element="U1" pad="22"/>
</signal>
<signal name="SWIM">
<contactref element="SWIM" pad="TP"/>
<contactref element="U2" pad="26"/>
</signal>
<signal name="RST">
<contactref element="RST" pad="TP"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$5">
</signal>
<signal name="N$6">
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
<signal name="N$9">
</signal>
<signal name="N$10">
</signal>
<signal name="N$11">
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="N$14">
</signal>
<signal name="N$15">
</signal>
<signal name="N$16">
</signal>
</signals>
</board>
</drawing>
</eagle>
