(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 96)
    (no_connects 3)
    (area 104.869999 71.019999 169.970001 127.620001)
    (thickness 1.6)
    (drawings 29)
    (tracks 382)
    (zones 0)
    (modules 47)
    (nets 52)
  )
  (page A4)
  (title_block
    (title "Raspberry Pi Hat Template")
    (date 2015-12-24)
    (rev 0.1)
    (company OpenFet)
    (comment 1 "Author: Julien")
    (comment 2 "License: CERN OHL V1.2")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.1)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (trace_clearance 0.15)
    (zone_clearance 0.23)
    (zone_45_only no)
    (trace_min 0.1)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.26)
    (via_min_drill 0.16)
    (user_via 0.4 0.22)
    (user_via 1.5 0.8)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.99898)
    (pad_drill 1.00076)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory /home/mangokid/Desktop/hat_gerber/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 +24V)
  (net 4 +5V)
  (net 5 "Net-(C3-Pad2)")
  (net 6 "Net-(C5-Pad2)")
  (net 7 "Net-(D1-Pad2)")
  (net 8 "Net-(D3-Pad2)")
  (net 9 "Net-(JP1-Pad1)")
  (net 10 "Net-(P3-Pad27)")
  (net 11 "Net-(P3-Pad28)")
  (net 12 "Net-(Q1-Pad1)")
  (net 13 "Net-(R4-Pad2)")
  (net 14 "Net-(R8-Pad1)")
  (net 15 "Net-(R11-Pad1)")
  (net 16 "Net-(U1-Pad3)")
  (net 17 "Net-(U1-Pad7)")
  (net 18 "Net-(P3-Pad1)")
  (net 19 "Net-(P3-Pad3)")
  (net 20 "Net-(P3-Pad5)")
  (net 21 "Net-(P3-Pad7)")
  (net 22 "Net-(P3-Pad8)")
  (net 23 "Net-(P3-Pad10)")
  (net 24 "Net-(P3-Pad11)")
  (net 25 "Net-(P3-Pad15)")
  (net 26 "Net-(P3-Pad17)")
  (net 27 "Net-(P3-Pad29)")
  (net 28 "Net-(P3-Pad31)")
  (net 29 /GPIO12)
  (net 30 /GPIO13)
  (net 31 /GPIO16)
  (net 32 /GPIO18)
  (net 33 /GPIO19)
  (net 34 /GPIO20)
  (net 35 /GPIO21)
  (net 36 /GPIO23)
  (net 37 /GPIO24)
  (net 38 /GPIO25)
  (net 39 /GPIO26)
  (net 40 "Net-(P5-Pad3)")
  (net 41 /5V)
  (net 42 "Net-(P6-Pad3)")
  (net 43 "Net-(P6-Pad4)")
  (net 44 "Net-(P6-Pad1)")
  (net 45 "Net-(P3-Pad19)")
  (net 46 "Net-(P3-Pad13)")
  (net 47 "Net-(P3-Pad21)")
  (net 48 "Net-(P3-Pad23)")
  (net 49 "Net-(P3-Pad24)")
  (net 50 "Net-(P3-Pad26)")
  (net 51 "Net-(P4-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.2)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +24V)
    (add_net +3V3)
    (add_net +5V)
    (add_net /5V)
    (add_net /GPIO12)
    (add_net /GPIO13)
    (add_net /GPIO16)
    (add_net /GPIO18)
    (add_net /GPIO19)
    (add_net /GPIO20)
    (add_net /GPIO21)
    (add_net /GPIO23)
    (add_net /GPIO24)
    (add_net /GPIO25)
    (add_net /GPIO26)
    (add_net GND)
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad10)")
    (add_net "Net-(P3-Pad11)")
    (add_net "Net-(P3-Pad13)")
    (add_net "Net-(P3-Pad15)")
    (add_net "Net-(P3-Pad17)")
    (add_net "Net-(P3-Pad19)")
    (add_net "Net-(P3-Pad21)")
    (add_net "Net-(P3-Pad23)")
    (add_net "Net-(P3-Pad24)")
    (add_net "Net-(P3-Pad26)")
    (add_net "Net-(P3-Pad27)")
    (add_net "Net-(P3-Pad28)")
    (add_net "Net-(P3-Pad29)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P3-Pad31)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(P3-Pad7)")
    (add_net "Net-(P3-Pad8)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P5-Pad3)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P6-Pad3)")
    (add_net "Net-(P6-Pad4)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad7)")
  )
  (module w_pin_strip:pin_socket_20x2 (layer F.Cu) (tedit 580A3347)
    (at 137.42 74.82)
    (descr "Pin socket 20x2pin")
    (tags "CONN DEV")
    (fp_text reference P3 (at 24.29 3.13) (layer F.SilkS))
    (fp_text value Raspberry_Pi_+_Conn (at 0 -5.08) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -24.13 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P3-Pad1)"))
    (pad 2 thru_hole oval (at -24.13 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 41 /5V))
    (pad 3 thru_hole oval (at -21.59 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P3-Pad3)"))
    (pad 4 thru_hole oval (at -21.59 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 41 /5V))
    (pad 5 thru_hole oval (at -19.05 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(P3-Pad5)"))
    (pad 6 thru_hole oval (at -19.05 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 7 thru_hole oval (at -16.51 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(P3-Pad7)"))
    (pad 8 thru_hole oval (at -16.51 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P3-Pad8)"))
    (pad 9 thru_hole oval (at -13.97 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 10 thru_hole oval (at -13.97 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(P3-Pad10)"))
    (pad 11 thru_hole oval (at -11.43 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(P3-Pad11)"))
    (pad 12 thru_hole oval (at -11.43 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 32 /GPIO18))
    (pad 13 thru_hole oval (at -8.89 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(P3-Pad13)"))
    (pad 14 thru_hole oval (at -8.89 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 15 thru_hole oval (at -6.35 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(P3-Pad15)"))
    (pad 16 thru_hole oval (at -6.35 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 36 /GPIO23))
    (pad 17 thru_hole oval (at -3.81 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(P3-Pad17)"))
    (pad 18 thru_hole oval (at -3.81 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 37 /GPIO24))
    (pad 19 thru_hole oval (at -1.27 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(P3-Pad19)"))
    (pad 20 thru_hole oval (at -1.27 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 21 thru_hole oval (at 1.27 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(P3-Pad21)"))
    (pad 22 thru_hole oval (at 1.27 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 38 /GPIO25))
    (pad 23 thru_hole oval (at 3.81 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(P3-Pad23)"))
    (pad 24 thru_hole oval (at 3.81 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(P3-Pad24)"))
    (pad 25 thru_hole oval (at 6.35 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 26 thru_hole oval (at 6.35 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(P3-Pad26)"))
    (pad 27 thru_hole oval (at 8.89 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P3-Pad27)"))
    (pad 28 thru_hole oval (at 8.89 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P3-Pad28)"))
    (pad 29 thru_hole oval (at 11.43 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(P3-Pad29)"))
    (pad 30 thru_hole oval (at 11.43 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 31 thru_hole oval (at 13.97 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(P3-Pad31)"))
    (pad 32 thru_hole oval (at 13.97 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 29 /GPIO12))
    (pad 33 thru_hole oval (at 16.51 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 30 /GPIO13))
    (pad 34 thru_hole oval (at 16.51 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 35 thru_hole oval (at 19.05 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 33 /GPIO19))
    (pad 36 thru_hole oval (at 19.05 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 31 /GPIO16))
    (pad 37 thru_hole oval (at 21.59 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 39 /GPIO26))
    (pad 38 thru_hole oval (at 21.59 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 34 /GPIO20))
    (pad 39 thru_hole oval (at 24.13 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 40 thru_hole oval (at 24.13 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 35 /GPIO21))
    (model walter/pin_strip/pin_socket_20x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3mm locked (layer F.Cu) (tedit 5509CE9A)
    (at 166.42 74.82)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 1.00076 5.00126) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.99974 2.99974) (drill 2.99974) (layers))
  )
  (module Mounting_Holes:MountingHole_3mm locked (layer F.Cu) (tedit 5509CEA9)
    (at 166.42 123.82)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 1.00076 5.00126) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.99974 2.99974) (drill 2.99974) (layers))
  )
  (module Mounting_Holes:MountingHole_3mm locked (layer F.Cu) (tedit 5509CEA3)
    (at 108.42 123.82)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 1.00076 5.00126) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.99974 2.99974) (drill 2.99974) (layers))
  )
  (module Mounting_Holes:MountingHole_3mm locked (layer F.Cu) (tedit 5509CE9D)
    (at 108.42 74.82)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 1.00076 5.00126) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.99974 2.99974) (drill 2.99974) (layers))
  )
  (module w_smd_cap:c_elec_6.3x7.7 (layer F.Cu) (tedit 0)
    (at 108.6 113.2 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (fp_text reference C1 (at 3.7 -1.4 360) (layer F.SilkS))
    (fp_text value 50uf/50v (at 0 3.81 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 3 +24V))
    (pad 2 smd rect (at -2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_elec_6_3x7_7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0402 (layer F.Cu) (tedit 0)
    (at 123.2 124.44864 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C2 (at -1.45136 0 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 0.4826 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 3 +24V))
    (pad 2 smd rect (at -0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0402 (layer F.Cu) (tedit 0)
    (at 123.2 119.2 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C3 (at 1.5 0 90) (layer F.SilkS))
    (fp_text value 1nf (at 0 0.4826 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 3 +24V))
    (pad 2 smd rect (at -0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0402 (layer F.Cu) (tedit 0)
    (at 168.7 78.5)
    (descr "SMT capacitor, 0402")
    (fp_text reference C4 (at -1.7 0) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0402 (layer F.Cu) (tedit 0)
    (at 126 118.8 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C5 (at 1.5 0 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 0.4826 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at -0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad2)"))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_elec_4x5.3 (layer F.Cu) (tedit 0)
    (at 144.3 124 90)
    (descr "SMT capacitor, aluminium electrolytic, 4x5.3")
    (fp_text reference C6 (at -1.9 2.8 90) (layer F.SilkS))
    (fp_text value 10uf/6.3V (at 0 2.794 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.80086 0 90) (size 2.60096 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at -1.80086 0 90) (size 2.60096 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_elec_4x5_3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0402 (layer F.Cu) (tedit 0)
    (at 142.34864 121 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference C7 (at -0.45136 0.7 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_diode:do214aa (layer F.Cu) (tedit 0)
    (at 139.7 124 90)
    (descr DO214AA)
    (fp_text reference D1 (at -2 -2.4 90) (layer F.SilkS))
    (fp_text value DIODESCH (at 0 2.49936 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 2.00914 0 90) (size 1.99898 2.30124) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -2.00914 0 90) (size 1.99898 2.30124) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_diode/do214aa.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_leds:Led_0603 (layer F.Cu) (tedit 567BA339)
    (at 106.3 81.9493 90)
    (descr "SMD LED, 0603")
    (fp_text reference D3 (at -0.0507 1 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.19888 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D3-Pad2)"))
    (model walter/smd_leds/led_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0603 (layer F.Cu) (tedit 0)
    (at 167.2 85.3 90)
    (descr "SMT resistor, 0603")
    (fp_text reference JP1 (at -1.3 -0.9 90) (layer F.SilkS))
    (fp_text value JUMPER (at 0 0.6096 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 90) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(JP1-Pad1)"))
    (pad 2 smd rect (at -0.75184 0 90) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_resistors/r_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_inductors:inductor_smd_8x5mm (layer F.Cu) (tedit 567B9F50)
    (at 133 122.8 90)
    (descr "Inductor SMD, d.8mm x h.5mm")
    (fp_text reference L1 (at 2.5 -4.1 90) (layer F.SilkS))
    (fp_text value 22uH (at 0 5.4991 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.49936 0 90) (size 2.9972 7.49808) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 2.49936 0 90) (size 2.9972 7.49808) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (model walter/smd_inductors/inductor_smd_8x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_strip_2 (layer F.Cu) (tedit 0)
    (at 168.2 85.3 90)
    (descr "Pin strip 2pin")
    (tags "CONN DEV")
    (fp_text reference P1 (at -3.1 1 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0.254 -3.556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(JP1-Pad1)"))
    (model walter/pin_strip/pin_strip_2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_mkds:mkds_1,5-2 (layer F.Cu) (tedit 567BA183)
    (at 117.1 122.7)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference P2 (at -5.6 -4.9 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 5.9) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 +24V))
    (pad 2 thru_hole circle (at 2.5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model walter/conn_mkds/mkds_1,5-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_trans:sot23 (layer F.Cu) (tedit 0)
    (at 110.8 79.3 90)
    (descr SOT23)
    (fp_text reference Q1 (at 0.9 -1.1 90) (layer F.SilkS))
    (fp_text value BSS138 (at 0 0.3302 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 1.05664 90) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0 -1.05664 90) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 41 /5V))
    (pad 3 smd rect (at 0.9525 1.05664 90) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (model walter/smd_trans/sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 0)
    (at 165 84.6 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R1 (at 0 -0.4826 180) (layer F.SilkS))
    (fp_text value 1k (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(JP1-Pad1)"))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 0)
    (at 124.8 118.8 90)
    (descr "SMT resistor, 0402")
    (fp_text reference R2 (at 1.5 0 90) (layer F.SilkS))
    (fp_text value 24k (at 0 0.4826 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 3 +24V))
    (pad 2 smd rect (at -0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 0)
    (at 165 82.7 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R3 (at 1.5 0 180) (layer F.SilkS))
    (fp_text value 3.9k (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P3-Pad28)"))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 0)
    (at 165 83.6 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R5 (at 1.5 0 180) (layer F.SilkS))
    (fp_text value 3.9k (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P3-Pad27)"))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 567B9F3B)
    (at 127.1 118.8 90)
    (descr "SMT resistor, 0402")
    (fp_text reference R6 (at 1.5 0 90) (layer F.SilkS))
    (fp_text value 30k (at 0 0.4826 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at -0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad2)"))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 0)
    (at 128.4 118.8 270)
    (descr "SMT resistor, 0402")
    (fp_text reference R7 (at -1.5 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0.4826 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad2)"))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 0)
    (at 137.7 117.4 270)
    (descr "SMT resistor, 0402")
    (fp_text reference R8 (at 0 0.7 270) (layer F.SilkS))
    (fp_text value 390 (at 0 0.4826 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 0)
    (at 137.9 119.6 270)
    (descr "SMT resistor, 0402")
    (fp_text reference R9 (at 0 0.7 270) (layer F.SilkS))
    (fp_text value 240 (at 0 0.4826 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R8-Pad1)"))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 0)
    (at 106.3 79.6 270)
    (descr "SMT resistor, 0402")
    (fp_text reference R10 (at 0 -0.8 270) (layer F.SilkS))
    (fp_text value 360 (at 0 0.4826 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 0)
    (at 112.9 81.5)
    (descr "SMT resistor, 0402")
    (fp_text reference R11 (at 1.7 0) (layer F.SilkS))
    (fp_text value 10k (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 0)
    (at 110.8 81.5 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R12 (at 1.3 0.5 270) (layer F.SilkS))
    (fp_text value 47k (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_dil:msoic-8 (layer F.Cu) (tedit 567B9F54)
    (at 125.5 121.7 90)
    (descr MSOIC-8)
    (fp_text reference U1 (at 1.9 -1.4 180) (layer F.SilkS))
    (fp_text value LM3489 (at 0 0.29972 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.97536 2.30124 90) (size 0.40894 1.02108) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R4-Pad2)"))
    (pad 2 smd rect (at -0.32512 2.30124 90) (size 0.40894 1.02108) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.32512 2.30124 90) (size 0.40894 1.02108) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at 0.97536 2.30124 90) (size 0.40894 1.02108) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad2)"))
    (pad 5 smd rect (at 0.97536 -2.30124 90) (size 0.40894 1.02108) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 6 smd rect (at 0.32512 -2.30124 90) (size 0.40894 1.02108) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -0.32512 -2.30124 90) (size 0.40894 1.02108) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at -0.97536 -2.30124 90) (size 0.40894 1.02108) (layers F.Cu F.Paste F.Mask)
      (net 3 +24V))
    (model walter/smd_dil/msoic-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_dil:tssop-8 (layer F.Cu) (tedit 567BA5EA)
    (at 165.9 80.6 270)
    (descr TSSOP-8)
    (fp_text reference U2 (at -2 2 360) (layer F.SilkS))
    (fp_text value CAT24C32HU4I-GT3 (at 0 -1.143 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at -0.32258 2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.32258 2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.97536 2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.97536 2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.97536 -2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P3-Pad27)"))
    (pad 6 smd rect (at 0.32258 -2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P3-Pad28)"))
    (pad 7 smd rect (at -0.32258 -2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(JP1-Pad1)"))
    (pad 8 smd rect (at -0.97536 -2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model walter/smd_dil/tssop-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_trans:sot23-6 (layer F.Cu) (tedit 567B9E4B)
    (at 125.4 125.7 90)
    (descr SOT23-6)
    (fp_text reference U3 (at 1.9 -0.3 180) (layer F.SilkS))
    (fp_text value FDC5614P (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 1.05664 90) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (pad 3 smd rect (at 0.9525 1.05664 90) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad7)"))
    (pad 2 smd rect (at 0 1.05664 90) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (pad 4 smd rect (at 0.9525 -1.05664 90) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 3 +24V))
    (pad 6 smd rect (at -0.9525 -1.05664 90) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (pad 5 smd rect (at 0 -1.05664 90) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (model walter/smd_trans/sot23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_trans:sot223 (layer F.Cu) (tedit 0)
    (at 141.7 116.5)
    (descr SOT223)
    (fp_text reference U4 (at -2.9 -2.3) (layer F.SilkS))
    (fp_text value LM1117IMPX-ADJ (at 0 1.0414) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.30124 2.99974) (size 1.30048 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 0 2.99974) (size 1.30048 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 3 smd rect (at 2.30124 2.99974) (size 1.30048 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 4 smd rect (at 0 -2.99974) (size 3.79984 1.80086) (layers F.Cu F.Paste F.Mask))
    (model walter/smd_trans/sot223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_trans:sot23-6 (layer F.Cu) (tedit 0)
    (at 115 79.4)
    (descr SOT23-6)
    (fp_text reference U5 (at 2 -0.3 90) (layer F.SilkS))
    (fp_text value DMMT5401 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R11-Pad1)"))
    (pad 3 smd rect (at 0.9525 1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 0 1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R11-Pad1)"))
    (pad 4 smd rect (at 0.9525 -1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(Q1-Pad1)"))
    (pad 6 smd rect (at -0.9525 -1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 5 smd rect (at 0 -1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 41 /5V))
    (model walter/smd_trans/sot23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 567BA0FF)
    (at 128 124.4 270)
    (descr "SMT resistor, 0402")
    (fp_text reference R4 (at -0.6 0.7 270) (layer F.SilkS))
    (fp_text value 270 (at 0 0.4826 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R4-Pad2)"))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0402 (layer F.Cu) (tedit 567BA1DF)
    (at 144.4 113.3 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference C8 (at 0.05136 -0.720001 270) (layer F.SilkS))
    (fp_text value 1uf (at 0 0.4826 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x03 (layer F.Cu) (tedit 54E9F429)
    (at 119.6 89.6 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P5 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /GPIO18))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(P5-Pad3)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x03.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04 (layer F.Cu) (tedit 0)
    (at 156 89.6 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P6 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(P6-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /5V))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(P6-Pad3)"))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(P6-Pad4)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x04.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_ThroughHole:Resistor_Vertical_RM5mm (layer F.Cu) (tedit 0)
    (at 157.6 82.6 270)
    (descr "Resistor, Vertical, RM 5mm, 1/3W,")
    (tags "Resistor, Vertical, RM 5mm, 1/3W,")
    (fp_text reference R13 (at 2.70002 -3.29946 270) (layer F.SilkS))
    (fp_text value R (at 0 4.50088 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.49936 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 39 /GPIO26))
    (pad 2 thru_hole circle (at 2.5019 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 44 "Net-(P6-Pad1)"))
  )
  (module Resistors_ThroughHole:Resistor_Vertical_RM5mm (layer F.Cu) (tedit 0)
    (at 153.4 82 90)
    (descr "Resistor, Vertical, RM 5mm, 1/3W,")
    (tags "Resistor, Vertical, RM 5mm, 1/3W,")
    (fp_text reference R14 (at 2.70002 -3.29946 90) (layer F.SilkS))
    (fp_text value R (at 0 4.50088 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.49936 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 42 "Net-(P6-Pad3)"))
    (pad 2 thru_hole circle (at 2.5019 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 33 /GPIO19))
  )
  (module Resistors_ThroughHole:Resistor_Vertical_RM5mm (layer F.Cu) (tedit 0)
    (at 149.4 82.6 270)
    (descr "Resistor, Vertical, RM 5mm, 1/3W,")
    (tags "Resistor, Vertical, RM 5mm, 1/3W,")
    (fp_text reference R15 (at 2.70002 -3.29946 270) (layer F.SilkS))
    (fp_text value R (at 0 4.50088 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.49936 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 30 /GPIO13))
    (pad 2 thru_hole circle (at 2.5019 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 43 "Net-(P6-Pad4)"))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x08 (layer F.Cu) (tedit 0)
    (at 125.3 89.6)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P4 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(P4-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /GPIO23))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /GPIO24))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /GPIO25))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /GPIO12))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /GPIO16))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /GPIO21))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /GPIO20))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x08.wrl
      (at (xyz 0.35 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module IMAGES:CI (layer F.Cu) (tedit 0)
    (at 163 102.6 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module IMAGES:Paw (layer F.Cu) (tedit 0)
    (at 163.3 113.3 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module IMAGES:Makerspace (layer F.Cu) (tedit 0)
    (at 188.1 103.4)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module IMAGES:MakerspaceINV (layer F.Cu) (tedit 0)
    (at 154.7 108.9 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (gr_text "Stefan Abare\nGiandre Acosta\nMaurice Barnett\nYvon Feaster\nMatthew Grooms\nJonathan Hord\nOwen Phillips\nGarrett Ross\nAvery White" (at 119 103.5) (layer F.SilkS))
  (gr_text "CERN OHL V1.2" (at 169.1 116 270) (layer B.SilkS))
  (gr_text "Julien M." (at 169 116.6 90) (layer F.SilkS))
  (gr_text GND (at 119.8 114.8 90) (layer F.SilkS))
  (gr_text VPP (at 114.8 114.8 90) (layer F.SilkS))
  (gr_arc (start 149.92 108.57) (end 149.92 107.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 149.92 108.57) (end 148.92 108.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 65 (width 0.3) (layer Dwgs.User)
    (gr_text "65.000 mm" (at 137.6 135.05) (layer Dwgs.User))
    (feature1 (pts (xy 105.1 125.2) (xy 105.1 136.4)))
    (feature2 (pts (xy 170.1 125.2) (xy 170.1 136.4)))
    (crossbar (pts (xy 170.1 133.7) (xy 105.1 133.7)))
    (arrow1a (pts (xy 105.1 133.7) (xy 106.226504 133.113579)))
    (arrow1b (pts (xy 105.1 133.7) (xy 106.226504 134.286421)))
    (arrow2a (pts (xy 170.1 133.7) (xy 168.973496 133.113579)))
    (arrow2b (pts (xy 170.1 133.7) (xy 168.973496 134.286421)))
  )
  (dimension 56.5 (width 0.3) (layer Dwgs.User)
    (gr_text "56.500 mm" (at 175.45 99.45 270) (layer Dwgs.User))
    (feature1 (pts (xy 167.1 127.7) (xy 176.8 127.7)))
    (feature2 (pts (xy 167.1 71.2) (xy 176.8 71.2)))
    (crossbar (pts (xy 174.1 71.2) (xy 174.1 127.7)))
    (arrow1a (pts (xy 174.1 127.7) (xy 173.513579 126.573496)))
    (arrow1b (pts (xy 174.1 127.7) (xy 174.686421 126.573496)))
    (arrow2a (pts (xy 174.1 71.2) (xy 173.513579 72.326504)))
    (arrow2b (pts (xy 174.1 71.2) (xy 174.686421 72.326504)))
  )
  (gr_line (start 104.92 109.07) (end 104.92 124.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.92 90.07) (end 104.92 74.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 108.92 108.07) (end 105.92 108.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.92 92.07) (end 109.92 107.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.92 91.07) (end 108.92 91.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 108.92 107.07) (end 109.92 107.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 108.92 92.07) (end 108.92 91.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 105.92 109.07) (end 104.92 109.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 105.92 90.07) (end 105.92 91.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.92 123.57) (end 148.92 108.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 150.92 108.57) (end 150.92 123.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 149.92 123.57) (end 150.92 123.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 149.92 123.57) (end 149.92 124.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.92 127.57) (end 107.92 127.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.92 74.07) (end 169.92 124.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 107.92 71.07) (end 166.92 71.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 166.92 124.57) (end 169.92 124.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 107.92 74.07) (end 104.92 74.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 166.92 74.07) (end 166.92 71.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 107.92 124.57) (end 107.92 127.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 169.87 119.32) (xy 162.87 119.32) (xy 162.87 126.32) (xy 112.37 126.32) (xy 112.37 119.32)
        (xy 105.87 119.32) (xy 105.87 107.82) (xy 110.87 107.82) (xy 110.87 89.82) (xy 105.87 89.82)
        (xy 105.87 77.82) (xy 112.37 77.82) (xy 112.37 70.82) (xy 163.37 70.82) (xy 163.37 77.82)
        (xy 169.87 77.82)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 169.87 119.32) (xy 162.87 119.32) (xy 162.87 126.32) (xy 112.37 126.32) (xy 112.37 119.32)
        (xy 105.87 119.32) (xy 105.87 107.82) (xy 110.87 107.82) (xy 110.87 89.82) (xy 105.87 89.82)
        (xy 105.87 77.82) (xy 112.37 77.82) (xy 112.37 70.82) (xy 163.37 70.82) (xy 163.37 77.82)
        (xy 169.87 77.82)
      )
    )
  )
  (zone (net 7) (net_name "Net-(D1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.23))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 123.8 125.4) (xy 123.8 127) (xy 126.9 127) (xy 136.8 126.8) (xy 138.1 123.7)
        (xy 140.9 123) (xy 140.9 121) (xy 138.5 121) (xy 133.8 123.8) (xy 129.3 123.8)
        (xy 129.2 123.8) (xy 128.4 124.5) (xy 127.6 124.5) (xy 127 125.4)
      )
    )
  )
)
