(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 29)
    (no_connects 0)
    (area 118.669999 86.1592 192.909 116.212333)
    (thickness 1.6)
    (drawings 5)
    (tracks 16)
    (zones 0)
    (modules 12)
    (nets 39)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.635)
    (user_trace_width 0.635)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.381)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 1.6)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 67.945 40.005)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x000b0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "METARmap GERBER Files/"))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(J3-Pad1)")
  (net 6 "Net-(J3-Pad3)")
  (net 7 "Net-(J3-Pad5)")
  (net 8 "Net-(J3-Pad7)")
  (net 9 "Net-(J3-Pad8)")
  (net 10 "Net-(J3-Pad10)")
  (net 11 "Net-(J3-Pad11)")
  (net 12 "Net-(J3-Pad12)")
  (net 13 "Net-(J3-Pad13)")
  (net 14 "Net-(J3-Pad15)")
  (net 15 "Net-(J3-Pad16)")
  (net 16 "Net-(J3-Pad17)")
  (net 17 "Net-(J3-Pad18)")
  (net 18 "Net-(J3-Pad19)")
  (net 19 "Net-(J3-Pad21)")
  (net 20 "Net-(J3-Pad22)")
  (net 21 "Net-(J3-Pad23)")
  (net 22 "Net-(J3-Pad24)")
  (net 23 "Net-(J3-Pad26)")
  (net 24 "Net-(J3-Pad27)")
  (net 25 "Net-(J3-Pad28)")
  (net 26 "Net-(J3-Pad29)")
  (net 27 "Net-(J3-Pad31)")
  (net 28 "Net-(J3-Pad32)")
  (net 29 "Net-(J3-Pad33)")
  (net 30 "Net-(J3-Pad35)")
  (net 31 "Net-(J3-Pad36)")
  (net 32 "Net-(J3-Pad37)")
  (net 33 "Net-(J3-Pad38)")
  (net 34 "Net-(J3-Pad40)")
  (net 35 "Net-(J4-Pad3)")
  (net 36 "Net-(U1-Pad6)")
  (net 37 "Net-(U1-Pad8)")
  (net 38 "Net-(U1-Pad11)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.381)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad10)")
    (add_net "Net-(J3-Pad11)")
    (add_net "Net-(J3-Pad12)")
    (add_net "Net-(J3-Pad13)")
    (add_net "Net-(J3-Pad15)")
    (add_net "Net-(J3-Pad16)")
    (add_net "Net-(J3-Pad17)")
    (add_net "Net-(J3-Pad18)")
    (add_net "Net-(J3-Pad19)")
    (add_net "Net-(J3-Pad21)")
    (add_net "Net-(J3-Pad22)")
    (add_net "Net-(J3-Pad23)")
    (add_net "Net-(J3-Pad24)")
    (add_net "Net-(J3-Pad26)")
    (add_net "Net-(J3-Pad27)")
    (add_net "Net-(J3-Pad28)")
    (add_net "Net-(J3-Pad29)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad31)")
    (add_net "Net-(J3-Pad32)")
    (add_net "Net-(J3-Pad33)")
    (add_net "Net-(J3-Pad35)")
    (add_net "Net-(J3-Pad36)")
    (add_net "Net-(J3-Pad37)")
    (add_net "Net-(J3-Pad38)")
    (add_net "Net-(J3-Pad40)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad8)")
    (add_net VCC)
  )
  (net_class PWR-GND ""
    (clearance 0.254)
    (trace_width 0.635)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5971399F)
    (at 183.515 92.075)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 4.572 4.572) (drill 3.4544) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5971399C)
    (at 183.515 111.125)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 4.572 4.572) (drill 3.4544) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 597139A2)
    (at 122.555 111.125)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 4.572 4.572) (drill 3.4544) (layers *.Cu *.Mask))
  )
  (module Capacitors_THT:CP_Radial_D8.0mm_P3.50mm (layer F.Cu) (tedit 59713F71)
    (at 142.24 101.6)
    (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C1 (at -1.905 3.81) (layer F.SilkS))
    (fp_text value 1000uF (at 1.75 5.06) (layer F.Fab))
    (fp_text user %R (at 1.75 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 3.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D8.0mm_P3.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 597140EC)
    (at 160.655 92.71)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0 -1.778) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.905 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "MetarMap V2:PJ-102AH" (layer F.Cu) (tedit 597139B5)
    (at 133.35 103.505)
    (fp_text reference J1 (at 3.81 0.889) (layer F.SilkS))
    (fp_text value BARREL_JACK (at 0 -13) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 -6) (size 2.032 2.032) (drill 1.143) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.143) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 3 thru_hole circle (at -4.7 -3) (size 2.032 2.032) (drill 1.143) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad3)"))
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 597139B0)
    (at 121.92 101.6 180)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J2 (at 0 -2.921 360) (layer F.SilkS))
    (fp_text value GS3 (at 1.8 0 270) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.27 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at 0 0 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 1.27 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
  )
  (module Pin_Headers:Pin_Header_Straight_2x20_Pitch2.54mm (layer F.Cu) (tedit 59650533)
    (at 128.905 112.395 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J3 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_02X20 (at 1.27 50.59 90) (layer F.Fab))
    (fp_text user %R (at 1.27 24.13 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J3-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J3-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J3-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J3-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J3-Pad16)"))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J3-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J3-Pad18)"))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J3-Pad19)"))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J3-Pad21)"))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J3-Pad22)"))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad23)"))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J3-Pad24)"))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad26)"))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad27)"))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J3-Pad28)"))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J3-Pad29)"))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-Pad31)"))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-Pad32)"))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J3-Pad33)"))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J3-Pad35)"))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J3-Pad36)"))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J3-Pad37)"))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J3-Pad38)"))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J3-Pad40)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x20_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "MetarMap V2:TE_Connectivity_3-Pos_Screw_Terminal_282834-3" (layer F.Cu) (tedit 597139C2)
    (at 182.88 101.6 270)
    (fp_text reference J4 (at 4.953 -2.54 360) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x03 (at 0.2 -8.9 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 35 "Net-(J4-Pad3)"))
  )
  (module "MetarMap V2:74AHCT125" (layer F.Cu) (tedit 597139B9)
    (at 158.75 100.33)
    (fp_text reference U1 (at -1.143 0.127) (layer F.SilkS))
    (fp_text value 74AHCT125 (at 7.62 -1.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad12)"))
    (pad 3 thru_hole circle (at 5.08 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 "Net-(J4-Pad3)"))
    (pad 4 thru_hole circle (at 7.62 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 5 thru_hole circle (at 10.16 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 12.7 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 "Net-(U1-Pad6)"))
    (pad 7 thru_hole circle (at 15.24 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole circle (at 15.24 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 "Net-(U1-Pad8)"))
    (pad 9 thru_hole circle (at 12.7 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole circle (at 10.16 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 11 thru_hole circle (at 7.62 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 "Net-(U1-Pad11)"))
    (pad 12 thru_hole circle (at 5.08 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 13 thru_hole circle (at 2.54 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 14 thru_hole circle (at 0 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 VCC))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 597139A5)
    (at 122.555 92.075)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 4.572 4.572) (drill 3.4544) (layers *.Cu *.Mask))
  )
  (module F16:F16 (layer F.Cu) (tedit 59713F6A)
    (at 149.225 93.345)
    (fp_text reference G*** (at -3.175 -5.715) (layer F.SilkS) hide)
    (fp_text value LOGO (at 1.905 -5.715) (layer F.SilkS) hide)
  )
  (gr_text "METARmap v1\nBy FHT" (at 172.72 91.44) (layer F.SilkS))
  (gr_line (start 187.325 114.935) (end 187.325 88.265) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.745 88.265) (end 118.745 114.935) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 187.325 88.265) (end 118.745 88.265) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.745 114.935) (end 187.325 114.935) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.635))
    (polygon
      (pts
        (xy 118.745 88.265) (xy 118.745 114.935) (xy 187.325 114.935) (xy 187.325 88.265)
      )
    )
  )
  (zone (net 1) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 118.745 88.265) (xy 118.745 114.935) (xy 187.325 114.935) (xy 187.325 88.265)
      )
    )
  )
)
