<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="64.75" y2="0" width="0" layer="20"/>
<wire x1="64.75" y1="0" x2="64.75" y2="19.99" width="0" layer="20"/>
<wire x1="64.75" y1="19.99" x2="0" y2="19.99" width="0" layer="20"/>
<wire x1="0" y1="19.99" x2="0" y2="0" width="0" layer="20"/>
<text>goboxgizmos.com</text>
<text>Solar NiCAD Charger</text>
<text>NI2O 03/2011</text>
<text>PV-</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="INDUCTOR-1206">
</package>
<package name="DIODE-1N4001">
</package>
<package name="CPOL-RADIAL-100UF-25V">
</package>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="maxim-10">
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="0207/2V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 2.5 mm</description>
</package>
</packages>
</library>
<library name="testpad">
<packages>
<package name="P1-20Y">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="maxim-10" package="DIL08" value="MAX639">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="resistor" package="0207/2V" value="820k"/>
<element name="R2" library="resistor" package="0207/2V" value="75K"/>
<element name="R3" library="resistor" package="0207/2V" value="75K"/>
<element name="R4" library="resistor" package="0207/2V" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="SparkFun" package="INDUCTOR-1206" value="100uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun" package="CPOL-RADIAL-100UF-25V" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun" package="CPOL-RADIAL-100UF-25V" value="47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun" package="DIODE-1N4001" value="1n5817">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun" package="DIODE-1N4001" value="1n5817">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PV+" library="testpad" package="P1-20Y" value="TPPAD1-20Y">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="PV-" library="testpad" package="P1-20Y" value="TPPAD1-20Y">
<attribute name="VALUE"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="BAT+" library="testpad" package="P1-20Y" value="TPPAD1-20Y">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="BAT-" library="testpad" package="P1-20Y" value="TPPAD1-20Y">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP1" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP2" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="4"/>
<contactref element="D1" pad="A"/>
<contactref element="C2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="BAT-" pad="TP"/>
<contactref element="C1" pad="2"/>
<contactref element="PV-" pad="TP"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="5"/>
<contactref element="L1" pad="P$2"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$2">
<contactref element="L1" pad="P$1"/>
<contactref element="IC1" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="8"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="3"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="7"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="6"/>
<contactref element="R1" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="PV+" pad="TP"/>
</signal>
<signal name="N$11">
<contactref element="D2" pad="C"/>
<contactref element="BAT+" pad="TP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
