(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 283)
    (no_connects 0)
    (area 101.193599 46.799499 212.915501 134.810501)
    (thickness 1.6002)
    (drawings 29)
    (tracks 1898)
    (zones 0)
    (modules 62)
    (nets 154)
  )
  (page User 279.4 215.9)
  (title_block
    (date "6 apr 2013")
  )
  (layers
    (0 Front signal)
    (31 Back signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.762)
    (user_trace_width 0.50546)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (user_trace_width 1.524)
    (trace_clearance 0.254)
    (zone_clearance 0.37846)
    (zone_45_only no)
    (trace_min 0.2032)
    (segment_width 0.381)
    (edge_width 0.381)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3048)
    (pcb_text_size 1.524 2.032)
    (mod_edge_width 0.381)
    (mod_text_size 1.524 1.524)
    (mod_text_width 0.3048)
    (pad_size 1.524 1.524)
    (pad_drill 0.8128)
    (pad_to_mask_clearance 0.254)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x000f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 0)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber))
  )
  (net 0 "")
  (net 1 /A0)
  (net 2 /A1)
  (net 3 /A10)
  (net 4 /A11)
  (net 5 /A12)
  (net 6 /A13)
  (net 7 /A14)
  (net 8 /A15)
  (net 9 /A16)
  (net 10 /A17)
  (net 11 /A18)
  (net 12 /A19)
  (net 13 /A2)
  (net 14 /A3)
  (net 15 /A4)
  (net 16 /A5)
  (net 17 /A6)
  (net 18 /A7)
  (net 19 /A8)
  (net 20 /A9)
  (net 21 /AEN)
  (net 22 /AVDD1)
  (net 23 /AVDD2)
  (net 24 /B)
  (net 25 /BLUE)
  (net 26 /D0)
  (net 27 /D1)
  (net 28 /D2)
  (net 29 /D3)
  (net 30 /D4)
  (net 31 /D5)
  (net 32 /D6)
  (net 33 /D7)
  (net 34 /G)
  (net 35 /GREEN)
  (net 36 /HSYNC)
  (net 37 /IOCHRDY)
  (net 38 /MAA0)
  (net 39 /MAA1)
  (net 40 /MAA2)
  (net 41 /MAA3)
  (net 42 /MAA4)
  (net 43 /MAA5)
  (net 44 /MAA6)
  (net 45 /MAA7)
  (net 46 /MAA8)
  (net 47 /MAB0)
  (net 48 /MAB1)
  (net 49 /MAB2)
  (net 50 /MAB3)
  (net 51 /MAB4)
  (net 52 /MAB5)
  (net 53 /MAB6)
  (net 54 /MAB7)
  (net 55 /MAB8)
  (net 56 /MD0)
  (net 57 /MD1)
  (net 58 /MD16)
  (net 59 /MD17)
  (net 60 /MD18)
  (net 61 /MD19)
  (net 62 /MD2)
  (net 63 /MD20)
  (net 64 /MD21)
  (net 65 /MD22)
  (net 66 /MD23)
  (net 67 /MD3)
  (net 68 /MD4)
  (net 69 /MD5)
  (net 70 /MD6)
  (net 71 /MD7)
  (net 72 /MONITOR)
  (net 73 /OSC)
  (net 74 /R)
  (net 75 /RED)
  (net 76 /RESET)
  (net 77 /RMD0)
  (net 78 /RMD1)
  (net 79 /RMD2)
  (net 80 /RMD3)
  (net 81 /RMD4)
  (net 82 /RMD5)
  (net 83 /RMD6)
  (net 84 /RMD7)
  (net 85 /ROMA0)
  (net 86 /VSYNC)
  (net 87 /~CAS)
  (net 88 /~IOR)
  (net 89 /~IOW)
  (net 90 /~MEMR)
  (net 91 /~MEMW)
  (net 92 /~NMI)
  (net 93 /~RAS)
  (net 94 /~REFRESH)
  (net 95 /~ROMCS)
  (net 96 /~WE0)
  (net 97 /~WE2)
  (net 98 GND)
  (net 99 VCC)
  (net 100 "Net-(C11-Pad1)")
  (net 101 "Net-(C12-Pad2)")
  (net 102 "Net-(C17-Pad1)")
  (net 103 "Net-(C18-Pad1)")
  (net 104 "Net-(C19-Pad1)")
  (net 105 "Net-(C26-Pad1)")
  (net 106 "Net-(C27-Pad1)")
  (net 107 "Net-(JP1-Pad1)")
  (net 108 "Net-(L2-Pad2)")
  (net 109 "Net-(P1-Pad4)")
  (net 110 "Net-(P1-Pad9)")
  (net 111 "Net-(P1-Pad11)")
  (net 112 "Net-(P1-Pad15)")
  (net 113 "Net-(R1-Pad1)")
  (net 114 "Net-(R15-Pad1)")
  (net 115 "Net-(R16-Pad1)")
  (net 116 "Net-(U1-Pad9)")
  (net 117 "Net-(U1-Pad10)")
  (net 118 "Net-(U1-Pad11)")
  (net 119 "Net-(U1-Pad12)")
  (net 120 "Net-(U1-Pad14)")
  (net 121 "Net-(U1-Pad15)")
  (net 122 "Net-(U1-Pad16)")
  (net 123 "Net-(U1-Pad17)")
  (net 124 "Net-(U1-Pad20)")
  (net 125 "Net-(U1-Pad99)")
  (net 126 "Net-(U1-Pad100)")
  (net 127 "Net-(U1-Pad103)")
  (net 128 "Net-(U1-Pad104)")
  (net 129 "Net-(U1-Pad105)")
  (net 130 "Net-(U1-Pad106)")
  (net 131 "Net-(U1-Pad107)")
  (net 132 "Net-(U1-Pad108)")
  (net 133 "Net-(U1-Pad109)")
  (net 134 "Net-(U1-Pad110)")
  (net 135 "Net-(U1-Pad111)")
  (net 136 "Net-(U1-Pad112)")
  (net 137 "Net-(U1-Pad116)")
  (net 138 "Net-(U1-Pad117)")
  (net 139 "Net-(U1-Pad118)")
  (net 140 "Net-(U1-Pad119)")
  (net 141 "Net-(U1-Pad63)")
  (net 142 "Net-(U1-Pad44)")
  (net 143 "Net-(U1-Pad123)")
  (net 144 "Net-(U1-Pad127)")
  (net 145 "Net-(U1-Pad129)")
  (net 146 "Net-(U1-Pad132)")
  (net 147 "Net-(U1-Pad133)")
  (net 148 "Net-(U1-Pad159)")
  (net 149 "Net-(U3-Pad5)")
  (net 150 "Net-(U4-Pad5)")
  (net 151 "Net-(U5-Pad5)")
  (net 152 "Net-(U6-Pad5)")
  (net 153 "Net-(R10-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.3683)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A16)
    (add_net /A17)
    (add_net /A18)
    (add_net /A19)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /AEN)
    (add_net /AVDD1)
    (add_net /AVDD2)
    (add_net /B)
    (add_net /BLUE)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /G)
    (add_net /GREEN)
    (add_net /HSYNC)
    (add_net /IOCHRDY)
    (add_net /MAA0)
    (add_net /MAA1)
    (add_net /MAA2)
    (add_net /MAA3)
    (add_net /MAA4)
    (add_net /MAA5)
    (add_net /MAA6)
    (add_net /MAA7)
    (add_net /MAA8)
    (add_net /MAB0)
    (add_net /MAB1)
    (add_net /MAB2)
    (add_net /MAB3)
    (add_net /MAB4)
    (add_net /MAB5)
    (add_net /MAB6)
    (add_net /MAB7)
    (add_net /MAB8)
    (add_net /MD0)
    (add_net /MD1)
    (add_net /MD16)
    (add_net /MD17)
    (add_net /MD18)
    (add_net /MD19)
    (add_net /MD2)
    (add_net /MD20)
    (add_net /MD21)
    (add_net /MD22)
    (add_net /MD23)
    (add_net /MD3)
    (add_net /MD4)
    (add_net /MD5)
    (add_net /MD6)
    (add_net /MD7)
    (add_net /MONITOR)
    (add_net /OSC)
    (add_net /R)
    (add_net /RED)
    (add_net /RESET)
    (add_net /RMD0)
    (add_net /RMD1)
    (add_net /RMD2)
    (add_net /RMD3)
    (add_net /RMD4)
    (add_net /RMD5)
    (add_net /RMD6)
    (add_net /RMD7)
    (add_net /ROMA0)
    (add_net /VSYNC)
    (add_net /~CAS)
    (add_net /~IOR)
    (add_net /~IOW)
    (add_net /~MEMR)
    (add_net /~MEMW)
    (add_net /~NMI)
    (add_net /~RAS)
    (add_net /~REFRESH)
    (add_net /~ROMCS)
    (add_net /~WE0)
    (add_net /~WE2)
    (add_net GND)
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C26-Pad1)")
    (add_net "Net-(C27-Pad1)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(L2-Pad2)")
    (add_net "Net-(P1-Pad11)")
    (add_net "Net-(P1-Pad15)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad9)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad100)")
    (add_net "Net-(U1-Pad103)")
    (add_net "Net-(U1-Pad104)")
    (add_net "Net-(U1-Pad105)")
    (add_net "Net-(U1-Pad106)")
    (add_net "Net-(U1-Pad107)")
    (add_net "Net-(U1-Pad108)")
    (add_net "Net-(U1-Pad109)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad110)")
    (add_net "Net-(U1-Pad111)")
    (add_net "Net-(U1-Pad112)")
    (add_net "Net-(U1-Pad116)")
    (add_net "Net-(U1-Pad117)")
    (add_net "Net-(U1-Pad118)")
    (add_net "Net-(U1-Pad119)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad123)")
    (add_net "Net-(U1-Pad127)")
    (add_net "Net-(U1-Pad129)")
    (add_net "Net-(U1-Pad132)")
    (add_net "Net-(U1-Pad133)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad159)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad44)")
    (add_net "Net-(U1-Pad63)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U1-Pad99)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U5-Pad5)")
    (add_net "Net-(U6-Pad5)")
    (add_net VCC)
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 0.63246)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module DIP28_600 (layer Front) (tedit 5110BF96)
    (at 184.15 110.49)
    (descr "Module Dil 28 pins, pads ronds, e=600 mils")
    (tags DIL)
    (fp_text reference U2 (at -15.24 9.8425) (layer F.SilkS))
    (fp_text value 27C256 (at -15.24 12.065) (layer F.SilkS))
    (pad 1 thru_hole rect (at -16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 VCC))
    (pad 2 thru_hole circle (at -13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A13))
    (pad 3 thru_hole circle (at -11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A8))
    (pad 4 thru_hole circle (at -8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A7))
    (pad 5 thru_hole circle (at -6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A6))
    (pad 6 thru_hole circle (at -3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A5))
    (pad 7 thru_hole circle (at -1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A4))
    (pad 8 thru_hole circle (at 1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A3))
    (pad 9 thru_hole circle (at 3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A2))
    (pad 10 thru_hole circle (at 6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 /A1))
    (pad 11 thru_hole circle (at 8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 77 /RMD0))
    (pad 12 thru_hole circle (at 11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 78 /RMD1))
    (pad 13 thru_hole circle (at 13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 79 /RMD2))
    (pad 14 thru_hole circle (at 16.51 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (pad 15 thru_hole circle (at 16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 80 /RMD3))
    (pad 16 thru_hole circle (at 13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 81 /RMD4))
    (pad 17 thru_hole circle (at 11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 82 /RMD5))
    (pad 18 thru_hole circle (at 8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 83 /RMD6))
    (pad 19 thru_hole circle (at 6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 84 /RMD7))
    (pad 20 thru_hole circle (at 3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (pad 21 thru_hole circle (at 1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 /A11))
    (pad 22 thru_hole circle (at -1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 95 /~ROMCS))
    (pad 23 thru_hole circle (at -3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A12))
    (pad 24 thru_hole circle (at -6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 /A10))
    (pad 25 thru_hole circle (at -8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A9))
    (pad 26 thru_hole circle (at -11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A14))
    (pad 27 thru_hole circle (at -13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 85 /ROMA0))
    (pad 28 thru_hole circle (at -16.51 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 VCC))
    (model dil/dil_28-w600.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_762 (layer Front) (tedit 5110BEF2)
    (at 113.03 74.93 90)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R15 (at -6.35 0.3175 90) (layer F.SilkS))
    (fp_text value 33 (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 114 "Net-(R15-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 93 /~RAS))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_762 (layer Front) (tedit 5110BBAD)
    (at 175.26 52.07)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R7 (at -6.0325 0) (layer F.SilkS))
    (fp_text value 4.7k (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 67 /MD3))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_762 (layer Front) (tedit 5110BFB2)
    (at 175.26 57.15 180)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R8 (at 7.62 0 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 72 /MONITOR))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 VCC))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_762 (layer Front) (tedit 5110BE8A)
    (at 176.53 120.65 180)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R9 (at 0 -2.2225 180) (layer F.SilkS))
    (fp_text value 1k (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 76 /RESET))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 103 "Net-(C18-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_762 (layer Front) (tedit 5110BBAB)
    (at 175.26 54.61)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R6 (at -6.0325 0) (layer F.SilkS))
    (fp_text value 4.7k (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 62 /MD2))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 107 "Net-(JP1-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_762 (layer Front) (tedit 5110BE80)
    (at 168.91 92.71)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R10 (at -0.3175 -1.905) (layer F.SilkS))
    (fp_text value 150 (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 153 "Net-(R10-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_762 (layer Front) (tedit 515F9312)
    (at 175.26 70.485)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R11 (at -7.62 0) (layer F.SilkS))
    (fp_text value 150 (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 74 /R))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_762 (layer Front) (tedit 5110BFAC)
    (at 175.26 76.835)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R12 (at -7.62 0) (layer F.SilkS))
    (fp_text value 150 (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /G))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_762 (layer Front) (tedit 5110C676)
    (at 175.26 83.185)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R13 (at -7.62 0) (layer F.SilkS))
    (fp_text value 150 (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 /B))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_762 (layer Front) (tedit 5110BEA0)
    (at 147.955 116.84 90)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R14 (at 0 -1.905 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 /~IOW))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 104 "Net-(C19-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_762 (layer Front) (tedit 5110BEF4)
    (at 115.57 74.93 90)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R16 (at -6.35 0 90) (layer F.SilkS))
    (fp_text value 33 (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 115 "Net-(R16-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 87 /~CAS))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_762 (layer Front) (tedit 5110BE8F)
    (at 194.31 120.65 180)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R5 (at 0 -2.2225 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 78 /RMD1))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_762 (layer Front) (tedit 5110BDF9)
    (at 184.15 97.79 180)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R4 (at 5.715 0 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 81 /RMD4))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_762 (layer Front) (tedit 5110BDFC)
    (at 184.15 100.33 180)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R3 (at 5.715 0 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 83 /RMD6))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_762 (layer Front) (tedit 5110BBAF)
    (at 175.26 49.53)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R2 (at -6.0325 0) (layer F.SilkS))
    (fp_text value 4.7k (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 71 /MD7))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_762 (layer Front) (tedit 5110BECB)
    (at 110.49 93.98)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R1 (at -5.715 0) (layer F.SilkS))
    (fp_text value 4.7k (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 113 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 VCC))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module DIP20_300 (layer Front) (tedit 5110BF45)
    (at 149.86 53.34)
    (descr "20 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference U5 (at -13.97 -4.445) (layer F.SilkS))
    (fp_text value MT4C4256 (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 68 /MD4))
    (pad 2 thru_hole circle (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 69 /MD5))
    (pad 3 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 96 /~WE0))
    (pad 4 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 93 /~RAS))
    (pad 5 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 151 "Net-(U5-Pad5)"))
    (pad 6 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /MAA0))
    (pad 7 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /MAA1))
    (pad 8 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /MAA2))
    (pad 9 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 41 /MAA3))
    (pad 10 thru_hole circle (at 11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 VCC))
    (pad 11 thru_hole circle (at 11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 42 /MAA4))
    (pad 12 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 43 /MAA5))
    (pad 13 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 44 /MAA6))
    (pad 14 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 45 /MAA7))
    (pad 15 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 46 /MAA8))
    (pad 16 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (pad 17 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 87 /~CAS))
    (pad 18 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 70 /MD6))
    (pad 19 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 71 /MD7))
    (pad 20 thru_hole circle (at -11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model dil/dil_20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DIP20_300 (layer Front) (tedit 5110BF41)
    (at 119.38 53.34)
    (descr "20 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference U6 (at -13.97 -4.445) (layer F.SilkS))
    (fp_text value MT4C4256 (at -0.3175 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 63 /MD20))
    (pad 2 thru_hole circle (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 64 /MD21))
    (pad 3 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 97 /~WE2))
    (pad 4 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 93 /~RAS))
    (pad 5 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 152 "Net-(U6-Pad5)"))
    (pad 6 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 /MAB0))
    (pad 7 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 /MAB1))
    (pad 8 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 49 /MAB2))
    (pad 9 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 /MAB3))
    (pad 10 thru_hole circle (at 11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 VCC))
    (pad 11 thru_hole circle (at 11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 /MAB4))
    (pad 12 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 /MAB5))
    (pad 13 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 /MAB6))
    (pad 14 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 /MAB7))
    (pad 15 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 55 /MAB8))
    (pad 16 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (pad 17 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 87 /~CAS))
    (pad 18 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 65 /MD22))
    (pad 19 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 66 /MD23))
    (pad 20 thru_hole circle (at -11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model dil/dil_20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DIP20_300 (layer Front) (tedit 5110BF51)
    (at 149.86 63.5)
    (descr "20 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference U3 (at -10.16 6.0325) (layer F.SilkS))
    (fp_text value MT4C4256 (at 7.62 6.0325) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 56 /MD0))
    (pad 2 thru_hole circle (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 /MD1))
    (pad 3 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 96 /~WE0))
    (pad 4 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 93 /~RAS))
    (pad 5 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 149 "Net-(U3-Pad5)"))
    (pad 6 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /MAA0))
    (pad 7 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /MAA1))
    (pad 8 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /MAA2))
    (pad 9 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 41 /MAA3))
    (pad 10 thru_hole circle (at 11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 VCC))
    (pad 11 thru_hole circle (at 11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 42 /MAA4))
    (pad 12 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 43 /MAA5))
    (pad 13 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 44 /MAA6))
    (pad 14 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 45 /MAA7))
    (pad 15 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 46 /MAA8))
    (pad 16 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (pad 17 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 87 /~CAS))
    (pad 18 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 62 /MD2))
    (pad 19 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 67 /MD3))
    (pad 20 thru_hole circle (at -11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model dil/dil_20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DIP20_300 (layer Front) (tedit 5110BF4C)
    (at 119.38 63.5)
    (descr "20 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference U4 (at -10.16 6.0325) (layer F.SilkS))
    (fp_text value MT4C4256 (at 7.62 6.0325) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 /MD16))
    (pad 2 thru_hole circle (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 59 /MD17))
    (pad 3 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 97 /~WE2))
    (pad 4 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 93 /~RAS))
    (pad 5 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 150 "Net-(U4-Pad5)"))
    (pad 6 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 /MAB0))
    (pad 7 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 /MAB1))
    (pad 8 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 49 /MAB2))
    (pad 9 thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 /MAB3))
    (pad 10 thru_hole circle (at 11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 VCC))
    (pad 11 thru_hole circle (at 11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 /MAB4))
    (pad 12 thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 /MAB5))
    (pad 13 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 /MAB6))
    (pad 14 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 /MAB7))
    (pad 15 thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 55 /MAB8))
    (pad 16 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (pad 17 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 87 /~CAS))
    (pad 18 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 /MD18))
    (pad 19 thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 61 /MD19))
    (pad 20 thru_hole circle (at -11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model dil/dil_20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Tant_504 (layer Front) (tedit 511345AD)
    (at 110.49 99.06 180)
    (descr "Tantalum Capacitor - 5.04mm")
    (tags Cap_Tant_504)
    (fp_text reference C15 (at 5.3975 0.635 180) (layer F.SilkS))
    (fp_text value 10uF (at 5.3975 -0.9525 180) (layer F.SilkS))
    (fp_text user + (at -2.54 -2.54 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /AVDD1))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Cer_504 (layer Front) (tedit 5110BE76)
    (at 163.83 79.375)
    (descr "Ceramic Capacitor 5.04mm")
    (tags Cap_Cer_504)
    (fp_text reference C1 (at 0 1.905) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 VCC))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Cer_504 (layer Front) (tedit 5110BE03)
    (at 168.91 100.33)
    (descr "Ceramic Capacitor 5.04mm")
    (tags Cap_Cer_504)
    (fp_text reference C2 (at -4.7625 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 VCC))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Cer_504 (layer Front) (tedit 5110BF19)
    (at 165.1 63.5 90)
    (descr "Ceramic Capacitor 5.04mm")
    (tags Cap_Cer_504)
    (fp_text reference C3 (at -4.7625 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 VCC))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Cer_504 (layer Front) (tedit 5110BF10)
    (at 134.62 63.5 90)
    (descr "Ceramic Capacitor 5.04mm")
    (tags Cap_Cer_504)
    (fp_text reference C4 (at -4.7625 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 VCC))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Cer_504 (layer Front) (tedit 5110BF0A)
    (at 134.62 53.34 90)
    (descr "Ceramic Capacitor 5.04mm")
    (tags Cap_Cer_504)
    (fp_text reference C6 (at -4.7625 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 VCC))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Cer_504 (layer Front) (tedit 5113459C)
    (at 110.49 104.14 180)
    (descr "Ceramic Capacitor 5.04mm")
    (tags Cap_Cer_504)
    (fp_text reference C8 (at 5.3975 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 VCC))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Cer_504 (layer Front) (tedit 51134598)
    (at 110.49 109.22 180)
    (descr "Ceramic Capacitor 5.04mm")
    (tags Cap_Cer_504)
    (fp_text reference C9 (at 5.3975 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /AVDD1))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Cer_504 (layer Front) (tedit 5110BE21)
    (at 168.91 95.25)
    (descr "Ceramic Capacitor 5.04mm")
    (tags Cap_Cer_504)
    (fp_text reference C10 (at -5.3975 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /AVDD2))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Cer_504 (layer Front) (tedit 5110BEB7)
    (at 110.49 114.3)
    (descr "Ceramic Capacitor 5.04mm")
    (tags Cap_Cer_504)
    (fp_text reference C11 (at -5.3975 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 100 "Net-(C11-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Cer_504 (layer Front) (tedit 51134594)
    (at 110.49 111.76 180)
    (descr "Ceramic Capacitor 5.04mm")
    (tags Cap_Cer_504)
    (fp_text reference C12 (at 5.3975 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /AVDD1))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(C12-Pad2)"))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Cer_504 (layer Front) (tedit 5110BDBB)
    (at 185.42 71.12)
    (descr "Ceramic Capacitor 5.04mm")
    (tags Cap_Cer_504)
    (fp_text reference C17 (at 5.3975 -2.2225) (layer F.SilkS))
    (fp_text value 1uF (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(C17-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Cer_504 (layer Front) (tedit 5110BEA8)
    (at 157.48 116.84 270)
    (descr "Ceramic Capacitor 5.04mm")
    (tags Cap_Cer_504)
    (fp_text reference C18 (at 5.3975 0 270) (layer F.SilkS))
    (fp_text value 470pF (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 103 "Net-(C18-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Cer_504 (layer Front) (tedit 5110BE99)
    (at 153.035 116.84 270)
    (descr "Ceramic Capacitor 5.04mm")
    (tags Cap_Cer_504)
    (fp_text reference C19 (at 5.3975 0 270) (layer F.SilkS))
    (fp_text value 100pF (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 104 "Net-(C19-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Cer_504 (layer Front) (tedit 5110BE96)
    (at 150.495 116.84 270)
    (descr "Ceramic Capacitor 5.04mm")
    (tags Cap_Cer_504)
    (fp_text reference C20 (at 5.3975 0 270) (layer F.SilkS))
    (fp_text value 47pF (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 90 /~MEMR))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Cer_504 (layer Front) (tedit 5110BEDC)
    (at 107.95 74.93 270)
    (descr "Ceramic Capacitor 5.04mm")
    (tags Cap_Cer_504)
    (fp_text reference C21 (at 5.3975 0 270) (layer F.SilkS))
    (fp_text value 47pF (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 93 /~RAS))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Cer_504 (layer Front) (tedit 5110BEE4)
    (at 110.49 74.93 270)
    (descr "Ceramic Capacitor 5.04mm")
    (tags Cap_Cer_504)
    (fp_text reference C22 (at 5.3975 0 270) (layer F.SilkS))
    (fp_text value 47pF (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 87 /~CAS))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Cer_504 (layer Front) (tedit 5110BDC6)
    (at 185.42 73.66)
    (descr "Ceramic Capacitor 5.04mm")
    (tags Cap_Cer_504)
    (fp_text reference C23 (at 0 2.2225) (layer F.SilkS))
    (fp_text value 47pF (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 75 /RED))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Cer_504 (layer Front) (tedit 5110BDD3)
    (at 185.42 86.36)
    (descr "Ceramic Capacitor 5.04mm")
    (tags Cap_Cer_504)
    (fp_text reference C25 (at 0 2.2225) (layer F.SilkS))
    (fp_text value 47pF (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 /BLUE))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Conn_Bus_ISA8 (layer Front) (tedit 5A345C61)
    (at 142.24 130.4925)
    (descr "ISA8 PCB edge connector")
    (tags "CONN BUS ISA")
    (fp_text reference BUS1 (at -22.86 -6.985) (layer F.SilkS) hide)
    (fp_text value BUSPC_DEV (at -13.0175 -6.985) (layer F.SilkS) hide)
    (pad 1 connect rect (at 38.1 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 98 GND))
    (pad 2 connect rect (at 35.56 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 76 /RESET))
    (pad 3 connect rect (at 33.02 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 99 VCC))
    (pad 10 connect rect (at 15.24 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 98 GND))
    (pad 11 connect rect (at 12.7 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 91 /~MEMW))
    (pad 12 connect rect (at 10.16 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 90 /~MEMR))
    (pad 13 connect rect (at 7.62 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 89 /~IOW))
    (pad 14 connect rect (at 5.08 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 88 /~IOR))
    (pad 19 connect rect (at -7.62 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 94 /~REFRESH))
    (pad 29 connect rect (at -33.02 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 99 VCC))
    (pad 30 connect rect (at -35.56 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 73 /OSC))
    (pad 31 connect rect (at -38.1 0) (size 1.778 7.62) (layers Back B.Mask)
      (net 98 GND))
    (pad 32 connect rect (at 38.1 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 92 /~NMI))
    (pad 33 connect rect (at 35.56 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 33 /D7))
    (pad 34 connect rect (at 33.02 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 32 /D6))
    (pad 35 connect rect (at 30.48 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 31 /D5))
    (pad 36 connect rect (at 27.94 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 30 /D4))
    (pad 37 connect rect (at 25.4 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 29 /D3))
    (pad 38 connect rect (at 22.86 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 28 /D2))
    (pad 39 connect rect (at 20.32 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 27 /D1))
    (pad 40 connect rect (at 17.78 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 26 /D0))
    (pad 41 connect rect (at 15.24 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 37 /IOCHRDY))
    (pad 42 connect rect (at 12.7 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 21 /AEN))
    (pad 43 connect rect (at 10.16 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 12 /A19))
    (pad 44 connect rect (at 7.62 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 11 /A18))
    (pad 45 connect rect (at 5.08 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 10 /A17))
    (pad 46 connect rect (at 2.54 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 9 /A16))
    (pad 47 connect rect (at 0 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 8 /A15))
    (pad 48 connect rect (at -2.54 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 7 /A14))
    (pad 49 connect rect (at -5.08 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 6 /A13))
    (pad 50 connect rect (at -7.62 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 5 /A12))
    (pad 51 connect rect (at -10.16 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 4 /A11))
    (pad 52 connect rect (at -12.7 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 3 /A10))
    (pad 53 connect rect (at -15.24 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 20 /A9))
    (pad 54 connect rect (at -17.78 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 19 /A8))
    (pad 55 connect rect (at -20.32 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 18 /A7))
    (pad 56 connect rect (at -22.86 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 17 /A6))
    (pad 57 connect rect (at -25.4 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 16 /A5))
    (pad 58 connect rect (at -27.94 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 15 /A4))
    (pad 59 connect rect (at -30.48 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 14 /A3))
    (pad 60 connect rect (at -33.02 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 13 /A2))
    (pad 61 connect rect (at -35.56 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 2 /A1))
    (pad 62 connect rect (at -38.1 0) (size 1.778 7.62) (layers Front F.Mask)
      (net 1 /A0))
  )
  (module Conn_Dsub_DE15F (layer Front) (tedit 5A3995FE)
    (at 194.945 84.1248 270)
    (descr "Connector DE15 Female Right Angle Through Hole")
    (tags "CONN DSUB DE15F 15PIN")
    (fp_text reference P1 (at 10.8077 6.35 270) (layer F.SilkS))
    (fp_text value VGA (at 6.3627 6.35 270) (layer F.SilkS))
    (pad "" thru_hole circle (at 12.49426 0 270) (size 4.04876 4.04876) (drill 3.05054) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (pad "" thru_hole circle (at -12.49426 0 270) (size 4.04876 4.04876) (drill 3.05054) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (pad 1 thru_hole rect (at -4.34086 2.54 90) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 75 /RED))
    (pad 2 thru_hole circle (at -2.04978 2.54 90) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 35 /GREEN))
    (pad 3 thru_hole circle (at 0.24892 2.54 90) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 25 /BLUE))
    (pad 4 thru_hole circle (at 2.54 2.54 90) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(P1-Pad4)"))
    (pad 5 thru_hole circle (at 4.83108 2.54 90) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (pad 9 thru_hole circle (at 1.39446 0 90) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 110 "Net-(P1-Pad9)"))
    (pad 8 thru_hole circle (at -0.89408 0 90) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (pad 7 thru_hole circle (at -3.18516 0 90) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (pad 6 thru_hole circle (at -5.47624 0 90) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (pad 10 thru_hole circle (at 3.68554 0 90) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (pad 11 thru_hole circle (at -4.34086 -2.54 90) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 111 "Net-(P1-Pad11)"))
    (pad 12 thru_hole circle (at -2.04978 -2.54 90) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(C17-Pad1)"))
    (pad 13 thru_hole circle (at 0.24892 -2.54 90) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 105 "Net-(C26-Pad1)"))
    (pad 14 thru_hole circle (at 2.54 -2.54 90) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(C27-Pad1)"))
    (pad 15 thru_hole circle (at 4.83108 -2.54 90) (size 1.524 1.524) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 112 "Net-(P1-Pad15)"))
    (model conn_DBxx/db9_male_pin90deg.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PQFP-160 (layer Front) (tedit 5110B1B1)
    (at 138.43 92.71 90)
    (fp_text reference U1 (at -7.3025 22.225 90) (layer F.SilkS))
    (fp_text value TVGA9000I (at 0.635 22.225 90) (layer F.SilkS))
    (fp_text user 150 (at -20.47494 6.17474 90) (layer F.SilkS))
    (fp_text user 140 (at -20.47494 -0.32512 90) (layer F.SilkS))
    (fp_text user 130 (at -19.685 -6.6675 180) (layer F.SilkS))
    (fp_text user 120 (at -12.6746 -19.49958 90) (layer F.SilkS))
    (fp_text user 110 (at -6.17474 -19.49958 90) (layer F.SilkS))
    (fp_text user 100 (at 0.32512 -19.49958 90) (layer F.SilkS))
    (fp_text user 90 (at 6.82498 -19.49958 90) (layer F.SilkS))
    (fp_text user 80 (at 20.14982 -12.6746 90) (layer F.SilkS))
    (fp_text user 70 (at 20.14982 -6.17474 90) (layer F.SilkS))
    (fp_text user 60 (at 20.14982 0.32512 90) (layer F.SilkS))
    (fp_text user 50 (at 20.14982 6.82498 90) (layer F.SilkS))
    (fp_text user 121 (at -15.60068 -13.64996 90) (layer F.SilkS))
    (fp_text user 81 (at 14.3002 -15.60068 90) (layer F.SilkS))
    (fp_text user 41 (at 15.60068 13.97508 90) (layer F.SilkS))
    (fp_text user 30 (at 6.17474 19.8247 90) (layer F.SilkS))
    (fp_text user 20 (at -0.32512 19.8247 90) (layer F.SilkS))
    (fp_text user 10 (at -6.82498 19.8247 90) (layer F.SilkS))
    (fp_text user 40 (at 12.6746 19.8247 90) (layer F.SilkS))
    (fp_text user 160 (at -19.685 12.7 180) (layer F.SilkS))
    (fp_text user 1 (at -13.64996 15.60068 90) (layer F.SilkS))
    (pad 1 smd rect (at -12.6746 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 98 GND))
    (pad 2 smd rect (at -12.02436 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 24 /B))
    (pad 3 smd rect (at -11.37412 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 34 /G))
    (pad 4 smd rect (at -10.72388 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 74 /R))
    (pad 5 smd rect (at -10.07364 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 103 "Net-(C18-Pad1)"))
    (pad 6 smd rect (at -9.4234 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 23 /AVDD2))
    (pad 7 smd rect (at -8.77316 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 98 GND))
    (pad 8 smd rect (at -8.12546 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 99 VCC))
    (pad 9 smd rect (at -7.47522 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 116 "Net-(U1-Pad9)"))
    (pad 10 smd rect (at -6.82498 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 117 "Net-(U1-Pad10)"))
    (pad 11 smd rect (at -6.17474 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 118 "Net-(U1-Pad11)"))
    (pad 12 smd rect (at -5.5245 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 119 "Net-(U1-Pad12)"))
    (pad 13 smd rect (at -4.87426 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 23 /AVDD2))
    (pad 14 smd rect (at -4.22402 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 120 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at -3.57378 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 121 "Net-(U1-Pad15)"))
    (pad 16 smd rect (at -2.92354 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 122 "Net-(U1-Pad16)"))
    (pad 17 smd rect (at -2.2733 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 123 "Net-(U1-Pad17)"))
    (pad 18 smd rect (at -1.62306 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 153 "Net-(R10-Pad1)"))
    (pad 19 smd rect (at -0.97536 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 99 VCC))
    (pad 20 smd rect (at -0.32512 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 124 "Net-(U1-Pad20)"))
    (pad 21 smd rect (at 0.32512 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 99 VCC))
    (pad 22 smd rect (at 0.97536 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 21 /AEN))
    (pad 23 smd rect (at 1.6256 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 98 GND))
    (pad 24 smd rect (at 2.27584 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 92 /~NMI))
    (pad 25 smd rect (at 2.92608 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 26 /D0))
    (pad 26 smd rect (at 3.57632 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 27 /D1))
    (pad 27 smd rect (at 4.22656 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 28 /D2))
    (pad 28 smd rect (at 4.8768 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 29 /D3))
    (pad 29 smd rect (at 5.5245 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 30 /D4))
    (pad 30 smd rect (at 6.17474 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 31 /D5))
    (pad 31 smd rect (at 6.82498 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 32 /D6))
    (pad 32 smd rect (at 7.47522 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 33 /D7))
    (pad 33 smd rect (at 8.12546 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 84 /RMD7))
    (pad 34 smd rect (at 8.7757 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 83 /RMD6))
    (pad 35 smd rect (at 9.42594 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 82 /RMD5))
    (pad 36 smd rect (at 10.07618 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 81 /RMD4))
    (pad 37 smd rect (at 10.72642 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 80 /RMD3))
    (pad 38 smd rect (at 11.37666 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 79 /RMD2))
    (pad 39 smd rect (at 12.0269 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 78 /RMD1))
    (pad 40 smd rect (at 12.6746 15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 99 VCC))
    (pad 81 smd rect (at 12.6746 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 99 VCC))
    (pad 82 smd rect (at 12.02436 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 53 /MAB6))
    (pad 83 smd rect (at 11.37412 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 54 /MAB7))
    (pad 84 smd rect (at 10.72388 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 55 /MAB8))
    (pad 85 smd rect (at 10.07364 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 115 "Net-(R16-Pad1)"))
    (pad 86 smd rect (at 9.42594 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 114 "Net-(R15-Pad1)"))
    (pad 87 smd rect (at 8.7757 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 97 /~WE2))
    (pad 88 smd rect (at 8.12546 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 96 /~WE0))
    (pad 89 smd rect (at 7.47522 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 58 /MD16))
    (pad 90 smd rect (at 6.82498 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 59 /MD17))
    (pad 91 smd rect (at 6.17474 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 60 /MD18))
    (pad 92 smd rect (at 5.5245 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 61 /MD19))
    (pad 93 smd rect (at 4.87426 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 63 /MD20))
    (pad 94 smd rect (at 4.22402 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 64 /MD21))
    (pad 95 smd rect (at 3.57378 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 65 /MD22))
    (pad 96 smd rect (at 2.92608 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 66 /MD23))
    (pad 97 smd rect (at 2.27584 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 85 /ROMA0))
    (pad 98 smd rect (at 1.6256 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 73 /OSC))
    (pad 99 smd rect (at 0.97536 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 125 "Net-(U1-Pad99)"))
    (pad 100 smd rect (at 0.32512 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 126 "Net-(U1-Pad100)"))
    (pad 101 smd rect (at -0.32512 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 98 GND))
    (pad 102 smd rect (at -0.97536 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 113 "Net-(R1-Pad1)"))
    (pad 103 smd rect (at -1.6256 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 127 "Net-(U1-Pad103)"))
    (pad 104 smd rect (at -2.27584 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 128 "Net-(U1-Pad104)"))
    (pad 105 smd rect (at -2.92608 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 129 "Net-(U1-Pad105)"))
    (pad 106 smd rect (at -3.57632 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 130 "Net-(U1-Pad106)"))
    (pad 107 smd rect (at -4.22402 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 131 "Net-(U1-Pad107)"))
    (pad 108 smd rect (at -4.87426 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 132 "Net-(U1-Pad108)"))
    (pad 109 smd rect (at -5.5245 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 133 "Net-(U1-Pad109)"))
    (pad 110 smd rect (at -6.17474 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 134 "Net-(U1-Pad110)"))
    (pad 111 smd rect (at -6.82498 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 135 "Net-(U1-Pad111)"))
    (pad 112 smd rect (at -7.47522 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 136 "Net-(U1-Pad112)"))
    (pad 113 smd rect (at -8.12546 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 10 /A17))
    (pad 114 smd rect (at -8.7757 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 11 /A18))
    (pad 115 smd rect (at -9.42594 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 12 /A19))
    (pad 116 smd rect (at -10.07618 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 137 "Net-(U1-Pad116)"))
    (pad 117 smd rect (at -10.72388 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 138 "Net-(U1-Pad117)"))
    (pad 118 smd rect (at -11.37412 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 139 "Net-(U1-Pad118)"))
    (pad 119 smd rect (at -12.02436 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 140 "Net-(U1-Pad119)"))
    (pad 120 smd rect (at -12.6746 -15.60068 90) (size 0.35052 2.99974) (layers Front F.Paste F.Mask)
      (net 99 VCC))
    (pad 61 smd rect (at 15.60068 -0.32512 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 46 /MAA8))
    (pad 62 smd rect (at 15.60068 -0.97536 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 99 VCC))
    (pad 63 smd rect (at 15.60068 -1.6256 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 141 "Net-(U1-Pad63)"))
    (pad 64 smd rect (at 15.60068 -2.27584 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 56 /MD0))
    (pad 65 smd rect (at 15.60068 -2.92608 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 57 /MD1))
    (pad 66 smd rect (at 15.60068 -3.57632 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 62 /MD2))
    (pad 67 smd rect (at 15.60068 -4.22402 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 67 /MD3))
    (pad 68 smd rect (at 15.60068 -4.87426 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 68 /MD4))
    (pad 69 smd rect (at 15.60068 -5.5245 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 99 VCC))
    (pad 70 smd rect (at 15.60068 -6.17474 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 69 /MD5))
    (pad 71 smd rect (at 15.60068 -6.82498 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 70 /MD6))
    (pad 72 smd rect (at 15.60068 -7.47522 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 71 /MD7))
    (pad 73 smd rect (at 15.60068 -8.12546 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 47 /MAB0))
    (pad 74 smd rect (at 15.60068 -8.7757 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 48 /MAB1))
    (pad 75 smd rect (at 15.60068 -9.42594 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 49 /MAB2))
    (pad 76 smd rect (at 15.60068 -10.07618 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 50 /MAB3))
    (pad 77 smd rect (at 15.60068 -10.72388 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 51 /MAB4))
    (pad 78 smd rect (at 15.60068 -11.37412 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 52 /MAB5))
    (pad 79 smd rect (at 15.60068 -12.02436 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 98 GND))
    (pad 80 smd rect (at 15.60068 -12.6746 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 98 GND))
    (pad 41 smd rect (at 15.60068 12.6746 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 98 GND))
    (pad 42 smd rect (at 15.60068 12.02436 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 98 GND))
    (pad 43 smd rect (at 15.60068 11.37412 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 77 /RMD0))
    (pad 44 smd rect (at 15.60068 10.72388 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 142 "Net-(U1-Pad44)"))
    (pad 45 smd rect (at 15.60068 10.07618 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 95 /~ROMCS))
    (pad 46 smd rect (at 15.60068 9.42594 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 72 /MONITOR))
    (pad 47 smd rect (at 15.60068 8.7757 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 86 /VSYNC))
    (pad 48 smd rect (at 15.60068 8.12546 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 36 /HSYNC))
    (pad 49 smd rect (at 15.60068 7.47522 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 98 GND))
    (pad 50 smd rect (at 15.60068 6.82498 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 98 GND))
    (pad 51 smd rect (at 15.60068 6.17474 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 99 VCC))
    (pad 52 smd rect (at 15.60068 5.5245 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 38 /MAA0))
    (pad 53 smd rect (at 15.60068 4.87426 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 39 /MAA1))
    (pad 54 smd rect (at 15.60068 4.22402 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 40 /MAA2))
    (pad 55 smd rect (at 15.60068 3.57632 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 41 /MAA3))
    (pad 56 smd rect (at 15.60068 2.92608 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 42 /MAA4))
    (pad 57 smd rect (at 15.60068 2.27584 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 43 /MAA5))
    (pad 58 smd rect (at 15.60068 1.6256 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 98 GND))
    (pad 59 smd rect (at 15.60068 0.97536 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 44 /MAA6))
    (pad 121 smd rect (at -15.60068 -12.6746 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 98 GND))
    (pad 122 smd rect (at -15.60068 -12.02436 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 98 GND))
    (pad 123 smd rect (at -15.60068 -11.37412 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 143 "Net-(U1-Pad123)"))
    (pad 124 smd rect (at -15.60068 -10.72388 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 22 /AVDD1))
    (pad 125 smd rect (at -15.60068 -10.07618 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 101 "Net-(C12-Pad2)"))
    (pad 126 smd rect (at -15.60068 -9.42594 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 98 GND))
    (pad 127 smd rect (at -15.60068 -8.7757 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 144 "Net-(U1-Pad127)"))
    (pad 128 smd rect (at -15.60068 -8.12546 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 98 GND))
    (pad 129 smd rect (at -15.60068 -7.47522 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 145 "Net-(U1-Pad129)"))
    (pad 130 smd rect (at -15.60068 -6.82498 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 99 VCC))
    (pad 131 smd rect (at -15.60068 -6.17474 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 108 "Net-(L2-Pad2)"))
    (pad 132 smd rect (at -15.60068 -5.5245 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 146 "Net-(U1-Pad132)"))
    (pad 133 smd rect (at -15.60068 -4.87426 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 147 "Net-(U1-Pad133)"))
    (pad 134 smd rect (at -15.60068 -4.22402 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 99 VCC))
    (pad 135 smd rect (at -15.60068 -3.57632 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 1 /A0))
    (pad 136 smd rect (at -15.60068 -2.92608 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 2 /A1))
    (pad 137 smd rect (at -15.60068 -2.27584 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 13 /A2))
    (pad 138 smd rect (at -15.60068 -1.6256 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 14 /A3))
    (pad 139 smd rect (at -15.60068 -0.97536 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 15 /A4))
    (pad 140 smd rect (at -15.60068 -0.32512 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 16 /A5))
    (pad 141 smd rect (at -15.60068 0.32512 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 17 /A6))
    (pad 142 smd rect (at -15.60068 0.97536 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 18 /A7))
    (pad 143 smd rect (at -15.60068 1.6256 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 98 GND))
    (pad 144 smd rect (at -15.60068 2.27584 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 19 /A8))
    (pad 145 smd rect (at -15.60068 2.92608 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 20 /A9))
    (pad 146 smd rect (at -15.60068 3.57378 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 3 /A10))
    (pad 147 smd rect (at -15.60068 4.22402 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 4 /A11))
    (pad 148 smd rect (at -15.60068 4.87426 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 5 /A12))
    (pad 149 smd rect (at -15.60068 5.5245 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 6 /A13))
    (pad 150 smd rect (at -15.60068 6.17474 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 7 /A14))
    (pad 151 smd rect (at -15.60068 6.82498 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 8 /A15))
    (pad 152 smd rect (at -15.60068 7.47522 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 9 /A16))
    (pad 153 smd rect (at -15.60068 8.12546 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 88 /~IOR))
    (pad 154 smd rect (at -15.60068 8.7757 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 104 "Net-(C19-Pad1)"))
    (pad 155 smd rect (at -15.60068 9.42594 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 90 /~MEMR))
    (pad 156 smd rect (at -15.60068 10.07364 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 91 /~MEMW))
    (pad 157 smd rect (at -15.60068 10.72388 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 37 /IOCHRDY))
    (pad 158 smd rect (at -15.60068 11.37412 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 94 /~REFRESH))
    (pad 159 smd rect (at -15.60068 12.02436 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 148 "Net-(U1-Pad159)"))
    (pad 160 smd rect (at -15.60068 12.6746 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 98 GND))
    (pad 60 smd rect (at 15.60068 0.32512 90) (size 2.99974 0.35052) (layers Front F.Paste F.Mask)
      (net 45 /MAA7))
  )
  (module Crystal_HC-49U_Vert (layer Front) (tedit 5110BF7C)
    (at 123.19 116.84 180)
    (descr "Quartz Crystal HC-49U Vertical")
    (tags "QUARTZ CRYSTAL HC49U VERT")
    (autoplace_cost180 10)
    (fp_text reference X1 (at 2.54 -3.4925 180) (layer F.SilkS))
    (fp_text value 40MHz (at -1.5875 -3.4925 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.44094 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 147 "Net-(U1-Pad133)"))
    (pad 2 thru_hole circle (at 2.44094 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 108 "Net-(L2-Pad2)"))
    (model discret/crystal_hc18u_vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Cer_504 (layer Front) (tedit 5110BF1D)
    (at 165.1 53.34 90)
    (descr "Ceramic Capacitor 5.04mm")
    (tags Cap_Cer_504)
    (fp_text reference C5 (at -4.7625 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 VCC))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Cer_504 (layer Front) (tedit 5110BF63)
    (at 130.81 116.84 270)
    (descr "Ceramic Capacitor 5.04mm")
    (tags Cap_Cer_504)
    (fp_text reference C7 (at 5.08 0 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Tant_504 (layer Front) (tedit 5110BF86)
    (at 106.68 122.555 180)
    (descr "Tantalum Capacitor - 5.04mm")
    (tags Cap_Tant_504)
    (fp_text reference C13 (at -5.715 0.635 180) (layer F.SilkS))
    (fp_text value 10uF (at -5.715 -0.9525 180) (layer F.SilkS))
    (fp_text user + (at -2.54 -2.54 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 VCC))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Tant_504 (layer Front) (tedit 5110B023)
    (at 185.42 122.555)
    (descr "Tantalum Capacitor - 5.04mm")
    (tags Cap_Tant_504)
    (fp_text reference C14 (at 4.445 1.5875) (layer F.SilkS))
    (fp_text value 10uF (at 4.445 3.175) (layer F.SilkS))
    (fp_text user + (at -2.54 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 VCC))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Tant_504 (layer Front) (tedit 5110B1EF)
    (at 177.8 92.71)
    (descr "Tantalum Capacitor - 5.04mm")
    (tags Cap_Tant_504)
    (fp_text reference C16 (at 5.08 -0.635) (layer F.SilkS))
    (fp_text value 10uF (at 5.08 0.9525) (layer F.SilkS))
    (fp_text user + (at -2.54 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /AVDD2))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Cer_504 (layer Front) (tedit 5110BDCB)
    (at 185.42 80.01)
    (descr "Ceramic Capacitor 5.04mm")
    (tags Cap_Cer_504)
    (fp_text reference C24 (at 0 2.2225) (layer F.SilkS))
    (fp_text value 47pF (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /GREEN))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Cer_504 (layer Front) (tedit 515F8EB7)
    (at 185.42 68.58)
    (descr "Ceramic Capacitor 5.04mm")
    (tags Cap_Cer_504)
    (fp_text reference C26 (at 5.3975 -1.27) (layer F.SilkS))
    (fp_text value 47pF (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 105 "Net-(C26-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_Cer_504 (layer Front) (tedit 515F8EB9)
    (at 185.42 66.04)
    (descr "Ceramic Capacitor 5.04mm")
    (tags Cap_Cer_504)
    (fp_text reference C27 (at 5.3975 -0.3175) (layer F.SilkS))
    (fp_text value 47pF (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(C27-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Conn_Pin_Header_2x1_Nokey (layer Front) (tedit 515F8F83)
    (at 185.42 60.96)
    (descr "Connector Pin Header 2x1 No Key")
    (tags "CONN PIN HEADER 2x1 NOKEY")
    (fp_text reference JP1 (at 5.08 0) (layer F.SilkS))
    (fp_text value HSYNC_SEL (at 0 2.54) (layer F.SilkS))
    (pad 1 thru_hole oval (at -1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 107 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 98 GND))
    (model pin_array/pins_array_5x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_1016 (layer Front) (tedit 5110BBEF)
    (at 175.26 73.66)
    (descr "Resistor 10.16mm between leads")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference FB1 (at -7.62 0) (layer F.SilkS))
    (fp_text value FILTER (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 74 /R))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 75 /RED))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_1016 (layer Front) (tedit 515F932C)
    (at 175.26 80.01)
    (descr "Resistor 10.16mm between leads")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference FB2 (at -7.62 1.27) (layer F.SilkS))
    (fp_text value FILTER (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /G))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /GREEN))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_1016 (layer Front) (tedit 5110B231)
    (at 175.26 86.36)
    (descr "Resistor 10.16mm between leads")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference FB3 (at -7.62 0) (layer F.SilkS))
    (fp_text value FILTER (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 /B))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 /BLUE))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_1016 (layer Front) (tedit 515F88C1)
    (at 175.26 60.325 180)
    (descr "Resistor 10.16mm between leads")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference FB4 (at 7.62 0 180) (layer F.SilkS))
    (fp_text value FILTER (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 105 "Net-(C26-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 /HSYNC))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_1016 (layer Front) (tedit 5110BBDA)
    (at 175.26 63.8175 180)
    (descr "Resistor 10.16mm between leads")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference FB5 (at 7.62 0 180) (layer F.SilkS))
    (fp_text value FILTER (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(C27-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 86 /VSYNC))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_1016 (layer Front) (tedit 5110BBEC)
    (at 175.26 67.31 180)
    (descr "Resistor 10.16mm between leads")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference FB6 (at 7.62 0 180) (layer F.SilkS))
    (fp_text value FILTER (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(C17-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 72 /MONITOR))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_1016 (layer Front) (tedit 5110BEBD)
    (at 110.49 106.68 180)
    (descr "Resistor 10.16mm between leads")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference L1 (at 6.985 0 180) (layer F.SilkS))
    (fp_text value 5.7uH (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 VCC))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /AVDD1))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_1016 (layer Front) (tedit 51133F16)
    (at 110.49 116.84)
    (descr "Resistor 10.16mm between leads")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference L2 (at -6.985 0) (layer F.SilkS))
    (fp_text value 2.7uH (at 0.3175 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 100 "Net-(C11-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 108 "Net-(L2-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_1016 (layer Front) (tedit 5110BE1E)
    (at 171.45 97.79)
    (descr "Resistor 10.16mm between leads")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference L3 (at -7.62 0) (layer F.SilkS))
    (fp_text value 5.7uH (at -0.3175 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 VCC))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /AVDD2))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "JP1: Select monitor's\nhorizontal frequency:\nOpen: >= 48.7 kHz\nClosed: < 48.7 kHz" (at 103.8225 86.36) (layer F.SilkS))
  (gr_text www.malinov.com (at 139.3825 122.555) (layer F.SilkS))
  (gr_text "ISA Super VGA\nVersion 1.1\nCopyright (C) 2017\nSergey Kiselev" (at 193.04 53.34) (layer F.SilkS))
  (gr_line (start 101.6 133.985) (end 101.6 49.53) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 205.74 124.46) (end 205.74 49.53) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 104.14 49.53) (end 101.6 49.53) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 104.14 46.99) (end 203.2 46.99) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 203.2 127) (end 182.88 127) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 203.2 124.46) (end 205.74 124.46) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 203.2 49.53) (end 203.2 46.99) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 182.88 133.985) (end 182.88 127) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 102.235 134.62) (end 182.245 134.62) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 182.245 133.985) (end 182.88 133.985) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 102.235 133.985) (end 102.235 134.62) (angle 90) (layer Edge.Cuts) (width 0.381))
  (zone (net 98) (net_name GND) (layer Front) (hatch edge 0.508)
    (connect_pads (clearance 0.37846))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 205.74 127) (xy 205.74 46.99) (xy 101.6 46.99) (xy 101.6 125.4125) (xy 182.88 125.4125)
        (xy 182.88 127)
      )
    )
  )
  (zone (net 99) (net_name VCC) (layer Back) (hatch edge 0.508)
    (connect_pads (clearance 0.37846))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 179.07 125.4125) (xy 179.07 124.1425) (xy 179.705 123.5075) (xy 183.8325 123.5075) (xy 183.8325 119.6975)
        (xy 183.1975 119.0625) (xy 168.91 119.0625) (xy 168.91 88.9) (xy 167.9575 87.9475) (xy 146.05 87.9475)
        (xy 144.78 86.6775) (xy 144.78 83.82) (xy 147.6375 80.9625) (xy 160.655 80.9625) (xy 162.8775 78.74)
        (xy 162.8775 71.755) (xy 167.005 67.6275) (xy 167.005 64.135) (xy 166.0525 63.1825) (xy 119.6975 63.1825)
        (xy 118.745 64.135) (xy 118.745 86.6775) (xy 111.76 93.6625) (xy 111.76 107.315) (xy 112.395 107.95)
        (xy 114.3 107.95) (xy 114.935 108.585) (xy 114.935 114.935) (xy 107.95 121.92) (xy 107.95 125.4125)
      )
    )
  )
  (zone (net 98) (net_name GND) (layer Back) (hatch edge 0.508)
    (connect_pads (clearance 0.37846))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 205.74 127) (xy 205.74 46.99) (xy 101.6 46.99) (xy 101.6 125.4125) (xy 107.315 125.4125)
        (xy 107.315 121.6025) (xy 114.3 114.6175) (xy 114.3 108.9025) (xy 113.9825 108.585) (xy 112.0775 108.585)
        (xy 111.125 107.6325) (xy 111.125 93.345) (xy 118.11 86.36) (xy 118.11 63.8175) (xy 119.38 62.5475)
        (xy 166.37 62.5475) (xy 167.64 63.8175) (xy 167.64 67.945) (xy 163.5125 72.0725) (xy 163.5125 79.0575)
        (xy 160.655 81.5975) (xy 147.955 81.5975) (xy 145.415 84.1375) (xy 145.415 86.36) (xy 146.3675 87.3125)
        (xy 168.275 87.3125) (xy 169.545 88.5825) (xy 169.545 118.4275) (xy 183.515 118.4275) (xy 184.4675 119.38)
        (xy 184.4675 123.825) (xy 184.15 124.1425) (xy 180.0225 124.1425) (xy 179.705 124.46) (xy 179.705 125.4125)
        (xy 182.88 125.4125) (xy 182.88 127)
      )
    )
  )
)
