<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="-0.254" y1="0.0254" x2="46.0048" y2="0" width="0" layer="20"/>
<wire x1="46.0048" y1="0" x2="45.9032" y2="40.4878" width="0" layer="20"/>
<wire x1="45.9032" y1="40.4878" x2="-0.2286" y2="40.691" width="0" layer="20"/>
<wire x1="-0.2286" y1="40.691" x2="-0.254" y2="0.0254" width="0" layer="20"/>
<text>                              
Solar Charge Rev1</text>
<text>4/15/16</text>
<text>GND</text>
<text>GND</text>
<text>Battery</text>
<text>Solar</text>
<text>Battery In</text>
<text>GND</text>
<text>1</text>
<text>GND</text>
<text>Solar In</text>
<text>Positive</text>
<text>Positive</text>
<text>VGate</text>
<hole x="2.0066" y="38.7096" drill="2.8"/>
<hole x="44.196" y="38.6334" drill="2.8"/>
<hole x="10.541" y="2.8448" drill="2.8"/>
<hole x="38.4556" y="2.5146" drill="2.8"/>
<text>1</text>
<text>RDF</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="TO92">
<description>&lt;b&gt;TO-92&lt;/b&gt;</description>
</package>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="DO35-7">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 7.62 mm</description>
</package>
<package name="C025-025X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.5 x 5 mm</description>
</package>
<package name="TO220H">
<description>&lt;b&gt;TO-220&lt;/b&gt;</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
<library name="motorola-sensor-driver">
<description>&lt;b&gt;Motorola pressure sensor&lt;/b&gt;&lt;p&gt;
SEMICONDUCTOR TECHNICAL DATA mpx2050.pdf</description>
<packages>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-wago-500">
<description>&lt;b&gt;Wago Screw Clamps&lt;/b&gt;&lt;p&gt;
Grid 5.00 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="W237-102">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="E$1" library="motorola-sensor-driver" package="DIP08" value="ATTINY 85">
<attribute name="VALUE"/>
</element>
<element name="E$2" library="adafruit" package="0204/7" value="4.7K">
<attribute name="VALUE"/>
</element>
<element name="E$3" library="adafruit" package="0204/7" value="220K">
<attribute name="VALUE"/>
</element>
<element name="E$4" library="adafruit" package="0204/7" value="220K">
<attribute name="VALUE"/>
</element>
<element name="E$5" library="adafruit" package="0204/7" value="20K">
<attribute name="VALUE"/>
</element>
<element name="E$6" library="adafruit" package="0204/7" value="220K">
<attribute name="VALUE"/>
</element>
<element name="E$7" library="adafruit" package="0204/7" value="82K">
<attribute name="VALUE"/>
</element>
<element name="E$8" library="adafruit" package="DO35-7" value="1N4148">
<attribute name="VALUE"/>
</element>
<element name="E$9" library="adafruit" package="DO35-7" value="1N4148">
<attribute name="VALUE"/>
</element>
<element name="E$10" library="adafruit" package="DO35-7" value="1N4148">
<attribute name="VALUE"/>
</element>
<element name="E$11" library="adafruit" package="DO35-7" value="1N4148">
<attribute name="VALUE"/>
</element>
<element name="E$12" library="adafruit" package="TO92" value="78L05">
<attribute name="VALUE"/>
</element>
<element name="E$14" library="adafruit" package="TO92" value="2N3906">
<attribute name="VALUE"/>
</element>
<element name="E$15" library="adafruit" package="TO92" value="2N3904">
<attribute name="VALUE"/>
</element>
<element name="E$16" library="adafruit" package="C025-025X050" value="1UF-T">
<attribute name="VALUE"/>
</element>
<element name="E$17" library="adafruit" package="C025-025X050" value="47N">
<attribute name="VALUE"/>
</element>
<element name="E$18" library="adafruit" package="C025-025X050" value="">
<attribute name="VALUE"/>
</element>
<element name="E$19" library="adafruit" package="C025-025X050" value="4.7UF-T">
<attribute name="VALUE"/>
</element>
<element name="E$20" library="adafruit" package="C025-025X050" value="1UF-T">
<attribute name="VALUE"/>
</element>
<element name="E$21" library="adafruit" package="C025-025X050" value="220P">
<attribute name="VALUE"/>
</element>
<element name="E$22" library="adafruit" package="C025-025X050" value="100N">
<attribute name="VALUE"/>
</element>
<element name="E$24" library="adafruit" package="TO220H" value="IRF3205">
<attribute name="VALUE"/>
</element>
<element name="E$23" library="adafruit" package="DO35-7" value="1N4148"/>
<element name="E$25" library="adafruit" package="LED3MM" value="Green">
<attribute name="VALUE"/>
</element>
<element name="E$26" library="adafruit" package="0204/7" value="1K">
<attribute name="VALUE"/>
</element>
<element name="E$13" library="con-wago-500" package="W237-102" value="">
<attribute name="VALUE"/>
</element>
<element name="E$28" library="con-wago-500" package="W237-102" value="">
<attribute name="VALUE"/>
</element>
<element name="E$29" library="adafruit" package="DO41-10" value="TVS">
<attribute name="VALUE"/>
</element>
<element name="E$30" library="adafruit" package="TO92" value="2N3906">
<attribute name="VALUE"/>
</element>
<element name="E$27" library="adafruit" package="LED3MM" value="RED">
<attribute name="VALUE"/>
</element>
<element name="E$31" library="adafruit" package="0204/7" value="1K">
<attribute name="VALUE"/>
</element>
<element name="E$32" library="SparkFun-Connectors" package="2X03" value="ICSP">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$1">
<contactref element="E$7" pad="2"/>
<contactref element="E$21" pad="1"/>
<contactref element="E$5" pad="1"/>
<contactref element="E$1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="E$5" pad="2"/>
<contactref element="E$21" pad="2"/>
<contactref element="E$1" pad="4"/>
<contactref element="E$20" pad="1"/>
<contactref element="E$3" pad="1"/>
<contactref element="E$12" pad="2"/>
<contactref element="E$16" pad="2"/>
<contactref element="E$22" pad="1"/>
<contactref element="E$19" pad="1"/>
<contactref element="E$26" pad="1"/>
<contactref element="E$28" pad="2"/>
<contactref element="E$29" pad="C"/>
<contactref element="E$13" pad="2"/>
<contactref element="E$32" pad="6"/>
</signal>
<signal name="S$3">
<contactref element="E$15" pad="1"/>
<contactref element="E$3" pad="2"/>
</signal>
<signal name="S$4">
<contactref element="E$1" pad="3"/>
<contactref element="E$15" pad="2"/>
</signal>
<signal name="S$5">
<contactref element="E$6" pad="1"/>
<contactref element="E$15" pad="3"/>
<contactref element="E$30" pad="2"/>
</signal>
<signal name="S$6">
<contactref element="E$6" pad="2"/>
<contactref element="E$10" pad="C"/>
<contactref element="E$20" pad="2"/>
<contactref element="E$30" pad="3"/>
</signal>
<signal name="S$7">
<contactref element="E$17" pad="1"/>
<contactref element="E$1" pad="5"/>
<contactref element="E$32" pad="4"/>
</signal>
<signal name="S$8">
<contactref element="E$1" pad="6"/>
<contactref element="E$18" pad="1"/>
<contactref element="E$32" pad="1"/>
</signal>
<signal name="S$9">
<contactref element="E$9" pad="C"/>
<contactref element="E$18" pad="2"/>
<contactref element="E$11" pad="A"/>
</signal>
<signal name="S$10">
<contactref element="E$10" pad="A"/>
<contactref element="E$17" pad="2"/>
<contactref element="E$11" pad="C"/>
</signal>
<signal name="S$11">
<contactref element="E$8" pad="A"/>
<contactref element="E$9" pad="A"/>
<contactref element="E$7" pad="1"/>
<contactref element="E$24" pad="3"/>
<contactref element="E$14" pad="1"/>
<contactref element="E$4" pad="2"/>
<contactref element="E$13" pad="1"/>
</signal>
<signal name="S$12">
<contactref element="E$24" pad="1"/>
<contactref element="E$2" pad="2"/>
</signal>
<signal name="S$16">
<contactref element="E$14" pad="2"/>
<contactref element="E$4" pad="1"/>
<contactref element="E$23" pad="A"/>
<contactref element="E$30" pad="1"/>
</signal>
<signal name="S$15">
<contactref element="E$16" pad="1"/>
<contactref element="E$12" pad="3"/>
<contactref element="E$8" pad="C"/>
</signal>
<signal name="S$17">
<contactref element="E$22" pad="2"/>
<contactref element="E$12" pad="1"/>
<contactref element="E$19" pad="2"/>
<contactref element="E$1" pad="8"/>
<contactref element="E$31" pad="2"/>
<contactref element="E$32" pad="2"/>
</signal>
<signal name="S$13">
<contactref element="E$24" pad="2"/>
</signal>
<signal name="S$2">
<contactref element="E$28" pad="1"/>
<contactref element="E$29" pad="A"/>
</signal>
<signal name="S$14">
<contactref element="E$27" pad="K"/>
<contactref element="E$1" pad="7"/>
<contactref element="E$25" pad="A"/>
<contactref element="E$32" pad="3"/>
</signal>
<signal name="S$18">
<contactref element="E$26" pad="2"/>
<contactref element="E$25" pad="K"/>
</signal>
<signal name="S$19">
<contactref element="E$31" pad="1"/>
<contactref element="E$27" pad="A"/>
</signal>
<signal name="S$20">
<contactref element="E$1" pad="1"/>
<contactref element="E$32" pad="5"/>
</signal>
<signal name="S$21">
<contactref element="E$2" pad="1"/>
<contactref element="E$14" pad="3"/>
<contactref element="E$23" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
