(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 0)
    (no_connects 7)
    (area 114.884999 77.419999 210.870001 130.860001)
    (thickness 1.6)
    (drawings 14)
    (tracks 302)
    (zones 0)
    (modules 80)
    (nets 62)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.4)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x00030_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 "Net-(J2-Pad2)")
  (net 4 /MOSI)
  (net 5 /~SS1)
  (net 6 /SCLK)
  (net 7 /RSSI1)
  (net 8 "Net-(J3-Pad2)")
  (net 9 /RSSI2)
  (net 10 /~SS2)
  (net 11 /RSSI3)
  (net 12 /~SS3)
  (net 13 /~SS4)
  (net 14 /RSSI4)
  (net 15 "Net-(D1-Pad2)")
  (net 16 "Net-(D2-Pad1)")
  (net 17 /RSSI7)
  (net 18 /BATTDIV)
  (net 19 /RSSI8)
  (net 20 /TEMP)
  (net 21 "Net-(NANO1-Pad1)")
  (net 22 "Net-(NANO1-Pad2)")
  (net 23 "Net-(NANO1-Pad3)")
  (net 24 /~SS5)
  (net 25 /~SS6)
  (net 26 /~SS7)
  (net 27 /~SS8)
  (net 28 "Net-(NANO1-Pad15)")
  (net 29 "Net-(NANO1-Pad16)")
  (net 30 "Net-(NANO1-Pad18)")
  (net 31 /RSSI6)
  (net 32 /RSSI5)
  (net 33 "Net-(NANO1-Pad28)")
  (net 34 "Net-(NANO1-Pad29)")
  (net 35 "Net-(NANO1-Pad30)")
  (net 36 +BATT)
  (net 37 "Net-(RX1-Pad11)")
  (net 38 "Net-(RX1-Pad3)")
  (net 39 "Net-(RX1-Pad2)")
  (net 40 "Net-(RX2-Pad11)")
  (net 41 "Net-(RX2-Pad3)")
  (net 42 "Net-(RX2-Pad2)")
  (net 43 "Net-(RX3-Pad11)")
  (net 44 "Net-(RX3-Pad3)")
  (net 45 "Net-(RX3-Pad2)")
  (net 46 "Net-(RX4-Pad11)")
  (net 47 "Net-(RX4-Pad3)")
  (net 48 "Net-(RX4-Pad2)")
  (net 49 "Net-(RX5-Pad11)")
  (net 50 "Net-(RX5-Pad3)")
  (net 51 "Net-(RX5-Pad2)")
  (net 52 "Net-(RX6-Pad11)")
  (net 53 "Net-(RX6-Pad3)")
  (net 54 "Net-(RX6-Pad2)")
  (net 55 "Net-(RX7-Pad11)")
  (net 56 "Net-(RX7-Pad3)")
  (net 57 "Net-(RX7-Pad2)")
  (net 58 "Net-(RX8-Pad11)")
  (net 59 "Net-(RX8-Pad3)")
  (net 60 "Net-(RX8-Pad2)")
  (net 61 "Net-(RX8-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net +BATT)
    (add_net /BATTDIV)
    (add_net /MOSI)
    (add_net /RSSI1)
    (add_net /RSSI2)
    (add_net /RSSI3)
    (add_net /RSSI4)
    (add_net /RSSI5)
    (add_net /RSSI6)
    (add_net /RSSI7)
    (add_net /RSSI8)
    (add_net /SCLK)
    (add_net /TEMP)
    (add_net /~SS1)
    (add_net /~SS2)
    (add_net /~SS3)
    (add_net /~SS4)
    (add_net /~SS5)
    (add_net /~SS6)
    (add_net /~SS7)
    (add_net /~SS8)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(NANO1-Pad1)")
    (add_net "Net-(NANO1-Pad15)")
    (add_net "Net-(NANO1-Pad16)")
    (add_net "Net-(NANO1-Pad18)")
    (add_net "Net-(NANO1-Pad2)")
    (add_net "Net-(NANO1-Pad28)")
    (add_net "Net-(NANO1-Pad29)")
    (add_net "Net-(NANO1-Pad3)")
    (add_net "Net-(NANO1-Pad30)")
    (add_net "Net-(RX1-Pad11)")
    (add_net "Net-(RX1-Pad2)")
    (add_net "Net-(RX1-Pad3)")
    (add_net "Net-(RX2-Pad11)")
    (add_net "Net-(RX2-Pad2)")
    (add_net "Net-(RX2-Pad3)")
    (add_net "Net-(RX3-Pad11)")
    (add_net "Net-(RX3-Pad2)")
    (add_net "Net-(RX3-Pad3)")
    (add_net "Net-(RX4-Pad11)")
    (add_net "Net-(RX4-Pad2)")
    (add_net "Net-(RX4-Pad3)")
    (add_net "Net-(RX5-Pad11)")
    (add_net "Net-(RX5-Pad2)")
    (add_net "Net-(RX5-Pad3)")
    (add_net "Net-(RX6-Pad11)")
    (add_net "Net-(RX6-Pad2)")
    (add_net "Net-(RX6-Pad3)")
    (add_net "Net-(RX7-Pad11)")
    (add_net "Net-(RX7-Pad2)")
    (add_net "Net-(RX7-Pad3)")
    (add_net "Net-(RX8-Pad1)")
    (add_net "Net-(RX8-Pad11)")
    (add_net "Net-(RX8-Pad2)")
    (add_net "Net-(RX8-Pad3)")
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 156.972 122.682)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 156.972 128.682)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 156.972 126.682)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 156.972 124.682)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 166.751 118.6815)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 166.751 117.4115)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 166.8145 116.205)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 170.6245 114.935)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 169.3545 114.935)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 168.0845 114.935)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 166.8145 114.935)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 165.5445 114.935)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 165.5445 116.1415)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 165.5445 117.4115)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 165.5445 118.6815)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 199.993 120.903)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 197.993 120.903)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 199.993 118.903)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 197.993 118.903)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 199.993 116.903)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 197.993 116.903)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 199.993 114.903)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 197.993 114.903)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 199.993 112.903)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 197.993 112.903)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 198.12 96.519)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 200.12 96.519)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 200.12 94.519)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 198.12 94.519)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 200.12 92.519)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 198.12 92.519)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 200.12 90.519)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 198.12 90.519)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 200.12 88.519)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 198.12 88.519)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 128.238 96.265)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 126.238 96.265)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 128.238 94.265)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 126.238 94.265)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 128.238 92.265)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 126.238 92.265)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 128.238 90.265)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 126.238 90.265)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 128.238 88.265)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 126.238 88.265)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 128.111 120.649)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 128.111 118.649)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 128.111 116.649)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 128.111 114.649)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 128.111 112.649)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 126.111 120.649)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 126.111 118.649)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 126.111 116.649)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 126.111 114.649)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:RX5808 (layer F.Cu) (tedit 59A58FA9)
    (at 121.666 127.762)
    (fp_text reference RX1 (at 7.874 -3.556) (layer F.SilkS))
    (fp_text value RX5808 (at 3.87 -20.785) (layer F.Fab))
    (fp_text user GND (at 24.892 -21.336) (layer F.SilkS))
    (fp_text user Video (at 24.384 -18.796) (layer F.SilkS))
    (fp_text user A6.5m (at 24.384 -16.256) (layer F.SilkS))
    (fp_text user RSSI (at 24.892 -13.716) (layer F.SilkS))
    (fp_text user 5V (at 25.4 -11.176) (layer F.SilkS))
    (fp_text user GND (at 24.892 -8.636) (layer F.SilkS))
    (fp_text user SCLK (at 24.892 -6.096) (layer F.SilkS))
    (fp_text user MOSI (at 24.892 -1.016) (layer F.SilkS))
    (fp_text user ~SS (at 25.4 -3.556) (layer F.SilkS))
    (fp_text user ANT (at 2.286 -3.556) (layer F.SilkS))
    (fp_text user GND (at 2.54 -1.016) (layer F.SilkS))
    (fp_text user GND (at 2.54 -6.096) (layer F.SilkS))
    (pad 9 smd oval (at 28 -1.1) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /MOSI))
    (pad 10 smd oval (at 0 -6.18) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd oval (at 0 -3.64) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(RX1-Pad11)"))
    (pad 12 smd oval (at 0 -1.1) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd oval (at 28 -3.64) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /~SS1))
    (pad 7 smd oval (at 28 -6.18) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /SCLK))
    (pad 6 smd oval (at 28 -8.72) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 28 -11.26) (size 2 1.6) (drill oval 0.75) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 4 smd oval (at 28 -13.8) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /RSSI1))
    (pad 3 smd oval (at 28 -16.34) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(RX1-Pad3)"))
    (pad 2 smd oval (at 28 -18.88) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(RX1-Pad2)"))
    (pad 1 smd oval (at 28 -21.42) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 599B42B2)
    (at 152.4 125.984)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at -1.016 -2.032) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-41_SOD81_P10.16mm_Horizontal (layer B.Cu) (tedit 599B4E00)
    (at 170.18 99.06 180)
    (descr "D, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D2 (at 5.08 2.41 180) (layer B.SilkS))
    (fp_text value D_Schottky (at 4.572 2.54 180) (layer B.Fab))
    (fp_text user %R (at 5.08 0 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS3 (layer B.Cu) (tedit 599B3DDC)
    (at 161.036 94.488 180)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J2 (at 1.524 0 270) (layer B.SilkS))
    (fp_text value GS3 (at 1.8 0 270) (layer B.Fab))
    (pad 1 smd rect (at 0 1.27 180) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 17 /RSSI7))
    (pad 2 smd rect (at 0 0 180) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (pad 3 smd rect (at 0 -1.27 180) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 18 /BATTDIV))
  )
  (module Connectors:GS3 (layer B.Cu) (tedit 599B3DF6)
    (at 161.036 89.916)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J3 (at -1.524 0 90) (layer B.SilkS))
    (fp_text value GS3 (at 2.54 0 90) (layer B.Fab))
    (pad 1 smd rect (at 0 1.27) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 19 /RSSI8))
    (pad 2 smd rect (at 0 0) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J3-Pad2)"))
    (pad 3 smd rect (at 0 -1.27) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 20 /TEMP))
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 599B42C2)
    (at 154.432 112.268 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 9.144 2.032 270) (layer F.SilkS))
    (fp_text value 330 (at 5.08 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer B.Cu) (tedit 599B3E75)
    (at 154.432 118.618 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 9.652 -2.032 90) (layer B.SilkS))
    (fp_text value 100k (at 5.461 0 90) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 +BATT))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /BATTDIV))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer B.Cu) (tedit 599B3E5D)
    (at 154.432 106.172 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 9.652 -2.032 90) (layer B.SilkS))
    (fp_text value 10k (at 5.334 0 90) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /BATTDIV))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module RX5808:5VBEC (layer B.Cu) (tedit 599F472F)
    (at 170.688 101.6 180)
    (fp_text reference REG1 (at 5.5 -8.5 180) (layer B.SilkS))
    (fp_text value 5VRegulator (at 5.5 -7 180) (layer B.Fab))
    (fp_text user GND (at 1.27 -3.302 180) (layer B.SilkS))
    (fp_text user 5V (at 9.652 -3.302 180) (layer B.SilkS))
    (fp_text user "VIN (6-23V)" (at 10.033 -20.32 360) (layer B.SilkS))
    (fp_text user GND (at 0.508 -20.32 360) (layer B.SilkS))
    (pad 4 smd rect (at 1.27 -1.27 180) (size 2.54 2.54) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 9.73 -1.27 180) (size 2.54 2.54) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.27 -15.77 180) (size 2.54 2.54) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 9.73 -15.77 180) (size 2.54 2.54) (layers B.Cu B.Paste B.Mask)
      (net 36 +BATT))
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 599B4854)
    (at 153.416 89.408 270)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U1 (at 2.54 -1.524 270) (layer F.SilkS))
    (fp_text value LM35-LP (at -3.556 0 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 90) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 20 /TEMP))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module RX5808:ArduinoNano (layer F.Cu) (tedit 599C83A3)
    (at 156.21 80.01)
    (fp_text reference NANO1 (at 8.89 1.27) (layer F.SilkS))
    (fp_text value ArduinoNano (at 8.636 3.556) (layer F.Fab))
    (fp_text user USB (at 8.89 41.783) (layer F.SilkS))
    (pad 1 thru_hole rect (at 1.27 3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(NANO1-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(NANO1-Pad2)"))
    (pad 3 thru_hole circle (at 1.27 8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(NANO1-Pad3)"))
    (pad 4 thru_hole circle (at 1.27 11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 1.27 13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /SCLK))
    (pad 6 thru_hole circle (at 1.27 16.51) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /MOSI))
    (pad 7 thru_hole circle (at 1.27 19.05) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /~SS8))
    (pad 8 thru_hole circle (at 1.27 21.59) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /~SS7))
    (pad 9 thru_hole circle (at 1.27 24.13) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /~SS6))
    (pad 10 thru_hole circle (at 1.27 26.67) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /~SS5))
    (pad 11 thru_hole circle (at 1.27 29.21) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /~SS4))
    (pad 12 thru_hole circle (at 1.27 31.75) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /~SS3))
    (pad 13 thru_hole circle (at 1.27 34.29) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /~SS2))
    (pad 14 thru_hole circle (at 1.27 36.83) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /~SS1))
    (pad 15 thru_hole circle (at 1.27 39.37) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(NANO1-Pad15)"))
    (pad 16 thru_hole circle (at 16.51 3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(NANO1-Pad16)"))
    (pad 17 thru_hole circle (at 16.51 6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 18 thru_hole circle (at 16.51 8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(NANO1-Pad18)"))
    (pad 19 thru_hole circle (at 16.51 11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(D2-Pad1)"))
    (pad 20 thru_hole circle (at 16.51 13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad2)"))
    (pad 21 thru_hole circle (at 16.51 16.51) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (pad 22 thru_hole circle (at 16.51 19.05) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /RSSI6))
    (pad 23 thru_hole circle (at 16.51 21.59) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /RSSI5))
    (pad 24 thru_hole circle (at 16.51 24.13) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /RSSI4))
    (pad 25 thru_hole circle (at 16.51 26.67) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /RSSI3))
    (pad 26 thru_hole circle (at 16.51 29.21) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /RSSI2))
    (pad 27 thru_hole circle (at 16.51 31.75) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /RSSI1))
    (pad 28 thru_hole circle (at 16.51 34.29) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(NANO1-Pad28)"))
    (pad 29 thru_hole circle (at 16.51 36.83) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(NANO1-Pad29)"))
    (pad 30 thru_hole circle (at 16.51 39.37) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(NANO1-Pad30)"))
  )
  (module RX5808:XT60_5V (layer B.Cu) (tedit 59A1F11B)
    (at 171.196 125.222 180)
    (fp_text reference J1 (at -2.54 1.27 180) (layer B.SilkS) hide)
    (fp_text value CONN_01X02 (at 6.35 -1.905 180) (layer B.Fab))
    (fp_text user GND (at 2.54 3.81 180) (layer B.SilkS))
    (fp_text user 6-23V (at 9.525 3.81 180) (layer B.SilkS))
    (pad 2 smd rect (at 9.54 2.54 180) (size 5.08 5.08) (layers B.Cu B.Paste B.Mask)
      (net 36 +BATT))
    (pad 1 smd rect (at 2.54 2.54 180) (size 5.08 5.08) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 59A31DBB)
    (at 118.364 91.948)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value "" (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 59A31DA9)
    (at 118.364 116.84)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value "" (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 59A31D94)
    (at 207.264 116.84)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value "" (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 59A31D83)
    (at 207.264 92.202)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value "" (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module RX5808:RX5808 (layer F.Cu) (tedit 59A58FA9)
    (at 204.216 81.026 180)
    (fp_text reference RX6 (at 7.874 -3.556 180) (layer F.SilkS))
    (fp_text value RX5808 (at 3.87 -20.785 180) (layer F.Fab))
    (fp_text user GND (at 24.892 -21.336 180) (layer F.SilkS))
    (fp_text user Video (at 24.384 -18.796 180) (layer F.SilkS))
    (fp_text user A6.5m (at 24.384 -16.256 180) (layer F.SilkS))
    (fp_text user RSSI (at 24.892 -13.716 180) (layer F.SilkS))
    (fp_text user 5V (at 25.4 -11.176 180) (layer F.SilkS))
    (fp_text user GND (at 24.892 -8.636 180) (layer F.SilkS))
    (fp_text user SCLK (at 24.892 -6.096 180) (layer F.SilkS))
    (fp_text user MOSI (at 24.892 -1.016 180) (layer F.SilkS))
    (fp_text user ~SS (at 25.4 -3.556 180) (layer F.SilkS))
    (fp_text user ANT (at 2.286 -3.556 180) (layer F.SilkS))
    (fp_text user GND (at 2.54 -1.016 180) (layer F.SilkS))
    (fp_text user GND (at 2.54 -6.096 180) (layer F.SilkS))
    (pad 9 smd oval (at 28 -1.1 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /MOSI))
    (pad 10 smd oval (at 0 -6.18 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd oval (at 0 -3.64 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(RX6-Pad11)"))
    (pad 12 smd oval (at 0 -1.1 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd oval (at 28 -3.64 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 25 /~SS6))
    (pad 7 smd oval (at 28 -6.18 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /SCLK))
    (pad 6 smd oval (at 28 -8.72 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 28 -11.26 180) (size 2 1.6) (drill oval 0.75) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 4 smd oval (at 28 -13.8 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 31 /RSSI6))
    (pad 3 smd oval (at 28 -16.34 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(RX6-Pad3)"))
    (pad 2 smd oval (at 28 -18.88 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(RX6-Pad2)"))
    (pad 1 smd oval (at 28 -21.42 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module RX5808:RX5808 (layer F.Cu) (tedit 59A58FA9)
    (at 204.216 105.664 180)
    (fp_text reference RX2 (at 7.874 -3.556 180) (layer F.SilkS))
    (fp_text value RX5808 (at 3.87 -20.785 180) (layer F.Fab))
    (fp_text user GND (at 24.892 -21.336 180) (layer F.SilkS))
    (fp_text user Video (at 24.384 -18.796 180) (layer F.SilkS))
    (fp_text user A6.5m (at 24.384 -16.256 180) (layer F.SilkS))
    (fp_text user RSSI (at 24.892 -13.716 180) (layer F.SilkS))
    (fp_text user 5V (at 25.4 -11.176 180) (layer F.SilkS))
    (fp_text user GND (at 24.892 -8.636 180) (layer F.SilkS))
    (fp_text user SCLK (at 24.892 -6.096 180) (layer F.SilkS))
    (fp_text user MOSI (at 24.892 -1.016 180) (layer F.SilkS))
    (fp_text user ~SS (at 25.4 -3.556 180) (layer F.SilkS))
    (fp_text user ANT (at 2.286 -3.556 180) (layer F.SilkS))
    (fp_text user GND (at 2.54 -1.016 180) (layer F.SilkS))
    (fp_text user GND (at 2.54 -6.096 180) (layer F.SilkS))
    (pad 9 smd oval (at 28 -1.1 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /MOSI))
    (pad 10 smd oval (at 0 -6.18 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd oval (at 0 -3.64 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(RX2-Pad11)"))
    (pad 12 smd oval (at 0 -1.1 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd oval (at 28 -3.64 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /~SS2))
    (pad 7 smd oval (at 28 -6.18 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /SCLK))
    (pad 6 smd oval (at 28 -8.72 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 28 -11.26 180) (size 2 1.6) (drill oval 0.75) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 4 smd oval (at 28 -13.8 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /RSSI2))
    (pad 3 smd oval (at 28 -16.34 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(RX2-Pad3)"))
    (pad 2 smd oval (at 28 -18.88 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(RX2-Pad2)"))
    (pad 1 smd oval (at 28 -21.42 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module RX5808:RX5808 (layer B.Cu) (tedit 59A58FA9)
    (at 204.216 128.27 180)
    (fp_text reference RX3 (at 7.874 3.556 180) (layer B.SilkS))
    (fp_text value RX5808 (at 3.87 20.785 180) (layer B.Fab))
    (fp_text user GND (at 24.892 21.336 180) (layer B.SilkS))
    (fp_text user Video (at 24.384 18.796 180) (layer B.SilkS))
    (fp_text user A6.5m (at 24.384 16.256 180) (layer B.SilkS))
    (fp_text user RSSI (at 24.892 13.716 180) (layer B.SilkS))
    (fp_text user 5V (at 25.4 11.176 180) (layer B.SilkS))
    (fp_text user GND (at 24.892 8.636 180) (layer B.SilkS))
    (fp_text user SCLK (at 24.892 6.096 180) (layer B.SilkS))
    (fp_text user MOSI (at 24.892 1.016 180) (layer B.SilkS))
    (fp_text user ~SS (at 25.4 3.556 180) (layer B.SilkS))
    (fp_text user ANT (at 2.286 3.556 180) (layer B.SilkS))
    (fp_text user GND (at 2.54 1.016 180) (layer B.SilkS))
    (fp_text user GND (at 2.54 6.096 180) (layer B.SilkS))
    (pad 9 smd oval (at 28 1.1 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 /MOSI))
    (pad 10 smd oval (at 0 6.18 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 11 smd oval (at 0 3.64 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(RX3-Pad11)"))
    (pad 12 smd oval (at 0 1.1 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd oval (at 28 3.64 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 /~SS3))
    (pad 7 smd oval (at 28 6.18 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 /SCLK))
    (pad 6 smd oval (at 28 8.72 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 28 11.26 180) (size 2 1.6) (drill oval 0.75) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 4 smd oval (at 28 13.8 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 /RSSI3))
    (pad 3 smd oval (at 28 16.34 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(RX3-Pad3)"))
    (pad 2 smd oval (at 28 18.88 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(RX3-Pad2)"))
    (pad 1 smd oval (at 28 21.42 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module RX5808:RX5808 (layer B.Cu) (tedit 59A58FA9)
    (at 121.666 105.156)
    (fp_text reference RX4 (at 7.874 3.556) (layer B.SilkS))
    (fp_text value RX5808 (at 3.87 20.785) (layer B.Fab))
    (fp_text user GND (at 24.892 21.336) (layer B.SilkS))
    (fp_text user Video (at 24.384 18.796) (layer B.SilkS))
    (fp_text user A6.5m (at 24.384 16.256) (layer B.SilkS))
    (fp_text user RSSI (at 24.892 13.716) (layer B.SilkS))
    (fp_text user 5V (at 25.4 11.176) (layer B.SilkS))
    (fp_text user GND (at 24.892 8.636) (layer B.SilkS))
    (fp_text user SCLK (at 24.892 6.096) (layer B.SilkS))
    (fp_text user MOSI (at 24.892 1.016) (layer B.SilkS))
    (fp_text user ~SS (at 25.4 3.556) (layer B.SilkS))
    (fp_text user ANT (at 2.286 3.556) (layer B.SilkS))
    (fp_text user GND (at 2.54 1.016) (layer B.SilkS))
    (fp_text user GND (at 2.54 6.096) (layer B.SilkS))
    (pad 9 smd oval (at 28 1.1) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 /MOSI))
    (pad 10 smd oval (at 0 6.18) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 11 smd oval (at 0 3.64) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(RX4-Pad11)"))
    (pad 12 smd oval (at 0 1.1) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd oval (at 28 3.64) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 13 /~SS4))
    (pad 7 smd oval (at 28 6.18) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 /SCLK))
    (pad 6 smd oval (at 28 8.72) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 28 11.26) (size 2 1.6) (drill oval 0.75) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 4 smd oval (at 28 13.8) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 14 /RSSI4))
    (pad 3 smd oval (at 28 16.34) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(RX4-Pad3)"))
    (pad 2 smd oval (at 28 18.88) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(RX4-Pad2)"))
    (pad 1 smd oval (at 28 21.42) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module RX5808:RX5808 (layer F.Cu) (tedit 59A58FA9)
    (at 121.666 103.124)
    (fp_text reference RX5 (at 7.874 -3.556) (layer F.SilkS))
    (fp_text value RX5808 (at 3.87 -20.785) (layer F.Fab))
    (fp_text user GND (at 24.892 -21.336) (layer F.SilkS))
    (fp_text user Video (at 24.384 -18.796) (layer F.SilkS))
    (fp_text user A6.5m (at 24.384 -16.256) (layer F.SilkS))
    (fp_text user RSSI (at 24.892 -13.716) (layer F.SilkS))
    (fp_text user 5V (at 25.4 -11.176) (layer F.SilkS))
    (fp_text user GND (at 24.892 -8.636) (layer F.SilkS))
    (fp_text user SCLK (at 24.892 -6.096) (layer F.SilkS))
    (fp_text user MOSI (at 24.892 -1.016) (layer F.SilkS))
    (fp_text user ~SS (at 25.4 -3.556) (layer F.SilkS))
    (fp_text user ANT (at 2.286 -3.556) (layer F.SilkS))
    (fp_text user GND (at 2.54 -1.016) (layer F.SilkS))
    (fp_text user GND (at 2.54 -6.096) (layer F.SilkS))
    (pad 9 smd oval (at 28 -1.1) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /MOSI))
    (pad 10 smd oval (at 0 -6.18) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd oval (at 0 -3.64) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(RX5-Pad11)"))
    (pad 12 smd oval (at 0 -1.1) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd oval (at 28 -3.64) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 24 /~SS5))
    (pad 7 smd oval (at 28 -6.18) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /SCLK))
    (pad 6 smd oval (at 28 -8.72) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 28 -11.26) (size 2 1.6) (drill oval 0.75) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 4 smd oval (at 28 -13.8) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 32 /RSSI5))
    (pad 3 smd oval (at 28 -16.34) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(RX5-Pad3)"))
    (pad 2 smd oval (at 28 -18.88) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(RX5-Pad2)"))
    (pad 1 smd oval (at 28 -21.42) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module RX5808:RX5808 (layer B.Cu) (tedit 59A58FA9)
    (at 204.216 103.632 180)
    (fp_text reference RX7 (at 7.874 3.556 180) (layer B.SilkS))
    (fp_text value RX5808 (at 3.87 20.785 180) (layer B.Fab))
    (fp_text user GND (at 24.892 21.336 180) (layer B.SilkS))
    (fp_text user Video (at 24.384 18.796 180) (layer B.SilkS))
    (fp_text user A6.5m (at 24.384 16.256 180) (layer B.SilkS))
    (fp_text user RSSI (at 24.892 13.716 180) (layer B.SilkS))
    (fp_text user 5V (at 25.4 11.176 180) (layer B.SilkS))
    (fp_text user GND (at 24.892 8.636 180) (layer B.SilkS))
    (fp_text user SCLK (at 24.892 6.096 180) (layer B.SilkS))
    (fp_text user MOSI (at 24.892 1.016 180) (layer B.SilkS))
    (fp_text user ~SS (at 25.4 3.556 180) (layer B.SilkS))
    (fp_text user ANT (at 2.286 3.556 180) (layer B.SilkS))
    (fp_text user GND (at 2.54 1.016 180) (layer B.SilkS))
    (fp_text user GND (at 2.54 6.096 180) (layer B.SilkS))
    (pad 9 smd oval (at 28 1.1 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 /MOSI))
    (pad 10 smd oval (at 0 6.18 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 11 smd oval (at 0 3.64 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(RX7-Pad11)"))
    (pad 12 smd oval (at 0 1.1 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd oval (at 28 3.64 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 26 /~SS7))
    (pad 7 smd oval (at 28 6.18 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 /SCLK))
    (pad 6 smd oval (at 28 8.72 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 28 11.26 180) (size 2 1.6) (drill oval 0.75) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 4 smd oval (at 28 13.8 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 17 /RSSI7))
    (pad 3 smd oval (at 28 16.34 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(RX7-Pad3)"))
    (pad 2 smd oval (at 28 18.88 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(RX7-Pad2)"))
    (pad 1 smd oval (at 28 21.42 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module RX5808:RX5808 (layer B.Cu) (tedit 59A58FA9)
    (at 121.666 80.518)
    (fp_text reference RX8 (at 7.874 3.556) (layer B.SilkS))
    (fp_text value RX5808 (at 3.87 20.785) (layer B.Fab))
    (fp_text user GND (at 24.892 21.336) (layer B.SilkS))
    (fp_text user Video (at 24.384 18.796) (layer B.SilkS))
    (fp_text user A6.5m (at 24.384 16.256) (layer B.SilkS))
    (fp_text user RSSI (at 24.892 13.716) (layer B.SilkS))
    (fp_text user 5V (at 25.4 11.176) (layer B.SilkS))
    (fp_text user GND (at 24.892 8.636) (layer B.SilkS))
    (fp_text user SCLK (at 24.892 6.096) (layer B.SilkS))
    (fp_text user MOSI (at 24.892 1.016) (layer B.SilkS))
    (fp_text user ~SS (at 25.4 3.556) (layer B.SilkS))
    (fp_text user ANT (at 2.286 3.556) (layer B.SilkS))
    (fp_text user GND (at 2.54 1.016) (layer B.SilkS))
    (fp_text user GND (at 2.54 6.096) (layer B.SilkS))
    (pad 9 smd oval (at 28 1.1) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 /MOSI))
    (pad 10 smd oval (at 0 6.18) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 11 smd oval (at 0 3.64) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(RX8-Pad11)"))
    (pad 12 smd oval (at 0 1.1) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd oval (at 28 3.64) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 27 /~SS8))
    (pad 7 smd oval (at 28 6.18) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 /SCLK))
    (pad 6 smd oval (at 28 8.72) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 28 11.26) (size 2 1.6) (drill oval 0.75) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 4 smd oval (at 28 13.8) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 19 /RSSI8))
    (pad 3 smd oval (at 28 16.34) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(RX8-Pad3)"))
    (pad 2 smd oval (at 28 18.88) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(RX8-Pad2)"))
    (pad 1 smd oval (at 28 21.42) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(RX8-Pad1)"))
  )
  (module Symbols:OSHW-Logo_11.4x12mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 136.652 91.948 180)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo_11.4x12mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module RX5808:VIA_STITCH (layer F.Cu) (tedit 59A5EEDA)
    (at 126.111 112.649)
    (fp_text reference REF** (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value VIA_STITCH (at 0 -1.27) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module RX5808:LOGO (layer B.Cu) (tedit 0)
    (at 188.722 91.8845 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_text "http://propnuts.co.uk/\n" (at 204.216 78.867) (layer F.SilkS))
  (gr_line (start 114.935 128.27) (end 114.935 80.01) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 158.242 130.81) (end 117.475 130.81) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 208.28 130.81) (end 172.085 130.81) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 210.82 80.01) (end 210.82 128.27) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.475 77.47) (end 208.28 77.47) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 208.28 80.01) (end 208.28 77.47) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 208.28 128.27) (end 210.82 128.27) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 117.475 128.27) (end 117.475 130.81) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 117.475 80.01) (end 114.935 80.01) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "PropNuts WizardTracker (v2)" (at 132.334 78.74) (layer F.SilkS))
  (gr_line (start 172.085 125.73) (end 172.085 130.81) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 158.242 125.73) (end 172.085 125.73) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 158.242 130.81) (end 158.242 125.73) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.92 123.19) (xy 120.015 121.285) (xy 113.03 121.285) (xy 113.03 127) (xy 120.015 127)
        (xy 121.92 125.095)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.92 123.19) (xy 120.015 121.285) (xy 113.03 121.285) (xy 113.03 127) (xy 120.015 127)
        (xy 121.92 125.095)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.92 107.95) (xy 120.015 106.045) (xy 113.03 106.045) (xy 113.03 111.76) (xy 120.015 111.76)
        (xy 121.92 109.855)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.92 107.95) (xy 120.015 106.045) (xy 113.03 106.045) (xy 113.03 111.76) (xy 120.015 111.76)
        (xy 121.92 109.855)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.92 98.425) (xy 120.015 96.52) (xy 113.03 96.52) (xy 113.03 102.235) (xy 120.015 102.235)
        (xy 121.92 100.33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.92 98.425) (xy 120.015 96.52) (xy 113.03 96.52) (xy 113.03 102.235) (xy 120.015 102.235)
        (xy 121.92 100.33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.92 85.09) (xy 120.015 86.995) (xy 113.03 86.995) (xy 113.03 81.28) (xy 120.015 81.28)
        (xy 121.92 83.185)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.92 85.09) (xy 120.015 86.995) (xy 113.03 86.995) (xy 113.03 81.28) (xy 120.015 81.28)
        (xy 121.92 83.185)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 203.835 83.82) (xy 205.74 81.915) (xy 212.725 81.915) (xy 212.725 87.63) (xy 205.74 87.63)
        (xy 203.835 85.725)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 203.835 83.82) (xy 205.74 81.915) (xy 212.725 81.915) (xy 212.725 87.63) (xy 205.74 87.63)
        (xy 203.835 85.725)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 203.835 99.06) (xy 205.74 97.155) (xy 212.725 97.155) (xy 212.725 102.87) (xy 205.74 102.87)
        (xy 203.835 100.965)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 203.835 99.06) (xy 205.74 97.155) (xy 212.725 97.155) (xy 212.725 102.87) (xy 205.74 102.87)
        (xy 203.835 100.965)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 203.835 108.585) (xy 205.74 106.68) (xy 212.725 106.68) (xy 212.725 111.76) (xy 205.74 111.76)
        (xy 204.47 110.49) (xy 203.835 110.49)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 203.835 108.585) (xy 205.74 106.68) (xy 212.725 106.68) (xy 212.725 111.76) (xy 205.74 111.76)
        (xy 204.47 110.49) (xy 203.835 110.49)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 203.835 123.825) (xy 205.74 121.92) (xy 212.725 121.92) (xy 212.725 127) (xy 205.74 127)
        (xy 204.47 125.73) (xy 203.835 125.73)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 203.835 123.825) (xy 205.74 121.92) (xy 212.725 121.92) (xy 212.725 127) (xy 205.74 127)
        (xy 204.47 125.73) (xy 203.835 125.73)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 210.82 77.47) (xy 114.935 77.47) (xy 114.935 130.81) (xy 158.242 130.81) (xy 158.242 125.73)
        (xy 172.085 125.73) (xy 172.085 130.81) (xy 210.82 130.81)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.935 77.47) (xy 210.82 77.47) (xy 210.82 130.81) (xy 171.45 130.81) (xy 171.45 125.73)
        (xy 158.75 125.73) (xy 158.75 130.81) (xy 114.935 130.81)
      )
    )
  )
)
