<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="40.62" y2="0" width="0" layer="20"/>
<wire x1="40.62" y1="0" x2="40.62" y2="22.53" width="0" layer="20"/>
<wire x1="40.62" y1="22.53" x2="0" y2="22.53" width="0" layer="20"/>
<wire x1="0" y1="22.53" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="1_eagle_lib">
<packages>
<package name="RK27112">
<description>ALPS Single-shaft, dual-unit
RK27112</description>
</package>
<package name="WIREPAD">
<description>Pad for soldered wire</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="P1" library="1_eagle_lib" package="RK27112" value=""/>
<element name="1IN" library="1_eagle_lib" package="WIREPAD" value="WIREPAD"/>
<element name="1G" library="1_eagle_lib" package="WIREPAD" value="WIREPAD"/>
<element name="2IN" library="1_eagle_lib" package="WIREPAD" value="WIREPAD"/>
<element name="2G" library="1_eagle_lib" package="WIREPAD" value="WIREPAD"/>
<element name="1OUT" library="1_eagle_lib" package="WIREPAD" value="WIREPAD"/>
<element name="1G'" library="1_eagle_lib" package="WIREPAD" value="WIREPAD">
<attribute name="NAME"/>
</element>
<element name="2OUT" library="1_eagle_lib" package="WIREPAD" value="WIREPAD"/>
<element name="2G'" library="1_eagle_lib" package="WIREPAD" value="WIREPAD">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="P1" pad="1.CW"/>
<contactref element="1IN" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="P1" pad="1.CCW"/>
<contactref element="1G" pad="P$1"/>
<contactref element="1G'" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="P1" pad="1.W"/>
<contactref element="1OUT" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="P1" pad="2.CW"/>
<contactref element="2IN" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="P1" pad="2.CCW"/>
<contactref element="2G" pad="P$1"/>
<contactref element="2G'" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="P1" pad="2.W"/>
<contactref element="2OUT" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
