<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<hole x="1.27" y="57.785" drill="2.2"/>
<hole x="19.05" y="57.785" drill="2.2"/>
<wire x1="-0.635" y1="80.645" x2="21.59" y2="80.645" width="0" layer="20"/>
<wire x1="21.59" y1="80.645" x2="21.59" y2="55.88" width="0" layer="20"/>
<wire x1="21.59" y1="55.88" x2="16.51" y2="55.88" width="0" layer="20"/>
<wire x1="16.51" y1="55.88" x2="16.51" y2="43.815" width="0" layer="20"/>
<wire x1="16.51" y1="43.815" x2="4.445" y2="43.815" width="0" layer="20"/>
<wire x1="4.445" y1="43.815" x2="4.445" y2="55.88" width="0" layer="20"/>
<wire x1="4.445" y1="55.88" x2="-0.635" y2="55.88" width="0" layer="20"/>
<wire x1="-0.635" y1="55.88" x2="-0.635" y2="80.645" width="0" layer="20"/>
<text>Charlie Hoey 4.16.16</text>
<text>Flimshaw Industries</text>
<text>LED Matrix Minidriver</text>
</plain>
<libraries>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="SEGMENT_BL-M07C881UR">
</package>
</packages>
</library>
<library name="GeekAmmo">
<description>&lt;h3&gt;GeekAmmo  Library&lt;/h3&gt;

These are parts used by the GeekAmmo company (now part of SparkFun Electronics)!

 If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-MALE-A-PCB">
<description>&lt;b&gt;USB Male A for direct PCB&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="atmel" package="TQFP32-08" value="MEGA8-AI">
<attribute name="OC_FARNELL" value="9171371"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA8-16AU"/>
<attribute name="OC_NEWARK" value="73M8863"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="2X3" value="AVR_SPI">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="adafruit" package="SEGMENT_BL-M07C881UR" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="GeekAmmo" package="USB-MALE-A-PCB" value="USB-CON-4PIN"/>
</elements>
<signals>
<signal name="AVCC">
<contactref element="IC1" pad="18"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="30"/>
<contactref element="LED1" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="31"/>
<contactref element="LED1" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="32"/>
<contactref element="LED1" pad="7"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="1"/>
<contactref element="LED1" pad="8"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="2"/>
<contactref element="LED1" pad="16"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="9"/>
<contactref element="LED1" pad="15"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="10"/>
<contactref element="LED1" pad="14"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="11"/>
<contactref element="LED1" pad="13"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="12"/>
<contactref element="LED1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="13"/>
<contactref element="LED1" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="14"/>
<contactref element="LED1" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="15"/>
<contactref element="LED1" pad="4"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="16"/>
<contactref element="LED1" pad="12"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="17"/>
<contactref element="LED1" pad="11"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="IC1" pad="7"/>
<contactref element="LED1" pad="10"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="8"/>
<contactref element="LED1" pad="9"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="21"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="5"/>
<contactref element="JP1" pad="6"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="6"/>
<contactref element="JP1" pad="2"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="JP1" pad="5"/>
<contactref element="IC1" pad="29"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
