(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 114)
    (no_connects 0)
    (area 79.680999 70.917999 192.607001 161.873001)
    (thickness 1.6)
    (drawings 33)
    (tracks 494)
    (zones 0)
    (modules 56)
    (nets 52)
  )
  (page USLetter)
  (title_block
    (title "2CHAINZ INTERFACE BOARD")
    (date 2017-07-10)
    (rev 0)
    (company 2WILLZ)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 2)
    (user_trace_width 1)
    (user_trace_width 2)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory mk0-renders/))
  )
  (net 0 "")
  (net 1 MLE)
  (net 2 "Net-(DRV-L1-Pad2)")
  (net 3 "Net-(DRV-L1-Pad3)")
  (net 4 "Net-(DRV-L1-Pad4)")
  (net 5 MLS)
  (net 6 MLD)
  (net 7 "Net-(DRV-L1-Pad11)")
  (net 8 "Net-(DRV-L1-Pad12)")
  (net 9 "Net-(DRV-L1-Pad13)")
  (net 10 "Net-(DRV-L1-Pad14)")
  (net 11 MRE)
  (net 12 MRS)
  (net 13 MRD)
  (net 14 "Net-(DRV-R1-Pad11)")
  (net 15 "Net-(DRV-R1-Pad12)")
  (net 16 "Net-(DRV-R1-Pad13)")
  (net 17 "Net-(DRV-R1-Pad14)")
  (net 18 SDA)
  (net 19 "Net-(ENCODER-SP1-Pad2)")
  (net 20 "Net-(ENCODER-SP1-Pad3)")
  (net 21 SCL)
  (net 22 "Net-(PHOTO-L1-Pad2)")
  (net 23 VCC)
  (net 24 GND)
  (net 25 +12V)
  (net 26 "Net-(D1-Pad1)")
  (net 27 "Net-(D2-Pad1)")
  (net 28 "Net-(D3-Pad1)")
  (net 29 INETRDY)
  (net 30 "Net-(D4-Pad1)")
  (net 31 "Net-(D5-Pad1)")
  (net 32 IRUN)
  (net 33 "Net-(D6-Pad1)")
  (net 34 IFAULT)
  (net 35 "Net-(D7-Pad1)")
  (net 36 LFR)
  (net 37 LFF)
  (net 38 "Net-(D10-Pad1)")
  (net 39 RFR)
  (net 40 RFF)
  (net 41 MLARM_)
  (net 42 MRARM_)
  (net 43 "Net-(R7-Pad1)")
  (net 44 "Net-(R8-Pad1)")
  (net 45 INETCON)
  (net 46 "Net-(Q1-Pad2)")
  (net 47 "Net-(Q1-Pad1)")
  (net 48 "Net-(Q2-Pad2)")
  (net 49 "Net-(Q3-Pad2)")
  (net 50 "Net-(D11-Pad2)")
  (net 51 ARM+)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +12V)
    (add_net ARM+)
    (add_net GND)
    (add_net IFAULT)
    (add_net INETCON)
    (add_net INETRDY)
    (add_net IRUN)
    (add_net LFF)
    (add_net LFR)
    (add_net MLARM_)
    (add_net MLD)
    (add_net MLE)
    (add_net MLS)
    (add_net MRARM_)
    (add_net MRD)
    (add_net MRE)
    (add_net MRS)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(DRV-L1-Pad11)")
    (add_net "Net-(DRV-L1-Pad12)")
    (add_net "Net-(DRV-L1-Pad13)")
    (add_net "Net-(DRV-L1-Pad14)")
    (add_net "Net-(DRV-L1-Pad2)")
    (add_net "Net-(DRV-L1-Pad3)")
    (add_net "Net-(DRV-L1-Pad4)")
    (add_net "Net-(DRV-R1-Pad11)")
    (add_net "Net-(DRV-R1-Pad12)")
    (add_net "Net-(DRV-R1-Pad13)")
    (add_net "Net-(DRV-R1-Pad14)")
    (add_net "Net-(ENCODER-SP1-Pad2)")
    (add_net "Net-(ENCODER-SP1-Pad3)")
    (add_net "Net-(PHOTO-L1-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(Q3-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net RFF)
    (add_net RFR)
    (add_net SCL)
    (add_net SDA)
    (add_net VCC)
  )
  (net_class HighI ""
    (clearance 1)
    (trace_width 5.5)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
  )
  (module Mounting_Holes:MountingHole_3.7mm (layer F.Cu) (tedit 59B195F9)
    (at 88.265 134.874)
    (descr "Mounting Hole 3.7mm, no annular")
    (tags "mounting hole 3.7mm no annular")
    (fp_text reference REF** (at 0 -4.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.7mm (at 0 4.7) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.7mm (layer F.Cu) (tedit 59B195F9)
    (at 88.265 88.392)
    (descr "Mounting Hole 3.7mm, no annular")
    (tags "mounting hole 3.7mm no annular")
    (fp_text reference REF** (at 0 -4.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.7mm (at 0 4.7) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.7mm (layer F.Cu) (tedit 59B195F9)
    (at 122.301 85.852)
    (descr "Mounting Hole 3.7mm, no annular")
    (tags "mounting hole 3.7mm no annular")
    (fp_text reference REF** (at 0 -4.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.7mm (at 0 4.7) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.7mm (layer F.Cu) (tedit 59B195F9)
    (at 88.392 110.998)
    (descr "Mounting Hole 3.7mm, no annular")
    (tags "mounting hole 3.7mm no annular")
    (fp_text reference REF** (at 0 -4.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.7mm (at 0 4.7) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.7mm (layer F.Cu) (tedit 59B195F9)
    (at 122.301 134.874)
    (descr "Mounting Hole 3.7mm, no annular")
    (tags "mounting hole 3.7mm no annular")
    (fp_text reference REF** (at 0 -4.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.7mm (at 0 4.7) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.7mm (layer F.Cu) (tedit 59B195F9)
    (at 187.579 130.175)
    (descr "Mounting Hole 3.7mm, no annular")
    (tags "mounting hole 3.7mm no annular")
    (fp_text reference REF** (at 0 -4.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.7mm (at 0 4.7) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.7) (layers *.Cu *.Mask))
  )
  (module bbb:BBB (layer F.Cu) (tedit 596FEEEF)
    (at 182.372 67.818 270)
    (descr "Beagle Bone Black")
    (tags Beagle)
    (fp_text reference U1 (at 44.8945 23.9395 270) (layer F.SilkS) hide)
    (fp_text value bbb (at 44.7675 26.67 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 71.4248 4.4196 90) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
    (pad 46 thru_hole circle (at 15.5448 1.8796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 RFR))
    (pad 45 thru_hole circle (at 15.5448 4.4196 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 RFF))
    (pad 44 thru_hole circle (at 18.0848 1.8796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 LFF))
    (pad 43 thru_hole circle (at 18.0848 4.4196 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 LFR))
    (pad 42 thru_hole circle (at 20.6248 1.8796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 IFAULT))
    (pad 41 thru_hole circle (at 20.6248 4.4196 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 IRUN))
    (pad 30 thru_hole circle (at 35.8648 1.8796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 40 thru_hole circle (at 23.1648 1.8796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 INETCON))
    (pad 39 thru_hole circle (at 23.1648 4.4196 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 INETRDY))
    (pad 9 thru_hole circle (at 61.2648 4.4196 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole circle (at 63.8048 4.4196 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at 66.3448 4.4196 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at 68.8848 4.4196 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 37 thru_hole circle (at 25.7048 4.4196 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 35 thru_hole circle (at 28.2448 4.4196 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 38 thru_hole circle (at 25.7048 1.8796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 36 thru_hole circle (at 28.2448 1.8796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 34 thru_hole circle (at 30.7848 1.8796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 32 thru_hole circle (at 33.3248 1.8796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 28 thru_hole circle (at 38.4048 1.8796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 33 thru_hole circle (at 30.7848 4.4196 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 26 thru_hole circle (at 40.9448 1.8796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 24 thru_hole circle (at 43.4848 1.8796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 31 thru_hole circle (at 33.3248 4.4196 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 22 thru_hole circle (at 46.0248 1.8796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 29 thru_hole circle (at 35.8648 4.4196 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 20 thru_hole circle (at 48.5648 1.8796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 27 thru_hole circle (at 38.4048 4.4196 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 18 thru_hole circle (at 51.1048 1.8796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 25 thru_hole circle (at 40.9448 4.4196 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 16 thru_hole circle (at 53.6448 1.8796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 23 thru_hole circle (at 43.4848 4.4196 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole circle (at 56.1848 1.8796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 MRD))
    (pad 21 thru_hole circle (at 46.0248 4.4196 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole circle (at 58.7248 1.8796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 MRE))
    (pad 19 thru_hole circle (at 48.5648 4.4196 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole circle (at 61.2648 1.8796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 17 thru_hole circle (at 51.1048 4.4196 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole circle (at 63.8048 1.8796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole circle (at 53.6448 4.4196 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole circle (at 66.3448 1.8796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole circle (at 56.1848 4.4196 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 MLD))
    (pad 4 thru_hole circle (at 68.8848 1.8796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole circle (at 58.7248 4.4196 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 MLE))
    (pad 2 thru_hole circle (at 71.4248 1.8796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 902 thru_hole circle (at 71.4248 50.1396 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 911 thru_hole circle (at 58.7248 52.6796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 904 thru_hole circle (at 68.8848 50.1396 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 913 thru_hole circle (at 56.1848 52.6796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 906 thru_hole circle (at 66.3448 50.1396 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 915 thru_hole circle (at 53.6448 52.6796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 908 thru_hole circle (at 63.8048 50.1396 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 917 thru_hole circle (at 51.1048 52.6796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 910 thru_hole circle (at 61.2648 50.1396 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 919 thru_hole circle (at 48.5648 52.6796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 SCL))
    (pad 912 thru_hole circle (at 58.7248 50.1396 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 921 thru_hole circle (at 46.0248 52.6796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 914 thru_hole circle (at 56.1848 50.1396 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 MLS))
    (pad 923 thru_hole circle (at 43.4848 52.6796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 916 thru_hole circle (at 53.6448 50.1396 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 925 thru_hole circle (at 40.9448 52.6796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 918 thru_hole circle (at 51.1048 50.1396 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 927 thru_hole circle (at 38.4048 52.6796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 920 thru_hole circle (at 48.5648 50.1396 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 SDA))
    (pad 929 thru_hole circle (at 35.8648 52.6796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 922 thru_hole circle (at 46.0248 50.1396 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 931 thru_hole circle (at 33.3248 52.6796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 MRS))
    (pad 924 thru_hole circle (at 43.4848 50.1396 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 926 thru_hole circle (at 40.9448 50.1396 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 933 thru_hole circle (at 30.7848 52.6796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 928 thru_hole circle (at 38.4048 50.1396 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 932 thru_hole circle (at 33.3248 50.1396 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 934 thru_hole circle (at 30.7848 50.1396 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 936 thru_hole circle (at 28.2448 50.1396 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 938 thru_hole circle (at 25.7048 50.1396 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 935 thru_hole circle (at 28.2448 52.6796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 937 thru_hole circle (at 25.7048 52.6796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 903 thru_hole circle (at 68.8848 52.6796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 905 thru_hole circle (at 66.3448 52.6796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 VCC))
    (pad 907 thru_hole circle (at 63.8048 52.6796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 909 thru_hole circle (at 61.2648 52.6796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 939 thru_hole circle (at 23.1648 52.6796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 940 thru_hole circle (at 23.1648 50.1396 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 930 thru_hole circle (at 35.8648 50.1396 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 941 thru_hole circle (at 20.6248 52.6796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 942 thru_hole circle (at 20.6248 50.1396 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 943 thru_hole circle (at 18.0848 52.6796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 944 thru_hole circle (at 18.0848 50.1396 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 945 thru_hole circle (at 15.5448 52.6796 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 946 thru_hole circle (at 15.5448 50.1396 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 901 thru_hole circle (at 71.4248 52.6796 90) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 24 GND))
  )
  (module Capacitors_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 596EDE11)
    (at 128.651 146.431 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C1 (at 2.5 -6.06 270) (layer F.SilkS))
    (fp_text value 100uF (at 2.5 6.06 270) (layer F.Fab))
    (fp_text user %R (at 2.4 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 25 +12V))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 24 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5920C257)
    (at 107.188 140.208 270)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C2 (at 1 -3.56 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 1 3.56 270) (layer F.Fab))
    (fp_text user %R (at 0.65 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 VCC))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 595FC724)
    (at 120.142 117.729 90)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 MLS))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 595FC724)
    (at 120.142 93.853 90)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D2 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 MRS))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 595FC724)
    (at 171.704 93.98)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D3 (at 0 -1.85) (layer F.SilkS))
    (fp_text value LED (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 INETRDY))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 595FC724)
    (at 171.704 97.536)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D4 (at 0 -1.85) (layer F.SilkS))
    (fp_text value LED (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 45 INETCON))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 595FC724)
    (at 171.704 86.868)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D5 (at 0 -1.85) (layer F.SilkS))
    (fp_text value LED (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 32 IRUN))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 595FC724)
    (at 171.704 90.424)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D6 (at 0 -1.85) (layer F.SilkS))
    (fp_text value LED (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 34 IFAULT))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:D_1206 (layer F.Cu) (tedit 590CEAF5)
    (at 159.512 117.602)
    (descr "Diode SMD 1206, reflow soldering http://datasheets.avx.com/schottky.pdf")
    (tags "Diode 1206")
    (attr smd)
    (fp_text reference D7 (at 0 -1.8) (layer F.SilkS))
    (fp_text value D (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.8) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D7-Pad1)"))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 36 LFR))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_1206 (layer F.Cu) (tedit 590CEAF5)
    (at 159.512 113.792)
    (descr "Diode SMD 1206, reflow soldering http://datasheets.avx.com/schottky.pdf")
    (tags "Diode 1206")
    (attr smd)
    (fp_text reference D8 (at 0 -1.8) (layer F.SilkS))
    (fp_text value D (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.8) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D7-Pad1)"))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 37 LFF))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_1206 (layer F.Cu) (tedit 590CEAF5)
    (at 165.862 117.602)
    (descr "Diode SMD 1206, reflow soldering http://datasheets.avx.com/schottky.pdf")
    (tags "Diode 1206")
    (attr smd)
    (fp_text reference D9 (at 0 -1.8) (layer F.SilkS))
    (fp_text value D (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.8) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 39 RFR))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_1206 (layer F.Cu) (tedit 590CEAF5)
    (at 165.862 113.792)
    (descr "Diode SMD 1206, reflow soldering http://datasheets.avx.com/schottky.pdf")
    (tags "Diode 1206")
    (attr smd)
    (fp_text reference D10 (at 0 -1.8) (layer F.SilkS))
    (fp_text value D (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.8) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 40 RFF))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module POLOLU-DRV8825:POLOLU-DRV8825 (layer F.Cu) (tedit 596EDEFC)
    (at 107.95 122.174 180)
    (fp_text reference DRV-L1 (at -1.27 -13.97 180) (layer F.SilkS))
    (fp_text value POLOLU-DRV8825 (at 0 -16.51 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -7.62 -10.16 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 41 MLARM_))
    (pad 2 thru_hole circle (at -7.62 -7.62 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(DRV-L1-Pad2)"))
    (pad 3 thru_hole circle (at -7.62 -5.08 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(DRV-L1-Pad3)"))
    (pad 4 thru_hole circle (at -7.62 -2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(DRV-L1-Pad4)"))
    (pad 5 thru_hole circle (at -7.62 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 23 VCC))
    (pad 6 thru_hole circle (at -7.62 2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 23 VCC))
    (pad 7 thru_hole circle (at -7.62 5.08 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 5 MLS))
    (pad 8 thru_hole circle (at -7.62 7.62 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 6 MLD))
    (pad 9 thru_hole circle (at 5.08 7.62 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 24 GND))
    (pad 10 thru_hole circle (at 5.08 5.08 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole circle (at 5.08 2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(DRV-L1-Pad11)"))
    (pad 12 thru_hole circle (at 5.08 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(DRV-L1-Pad12)"))
    (pad 13 thru_hole circle (at 5.08 -2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(DRV-L1-Pad13)"))
    (pad 14 thru_hole circle (at 5.08 -5.08 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(DRV-L1-Pad14)"))
    (pad 15 thru_hole circle (at 5.08 -7.62 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 24 GND))
    (pad 16 thru_hole circle (at 5.08 -10.16 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 25 +12V))
  )
  (module POLOLU-DRV8825:POLOLU-DRV8825 (layer F.Cu) (tedit 596EDFED)
    (at 107.95 97.028 180)
    (fp_text reference DRV-R1 (at -1.27 -13.97 180) (layer F.SilkS))
    (fp_text value POLOLU-DRV8825 (at 0 -16.51 180) (layer Cmts.User) hide)
    (pad 1 thru_hole rect (at -7.62 -10.16 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 42 MRARM_))
    (pad 2 thru_hole circle (at -7.62 -7.62 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(DRV-L1-Pad2)"))
    (pad 3 thru_hole circle (at -7.62 -5.08 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(DRV-L1-Pad3)"))
    (pad 4 thru_hole circle (at -7.62 -2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(DRV-L1-Pad4)"))
    (pad 5 thru_hole circle (at -7.62 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 23 VCC))
    (pad 6 thru_hole circle (at -7.62 2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 23 VCC))
    (pad 7 thru_hole circle (at -7.62 5.08 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 12 MRS))
    (pad 8 thru_hole circle (at -7.62 7.62 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 13 MRD))
    (pad 9 thru_hole circle (at 5.08 7.62 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 24 GND))
    (pad 10 thru_hole circle (at 5.08 5.08 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole circle (at 5.08 2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(DRV-R1-Pad11)"))
    (pad 12 thru_hole circle (at 5.08 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(DRV-R1-Pad12)"))
    (pad 13 thru_hole circle (at 5.08 -2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(DRV-R1-Pad13)"))
    (pad 14 thru_hole circle (at 5.08 -5.08 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(DRV-R1-Pad14)"))
    (pad 15 thru_hole circle (at 5.08 -7.62 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 24 GND))
    (pad 16 thru_hole circle (at 5.08 -10.16 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 25 +12V))
  )
  (module Connectors_Molex:Molex_KK-6410-04_04x2.54mm_Straight (layer F.Cu) (tedit 58EE6EE8)
    (at 141.224 76.708)
    (descr "Connector Headers with Friction Lock, 22-27-2041, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2041")
    (fp_text reference PHOTO-L1 (at 1 -4.5) (layer F.SilkS))
    (fp_text value 01x04 (at 3.81 4.5) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 24 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 22 "Net-(PHOTO-L1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 24 GND))
    (pad 4 thru_hole oval (at 7.62 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 19 "Net-(ENCODER-SP1-Pad2)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-04_04x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_KK-6410-04_04x2.54mm_Straight (layer F.Cu) (tedit 58EE6EE8)
    (at 128.016 76.6445)
    (descr "Connector Headers with Friction Lock, 22-27-2041, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2041")
    (fp_text reference PHOTO-R1 (at 1 -4.5) (layer F.SilkS))
    (fp_text value 01x04 (at 3.81 4.5) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 24 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 22 "Net-(PHOTO-L1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 24 GND))
    (pad 4 thru_hole oval (at 7.62 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 20 "Net-(ENCODER-SP1-Pad3)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-04_04x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 139.7 83.058)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R0 (at 0 -1.85) (layer F.SilkS))
    (fp_text value 250 (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 23 VCC))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(PHOTO-L1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 164.592 93.98 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 150 (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 24 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 164.592 97.536 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 150 (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 24 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 164.592 86.868 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 150 (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 24 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 164.592 90.424 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 150 (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 24 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 124.46 117.729 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 150 (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 24 GND))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 124.46 93.853 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 150 (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 24 GND))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 158.496 134.112 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value 240 (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 24 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 164.846 134.112 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value 240 (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 24 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 152.146 134.112 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value 240 (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 51 ARM+))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(D11-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 596EE0F4)
    (at 106.68 81.534)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference SM0 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 4.87) (layer Cmts.User) hide)
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 VCC))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(DRV-L1-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 596EE0D6)
    (at 110.49 81.534)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference SM1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 4.87) (layer Cmts.User) hide)
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 VCC))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(DRV-L1-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 596EE0F9)
    (at 114.3 81.534)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference SM2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 4.87) (layer Cmts.User) hide)
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 VCC))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(DRV-L1-Pad4)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_MiniFit-JR-5569-04A2_2x02x4.20mm_Angled (layer F.Cu) (tedit 58A28C61)
    (at 90.932 125.476 90)
    (descr "Molex Mini-Fit JR, PN:5569-04A2, dual row, side entry type, through hole, with plastic peg mount")
    (tags "connector molex mini-fit 5569")
    (fp_text reference STEPPER-L1 (at 2.1 8.5 90) (layer F.SilkS))
    (fp_text value 01x04 (at 2.1 10 90) (layer F.Fab))
    (fp_text user %R (at 2.1 -4.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 10 "Net-(DRV-L1-Pad14)"))
    (pad 2 thru_hole circle (at 4.2 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 7 "Net-(DRV-L1-Pad11)"))
    (pad 3 thru_hole circle (at 0 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 9 "Net-(DRV-L1-Pad13)"))
    (pad 4 thru_hole circle (at 4.2 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 8 "Net-(DRV-L1-Pad12)"))
    (pad "" np_thru_hole circle (at 2.1 -7.3 90) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_MiniFit-JR-5569-04A2_2x02x4.20mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_MiniFit-JR-5569-04A2_2x02x4.20mm_Angled (layer F.Cu) (tedit 58A28C61)
    (at 90.932 100.584 90)
    (descr "Molex Mini-Fit JR, PN:5569-04A2, dual row, side entry type, through hole, with plastic peg mount")
    (tags "connector molex mini-fit 5569")
    (fp_text reference STEPPER-R1 (at 2.1 8.5 90) (layer F.SilkS))
    (fp_text value 01X04 (at 2.1 10 90) (layer F.Fab))
    (fp_text user %R (at 2.1 -4.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 17 "Net-(DRV-R1-Pad14)"))
    (pad 2 thru_hole circle (at 4.2 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 14 "Net-(DRV-R1-Pad11)"))
    (pad 3 thru_hole circle (at 0 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 16 "Net-(DRV-R1-Pad13)"))
    (pad 4 thru_hole circle (at 4.2 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 15 "Net-(DRV-R1-Pad12)"))
    (pad "" np_thru_hole circle (at 2.1 -7.3 90) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_MiniFit-JR-5569-04A2_2x02x4.20mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module spdt-illuminated:spdt-illuminated (layer F.Cu) (tedit 596EE4A6)
    (at 159.766 125.984)
    (fp_text reference SWITCH-LF1 (at 0 -4.572) (layer Cmts.User))
    (fp_text value SPDT-ILLUMINATED (at 0 -0.5) (layer Cmts.User) hide)
    (pad 5 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 "Net-(D7-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 VCC))
    (pad 1 thru_hole circle (at 1.27 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 LFR))
    (pad 4 thru_hole circle (at -1.27 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -1.27 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 "Net-(R7-Pad1)"))
    (pad 3 thru_hole circle (at 1.27 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 LFF))
  )
  (module spdt-illuminated:spdt-illuminated (layer F.Cu) (tedit 596EE4A1)
    (at 166.116 125.984)
    (fp_text reference SWITCH-RF1 (at 0 -4.572) (layer Cmts.User))
    (fp_text value SPDT-ILLUMINATED (at 0 -0.5) (layer Cmts.User) hide)
    (pad 5 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 "Net-(D10-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 VCC))
    (pad 1 thru_hole circle (at 1.27 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 RFR))
    (pad 4 thru_hole circle (at -1.27 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -1.27 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 44 "Net-(R8-Pad1)"))
    (pad 3 thru_hole circle (at 1.27 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 40 RFF))
  )
  (module lm78xx:LM78XX-Linear-Regulator (layer F.Cu) (tedit 5964489F)
    (at 101.346 151.257 180)
    (descr "LM78XX Linear Regulator")
    (tags "LM78XX Linear Regulator TO-220")
    (fp_text reference U2 (at 2.54 -3.62 180) (layer F.SilkS))
    (fp_text value 7805 (at 2.54 3.92 180) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 180) (layer F.Fab))
    (pad VI thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 25 +12V))
    (pad GND thru_hole oval (at 2.54 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 24 GND))
    (pad VO thru_hole oval (at 5.08 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 23 VCC))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 58EE6EE4)
    (at 122.301 76.581 180)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference MEDIA-I2C1 (at 1 -4.5 180) (layer F.SilkS))
    (fp_text value 01X02 (at 1.27 4.5 180) (layer F.Fab))
    (fp_text user %R (at 1.27 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 SDA))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 21 SCL))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-02_02x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_MiniFit-JR-5569-04A2_2x02x4.20mm_Angled (layer F.Cu) (tedit 58A28C61)
    (at 142.748 151.892 180)
    (descr "Molex Mini-Fit JR, PN:5569-04A2, dual row, side entry type, through hole, with plastic peg mount")
    (tags "connector molex mini-fit 5569")
    (fp_text reference MEDIA-PWR1 (at 2.1 8.5 180) (layer F.SilkS))
    (fp_text value 01X04 (at 2.1 10 180) (layer F.Fab))
    (fp_text user %R (at 2.1 -4.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 3 3) (drill 1.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 4.2 0 180) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 24 GND))
    (pad 3 thru_hole circle (at 0 5.5 180) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 23 VCC))
    (pad 4 thru_hole circle (at 4.2 5.5 180) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 25 +12V))
    (pad "" np_thru_hole circle (at 2.1 -7.3 180) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_MiniFit-JR-5569-04A2_2x02x4.20mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 596FE3E5)
    (at 113.792 75.692 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference DEBUG-I2C1 (at 0 -2.33 270) (layer Cmts.User) hide)
    (fp_text value 01X02 (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 SDA))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 SCL))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 58CC8E33)
    (at 143.764 95.25 180)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference ENCODER-SP1 (at 3.81 -2.39 180) (layer F.SilkS))
    (fp_text value ATTINY25-P (at 3.81 10.01 180) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 VCC))
    (pad 5 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 SDA))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(ENCODER-SP1-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(ENCODER-SP1-Pad3)"))
    (pad 7 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 SCL))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 GND))
    (pad 8 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 VCC))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 59A5BD2D)
    (at 138.938 112.776 270)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 -3.56 270) (layer F.SilkS))
    (fp_text value Q_NPN_EBC (at 1.27 2.79 270) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -3.56 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 90) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 46 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 41 MLARM_))
    (pad 1 thru_hole rect (at 0 0 90) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 47 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 59A5BD33)
    (at 145.288 112.776 270)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 1.27 -3.56 270) (layer F.SilkS))
    (fp_text value Q_NPN_EBC (at 1.27 2.79 270) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -3.56 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 90) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 48 "Net-(Q2-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 42 MRARM_))
    (pad 1 thru_hole rect (at 0 0 90) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 47 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 58CE52AF)
    (at 151.638 112.776 270)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q3 (at 1.27 -3.56 270) (layer F.SilkS))
    (fp_text value Q_NPN_EBC (at 1.27 2.79 270) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 90) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 49 "Net-(Q3-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 47 "Net-(Q1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 24 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 59A5BE1C)
    (at 136.144 128.524 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value 5.1K (at 0 1.9 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(Q1-Pad2)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 MLE))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 59A5BE17)
    (at 143.764 120.904 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R11 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value 5.1K (at 0 1.9 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(Q3-Pad2)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 51 ARM+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 59A5BE28)
    (at 136.144 120.904 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R12 (at 0 1.778 90) (layer F.SilkS))
    (fp_text value 510 (at 0 1.9 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 23 VCC))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 41 MLARM_))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 59A5BE13)
    (at 139.954 120.904 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R13 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value 5.1K (at 0 1.9 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(Q2-Pad2)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 MRE))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 59A5BE1F)
    (at 139.954 128.524 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R14 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value 510 (at 0 1.9 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 42 MRARM_))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 23 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 595FC724)
    (at 171.704 83.058)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D11 (at 0 -1.85) (layer F.SilkS))
    (fp_text value LED (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 24 GND))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(D11-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connectors_Molex:Molex_MiniFit-JR-5569-04A2_2x02x4.20mm_Angled (layer F.Cu) (tedit 58A28C61)
    (at 118.872 151.892 180)
    (descr "Molex Mini-Fit JR, PN:5569-04A2, dual row, side entry type, through hole, with plastic peg mount")
    (tags "connector molex mini-fit 5569")
    (fp_text reference GCTRL1 (at 2.1 8.5 180) (layer F.SilkS))
    (fp_text value 01X04 (at 2.1 10 180) (layer F.Fab))
    (fp_text user %R (at 2.1 -4.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 24 GND))
    (pad 2 thru_hole circle (at 4.2 0 180) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 25 +12V))
    (pad 3 thru_hole circle (at 0 5.5 180) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 51 ARM+))
    (pad 4 thru_hole circle (at 4.2 5.5 180) (size 3 3) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.1 -7.3 180) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_MiniFit-JR-5569-04A2_2x02x4.20mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.7mm (layer F.Cu) (tedit 59B195F9)
    (at 187.452 92.964)
    (descr "Mounting Hole 3.7mm, no annular")
    (tags "mounting hole 3.7mm no annular")
    (fp_text reference REF** (at 0 -4.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.7mm (at 0 4.7) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.7) (layers *.Cu *.Mask))
  )
  (gr_line (start 91.44 161.798) (end 99.822 161.798) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.756 150.114) (end 91.44 161.798) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.756 89.281) (end 79.756 150.114) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 98.044 70.993) (end 79.756 89.281) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.442 70.993) (end 98.044 70.993) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.442 70.993) (end 107.823 70.993) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.965 161.798) (end 99.822 161.798) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102.87 161.798) (end 100.965 161.798) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.304 161.798) (end 102.87 161.798) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150.241 70.993) (end 107.823 70.993) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.131 79.883) (end 150.241 70.993) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 181.483 79.883) (end 159.131 79.883) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 192.532 90.932) (end 181.483 79.883) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "MK1\n1709" (at 135.382 137.795) (layer F.SilkS))
  (gr_line (start 148.336 159.766) (end 148.336 137.922) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.304 161.798) (end 148.336 159.766) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text ARMED (at 160.782 83.312) (layer F.SilkS))
  (gr_line (start 192.532 90.932) (end 192.532 99.06) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 192.532 132.588) (end 192.532 99.06) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 189.23 135.89) (end 192.532 132.588) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 183.388 141.732) (end 189.23 135.89) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.878 141.732) (end 183.388 141.732) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.878 137.922) (end 166.878 141.732) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.336 137.922) (end 166.878 137.922) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text haldean.org/wallbot (at 81.153 149.733 90) (layer F.SilkS))
  (gr_text "WILLIAM BURKE + HALDEAN BROWN" (at 135.382 109.22) (layer F.SilkS))
  (gr_text WALL&CHAIN (at 135.382 105.156) (layer F.SilkS))
  (gr_text CONN (at 160.782 97.79) (layer F.SilkS))
  (gr_text "NET OK" (at 160.782 94.234) (layer F.SilkS))
  (gr_text FAULT (at 160.782 90.678) (layer F.SilkS))
  (gr_text RUN (at 160.782 87.122) (layer F.SilkS))
  (gr_text L (at 159.766 120.65) (layer F.SilkS))
  (gr_text R (at 166.116 120.65) (layer F.SilkS))
)
