(kicad_pcb (version 20171130) (host pcbnew "(5.0.1)-4")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 107)
    (zones 0)
    (modules 15)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.4064)
    (user_trace_width 0.1524)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.508)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 17.78 17.78)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 176.276 122.682)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "GERBERS/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /PB2)
  (net 3 /PB0)
  (net 4 /PB3)
  (net 5 /PB5)
  (net 6 /PB1)
  (net 7 /PB4)
  (net 8 VCC)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /PB0)
    (add_net /PB1)
    (add_net /PB2)
    (add_net /PB3)
    (add_net /PB4)
    (add_net /PB5)
    (add_net GND)
    (add_net VCC)
  )
  (module bobness_card:SMTU2032 (layer B.Cu) (tedit 5BCB83E7)
    (at 157.226 112.522 180)
    (descr SMTU2032-LF)
    (tags "Undefined or Miscellaneous")
    (attr smd)
    (fp_text reference BT1 (at 0 6.985 180) (layer B.SilkS))
    (fp_text value CR2032 (at 0 -6.985 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -14.7 0 180) (size 2.6 3.5) (layers B.Cu B.Paste B.Mask)
      (net 8 VCC))
    (pad 2 smd rect (at 14.7 0 180) (size 2.6 3.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ../../../../../../Users/Dday/Documents/Documents/pcb/bobness_card-simple/bobness_card.3d/smtu2032.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C81FE79)
    (at 141.351 115.697 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 22K (at 3.81 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /PB3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C81FE86)
    (at 160.401 115.697 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 22K (at 3.81 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /PB4))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C81FE8A)
    (at 179.451 115.697 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 22K (at 3.81 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /PB1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5BE7778A)
    (at 134.366 111.252 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 1.905 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C81FE66)
    (at 134.366 103.632 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -1.905 270) (layer F.SilkS))
    (fp_text value 22K (at 0 -1.905 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /PB5))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module bobness_card:ATTINY85-20SU (layer F.Cu) (tedit 5BE77796)
    (at 130.326 107.462 270)
    (descr "8-Lead Plastic Small Outline (SM) - Medium, 5.28 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 1.27 -1.905 270) (layer F.SilkS))
    (fp_text value ATTINY85-20SU (at -4 6.25 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -4.5 -1.905 270) (size 1.905 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 /PB5))
    (pad 2 smd rect (at -4.5 -0.635 270) (size 1.905 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 /PB3))
    (pad 3 smd rect (at -4.5 0.635 270) (size 1.905 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 /PB4))
    (pad 4 smd rect (at -4.5 1.905 270) (size 1.905 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 4.5 1.905 270) (size 1.905 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 /PB0))
    (pad 6 smd rect (at 4.5 0.635 270) (size 1.905 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 /PB1))
    (pad 7 smd rect (at 4.5 -0.635 270) (size 1.905 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 /PB2))
    (pad 8 smd rect (at 4.5 -1.905 270) (size 1.905 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 VCC))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIJ-8_5.3x5.3mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5BCAB0ED)
    (at 181.991 110.617 180)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33 180) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 6.35 -6.35 180) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 -90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /PB1))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 VCC))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /PB2))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /PB0))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /PB5))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5D45F2F3)
    (at 144.526 106.172)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 1.905) (layer B.SilkS))
    (fp_text value 4.7k (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 /PB2))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5D45F2F9)
    (at 144.526 103.632)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -1.905) (layer B.SilkS))
    (fp_text value 4.7k (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 /PB0))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module bobness_card:SSD1306_OLED_Display_128x32 (layer F.Cu) (tedit 5C81FEA2)
    (at 139.446 103.632)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference DS1 (at 2.54 3.81 90) (layer F.SilkS))
    (fp_text value SSD1306-128x32 (at 19.05 7.62) (layer F.Fab))
    (fp_text user %R (at 3.175 -0.635 180) (layer F.Fab))
    (pad 4 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /PB0))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /PB2))
    (pad 2 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 VCC))
    (pad 1 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ../../../../../../Users/Dday/Documents/Documents/pcb/bobness_card-simple/bobness_card.3d/ssd1306-128x32.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module bobness_card:CHERRY_CHOC_PCB (layer F.Cu) (tedit 5D45E4A8)
    (at 175.006 123.952 180)
    (fp_text reference SW1 (at 3.81 5.08 180) (layer F.SilkS))
    (fp_text value SW_Push (at 0 3.175 180) (layer F.SilkS) hide)
    (fp_text user 1.00u (at 5.716 -8.414 180) (layer Dwgs.User))
    (pad 2 thru_hole circle (at 5 -3.8 180) (size 1.9874 1.9874) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 /PB1))
    (pad 1 thru_hole circle (at 0 -5.9 180) (size 1.9874 1.9874) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.54 -5.08 180) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -3.81 -2.54 180) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 6 /PB1))
    (pad HOLE np_thru_hole circle (at 0 0 180) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu))
    (pad "" np_thru_hole oval (at 5.33955 0 180) (size 2.2209 1.9) (drill oval 2.2209 1.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at -5.33955 0 180) (size 2.2209 1.9) (drill oval 2.2209 1.9) (layers *.Cu *.Mask))
  )
  (module bobness_card:CHERRY_CHOC_PCB (layer F.Cu) (tedit 5D45E4A8)
    (at 136.906 123.952 180)
    (fp_text reference SW2 (at 3.81 5.08 180) (layer F.SilkS))
    (fp_text value SW_Push (at 0 3.175 180) (layer F.SilkS) hide)
    (fp_text user 1.00u (at 5.716 -8.414 180) (layer Dwgs.User))
    (pad "" np_thru_hole oval (at -5.33955 0 180) (size 2.2209 1.9) (drill oval 2.2209 1.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 5.33955 0 180) (size 2.2209 1.9) (drill oval 2.2209 1.9) (layers *.Cu *.Mask))
    (pad HOLE np_thru_hole circle (at 0 0 180) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu))
    (pad 2 thru_hole circle (at -3.81 -2.54 180) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 4 /PB3))
    (pad 1 thru_hole circle (at 2.54 -5.08 180) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -5.9 180) (size 1.9874 1.9874) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 -3.8 180) (size 1.9874 1.9874) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 /PB3))
  )
  (module bobness_card:CHERRY_CHOC_PCB (layer F.Cu) (tedit 5D45E4A8)
    (at 155.956 123.952 180)
    (fp_text reference SW3 (at 3.81 5.08 180) (layer F.SilkS))
    (fp_text value SW_Push (at 0 3.175 180) (layer F.SilkS) hide)
    (fp_text user 1.00u (at 5.716 -8.414 180) (layer Dwgs.User))
    (pad 2 thru_hole circle (at 5 -3.8 180) (size 1.9874 1.9874) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 /PB4))
    (pad 1 thru_hole circle (at 0 -5.9 180) (size 1.9874 1.9874) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.54 -5.08 180) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -3.81 -2.54 180) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 7 /PB4))
    (pad HOLE np_thru_hole circle (at 0 0 180) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu))
    (pad "" np_thru_hole oval (at 5.33955 0 180) (size 2.2209 1.9) (drill oval 2.2209 1.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at -5.33955 0 180) (size 2.2209 1.9) (drill oval 2.2209 1.9) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 5D45ED7B)
    (at 183.896 101.092)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask))
  )
  (gr_line (start 125.476 101.092) (end 125.476 132.842) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 183.896 98.552) (end 128.016 98.552) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 186.436 132.842) (end 186.436 101.092) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.016 135.382) (end 183.896 135.382) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 183.896 132.842) (end 186.436 132.842) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 128.016 132.842) (end 128.016 135.382) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 128.016 101.092) (end 125.476 101.092) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 183.896 101.092) (end 183.896 98.552) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 187.706 137.287) (xy 124.206 137.287) (xy 124.841 97.917) (xy 187.706 97.917)
      )
    )
  )
  (zone (net 8) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 187.706 137.287) (xy 124.206 137.287) (xy 124.206 96.647) (xy 188.341 96.647)
      )
    )
  )
)
