(kicad_pcb (version 20171130) (host pcbnew "(5.1.8)-1")
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 1185)
    (zones 0)
    (modules 523)
    (nets 260)
  )
  (page A4)
  (title_block
    (title "Splendida")
    (company Wokwi)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.4)
    (user_trace_width 0.8)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.5 4)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 "Net-(D1-Pad2)")
  (net 3 /DIN)
  (net 4 GND)
  (net 5 "Net-(D2-Pad2)")
  (net 6 "Net-(D3-Pad2)")
  (net 7 "Net-(D4-Pad2)")
  (net 8 "Net-(D5-Pad2)")
  (net 9 "Net-(D6-Pad2)")
  (net 10 "Net-(D7-Pad2)")
  (net 11 "Net-(D8-Pad2)")
  (net 12 "Net-(D10-Pad4)")
  (net 13 "Net-(D10-Pad2)")
  (net 14 "Net-(D11-Pad2)")
  (net 15 "Net-(D12-Pad2)")
  (net 16 "Net-(D13-Pad2)")
  (net 17 "Net-(D14-Pad2)")
  (net 18 /LEDS/L16)
  (net 19 "Net-(D16-Pad2)")
  (net 20 "Net-(D17-Pad2)")
  (net 21 "Net-(D18-Pad2)")
  (net 22 "Net-(D19-Pad2)")
  (net 23 "Net-(D20-Pad2)")
  (net 24 "Net-(D21-Pad2)")
  (net 25 "Net-(D22-Pad2)")
  (net 26 "Net-(D23-Pad2)")
  (net 27 "Net-(D24-Pad2)")
  (net 28 "Net-(D25-Pad2)")
  (net 29 "Net-(D26-Pad2)")
  (net 30 "Net-(D27-Pad2)")
  (net 31 "Net-(D28-Pad2)")
  (net 32 "Net-(D29-Pad2)")
  (net 33 /LEDS/L31)
  (net 34 "Net-(D31-Pad2)")
  (net 35 "Net-(D32-Pad2)")
  (net 36 "Net-(D33-Pad2)")
  (net 37 "Net-(D34-Pad2)")
  (net 38 "Net-(D35-Pad2)")
  (net 39 "Net-(D36-Pad2)")
  (net 40 "Net-(D37-Pad2)")
  (net 41 "Net-(D38-Pad2)")
  (net 42 "Net-(D39-Pad2)")
  (net 43 "Net-(D40-Pad2)")
  (net 44 "Net-(D41-Pad2)")
  (net 45 "Net-(D42-Pad2)")
  (net 46 "Net-(D43-Pad2)")
  (net 47 "Net-(D44-Pad2)")
  (net 48 /LEDS/L46)
  (net 49 "Net-(D46-Pad2)")
  (net 50 "Net-(D47-Pad2)")
  (net 51 "Net-(D48-Pad2)")
  (net 52 "Net-(D49-Pad2)")
  (net 53 "Net-(D50-Pad2)")
  (net 54 "Net-(D51-Pad2)")
  (net 55 "Net-(D52-Pad2)")
  (net 56 "Net-(D53-Pad2)")
  (net 57 "Net-(D54-Pad2)")
  (net 58 "Net-(D55-Pad2)")
  (net 59 "Net-(D56-Pad2)")
  (net 60 "Net-(D57-Pad2)")
  (net 61 "Net-(D58-Pad2)")
  (net 62 "Net-(D59-Pad2)")
  (net 63 /LEDS/L61)
  (net 64 "Net-(D61-Pad2)")
  (net 65 "Net-(D62-Pad2)")
  (net 66 "Net-(D63-Pad2)")
  (net 67 "Net-(D64-Pad2)")
  (net 68 "Net-(D65-Pad2)")
  (net 69 "Net-(D66-Pad2)")
  (net 70 "Net-(D67-Pad2)")
  (net 71 "Net-(D68-Pad2)")
  (net 72 "Net-(D69-Pad2)")
  (net 73 "Net-(D70-Pad2)")
  (net 74 "Net-(D71-Pad2)")
  (net 75 "Net-(D72-Pad2)")
  (net 76 "Net-(D73-Pad2)")
  (net 77 "Net-(D74-Pad2)")
  (net 78 /LEDS/L76)
  (net 79 "Net-(D76-Pad2)")
  (net 80 "Net-(D77-Pad2)")
  (net 81 "Net-(D78-Pad2)")
  (net 82 "Net-(D79-Pad2)")
  (net 83 "Net-(D80-Pad2)")
  (net 84 "Net-(D81-Pad2)")
  (net 85 "Net-(D82-Pad2)")
  (net 86 "Net-(D83-Pad2)")
  (net 87 "Net-(D84-Pad2)")
  (net 88 "Net-(D85-Pad2)")
  (net 89 "Net-(D86-Pad2)")
  (net 90 "Net-(D87-Pad2)")
  (net 91 "Net-(D88-Pad2)")
  (net 92 "Net-(D89-Pad2)")
  (net 93 /LEDS/L91)
  (net 94 "Net-(D91-Pad2)")
  (net 95 "Net-(D92-Pad2)")
  (net 96 "Net-(D93-Pad2)")
  (net 97 "Net-(D94-Pad2)")
  (net 98 "Net-(D95-Pad2)")
  (net 99 "Net-(D96-Pad2)")
  (net 100 "Net-(D97-Pad2)")
  (net 101 "Net-(D98-Pad2)")
  (net 102 "Net-(D100-Pad4)")
  (net 103 "Net-(D100-Pad2)")
  (net 104 "Net-(D101-Pad2)")
  (net 105 "Net-(D102-Pad2)")
  (net 106 "Net-(D103-Pad2)")
  (net 107 "Net-(D104-Pad2)")
  (net 108 /LEDS/L106)
  (net 109 "Net-(D106-Pad2)")
  (net 110 "Net-(D107-Pad2)")
  (net 111 "Net-(D108-Pad2)")
  (net 112 "Net-(D109-Pad2)")
  (net 113 "Net-(D110-Pad2)")
  (net 114 "Net-(D111-Pad2)")
  (net 115 "Net-(D112-Pad2)")
  (net 116 "Net-(D113-Pad2)")
  (net 117 "Net-(D114-Pad2)")
  (net 118 "Net-(D115-Pad2)")
  (net 119 "Net-(D116-Pad2)")
  (net 120 "Net-(D117-Pad2)")
  (net 121 "Net-(D118-Pad2)")
  (net 122 "Net-(D119-Pad2)")
  (net 123 /LEDS/L121)
  (net 124 "Net-(D121-Pad2)")
  (net 125 "Net-(D122-Pad2)")
  (net 126 "Net-(D123-Pad2)")
  (net 127 "Net-(D124-Pad2)")
  (net 128 "Net-(D125-Pad2)")
  (net 129 "Net-(D126-Pad2)")
  (net 130 "Net-(D127-Pad2)")
  (net 131 "Net-(D128-Pad2)")
  (net 132 "Net-(D129-Pad2)")
  (net 133 "Net-(D130-Pad2)")
  (net 134 "Net-(D131-Pad2)")
  (net 135 "Net-(D132-Pad2)")
  (net 136 "Net-(D133-Pad2)")
  (net 137 "Net-(D134-Pad2)")
  (net 138 /LEDS/L136)
  (net 139 "Net-(D136-Pad2)")
  (net 140 "Net-(D137-Pad2)")
  (net 141 "Net-(D138-Pad2)")
  (net 142 "Net-(D139-Pad2)")
  (net 143 "Net-(D140-Pad2)")
  (net 144 "Net-(D141-Pad2)")
  (net 145 "Net-(D142-Pad2)")
  (net 146 "Net-(D143-Pad2)")
  (net 147 "Net-(D144-Pad2)")
  (net 148 "Net-(D145-Pad2)")
  (net 149 "Net-(D146-Pad2)")
  (net 150 "Net-(D147-Pad2)")
  (net 151 "Net-(D148-Pad2)")
  (net 152 "Net-(D149-Pad2)")
  (net 153 /LEDS/L151)
  (net 154 "Net-(D151-Pad2)")
  (net 155 "Net-(D152-Pad2)")
  (net 156 "Net-(D153-Pad2)")
  (net 157 "Net-(D154-Pad2)")
  (net 158 "Net-(D155-Pad2)")
  (net 159 "Net-(D156-Pad2)")
  (net 160 "Net-(D157-Pad2)")
  (net 161 "Net-(D158-Pad2)")
  (net 162 "Net-(D159-Pad2)")
  (net 163 "Net-(D160-Pad2)")
  (net 164 "Net-(D161-Pad2)")
  (net 165 "Net-(D162-Pad2)")
  (net 166 "Net-(D163-Pad2)")
  (net 167 "Net-(D164-Pad2)")
  (net 168 /LEDS/L166)
  (net 169 "Net-(D166-Pad2)")
  (net 170 "Net-(D167-Pad2)")
  (net 171 "Net-(D168-Pad2)")
  (net 172 "Net-(D169-Pad2)")
  (net 173 "Net-(D170-Pad2)")
  (net 174 "Net-(D171-Pad2)")
  (net 175 "Net-(D172-Pad2)")
  (net 176 "Net-(D173-Pad2)")
  (net 177 "Net-(D174-Pad2)")
  (net 178 "Net-(D175-Pad2)")
  (net 179 "Net-(D176-Pad2)")
  (net 180 "Net-(D177-Pad2)")
  (net 181 "Net-(D178-Pad2)")
  (net 182 "Net-(D179-Pad2)")
  (net 183 /LEDS/L181)
  (net 184 "Net-(D181-Pad2)")
  (net 185 "Net-(D182-Pad2)")
  (net 186 "Net-(D183-Pad2)")
  (net 187 "Net-(D184-Pad2)")
  (net 188 "Net-(D185-Pad2)")
  (net 189 "Net-(D186-Pad2)")
  (net 190 "Net-(D187-Pad2)")
  (net 191 "Net-(D188-Pad2)")
  (net 192 "Net-(D189-Pad2)")
  (net 193 "Net-(D190-Pad2)")
  (net 194 "Net-(D191-Pad2)")
  (net 195 "Net-(D192-Pad2)")
  (net 196 "Net-(D193-Pad2)")
  (net 197 "Net-(D194-Pad2)")
  (net 198 /LEDS/L196)
  (net 199 "Net-(D196-Pad2)")
  (net 200 "Net-(D197-Pad2)")
  (net 201 "Net-(D198-Pad2)")
  (net 202 "Net-(D199-Pad2)")
  (net 203 "Net-(D200-Pad2)")
  (net 204 "Net-(D201-Pad2)")
  (net 205 "Net-(D202-Pad2)")
  (net 206 "Net-(D203-Pad2)")
  (net 207 "Net-(D204-Pad2)")
  (net 208 "Net-(D205-Pad2)")
  (net 209 "Net-(D206-Pad2)")
  (net 210 "Net-(D207-Pad2)")
  (net 211 "Net-(D208-Pad2)")
  (net 212 "Net-(D209-Pad2)")
  (net 213 /LEDS/L211)
  (net 214 "Net-(D211-Pad2)")
  (net 215 "Net-(D212-Pad2)")
  (net 216 "Net-(D213-Pad2)")
  (net 217 "Net-(D214-Pad2)")
  (net 218 "Net-(D215-Pad2)")
  (net 219 "Net-(D216-Pad2)")
  (net 220 "Net-(D217-Pad2)")
  (net 221 "Net-(D218-Pad2)")
  (net 222 "Net-(D219-Pad2)")
  (net 223 "Net-(D220-Pad2)")
  (net 224 "Net-(D221-Pad2)")
  (net 225 "Net-(D222-Pad2)")
  (net 226 "Net-(D223-Pad2)")
  (net 227 "Net-(D224-Pad2)")
  (net 228 /LEDS/L226)
  (net 229 "Net-(D226-Pad2)")
  (net 230 "Net-(D227-Pad2)")
  (net 231 "Net-(D228-Pad2)")
  (net 232 "Net-(D229-Pad2)")
  (net 233 "Net-(D230-Pad2)")
  (net 234 "Net-(D231-Pad2)")
  (net 235 "Net-(D232-Pad2)")
  (net 236 "Net-(D233-Pad2)")
  (net 237 "Net-(D234-Pad2)")
  (net 238 "Net-(D235-Pad2)")
  (net 239 "Net-(D236-Pad2)")
  (net 240 "Net-(D237-Pad2)")
  (net 241 "Net-(D238-Pad2)")
  (net 242 "Net-(D239-Pad2)")
  (net 243 /LEDS/L241)
  (net 244 "Net-(D241-Pad2)")
  (net 245 "Net-(D242-Pad2)")
  (net 246 "Net-(D243-Pad2)")
  (net 247 "Net-(D244-Pad2)")
  (net 248 "Net-(D245-Pad2)")
  (net 249 "Net-(D246-Pad2)")
  (net 250 "Net-(D247-Pad2)")
  (net 251 "Net-(D248-Pad2)")
  (net 252 "Net-(D249-Pad2)")
  (net 253 "Net-(D250-Pad2)")
  (net 254 "Net-(D251-Pad2)")
  (net 255 "Net-(D252-Pad2)")
  (net 256 "Net-(D253-Pad2)")
  (net 257 "Net-(D254-Pad2)")
  (net 258 /LEDS/L256)
  (net 259 /DOUT)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /DIN)
    (add_net /DOUT)
    (add_net /LEDS/L106)
    (add_net /LEDS/L121)
    (add_net /LEDS/L136)
    (add_net /LEDS/L151)
    (add_net /LEDS/L16)
    (add_net /LEDS/L166)
    (add_net /LEDS/L181)
    (add_net /LEDS/L196)
    (add_net /LEDS/L211)
    (add_net /LEDS/L226)
    (add_net /LEDS/L241)
    (add_net /LEDS/L256)
    (add_net /LEDS/L31)
    (add_net /LEDS/L46)
    (add_net /LEDS/L61)
    (add_net /LEDS/L76)
    (add_net /LEDS/L91)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D10-Pad4)")
    (add_net "Net-(D100-Pad2)")
    (add_net "Net-(D100-Pad4)")
    (add_net "Net-(D101-Pad2)")
    (add_net "Net-(D102-Pad2)")
    (add_net "Net-(D103-Pad2)")
    (add_net "Net-(D104-Pad2)")
    (add_net "Net-(D106-Pad2)")
    (add_net "Net-(D107-Pad2)")
    (add_net "Net-(D108-Pad2)")
    (add_net "Net-(D109-Pad2)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D110-Pad2)")
    (add_net "Net-(D111-Pad2)")
    (add_net "Net-(D112-Pad2)")
    (add_net "Net-(D113-Pad2)")
    (add_net "Net-(D114-Pad2)")
    (add_net "Net-(D115-Pad2)")
    (add_net "Net-(D116-Pad2)")
    (add_net "Net-(D117-Pad2)")
    (add_net "Net-(D118-Pad2)")
    (add_net "Net-(D119-Pad2)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D121-Pad2)")
    (add_net "Net-(D122-Pad2)")
    (add_net "Net-(D123-Pad2)")
    (add_net "Net-(D124-Pad2)")
    (add_net "Net-(D125-Pad2)")
    (add_net "Net-(D126-Pad2)")
    (add_net "Net-(D127-Pad2)")
    (add_net "Net-(D128-Pad2)")
    (add_net "Net-(D129-Pad2)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D130-Pad2)")
    (add_net "Net-(D131-Pad2)")
    (add_net "Net-(D132-Pad2)")
    (add_net "Net-(D133-Pad2)")
    (add_net "Net-(D134-Pad2)")
    (add_net "Net-(D136-Pad2)")
    (add_net "Net-(D137-Pad2)")
    (add_net "Net-(D138-Pad2)")
    (add_net "Net-(D139-Pad2)")
    (add_net "Net-(D14-Pad2)")
    (add_net "Net-(D140-Pad2)")
    (add_net "Net-(D141-Pad2)")
    (add_net "Net-(D142-Pad2)")
    (add_net "Net-(D143-Pad2)")
    (add_net "Net-(D144-Pad2)")
    (add_net "Net-(D145-Pad2)")
    (add_net "Net-(D146-Pad2)")
    (add_net "Net-(D147-Pad2)")
    (add_net "Net-(D148-Pad2)")
    (add_net "Net-(D149-Pad2)")
    (add_net "Net-(D151-Pad2)")
    (add_net "Net-(D152-Pad2)")
    (add_net "Net-(D153-Pad2)")
    (add_net "Net-(D154-Pad2)")
    (add_net "Net-(D155-Pad2)")
    (add_net "Net-(D156-Pad2)")
    (add_net "Net-(D157-Pad2)")
    (add_net "Net-(D158-Pad2)")
    (add_net "Net-(D159-Pad2)")
    (add_net "Net-(D16-Pad2)")
    (add_net "Net-(D160-Pad2)")
    (add_net "Net-(D161-Pad2)")
    (add_net "Net-(D162-Pad2)")
    (add_net "Net-(D163-Pad2)")
    (add_net "Net-(D164-Pad2)")
    (add_net "Net-(D166-Pad2)")
    (add_net "Net-(D167-Pad2)")
    (add_net "Net-(D168-Pad2)")
    (add_net "Net-(D169-Pad2)")
    (add_net "Net-(D17-Pad2)")
    (add_net "Net-(D170-Pad2)")
    (add_net "Net-(D171-Pad2)")
    (add_net "Net-(D172-Pad2)")
    (add_net "Net-(D173-Pad2)")
    (add_net "Net-(D174-Pad2)")
    (add_net "Net-(D175-Pad2)")
    (add_net "Net-(D176-Pad2)")
    (add_net "Net-(D177-Pad2)")
    (add_net "Net-(D178-Pad2)")
    (add_net "Net-(D179-Pad2)")
    (add_net "Net-(D18-Pad2)")
    (add_net "Net-(D181-Pad2)")
    (add_net "Net-(D182-Pad2)")
    (add_net "Net-(D183-Pad2)")
    (add_net "Net-(D184-Pad2)")
    (add_net "Net-(D185-Pad2)")
    (add_net "Net-(D186-Pad2)")
    (add_net "Net-(D187-Pad2)")
    (add_net "Net-(D188-Pad2)")
    (add_net "Net-(D189-Pad2)")
    (add_net "Net-(D19-Pad2)")
    (add_net "Net-(D190-Pad2)")
    (add_net "Net-(D191-Pad2)")
    (add_net "Net-(D192-Pad2)")
    (add_net "Net-(D193-Pad2)")
    (add_net "Net-(D194-Pad2)")
    (add_net "Net-(D196-Pad2)")
    (add_net "Net-(D197-Pad2)")
    (add_net "Net-(D198-Pad2)")
    (add_net "Net-(D199-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D20-Pad2)")
    (add_net "Net-(D200-Pad2)")
    (add_net "Net-(D201-Pad2)")
    (add_net "Net-(D202-Pad2)")
    (add_net "Net-(D203-Pad2)")
    (add_net "Net-(D204-Pad2)")
    (add_net "Net-(D205-Pad2)")
    (add_net "Net-(D206-Pad2)")
    (add_net "Net-(D207-Pad2)")
    (add_net "Net-(D208-Pad2)")
    (add_net "Net-(D209-Pad2)")
    (add_net "Net-(D21-Pad2)")
    (add_net "Net-(D211-Pad2)")
    (add_net "Net-(D212-Pad2)")
    (add_net "Net-(D213-Pad2)")
    (add_net "Net-(D214-Pad2)")
    (add_net "Net-(D215-Pad2)")
    (add_net "Net-(D216-Pad2)")
    (add_net "Net-(D217-Pad2)")
    (add_net "Net-(D218-Pad2)")
    (add_net "Net-(D219-Pad2)")
    (add_net "Net-(D22-Pad2)")
    (add_net "Net-(D220-Pad2)")
    (add_net "Net-(D221-Pad2)")
    (add_net "Net-(D222-Pad2)")
    (add_net "Net-(D223-Pad2)")
    (add_net "Net-(D224-Pad2)")
    (add_net "Net-(D226-Pad2)")
    (add_net "Net-(D227-Pad2)")
    (add_net "Net-(D228-Pad2)")
    (add_net "Net-(D229-Pad2)")
    (add_net "Net-(D23-Pad2)")
    (add_net "Net-(D230-Pad2)")
    (add_net "Net-(D231-Pad2)")
    (add_net "Net-(D232-Pad2)")
    (add_net "Net-(D233-Pad2)")
    (add_net "Net-(D234-Pad2)")
    (add_net "Net-(D235-Pad2)")
    (add_net "Net-(D236-Pad2)")
    (add_net "Net-(D237-Pad2)")
    (add_net "Net-(D238-Pad2)")
    (add_net "Net-(D239-Pad2)")
    (add_net "Net-(D24-Pad2)")
    (add_net "Net-(D241-Pad2)")
    (add_net "Net-(D242-Pad2)")
    (add_net "Net-(D243-Pad2)")
    (add_net "Net-(D244-Pad2)")
    (add_net "Net-(D245-Pad2)")
    (add_net "Net-(D246-Pad2)")
    (add_net "Net-(D247-Pad2)")
    (add_net "Net-(D248-Pad2)")
    (add_net "Net-(D249-Pad2)")
    (add_net "Net-(D25-Pad2)")
    (add_net "Net-(D250-Pad2)")
    (add_net "Net-(D251-Pad2)")
    (add_net "Net-(D252-Pad2)")
    (add_net "Net-(D253-Pad2)")
    (add_net "Net-(D254-Pad2)")
    (add_net "Net-(D26-Pad2)")
    (add_net "Net-(D27-Pad2)")
    (add_net "Net-(D28-Pad2)")
    (add_net "Net-(D29-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D31-Pad2)")
    (add_net "Net-(D32-Pad2)")
    (add_net "Net-(D33-Pad2)")
    (add_net "Net-(D34-Pad2)")
    (add_net "Net-(D35-Pad2)")
    (add_net "Net-(D36-Pad2)")
    (add_net "Net-(D37-Pad2)")
    (add_net "Net-(D38-Pad2)")
    (add_net "Net-(D39-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D40-Pad2)")
    (add_net "Net-(D41-Pad2)")
    (add_net "Net-(D42-Pad2)")
    (add_net "Net-(D43-Pad2)")
    (add_net "Net-(D44-Pad2)")
    (add_net "Net-(D46-Pad2)")
    (add_net "Net-(D47-Pad2)")
    (add_net "Net-(D48-Pad2)")
    (add_net "Net-(D49-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D50-Pad2)")
    (add_net "Net-(D51-Pad2)")
    (add_net "Net-(D52-Pad2)")
    (add_net "Net-(D53-Pad2)")
    (add_net "Net-(D54-Pad2)")
    (add_net "Net-(D55-Pad2)")
    (add_net "Net-(D56-Pad2)")
    (add_net "Net-(D57-Pad2)")
    (add_net "Net-(D58-Pad2)")
    (add_net "Net-(D59-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D61-Pad2)")
    (add_net "Net-(D62-Pad2)")
    (add_net "Net-(D63-Pad2)")
    (add_net "Net-(D64-Pad2)")
    (add_net "Net-(D65-Pad2)")
    (add_net "Net-(D66-Pad2)")
    (add_net "Net-(D67-Pad2)")
    (add_net "Net-(D68-Pad2)")
    (add_net "Net-(D69-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D70-Pad2)")
    (add_net "Net-(D71-Pad2)")
    (add_net "Net-(D72-Pad2)")
    (add_net "Net-(D73-Pad2)")
    (add_net "Net-(D74-Pad2)")
    (add_net "Net-(D76-Pad2)")
    (add_net "Net-(D77-Pad2)")
    (add_net "Net-(D78-Pad2)")
    (add_net "Net-(D79-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D80-Pad2)")
    (add_net "Net-(D81-Pad2)")
    (add_net "Net-(D82-Pad2)")
    (add_net "Net-(D83-Pad2)")
    (add_net "Net-(D84-Pad2)")
    (add_net "Net-(D85-Pad2)")
    (add_net "Net-(D86-Pad2)")
    (add_net "Net-(D87-Pad2)")
    (add_net "Net-(D88-Pad2)")
    (add_net "Net-(D89-Pad2)")
    (add_net "Net-(D91-Pad2)")
    (add_net "Net-(D92-Pad2)")
    (add_net "Net-(D93-Pad2)")
    (add_net "Net-(D94-Pad2)")
    (add_net "Net-(D95-Pad2)")
    (add_net "Net-(D96-Pad2)")
    (add_net "Net-(D97-Pad2)")
    (add_net "Net-(D98-Pad2)")
    (add_net VDD)
  )
  (module TestPoint:TestPoint_Pad_D2.5mm (layer B.Cu) (tedit 60057767)
    (at 131.82854 175.93634)
    (descr "SMD pad as test Point, diameter 2.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference REF** (at -1.78054 4.12242) (layer B.SilkS) hide)
    (fp_text value TestPoint_Pad_D2.5mm (at 0 -2.25) (layer B.Fab))
    (fp_text user %R (at 0 2.15) (layer B.Fab))
    (pad 1 smd oval (at -0.09144 -0.57982) (size 2.5 4) (layers B.Cu B.Mask)
      (net 1 VDD))
  )
  (module TestPoint:TestPoint_Pad_D2.5mm (layer B.Cu) (tedit 60057746)
    (at 114.47272 173.92142)
    (descr "SMD pad as test Point, diameter 2.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference REF** (at -0.23876 3.79476) (layer B.SilkS) hide)
    (fp_text value TestPoint_Pad_D2.5mm (at 0 -2.25) (layer B.Fab))
    (fp_text user %R (at 0 2.15) (layer B.Fab))
    (pad 1 smd oval (at 0 0 348) (size 2.5 4) (layers B.Cu B.Mask)
      (net 4 GND))
  )
  (module Wokwi:border-text (layer F.Cu) (tedit 0)
    (at 130 90 271.5)
    (fp_text reference Ref** (at 0 0 91.5) (layer F.SilkS) hide)
    (fp_text value Val** (at 0 0 91.5) (layer F.SilkS) hide)
  )
  (module Wokwi:skull-spiral (layer B.Cu) (tedit 0)
    (at 130 90 180)
    (fp_text reference Ref** (at 0 0) (layer B.SilkS) hide)
    (fp_text value Val** (at 0 0) (layer B.SilkS) hide)
  )
  (module Symbol:KiCad-Logo2_5mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 203.51496 53.29174 116)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.08 296) (layer F.SilkS) hide)
    (fp_text value KiCad-Logo2_5mm_SilkScreen (at 0 5.08 296) (layer F.Fab) hide)
  )
  (module Symbol:OSHW-Logo2_9.8x8mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 171.64304 20.17776 145)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference 2 (at 0 0 325) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_9.8x8mm_SilkScreen (at 0.75 0 325) (layer F.Fab) hide)
  )
  (module MountingHole:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 51.657172 112.464445)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference HOLE2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 202.617032 127.000226)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference HOLE1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 128.577629 8.512413)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference HOLE3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 119.019726 12.029278 58.016)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D184 (at 0 -3.5 58.016) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 58.016) (layer F.Fab))
    (fp_text user %R (at 0 0 58.016) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 58.016) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 58.016) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 58.016) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(D184-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 58.016) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(D183-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 58.016) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 165.507573 52.393987 186.644)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D6 (at 0 -3.5 6.644) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 6.644) (layer F.Fab))
    (fp_text user %R (at 0 0 6.644) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 6.644) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 186.644) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 186.644) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D6-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 186.644) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D5-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 186.644) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 208.102719 68.974006 333.032)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C256 (at 0 -1.43 333.032) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 333.032) (layer F.Fab))
    (fp_text user %R (at 0 0 333.032) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 333.032) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 333.032) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 201.39773 59.950134 340.7)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C255 (at 0 -1.43 340.7) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 340.7) (layer F.Fab))
    (fp_text user %R (at 0 0 340.7) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 340.7) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 340.7) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 193.594526 52.395743 348.368)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C254 (at 0 -1.43 348.368) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 348.368) (layer F.Fab))
    (fp_text user %R (at 0 0 348.368) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 348.368) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 348.368) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 184.95514 46.467541 356.036)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C253 (at 0 -1.43 356.036) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 356.036) (layer F.Fab))
    (fp_text user %R (at 0 0 356.036) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 356.036) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 356.036) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 175.76402 42.287135 3.704)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C252 (at 0 -1.43 3.704) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 3.704) (layer F.Fab))
    (fp_text user %R (at 0 0 3.704) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 3.704) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 3.704) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 166.324051 39.941522 11.372)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C251 (at 0 -1.43 11.372) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 11.372) (layer F.Fab))
    (fp_text user %R (at 0 0 11.372) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 11.372) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 11.372) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 156.953658 39.48649 19.04)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C250 (at 0 -1.43 19.04) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 19.04) (layer F.Fab))
    (fp_text user %R (at 0 0 19.04) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 19.04) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 19.04) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 147.986347 40.955216 26.708)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C249 (at 0 -1.43 26.708) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 26.708) (layer F.Fab))
    (fp_text user %R (at 0 0 26.708) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 26.708) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 26.708) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 139.775663 44.377809 34.376)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C248 (at 0 -1.43 34.376) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 34.376) (layer F.Fab))
    (fp_text user %R (at 0 0 34.376) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 34.376) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 34.376) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 132.713581 49.829312 42.044)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C247 (at 0 -1.43 42.044) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 42.044) (layer F.Fab))
    (fp_text user %R (at 0 0 42.044) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 42.044) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 42.044) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 127.290281 57.575517 49.712)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C246 (at 0 -1.43 49.712) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 49.712) (layer F.Fab))
    (fp_text user %R (at 0 0 49.712) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 49.712) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 49.712) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 124.354097 68.774009 57.38)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C245 (at 0 -1.43 57.38) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 57.38) (layer F.Fab))
    (fp_text user %R (at 0 0 57.38) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 57.38) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 57.38) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 120.242798 77.44476 257.444)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C244 (at 0 -1.43 257.444) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 257.444) (layer F.Fab))
    (fp_text user %R (at 0 0 257.444) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 257.444) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 257.444) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 117.52946 63.806541 249.776)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C243 (at 0 -1.43 249.776) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 249.776) (layer F.Fab))
    (fp_text user %R (at 0 0 249.776) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 249.776) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 249.776) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 119.344207 54.024338 242.108)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C242 (at 0 -1.43 242.108) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 242.108) (layer F.Fab))
    (fp_text user %R (at 0 0 242.108) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 242.108) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 242.108) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 123.710844 46.111711 234.44)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C241 (at 0 -1.43 234.44) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 234.44) (layer F.Fab))
    (fp_text user %R (at 0 0 234.44) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 234.44) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 234.44) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 129.953411 39.810331 226.772)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C240 (at 0 -1.43 226.772) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 226.772) (layer F.Fab))
    (fp_text user %R (at 0 0 226.772) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 226.772) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 226.772) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 137.637125 35.128923 219.104)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C239 (at 0 -1.43 219.104) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 219.104) (layer F.Fab))
    (fp_text user %R (at 0 0 219.104) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 219.104) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 219.104) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 146.401953 32.137876 211.436)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C238 (at 0 -1.43 211.436) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 211.436) (layer F.Fab))
    (fp_text user %R (at 0 0 211.436) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 211.436) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 211.436) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 155.914429 30.909949 203.768)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C237 (at 0 -1.43 203.768) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 203.768) (layer F.Fab))
    (fp_text user %R (at 0 0 203.768) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 203.768) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 203.768) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 165.851442 31.496927 196.1)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C236 (at 0 -1.43 196.1) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 196.1) (layer F.Fab))
    (fp_text user %R (at 0 0 196.1) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 196.1) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 196.1) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 175.895709 33.918722 188.432)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C235 (at 0 -1.43 188.432) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 188.432) (layer F.Fab))
    (fp_text user %R (at 0 0 188.432) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 188.432) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 188.432) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 185.736393 38.157944 180.764)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C234 (at 0 -1.43 180.764) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 180.764) (layer F.Fab))
    (fp_text user %R (at 0 0 180.764) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180.764) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 180.764) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 195.072188 44.15745 173.096)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C233 (at 0 -1.43 173.096) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 173.096) (layer F.Fab))
    (fp_text user %R (at 0 0 173.096) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 173.096) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 173.096) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 185.171443 29.774907 5.492)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C232 (at 0 -1.43 5.492) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 5.492) (layer F.Fab))
    (fp_text user %R (at 0 0 5.492) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 5.492) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 5.492) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 174.611825 25.661747 13.16)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C231 (at 0 -1.43 13.16) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 13.16) (layer F.Fab))
    (fp_text user %R (at 0 0 13.16) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 13.16) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 13.16) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 163.900322 23.379389 20.828)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C230 (at 0 -1.43 20.828) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 20.828) (layer F.Fab))
    (fp_text user %R (at 0 0 20.828) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 20.828) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 20.828) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 153.341396 22.919851 28.496)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C229 (at 0 -1.43 28.496) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 28.496) (layer F.Fab))
    (fp_text user %R (at 0 0 28.496) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 28.496) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 28.496) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 143.239212 24.233102 36.164)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C228 (at 0 -1.43 36.164) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 36.164) (layer F.Fab))
    (fp_text user %R (at 0 0 36.164) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 36.164) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 36.164) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 133.894212 27.229357 43.832)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C227 (at 0 -1.43 43.832) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 43.832) (layer F.Fab))
    (fp_text user %R (at 0 0 43.832) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 43.832) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 43.832) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 125.601885 31.783028 51.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C226 (at 0 -1.43 51.5) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 51.5) (layer F.Fab))
    (fp_text user %R (at 0 0 51.5) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 51.5) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 51.5) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 118.655715 37.739225 59.168)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C225 (at 0 -1.43 59.168) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 59.168) (layer F.Fab))
    (fp_text user %R (at 0 0 59.168) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 59.168) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 59.168) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 113.358893 44.925187 66.836)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C224 (at 0 -1.43 66.836) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 66.836) (layer F.Fab))
    (fp_text user %R (at 0 0 66.836) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 66.836) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 66.836) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 110.057326 53.174038 74.504)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C223 (at 0 -1.43 74.504) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 74.504) (layer F.Fab))
    (fp_text user %R (at 0 0 74.504) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 74.504) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 74.504) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 109.237822 62.389519 82.172)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C222 (at 0 -1.43 82.172) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 82.172) (layer F.Fab))
    (fp_text user %R (at 0 0 82.172) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 82.172) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 82.172) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 111.924738 72.820184 89.84)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C221 (at 0 -1.43 89.84) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 89.84) (layer F.Fab))
    (fp_text user %R (at 0 0 89.84) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 89.84) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 89.84) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 111.488541 82.591295 289.904)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C220 (at 0 -1.43 289.904) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 289.904) (layer F.Fab))
    (fp_text user %R (at 0 0 289.904) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 289.904) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 289.904) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 103.628659 73.204619 282.236)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C219 (at 0 -1.43 282.236) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 282.236) (layer F.Fab))
    (fp_text user %R (at 0 0 282.236) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 282.236) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 282.236) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 100.477777 64.122746 274.568)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C218 (at 0 -1.43 274.568) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 274.568) (layer F.Fab))
    (fp_text user %R (at 0 0 274.568) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 274.568) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 274.568) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 100.25653 55.169844 266.9)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C217 (at 0 -1.43 266.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 266.9) (layer F.Fab))
    (fp_text user %R (at 0 0 266.9) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 266.9) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 266.9) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 102.392007 46.54846 259.232)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C216 (at 0 -1.43 259.232) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 259.232) (layer F.Fab))
    (fp_text user %R (at 0 0 259.232) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 259.232) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 259.232) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 106.56468 38.51623 251.564)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C215 (at 0 -1.43 251.564) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 251.564) (layer F.Fab))
    (fp_text user %R (at 0 0 251.564) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 251.564) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 251.564) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 112.52629 31.332326 243.896)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C214 (at 0 -1.43 243.896) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 243.896) (layer F.Fab))
    (fp_text user %R (at 0 0 243.896) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 243.896) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 243.896) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 120.04306 25.239917 236.228)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C213 (at 0 -1.43 236.228) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 236.228) (layer F.Fab))
    (fp_text user %R (at 0 0 236.228) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 236.228) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 236.228) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 128.874594 20.457264 228.56)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C212 (at 0 -1.43 228.56) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 228.56) (layer F.Fab))
    (fp_text user %R (at 0 0 228.56) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 228.56) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 228.56) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 138.766279 17.17174 220.892)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C211 (at 0 -1.43 220.892) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 220.892) (layer F.Fab))
    (fp_text user %R (at 0 0 220.892) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 220.892) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 220.892) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 149.447832 15.535286 213.224)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C210 (at 0 -1.43 213.224) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 213.224) (layer F.Fab))
    (fp_text user %R (at 0 0 213.224) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 213.224) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 213.224) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 160.63508 15.660866 205.556)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C209 (at 0 -1.43 205.556) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 205.556) (layer F.Fab))
    (fp_text user %R (at 0 0 205.556) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 205.556) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 205.556) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 144.392231 8.805181 37.952)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C208 (at 0 -1.43 37.952) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 37.952) (layer F.Fab))
    (fp_text user %R (at 0 0 37.952) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 37.952) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 37.952) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 133.173537 10.952504 45.62)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C207 (at 0 -1.43 45.62) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 45.62) (layer F.Fab))
    (fp_text user %R (at 0 0 45.62) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 45.62) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 45.62) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 122.79866 14.734989 53.288)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C206 (at 0 -1.43 53.288) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 53.288) (layer F.Fab))
    (fp_text user %R (at 0 0 53.288) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 53.288) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 53.288) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 113.519925 19.983285 60.956)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C205 (at 0 -1.43 60.956) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 60.956) (layer F.Fab))
    (fp_text user %R (at 0 0 60.956) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 60.956) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 60.956) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 105.566377 26.492611 68.624)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C204 (at 0 -1.43 68.624) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 68.624) (layer F.Fab))
    (fp_text user %R (at 0 0 68.624) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 68.624) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 68.624) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 99.141757 34.026501 76.292)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C203 (at 0 -1.43 76.292) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 76.292) (layer F.Fab))
    (fp_text user %R (at 0 0 76.292) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 76.292) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 76.292) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 94.424921 42.320758 83.96)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C202 (at 0 -1.43 83.96) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 83.96) (layer F.Fab))
    (fp_text user %R (at 0 0 83.96) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 83.96) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 83.96) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 91.574476 51.087274 91.628)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C201 (at 0 -1.43 91.628) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 91.628) (layer F.Fab))
    (fp_text user %R (at 0 0 91.628) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 91.628) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 91.628) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 90.741733 60.017147 99.296)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C200 (at 0 -1.43 99.296) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 99.296) (layer F.Fab))
    (fp_text user %R (at 0 0 99.296) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 99.296) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 99.296) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 92.103109 68.782265 106.964)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C199 (at 0 -1.43 106.964) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 106.964) (layer F.Fab))
    (fp_text user %R (at 0 0 106.964) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 106.964) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 106.964) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 95.949528 77.034171 114.632)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C198 (at 0 -1.43 114.632) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 114.632) (layer F.Fab))
    (fp_text user %R (at 0 0 114.632) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 114.632) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 114.632) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 103.013732 84.402995 122.3)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C197 (at 0 -1.43 122.3) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 122.3) (layer F.Fab))
    (fp_text user %R (at 0 0 122.3) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 122.3) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 122.3) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 117.278882 90.666867 129.968)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C196 (at 0 -1.43 129.968) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 129.968) (layer F.Fab))
    (fp_text user %R (at 0 0 129.968) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 129.968) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 129.968) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 107.112107 93.819993 322.364)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C195 (at 0 -1.43 322.364) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 322.364) (layer F.Fab))
    (fp_text user %R (at 0 0 322.364) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 322.364) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 322.364) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 96.644221 89.788349 314.696)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C194 (at 0 -1.43 314.696) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 314.696) (layer F.Fab))
    (fp_text user %R (at 0 0 314.696) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 314.696) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 314.696) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 89.580612 83.637149 307.028)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C193 (at 0 -1.43 307.028) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 307.028) (layer F.Fab))
    (fp_text user %R (at 0 0 307.028) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 307.028) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 307.028) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 84.880805 76.074549 299.36)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C192 (at 0 -1.43 299.36) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 299.36) (layer F.Fab))
    (fp_text user %R (at 0 0 299.36) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 299.36) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 299.36) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 82.275448 67.557249 291.692)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C191 (at 0 -1.43 291.692) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 291.692) (layer F.Fab))
    (fp_text user %R (at 0 0 291.692) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 291.692) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 291.692) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 81.668755 58.465948 284.024)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C190 (at 0 -1.43 284.024) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 284.024) (layer F.Fab))
    (fp_text user %R (at 0 0 284.024) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 284.024) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 284.024) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 83.005549 49.148656 276.356)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C189 (at 0 -1.43 276.356) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 276.356) (layer F.Fab))
    (fp_text user %R (at 0 0 276.356) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 276.356) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 276.356) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 86.226387 39.933826 268.688)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C188 (at 0 -1.43 268.688) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 268.688) (layer F.Fab))
    (fp_text user %R (at 0 0 268.688) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 268.688) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 268.688) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 91.249243 31.133216 261.02)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C187 (at 0 -1.43 261.02) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 261.02) (layer F.Fab))
    (fp_text user %R (at 0 0 261.02) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 261.02) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 261.02) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 97.961653 23.040521 253.352)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C186 (at 0 -1.43 253.352) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 253.352) (layer F.Fab))
    (fp_text user %R (at 0 0 253.352) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 253.352) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 253.352) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 106.217888 15.928109 245.684)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C185 (at 0 -1.43 245.684) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 245.684) (layer F.Fab))
    (fp_text user %R (at 0 0 245.684) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 245.684) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 245.684) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 115.838991 10.042969 238.016)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C184 (at 0 -1.43 238.016) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 238.016) (layer F.Fab))
    (fp_text user %R (at 0 0 238.016) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 238.016) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 238.016) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 89.870293 20.88347 78.08)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C183 (at 0 -1.43 78.08) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 78.08) (layer F.Fab))
    (fp_text user %R (at 0 0 78.08) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 78.08) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 78.08) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 83.031891 29.669464 85.748)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C182 (at 0 -1.43 85.748) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 85.748) (layer F.Fab))
    (fp_text user %R (at 0 0 85.748) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 85.748) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 85.748) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 77.901499 39.117887 93.416)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C181 (at 0 -1.43 93.416) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 93.416) (layer F.Fab))
    (fp_text user %R (at 0 0 93.416) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 93.416) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 93.416) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 74.562361 48.933949 101.084)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C180 (at 0 -1.43 101.084) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 101.084) (layer F.Fab))
    (fp_text user %R (at 0 0 101.084) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 101.084) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 101.084) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 73.058695 58.810006 108.752)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C179 (at 0 -1.43 108.752) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 108.752) (layer F.Fab))
    (fp_text user %R (at 0 0 108.752) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 108.752) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 108.752) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 73.397685 68.428962 116.42)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C178 (at 0 -1.43 116.42) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 116.42) (layer F.Fab))
    (fp_text user %R (at 0 0 116.42) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 116.42) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 116.42) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 75.554463 77.465573 124.088)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C177 (at 0 -1.43 124.088) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 124.088) (layer F.Fab))
    (fp_text user %R (at 0 0 124.088) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 124.088) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 124.088) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 79.482561 85.583383 131.756)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C176 (at 0 -1.43 131.756) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 131.756) (layer F.Fab))
    (fp_text user %R (at 0 0 131.756) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 131.756) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 131.756) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 85.136528 92.42178 139.424)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C175 (at 0 -1.43 139.424) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 139.424) (layer F.Fab))
    (fp_text user %R (at 0 0 139.424) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 139.424) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 139.424) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 92.528704 97.556798 147.092)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C174 (at 0 -1.43 147.092) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 147.092) (layer F.Fab))
    (fp_text user %R (at 0 0 147.092) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 147.092) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 147.092) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 101.918534 100.369168 154.76)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C173 (at 0 -1.43 154.76) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 154.76) (layer F.Fab))
    (fp_text user %R (at 0 0 154.76) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 154.76) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 154.76) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 115.002465 99.29785 162.428)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C172 (at 0 -1.43 162.428) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 162.428) (layer F.Fab))
    (fp_text user %R (at 0 0 162.428) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 162.428) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 162.428) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 110.409646 107.127193 354.824)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C171 (at 0 -1.43 354.824) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 354.824) (layer F.Fab))
    (fp_text user %R (at 0 0 354.824) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 354.824) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 354.824) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 99.99342 108.620728 347.156)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C170 (at 0 -1.43 347.156) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 347.156) (layer F.Fab))
    (fp_text user %R (at 0 0 347.156) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 347.156) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 347.156) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 90.977532 106.856622 339.488)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C169 (at 0 -1.43 339.488) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 339.488) (layer F.Fab))
    (fp_text user %R (at 0 0 339.488) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 339.488) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 339.488) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 83.108826 102.748058 331.82)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C168 (at 0 -1.43 331.82) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 331.82) (layer F.Fab))
    (fp_text user %R (at 0 0 331.82) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 331.82) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 331.82) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 76.460817 96.766805 324.152)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C167 (at 0 -1.43 324.152) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 324.152) (layer F.Fab))
    (fp_text user %R (at 0 0 324.152) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 324.152) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 324.152) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 71.176835 89.263816 316.484)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C166 (at 0 -1.43 316.484) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 316.484) (layer F.Fab))
    (fp_text user %R (at 0 0 316.484) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 316.484) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 316.484) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 67.40567 80.552429 308.816)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C165 (at 0 -1.43 308.816) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 308.816) (layer F.Fab))
    (fp_text user %R (at 0 0 308.816) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 308.816) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 308.816) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 65.277458 70.936583 301.148)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C164 (at 0 -1.43 301.148) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 301.148) (layer F.Fab))
    (fp_text user %R (at 0 0 301.148) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 301.148) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 301.148) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 64.892147 60.720518 293.48)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C163 (at 0 -1.43 293.48) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 293.48) (layer F.Fab))
    (fp_text user %R (at 0 0 293.48) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 293.48) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 293.48) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 66.313152 50.210725 285.812)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C162 (at 0 -1.43 285.812) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 285.812) (layer F.Fab))
    (fp_text user %R (at 0 0 285.812) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 285.812) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 285.812) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 69.5637 39.714164 278.144)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C161 (at 0 -1.43 278.144) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 278.144) (layer F.Fab))
    (fp_text user %R (at 0 0 278.144) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 278.144) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 278.144) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 74.624949 29.534537 270.476)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C160 (at 0 -1.43 270.476) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 270.476) (layer F.Fab))
    (fp_text user %R (at 0 0 270.476) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270.476) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 270.476) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 58.345402 52.825054 110.54)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C159 (at 0 -1.43 110.54) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 110.54) (layer F.Fab))
    (fp_text user %R (at 0 0 110.54) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 110.54) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 110.54) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 57.209964 63.991604 118.208)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C158 (at 0 -1.43 118.208) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 118.208) (layer F.Fab))
    (fp_text user %R (at 0 0 118.208) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 118.208) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 118.208) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 57.875954 74.813785 125.876)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C157 (at 0 -1.43 -54.124) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 -54.124) (layer F.Fab))
    (fp_text user %R (at 0 0 -54.124) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 125.876) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 125.876) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 60.2559 84.998913 133.544)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C156 (at 0 -1.43 133.544) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 133.544) (layer F.Fab))
    (fp_text user %R (at 0 0 133.544) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 133.544) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 133.544) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 64.222155 94.264941 141.212)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C155 (at 0 -1.43 141.212) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 141.212) (layer F.Fab))
    (fp_text user %R (at 0 0 141.212) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 141.212) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 141.212) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 69.610195 102.342711 148.88)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C154 (at 0 -1.43 148.88) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 148.88) (layer F.Fab))
    (fp_text user %R (at 0 0 148.88) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 148.88) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 148.88) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 76.223127 108.975241 156.548)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C153 (at 0 -1.43 156.548) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 156.548) (layer F.Fab))
    (fp_text user %R (at 0 0 156.548) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 156.548) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 156.548) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 83.837983 113.911363 164.216)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C152 (at 0 -1.43 164.216) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 164.216) (layer F.Fab))
    (fp_text user %R (at 0 0 164.216) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 164.216) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 164.216) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 92.21563 116.887176 171.884)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C151 (at 0 -1.43 171.884) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 171.884) (layer F.Fab))
    (fp_text user %R (at 0 0 171.884) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 171.884) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 171.884) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 101.120743 117.575945 179.552)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C150 (at 0 -1.43 179.552) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 179.552) (layer F.Fab))
    (fp_text user %R (at 0 0 179.552) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 179.552) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 179.552) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 110.380731 115.431301 187.22)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C149 (at 0 -1.43 187.22) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 187.22) (layer F.Fab))
    (fp_text user %R (at 0 0 187.22) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 187.22) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 187.22) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 120.20292 108.928038 194.888)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C148 (at 0 -1.43 194.888) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 194.888) (layer F.Fab))
    (fp_text user %R (at 0 0 194.888) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 194.888) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 194.888) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 128.968555 104.901088 34.952)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C147 (at 0 -1.43 34.952) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 34.952) (layer F.Fab))
    (fp_text user %R (at 0 0 34.952) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 34.952) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 34.952) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 121.68618 117.298235 27.284)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C146 (at 0 -1.43 27.284) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 27.284) (layer F.Fab))
    (fp_text user %R (at 0 0 27.284) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 27.284) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 27.284) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 113.73775 123.415607 19.616)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C145 (at 0 -1.43 19.616) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 19.616) (layer F.Fab))
    (fp_text user %R (at 0 0 19.616) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 19.616) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 19.616) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 105.176305 126.374083 11.948)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C144 (at 0 -1.43 11.948) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 11.948) (layer F.Fab))
    (fp_text user %R (at 0 0 11.948) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 11.948) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 11.948) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 96.320015 126.856435 4.28)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C143 (at 0 -1.43 4.28) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 4.28) (layer F.Fab))
    (fp_text user %R (at 0 0 4.28) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 4.28) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 4.28) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 87.493931 125.160395 356.612)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C142 (at 0 -1.43 356.612) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 356.612) (layer F.Fab))
    (fp_text user %R (at 0 0 356.612) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 356.612) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 356.612) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 79.010596 121.481472 348.944)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C141 (at 0 -1.43 348.944) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 348.944) (layer F.Fab))
    (fp_text user %R (at 0 0 348.944) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 348.944) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 348.944) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 71.164889 115.993243 341.276)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C140 (at 0 -1.43 341.276) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 341.276) (layer F.Fab))
    (fp_text user %R (at 0 0 341.276) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 341.276) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 341.276) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 64.230024 108.876789 333.608)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C139 (at 0 -1.43 333.608) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 333.608) (layer F.Fab))
    (fp_text user %R (at 0 0 333.608) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 333.608) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 333.608) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 58.453456 100.332275 325.94)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C138 (at 0 -1.43 325.94) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 325.94) (layer F.Fab))
    (fp_text user %R (at 0 0 325.94) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 325.94) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 325.94) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 54.052745 90.582763 318.272)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C137 (at 0 -1.43 318.272) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 318.272) (layer F.Fab))
    (fp_text user %R (at 0 0 318.272) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 318.272) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 318.272) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 51.211599 79.874048 310.604)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C136 (at 0 -1.43 310.604) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 310.604) (layer F.Fab))
    (fp_text user %R (at 0 0 310.604) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 310.604) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 310.604) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 48.794598 97.132403 143)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C135 (at 0 -1.43 143) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 143) (layer F.Fab))
    (fp_text user %R (at 0 0 143) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 143) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 143) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 53.807007 107.275936 150.668)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C134 (at 0 -1.43 150.668) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 150.668) (layer F.Fab))
    (fp_text user %R (at 0 0 150.668) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 150.668) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 150.668) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 60.165836 116.170447 158.336)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C133 (at 0 -1.43 158.336) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 158.336) (layer F.Fab))
    (fp_text user %R (at 0 0 158.336) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 158.336) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 158.336) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 67.641022 123.616138 166.004)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C132 (at 0 -1.43 166.004) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 166.004) (layer F.Fab))
    (fp_text user %R (at 0 0 166.004) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 166.004) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 166.004) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 75.974319 129.444308 173.672)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C131 (at 0 -1.43 173.672) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 173.672) (layer F.Fab))
    (fp_text user %R (at 0 0 173.672) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 173.672) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 173.672) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 84.883357 133.517904 181.34)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C130 (at 0 -1.43 181.34) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 181.34) (layer F.Fab))
    (fp_text user %R (at 0 0 181.34) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 181.34) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 181.34) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 94.065193 135.729299 189.008)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C129 (at 0 -1.43 189.008) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 189.008) (layer F.Fab))
    (fp_text user %R (at 0 0 189.008) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 189.008) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 189.008) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 103.198469 135.993202 196.676)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C128 (at 0 -1.43 196.676) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 196.676) (layer F.Fab))
    (fp_text user %R (at 0 0 196.676) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 196.676) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 196.676) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 111.94239 134.229639 204.344)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C127 (at 0 -1.43 204.344) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 204.344) (layer F.Fab))
    (fp_text user %R (at 0 0 204.344) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 204.344) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 204.344) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 119.928143 130.322234 212.012)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C126 (at 0 -1.43 212.012) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 212.012) (layer F.Fab))
    (fp_text user %R (at 0 0 212.012) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 212.012) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 212.012) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 126.72929 123.997285 219.68)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C125 (at 0 -1.43 219.68) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 219.68) (layer F.Fab))
    (fp_text user %R (at 0 0 219.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 219.68) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 219.68) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 131.749637 114.311941 227.348)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C124 (at 0 -1.43 227.348) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 227.348) (layer F.Fab))
    (fp_text user %R (at 0 0 227.348) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 227.348) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 227.348) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 138.424684 107.263628 67.412)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C123 (at 0 -1.43 67.412) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 67.412) (layer F.Fab))
    (fp_text user %R (at 0 0 67.412) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 67.412) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 67.412) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 138.026193 119.765727 59.744)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C122 (at 0 -1.43 59.744) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 59.744) (layer F.Fab))
    (fp_text user %R (at 0 0 59.744) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 59.744) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 59.744) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 134.276713 128.681466 52.076)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C121 (at 0 -1.43 52.076) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 52.076) (layer F.Fab))
    (fp_text user %R (at 0 0 52.076) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 52.076) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 52.076) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 128.432889 135.48584 44.408)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C120 (at 0 -1.43 44.408) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 44.408) (layer F.Fab))
    (fp_text user %R (at 0 0 44.408) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 44.408) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 44.408) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 121.065068 140.43978 36.74)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C119 (at 0 -1.43 36.74) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 36.74) (layer F.Fab))
    (fp_text user %R (at 0 0 36.74) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 36.74) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 36.74) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 112.586644 143.576592 29.072)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C118 (at 0 -1.43 29.072) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 29.072) (layer F.Fab))
    (fp_text user %R (at 0 0 29.072) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 29.072) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 29.072) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 103.357396 144.875954 21.404)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C117 (at 0 -1.43 21.404) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 21.404) (layer F.Fab))
    (fp_text user %R (at 0 0 21.404) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 21.404) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 21.404) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 93.714814 144.317925 13.736)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C116 (at 0 -1.43 13.736) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 13.736) (layer F.Fab))
    (fp_text user %R (at 0 0 13.736) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 13.736) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 13.736) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 83.984073 141.904659 6.068)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C115 (at 0 -1.43 6.068) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 6.068) (layer F.Fab))
    (fp_text user %R (at 0 0 6.068) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 6.068) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 6.068) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 74.479799 137.670317 358.4)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C114 (at 0 -1.43 358.4) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 358.4) (layer F.Fab))
    (fp_text user %R (at 0 0 358.4) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 358.4) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 358.4) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 65.504143 131.685566 350.732)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C113 (at 0 -1.43 350.732) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 350.732) (layer F.Fab))
    (fp_text user %R (at 0 0 350.732) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 350.732) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 350.732) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 57.343131 124.059071 343.064)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C112 (at 0 -1.43 343.064) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 343.064) (layer F.Fab))
    (fp_text user %R (at 0 0 343.064) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 343.064) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 343.064) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 64.668905 140.058254 175.46)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C111 (at 0 -1.43 175.46) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 175.46) (layer F.Fab))
    (fp_text user %R (at 0 0 175.46) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 175.46) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 175.46) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 74.383496 146.032092 183.128)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C110 (at 0 -1.43 183.128) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 183.128) (layer F.Fab))
    (fp_text user %R (at 0 0 183.128) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 183.128) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 183.128) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 84.577655 150.230118 190.796)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C109 (at 0 -1.43 190.796) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 190.796) (layer F.Fab))
    (fp_text user %R (at 0 0 190.796) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 190.796) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 190.796) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 94.950786 152.606846 198.464)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C108 (at 0 -1.43 198.464) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 198.464) (layer F.Fab))
    (fp_text user %R (at 0 0 198.464) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 198.464) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 198.464) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 105.195474 153.158575 206.132)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C107 (at 0 -1.43 206.132) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 206.132) (layer F.Fab))
    (fp_text user %R (at 0 0 206.132) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 206.132) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 206.132) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 115.001462 151.921929 213.8)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C106 (at 0 -1.43 213.8) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 213.8) (layer F.Fab))
    (fp_text user %R (at 0 0 213.8) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 213.8) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 213.8) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 124.057928 148.970578 221.468)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C105 (at 0 -1.43 221.468) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 221.468) (layer F.Fab))
    (fp_text user %R (at 0 0 221.468) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 221.468) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 221.468) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 132.052461 144.409112 229.136)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C104 (at 0 -1.43 229.136) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 229.136) (layer F.Fab))
    (fp_text user %R (at 0 0 229.136) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 229.136) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 229.136) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 138.663235 138.361585 236.804)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C103 (at 0 -1.43 236.804) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 236.804) (layer F.Fab))
    (fp_text user %R (at 0 0 236.804) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 236.804) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 236.804) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 143.535169 130.947378 244.472)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C102 (at 0 -1.43 244.472) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 244.472) (layer F.Fab))
    (fp_text user %R (at 0 0 244.472) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 244.472) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 244.472) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 146.209919 122.217992 252.14)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C101 (at 0 -1.43 252.14) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 252.14) (layer F.Fab))
    (fp_text user %R (at 0 0 252.14) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 252.14) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 252.14) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 145.867119 111.917677 259.808)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C100 (at 0 -1.43 259.808) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 259.808) (layer F.Fab))
    (fp_text user %R (at 0 0 259.808) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 259.808) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 259.808) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 139.015511 97.03799 267.476)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C99 (at 0 -1.43 267.476) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 267.476) (layer F.Fab))
    (fp_text user %R (at 0 0 267.476) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 267.476) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 267.476) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 148.986604 102.247019 99.872)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C98 (at 0 -1.43 99.872) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 99.872) (layer F.Fab))
    (fp_text user %R (at 0 0 99.872) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 99.872) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 99.872) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 154.178382 112.38505 92.204)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C97 (at 0 -1.43 92.204) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 92.204) (layer F.Fab))
    (fp_text user %R (at 0 0 92.204) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 92.204) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 92.204) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 155.32078 121.725308 84.536)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C96 (at 0 -1.43 84.536) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 84.536) (layer F.Fab))
    (fp_text user %R (at 0 0 84.536) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 84.536) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 84.536) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 153.736434 130.495554 76.868)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C95 (at 0 -1.43 76.868) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 76.868) (layer F.Fab))
    (fp_text user %R (at 0 0 76.868) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 76.868) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 76.868) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 149.948928 138.550469 69.2)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C94 (at 0 -1.43 69.2) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 69.2) (layer F.Fab))
    (fp_text user %R (at 0 0 69.2) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 69.2) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 69.2) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 144.291898 145.67723 61.532)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C93 (at 0 -1.43 61.532) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 61.532) (layer F.Fab))
    (fp_text user %R (at 0 0 61.532) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 61.532) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 61.532) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 137.043701 151.657824 53.864)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C92 (at 0 -1.43 53.864) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 53.864) (layer F.Fab))
    (fp_text user %R (at 0 0 53.864) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 53.864) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 53.864) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 128.47133 156.290811 46.196)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C91 (at 0 -1.43 46.196) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 46.196) (layer F.Fab))
    (fp_text user %R (at 0 0 46.196) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 46.196) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 46.196) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 118.846553 159.401966 38.528)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C90 (at 0 -1.43 38.528) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 38.528) (layer F.Fab))
    (fp_text user %R (at 0 0 38.528) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 38.528) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 38.528) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 108.451074 160.850763 30.86)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C89 (at 0 -1.43 30.86) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 30.86) (layer F.Fab))
    (fp_text user %R (at 0 0 30.86) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 30.86) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 30.86) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 97.576554 160.534766 23.192)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C88 (at 0 -1.43 23.192) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 23.192) (layer F.Fab))
    (fp_text user %R (at 0 0 23.192) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 23.192) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 23.192) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 86.521925 158.39263 15.524)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C87 (at 0 -1.43 15.524) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 15.524) (layer F.Fab))
    (fp_text user %R (at 0 0 15.524) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 15.524) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 15.524) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 112.94338 167.915217 215.588)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C86 (at 0 -1.43 215.588) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 215.588) (layer F.Fab))
    (fp_text user %R (at 0 0 215.588) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 215.588) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 215.588) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 123.900305 166.04443 223.256)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C85 (at 0 -1.43 223.256) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 223.256) (layer F.Fab))
    (fp_text user %R (at 0 0 223.256) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 223.256) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 223.256) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 134.04287 162.533033 230.924)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C84 (at 0 -1.43 230.924) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 230.924) (layer F.Fab))
    (fp_text user %R (at 0 0 230.924) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 230.924) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 230.924) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 143.110436 157.542295 238.592)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C83 (at 0 -1.43 238.592) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 238.592) (layer F.Fab))
    (fp_text user %R (at 0 0 238.592) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 238.592) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 238.592) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 150.862326 151.26928 246.26)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C82 (at 0 -1.43 246.26) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 246.26) (layer F.Fab))
    (fp_text user %R (at 0 0 246.26) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 246.26) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 246.26) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 157.07855 143.942976 253.928)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C81 (at 0 -1.43 253.928) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 253.928) (layer F.Fab))
    (fp_text user %R (at 0 0 253.928) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 253.928) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 253.928) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 161.556804 135.819921 261.596)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C80 (at 0 -1.43 261.596) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 261.596) (layer F.Fab))
    (fp_text user %R (at 0 0 261.596) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 261.596) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 261.596) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 164.102245 127.17932 269.264)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C79 (at 0 -1.43 269.264) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 269.264) (layer F.Fab))
    (fp_text user %R (at 0 0 269.264) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 269.264) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 269.264) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 164.500943 118.317058 276.932)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C78 (at 0 -1.43 276.932) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 276.932) (layer F.Fab))
    (fp_text user %R (at 0 0 276.932) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 276.932) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 276.932) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 162.448028 109.535422 284.6)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C77 (at 0 -1.43 284.6) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 284.6) (layer F.Fab))
    (fp_text user %R (at 0 0 284.6) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 284.6) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 284.6) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 157.303288 101.108545 292.268)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C76 (at 0 -1.43 292.268) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 292.268) (layer F.Fab))
    (fp_text user %R (at 0 0 292.268) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 292.268) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 292.268) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 146.533536 92.980365 299.936)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C75 (at 0 -1.43 299.936) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 299.936) (layer F.Fab))
    (fp_text user %R (at 0 0 299.936) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 299.936) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 299.936) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 155.480194 90.531982 132.332)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C74 (at 0 -1.43 132.332) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 132.332) (layer F.Fab))
    (fp_text user %R (at 0 0 132.332) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 132.332) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 132.332) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 164.334234 96.43724 124.664)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C73 (at 0 -1.43 124.664) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 124.664) (layer F.Fab))
    (fp_text user %R (at 0 0 124.664) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 124.664) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 124.664) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 169.871714 103.80698 116.996)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C72 (at 0 -1.43 116.996) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 116.996) (layer F.Fab))
    (fp_text user %R (at 0 0 116.996) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 116.996) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 116.996) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 172.953456 112.135598 109.328)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C71 (at 0 -1.43 109.328) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 109.328) (layer F.Fab))
    (fp_text user %R (at 0 0 109.328) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 109.328) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 109.328) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 173.85826 121.0244 101.66)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C70 (at 0 -1.43 101.66) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 101.66) (layer F.Fab))
    (fp_text user %R (at 0 0 101.66) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 101.66) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 101.66) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 172.722867 130.117225 93.992)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C69 (at 0 -1.43 93.992) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 93.992) (layer F.Fab))
    (fp_text user %R (at 0 0 93.992) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 93.992) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 93.992) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 169.651637 139.082196 86.324)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C68 (at 0 -1.43 86.324) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 86.324) (layer F.Fab))
    (fp_text user %R (at 0 0 86.324) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 86.324) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 86.324) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 164.755115 147.607072 78.656)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C67 (at 0 -1.43 78.656) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 78.656) (layer F.Fab))
    (fp_text user %R (at 0 0 78.656) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 78.656) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 78.656) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 158.16572 155.399825 70.988)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C66 (at 0 -1.43 70.988) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 70.988) (layer F.Fab))
    (fp_text user %R (at 0 0 70.988) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 70.988) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 70.988) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 150.044029 162.191461 63.32)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C65 (at 0 -1.43 63.32) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 63.32) (layer F.Fab))
    (fp_text user %R (at 0 0 63.32) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 63.32) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 63.32) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 140.580392 167.73979 55.652)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C64 (at 0 -1.43 55.652) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 55.652) (layer F.Fab))
    (fp_text user %R (at 0 0 55.652) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 55.652) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 55.652) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 129.993879 171.833428 47.984)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C63 (at 0 -1.43 47.984) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 47.984) (layer F.Fab))
    (fp_text user %R (at 0 0 47.984) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 47.984) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 47.984) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 157.675333 165.661504 248.048)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C62 (at 0 -1.43 248.048) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 248.048) (layer F.Fab))
    (fp_text user %R (at 0 0 248.048) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 248.048) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 248.048) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 166.032409 158.195933 255.716)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C61 (at 0 -1.43 255.716) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 255.716) (layer F.Fab))
    (fp_text user %R (at 0 0 255.716) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 255.716) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 255.716) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 172.827464 149.770063 263.384)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C60 (at 0 -1.43 263.384) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 263.384) (layer F.Fab))
    (fp_text user %R (at 0 0 263.384) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 263.384) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 263.384) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 177.927281 140.658972 271.052)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C59 (at 0 -1.43 271.052) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 271.052) (layer F.Fab))
    (fp_text user %R (at 0 0 271.052) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 271.052) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 271.052) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 181.235336 131.157061 278.72)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C58 (at 0 -1.43 278.72) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 278.72) (layer F.Fab))
    (fp_text user %R (at 0 0 278.72) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 278.72) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 278.72) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 182.690798 121.574207 286.388)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C57 (at 0 -1.43 286.388) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 286.388) (layer F.Fab))
    (fp_text user %R (at 0 0 286.388) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 286.388) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 286.388) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 182.264563 112.233313 294.056)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C56 (at 0 -1.43 294.056) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 294.056) (layer F.Fab))
    (fp_text user %R (at 0 0 294.056) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 294.056) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 294.056) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 179.94997 103.470895 301.724)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C55 (at 0 -1.43 301.724) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 301.724) (layer F.Fab))
    (fp_text user %R (at 0 0 301.724) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 301.724) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 301.724) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 175.742121 95.644401 309.392)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C54 (at 0 -1.43 309.392) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 309.392) (layer F.Fab))
    (fp_text user %R (at 0 0 309.392) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 309.392) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 309.392) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 169.586806 89.156637 317.06)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C53 (at 0 -1.43 317.06) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 317.06) (layer F.Fab))
    (fp_text user %R (at 0 0 317.06) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 317.06) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 317.06) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 161.221022 84.535329 324.728)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C52 (at 0 -1.43 324.728) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 324.728) (layer F.Fab))
    (fp_text user %R (at 0 0 324.728) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 324.728) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 324.728) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 149.345072 82.806892 332.396)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C51 (at 0 -1.43 332.396) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 332.396) (layer F.Fab))
    (fp_text user %R (at 0 0 332.396) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 332.396) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 332.396) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 139.925662 80.281818 172.46)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C50 (at 0 -1.43 172.46) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 172.46) (layer F.Fab))
    (fp_text user %R (at 0 0 172.46) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 172.46) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 172.46) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 154.129082 75.690586 164.792)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C49 (at 0 -1.43 164.792) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 164.792) (layer F.Fab))
    (fp_text user %R (at 0 0 164.792) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 164.792) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 164.792) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 164.216476 76.452027 157.124)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C48 (at 0 -1.43 157.124) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 157.124) (layer F.Fab))
    (fp_text user %R (at 0 0 157.124) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 157.124) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 157.124) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 172.57656 79.996498 149.456)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C47 (at 0 -1.43 149.456) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 149.456) (layer F.Fab))
    (fp_text user %R (at 0 0 149.456) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 149.456) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 149.456) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 179.466587 85.581755 141.788)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C46 (at 0 -1.43 141.788) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 141.788) (layer F.Fab))
    (fp_text user %R (at 0 0 141.788) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 141.788) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 141.788) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 184.856596 92.761665 134.12)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C45 (at 0 -1.43 134.12) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 134.12) (layer F.Fab))
    (fp_text user %R (at 0 0 134.12) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 134.12) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 134.12) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 188.65153 101.178076 126.452)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C44 (at 0 -1.43 126.452) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 126.452) (layer F.Fab))
    (fp_text user %R (at 0 0 126.452) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 126.452) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 126.452) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 190.752725 110.502426 118.784)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C43 (at 0 -1.43 118.784) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 118.784) (layer F.Fab))
    (fp_text user %R (at 0 0 118.784) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 118.784) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 118.784) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 191.081761 120.415893 111.116)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C42 (at 0 -1.43 111.116) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 111.116) (layer F.Fab))
    (fp_text user %R (at 0 0 111.116) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 111.116) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 111.116) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 189.591713 130.603294 103.448)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C41 (at 0 -1.43 103.448) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 103.448) (layer F.Fab))
    (fp_text user %R (at 0 0 103.448) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 103.448) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 103.448) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 186.272954 140.752921 95.78)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C40 (at 0 -1.43 95.78) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 95.78) (layer F.Fab))
    (fp_text user %R (at 0 0 95.78) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 95.78) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 95.78) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 181.156047 150.559244 88.112)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C39 (at 0 -1.43 88.112) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 88.112) (layer F.Fab))
    (fp_text user %R (at 0 0 88.112) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 88.112) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 88.112) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 174.312736 159.727103 80.444)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C38 (at 0 -1.43 80.444) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 80.444) (layer F.Fab))
    (fp_text user %R (at 0 0 80.444) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 80.444) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 80.444) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 194.574269 139.493326 280.508)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C37 (at 0 -1.43 280.508) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 280.508) (layer F.Fab))
    (fp_text user %R (at 0 0 280.508) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 280.508) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 280.508) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 197.711705 128.641401 288.176)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C36 (at 0 -1.43 288.176) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 288.176) (layer F.Fab))
    (fp_text user %R (at 0 0 288.176) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 288.176) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 288.176) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 199.013183 117.803721 295.844)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C35 (at 0 -1.43 295.844) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 295.844) (layer F.Fab))
    (fp_text user %R (at 0 0 295.844) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 295.844) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 295.844) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 198.513481 107.283152 303.512)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C34 (at 0 -1.43 303.512) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 303.512) (layer F.Fab))
    (fp_text user %R (at 0 0 303.512) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 303.512) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 303.512) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 196.2891 97.378747 311.18)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C33 (at 0 -1.43 311.18) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 311.18) (layer F.Fab))
    (fp_text user %R (at 0 0 311.18) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 311.18) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 311.18) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 192.455592 88.382666 318.848)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C32 (at 0 -1.43 318.848) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 318.848) (layer F.Fab))
    (fp_text user %R (at 0 0 318.848) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 318.848) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 318.848) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 187.163359 80.579544 326.516)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C31 (at 0 -1.43 326.516) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 326.516) (layer F.Fab))
    (fp_text user %R (at 0 0 326.516) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 326.516) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 326.516) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 180.591106 74.250517 334.184)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C30 (at 0 -1.43 334.184) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 334.184) (layer F.Fab))
    (fp_text user %R (at 0 0 334.184) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 334.184) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 334.184) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 172.9347 69.687079 341.852)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C29 (at 0 -1.43 341.852) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 341.852) (layer F.Fab))
    (fp_text user %R (at 0 0 341.852) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 341.852) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 341.852) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 164.384167 67.229309 349.52)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C28 (at 0 -1.43 349.52) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 349.52) (layer F.Fab))
    (fp_text user %R (at 0 0 349.52) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 349.52) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 349.52) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 155.059563 67.381125 357.188)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C27 (at 0 -1.43 357.188) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 357.188) (layer F.Fab))
    (fp_text user %R (at 0 0 357.188) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 357.188) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 357.188) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 144.720207 71.301208 4.856)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C26 (at 0 -1.43 4.856) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 4.856) (layer F.Fab))
    (fp_text user %R (at 0 0 4.856) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 4.856) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 4.856) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 135.122112 72.278497 204.92)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C25 (at 0 -1.43 204.92) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 204.92) (layer F.Fab))
    (fp_text user %R (at 0 0 204.92) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 204.92) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 204.92) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 143.947119 63.004655 197.252)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C24 (at 0 -1.43 197.252) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 197.252) (layer F.Fab))
    (fp_text user %R (at 0 0 197.252) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 197.252) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 197.252) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 152.751612 58.851214 189.584)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at 0 -1.43 189.584) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 189.584) (layer F.Fab))
    (fp_text user %R (at 0 0 189.584) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 189.584) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 189.584) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 161.663656 57.7134 181.916)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at 0 -1.43 181.916) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 181.916) (layer F.Fab))
    (fp_text user %R (at 0 0 181.916) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 181.916) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 181.916) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 170.447212 58.9873 174.248)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at 0 -1.43 174.248) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 174.248) (layer F.Fab))
    (fp_text user %R (at 0 0 174.248) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 174.248) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 174.248) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 178.822384 62.360726 166.58)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at 0 -1.43 166.58) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 166.58) (layer F.Fab))
    (fp_text user %R (at 0 0 166.58) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 166.58) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 166.58) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 186.51108 67.60212 158.912)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at 0 -1.43 158.912) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 158.912) (layer F.Fab))
    (fp_text user %R (at 0 0 158.912) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 158.912) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 158.912) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 193.251353 74.496526 151.244)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at 0 -1.43 151.244) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 151.244) (layer F.Fab))
    (fp_text user %R (at 0 0 151.244) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 151.244) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 151.244) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 198.805019 82.821819 143.576)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at 0 -1.43 143.576) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 143.576) (layer F.Fab))
    (fp_text user %R (at 0 0 143.576) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 143.576) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 143.576) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 202.963168 92.339817 135.908)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 0 -1.43 135.908) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 135.908) (layer F.Fab))
    (fp_text user %R (at 0 0 135.908) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 135.908) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 135.908) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 205.550661 102.79406 128.24)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at 0 -1.43 128.24) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 128.24) (layer F.Fab))
    (fp_text user %R (at 0 0 128.24) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 128.24) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 128.24) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 206.429873 113.911086 120.572)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 0 -1.43 120.572) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 120.572) (layer F.Fab))
    (fp_text user %R (at 0 0 120.572) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 120.572) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 120.572) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 211.831481 97.199599 312.968)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 0 -1.43 312.968) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 312.968) (layer F.Fab))
    (fp_text user %R (at 0 0 312.968) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 312.968) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 312.968) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 208.695403 86.25358 320.636)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 0 -1.43 320.636) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 320.636) (layer F.Fab))
    (fp_text user %R (at 0 0 320.636) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 320.636) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 320.636) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 204.008125 76.295002 328.304)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0 -1.43 328.304) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 328.304) (layer F.Fab))
    (fp_text user %R (at 0 0 328.304) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 328.304) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 328.304) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 197.96074 67.560495 335.972)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0 -1.43 335.972) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 335.972) (layer F.Fab))
    (fp_text user %R (at 0 0 335.972) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 335.972) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 335.972) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 190.777573 60.260572 343.64)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0 -1.43 343.64) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 343.64) (layer F.Fab))
    (fp_text user %R (at 0 0 343.64) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 343.64) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 343.64) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 182.712278 54.578094 351.308)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0 -1.43 351.308) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 351.308) (layer F.Fab))
    (fp_text user %R (at 0 0 351.308) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 351.308) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 351.308) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 174.043939 50.66928 358.976)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0 -1.43 358.976) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 358.976) (layer F.Fab))
    (fp_text user %R (at 0 0 358.976) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 358.976) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 358.976) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 165.073699 48.669172 6.644)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0 -1.43 6.644) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 6.644) (layer F.Fab))
    (fp_text user %R (at 0 0 6.644) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 6.644) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 6.644) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 156.122798 48.705956 14.312)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0 -1.43 14.312) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 14.312) (layer F.Fab))
    (fp_text user %R (at 0 0 14.312) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 14.312) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 14.312) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 147.533866 50.936424 21.98)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 -1.43 21.98) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 21.98) (layer F.Fab))
    (fp_text user %R (at 0 0 21.98) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 21.98) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 21.98) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 139.679768 55.645146 29.648)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 -1.43 29.648) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 29.648) (layer F.Fab))
    (fp_text user %R (at 0 0 29.648) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 29.648) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 29.648) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 132.991905 63.623643 37.316)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 -1.43 37.316) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 37.316) (layer F.Fab))
    (fp_text user %R (at 0 0 37.316) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 37.316) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 37.316) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 127.967342 80.303623 44.984)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.43 44.984) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.43 44.984) (layer F.Fab))
    (fp_text user %R (at 0 0 44.984) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 44.984) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.775 0 44.984) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 46 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 0 2.33 180) (layer B.SilkS) hide)
    (fp_text value Conn_01x03_Female (at 0 -7.41 180) (layer B.Fab))
    (fp_text user %R (at 0 -2.54 -270) (layer B.Fab))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /DIN))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 214 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 0 2.33 180) (layer B.SilkS) hide)
    (fp_text value Conn_01x03_Female (at 0 -7.41 180) (layer B.Fab))
    (fp_text user %R (at 0 -2.54 -270) (layer B.Fab))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 259 /DOUT))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 206.402122 72.31623 153.032)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D256 (at 0 -3.5 153.032) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 153.032) (layer F.Fab))
    (fp_text user %R (at 0 0 153.032) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 153.032) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 153.032) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 153.032) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 259 /DOUT))
    (pad 4 smd rect (at 2.45 -1.6 153.032) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 258 /LEDS/L256))
    (pad 3 smd rect (at 2.45 1.6 153.032) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 200.158302 63.489387 160.7)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D255 (at 0 -3.5 160.7) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 160.7) (layer F.Fab))
    (fp_text user %R (at 0 0 160.7) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 160.7) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 160.7) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 160.7) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 258 /LEDS/L256))
    (pad 4 smd rect (at 2.45 -1.6 160.7) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 257 "Net-(D254-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 160.7) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 192.838433 56.068728 168.368)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D254 (at 0 -3.5 168.368) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 168.368) (layer F.Fab))
    (fp_text user %R (at 0 0 168.368) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 168.368) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 168.368) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 168.368) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 257 "Net-(D254-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 168.368) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 256 "Net-(D253-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 168.368) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 184.695904 50.208569 176.036)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D253 (at 0 -3.5 176.036) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 176.036) (layer F.Fab))
    (fp_text user %R (at 0 0 176.036) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 176.036) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 176.036) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 176.036) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 256 "Net-(D253-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 176.036) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 255 "Net-(D252-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 176.036) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 176.006277 46.029301 183.704)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D252 (at 0 -3.5 183.704) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 183.704) (layer F.Fab))
    (fp_text user %R (at 0 0 183.704) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 183.704) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 183.704) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 183.704) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 255 "Net-(D252-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 183.704) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 254 "Net-(D251-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 183.704) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 167.063469 43.6179 191.372)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D251 (at 0 -3.5 191.372) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 191.372) (layer F.Fab))
    (fp_text user %R (at 0 0 191.372) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 191.372) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 191.372) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 191.372) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 254 "Net-(D251-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 191.372) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 253 "Net-(D250-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 191.372) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 158.177013 43.031331 199.04)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D250 (at 0 -3.5 199.04) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 199.04) (layer F.Fab))
    (fp_text user %R (at 0 0 199.04) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 199.04) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 199.04) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 199.04) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 253 "Net-(D250-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 199.04) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 252 "Net-(D249-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 199.04) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 149.67176 44.305123 206.708)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D249 (at 0 -3.5 206.708) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 206.708) (layer F.Fab))
    (fp_text user %R (at 0 0 206.708) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 206.708) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 206.708) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 206.708) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 252 "Net-(D249-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 206.708) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 251 "Net-(D248-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 206.708) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 141.892992 47.472871 214.376)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D248 (at 0 -3.5 214.376) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 214.376) (layer F.Fab))
    (fp_text user %R (at 0 0 214.376) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 214.376) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 214.376) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 214.376) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 251 "Net-(D248-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 214.376) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 250 "Net-(D247-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 214.376) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 135.22496 52.614177 222.044)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D247 (at 0 -3.5 222.044) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 222.044) (layer F.Fab))
    (fp_text user %R (at 0 0 222.044) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 222.044) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 222.044) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 222.044) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 250 "Net-(D247-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 222.044) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 249 "Net-(D246-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 222.044) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 130.150795 60.000379 229.712)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D246 (at 0 -3.5 229.712) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 229.712) (layer F.Fab))
    (fp_text user %R (at 0 0 229.712) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 229.712) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 229.712) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 229.712) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 249 "Net-(D246-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 229.712) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 248 "Net-(D245-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 229.712) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 127.512588 70.795502 237.38)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D245 (at 0 -3.5 237.38) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 237.38) (layer F.Fab))
    (fp_text user %R (at 0 0 237.38) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 237.38) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 237.38) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 237.38) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 248 "Net-(D245-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 237.38) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 247 "Net-(D244-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 237.38) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 123.903112 78.259986 77.444)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D244 (at 0 -3.5 77.444) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 77.444) (layer F.Fab))
    (fp_text user %R (at 0 0 77.444) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 77.444) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 77.444) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 77.444) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 247 "Net-(D244-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 77.444) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 246 "Net-(D243-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 77.444) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 121.048266 65.102883 69.776)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D243 (at 0 -3.5 69.776) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 69.776) (layer F.Fab))
    (fp_text user %R (at 0 0 69.776) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 69.776) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 69.776) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 69.776) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 246 "Net-(D243-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 69.776) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 245 "Net-(D242-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 69.776) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 122.658573 55.778612 62.108)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D242 (at 0 -3.5 62.108) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 62.108) (layer F.Fab))
    (fp_text user %R (at 0 0 62.108) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 62.108) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 62.108) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 62.108) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 245 "Net-(D242-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 62.108) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 244 "Net-(D241-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 62.108) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 126.761495 48.292542 54.44)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D241 (at 0 -3.5 54.44) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 54.44) (layer F.Fab))
    (fp_text user %R (at 0 0 54.44) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 54.44) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 54.44) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 54.44) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 244 "Net-(D241-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 54.44) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 243 /LEDS/L241))
    (pad 3 smd rect (at 2.45 1.6 54.44) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 132.685788 42.378718 46.772)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D240 (at 0 -3.5 46.772) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 46.772) (layer F.Fab))
    (fp_text user %R (at 0 0 46.772) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 46.772) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 46.772) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 46.772) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 243 /LEDS/L241))
    (pad 4 smd rect (at 2.45 -1.6 46.772) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 242 "Net-(D239-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 46.772) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 140.002362 38.038931 39.104)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D239 (at 0 -3.5 39.104) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 39.104) (layer F.Fab))
    (fp_text user %R (at 0 0 39.104) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 39.104) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 39.104) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 39.104) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 242 "Net-(D239-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 39.104) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 241 "Net-(D238-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 39.104) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 148.357749 35.337463 31.436)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D238 (at 0 -3.5 31.436) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 31.436) (layer F.Fab))
    (fp_text user %R (at 0 0 31.436) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 31.436) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 31.436) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 31.436) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 241 "Net-(D238-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 31.436) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 240 "Net-(D237-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 31.436) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 157.425807 34.341892 23.768)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D237 (at 0 -3.5 23.768) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 23.768) (layer F.Fab))
    (fp_text user %R (at 0 0 23.768) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 23.768) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 23.768) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 23.768) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 240 "Net-(D237-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 23.768) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 239 "Net-(D236-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 23.768) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 166.891371 35.099848 16.1)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D236 (at 0 -3.5 16.1) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 16.1) (layer F.Fab))
    (fp_text user %R (at 0 0 16.1) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 16.1) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 16.1) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 16.1) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 239 "Net-(D236-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 16.1) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 238 "Net-(D235-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 16.1) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 176.445592 37.628186 8.432)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D235 (at 0 -3.5 8.432) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 8.432) (layer F.Fab))
    (fp_text user %R (at 0 0 8.432) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 8.432) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 8.432) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 8.432) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 238 "Net-(D235-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 8.432) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 237 "Net-(D234-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 8.432) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 185.786395 41.90761 0.764)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D234 (at 0 -3.5 0.764) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 0.764) (layer F.Fab))
    (fp_text user %R (at 0 0 0.764) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 0.764) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 0.764) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 0.764) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 237 "Net-(D234-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 0.764) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 236 "Net-(D233-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 0.764) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 194.621415 47.880258 353.096)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D233 (at 0 -3.5 353.096) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 353.096) (layer F.Fab))
    (fp_text user %R (at 0 0 353.096) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 353.096) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 353.096) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 353.096) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 236 "Net-(D233-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 353.096) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 235 "Net-(D232-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 353.096) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 185.530343 33.507692 185.492)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D232 (at 0 -3.5 185.492) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 185.492) (layer F.Fab))
    (fp_text user %R (at 0 0 185.492) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 185.492) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 185.492) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 185.492) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 235 "Net-(D232-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 185.492) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 234 "Net-(D231-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 185.492) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 175.465591 29.313264 193.16)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D231 (at 0 -3.5 193.16) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 193.16) (layer F.Fab))
    (fp_text user %R (at 0 0 193.16) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 193.16) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 193.16) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 193.16) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 234 "Net-(D231-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 193.16) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 233 "Net-(D230-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 193.16) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 165.233686 26.884334 200.828)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D230 (at 0 -3.5 200.828) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 200.828) (layer F.Fab))
    (fp_text user %R (at 0 0 200.828) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 200.828) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 200.828) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 200.828) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 233 "Net-(D230-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 200.828) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 232 "Net-(D229-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 200.828) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 155.130511 26.21554 208.496)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D229 (at 0 -3.5 208.496) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 208.496) (layer F.Fab))
    (fp_text user %R (at 0 0 208.496) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 208.496) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 208.496) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 208.496) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 232 "Net-(D229-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 208.496) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 231 "Net-(D228-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 208.496) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 145.452081 27.260594 216.164)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D228 (at 0 -3.5 216.164) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 216.164) (layer F.Fab))
    (fp_text user %R (at 0 0 216.164) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 216.164) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 216.164) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 216.164) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 231 "Net-(D228-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 216.164) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 230 "Net-(D227-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 216.164) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 136.49126 29.934507 223.832)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D227 (at 0 -3.5 223.832) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 223.832) (layer F.Fab))
    (fp_text user %R (at 0 0 223.832) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 223.832) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 223.832) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 223.832) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 230 "Net-(D227-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 223.832) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 229 "Net-(D226-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 223.832) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 128.536665 34.117457 231.5)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D226 (at 0 -3.5 231.5) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 231.5) (layer F.Fab))
    (fp_text user %R (at 0 0 231.5) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 231.5) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 231.5) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 231.5) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 229 "Net-(D226-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 231.5) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 228 /LEDS/L226))
    (pad 3 smd rect (at 2.45 1.6 231.5) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 121.875741 39.661184 239.168)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D225 (at 0 -3.5 239.168) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 239.168) (layer F.Fab))
    (fp_text user %R (at 0 0 239.168) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 239.168) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 239.168) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 239.168) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 228 /LEDS/L226))
    (pad 4 smd rect (at 2.45 -1.6 239.168) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 227 "Net-(D224-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 239.168) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 116.806578 46.400303 246.836)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D224 (at 0 -3.5 246.836) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 246.836) (layer F.Fab))
    (fp_text user %R (at 0 0 246.836) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 246.836) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 246.836) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 246.836) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 227 "Net-(D224-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 246.836) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 226 "Net-(D223-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 246.836) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 113.67101 54.175929 254.504)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D223 (at 0 -3.5 254.504) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 254.504) (layer F.Fab))
    (fp_text user %R (at 0 0 254.504) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 254.504) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 254.504) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 254.504) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 226 "Net-(D223-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 254.504) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 225 "Net-(D222-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 254.504) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 112.952877 62.900267 262.172)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D222 (at 0 -3.5 262.172) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 262.172) (layer F.Fab))
    (fp_text user %R (at 0 0 262.172) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 262.172) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 262.172) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 262.172) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 225 "Net-(D222-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 262.172) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(D221-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 262.172) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 115.674723 72.830655 269.84)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D221 (at 0 -3.5 269.84) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 269.84) (layer F.Fab))
    (fp_text user %R (at 0 0 269.84) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 269.84) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 269.84) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 269.84) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(D221-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 269.84) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 223 "Net-(D220-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 269.84) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 115.014532 81.314626 109.904)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D220 (at 0 -3.5 109.904) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 109.904) (layer F.Fab))
    (fp_text user %R (at 0 0 109.904) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 109.904) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 109.904) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 109.904) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 223 "Net-(D220-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 109.904) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(D219-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 109.904) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 107.293469 72.409849 102.236)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D219 (at 0 -3.5 102.236) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 102.236) (layer F.Fab))
    (fp_text user %R (at 0 0 102.236) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 102.236) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 102.236) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 102.236) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(D219-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 102.236) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 221 "Net-(D218-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 102.236) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 104.215865 63.824088 94.568)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D218 (at 0 -3.5 94.568) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 94.568) (layer F.Fab))
    (fp_text user %R (at 0 0 94.568) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 94.568) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 94.568) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 94.568) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 221 "Net-(D218-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 94.568) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 220 "Net-(D217-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 94.568) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 104.001042 55.372639 86.9)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D217 (at 0 -3.5 86.9) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 86.9) (layer F.Fab))
    (fp_text user %R (at 0 0 86.9) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 86.9) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 86.9) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 86.9) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 220 "Net-(D217-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 86.9) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 219 "Net-(D216-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 86.9) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 106.075976 47.249082 79.232)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D216 (at 0 -3.5 79.232) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 79.232) (layer F.Fab))
    (fp_text user %R (at 0 0 79.232) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 79.232) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 79.232) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 79.232) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 219 "Net-(D216-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 79.232) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 218 "Net-(D215-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 79.232) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 110.12222 39.702149 71.564)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D215 (at 0 -3.5 71.564) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 71.564) (layer F.Fab))
    (fp_text user %R (at 0 0 71.564) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 71.564) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 71.564) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 71.564) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 218 "Net-(D215-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 71.564) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 217 "Net-(D214-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 71.564) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 115.893778 32.982332 63.896)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D214 (at 0 -3.5 63.896) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 63.896) (layer F.Fab))
    (fp_text user %R (at 0 0 63.896) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 63.896) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 63.896) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 63.896) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 217 "Net-(D214-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 63.896) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 216 "Net-(D213-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 63.896) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 123.16027 27.324502 56.228)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D213 (at 0 -3.5 56.228) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 56.228) (layer F.Fab))
    (fp_text user %R (at 0 0 56.228) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 56.228) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 56.228) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 56.228) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 216 "Net-(D213-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 56.228) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 215 "Net-(D212-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 56.228) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 131.685778 22.939146 48.56)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D212 (at 0 -3.5 48.56) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 48.56) (layer F.Fab))
    (fp_text user %R (at 0 0 48.56) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 48.56) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 48.56) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 48.56) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 215 "Net-(D212-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 48.56) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 214 "Net-(D211-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 48.56) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 141.221161 20.006533 40.892)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D211 (at 0 -3.5 40.892) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 40.892) (layer F.Fab))
    (fp_text user %R (at 0 0 40.892) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 40.892) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 40.892) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 40.892) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 214 "Net-(D211-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 40.892) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 213 /LEDS/L211))
    (pad 3 smd rect (at 2.45 1.6 40.892) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 151.502508 18.672291 33.224)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D210 (at 0 -3.5 33.224) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 33.224) (layer F.Fab))
    (fp_text user %R (at 0 0 33.224) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 33.224) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 33.224) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 33.224) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 213 /LEDS/L211))
    (pad 4 smd rect (at 2.45 -1.6 33.224) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 212 "Net-(D209-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 33.224) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 162.252803 19.043981 25.556)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D209 (at 0 -3.5 25.556) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 25.556) (layer F.Fab))
    (fp_text user %R (at 0 0 25.556) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 25.556) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 25.556) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 25.556) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 212 "Net-(D209-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 25.556) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(D208-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 25.556) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 146.698485 11.762154 217.952)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D208 (at 0 -3.5 217.952) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 217.952) (layer F.Fab))
    (fp_text user %R (at 0 0 217.952) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 217.952) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 217.952) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 217.952) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(D208-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 217.952) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(D207-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 217.952) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 135.853725 13.575306 225.62)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D207 (at 0 -3.5 225.62) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 225.62) (layer F.Fab))
    (fp_text user %R (at 0 0 225.62) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 225.62) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 225.62) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 225.62) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(D207-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 225.62) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(D206-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 225.62) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 125.804849 16.976712 233.288)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D206 (at 0 -3.5 233.288) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 233.288) (layer F.Fab))
    (fp_text user %R (at 0 0 233.288) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 233.288) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 233.288) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 233.288) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(D206-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 233.288) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(D205-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 233.288) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 116.798351 21.803839 240.956)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D205 (at 0 -3.5 240.956) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 240.956) (layer F.Fab))
    (fp_text user %R (at 0 0 240.956) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 240.956) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 240.956) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 240.956) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(D205-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 240.956) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 207 "Net-(D204-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 240.956) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 109.058409 27.859436 248.624)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D204 (at 0 -3.5 248.624) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 248.624) (layer F.Fab))
    (fp_text user %R (at 0 0 248.624) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 248.624) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 248.624) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 248.624) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 207 "Net-(D204-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 248.624) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 206 "Net-(D203-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 248.624) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 102.784942 34.915152 256.292)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D203 (at 0 -3.5 256.292) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 256.292) (layer F.Fab))
    (fp_text user %R (at 0 0 256.292) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 256.292) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 256.292) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 256.292) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 206 "Net-(D203-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 256.292) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 205 "Net-(D202-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 256.292) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 98.154103 42.715343 263.96)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D202 (at 0 -3.5 263.96) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 263.96) (layer F.Fab))
    (fp_text user %R (at 0 0 263.96) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 263.96) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 263.96) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 263.96) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 205 "Net-(D202-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 263.96) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 204 "Net-(D201-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 263.96) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 95.322962 50.980736 271.628)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D201 (at 0 -3.5 271.628) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 271.628) (layer F.Fab))
    (fp_text user %R (at 0 0 271.628) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 271.628) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 271.628) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 271.628) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 204 "Net-(D201-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 271.628) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 203 "Net-(D200-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 271.628) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 94.442484 59.411392 279.296)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D200 (at 0 -3.5 279.296) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 279.296) (layer F.Fab))
    (fp_text user %R (at 0 0 279.296) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 279.296) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 279.296) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 279.296) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 203 "Net-(D200-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 279.296) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 202 "Net-(D199-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 279.296) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 95.68994 67.688125 286.964)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D199 (at 0 -3.5 286.964) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 286.964) (layer F.Fab))
    (fp_text user %R (at 0 0 286.964) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 286.964) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 286.964) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 286.964) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 202 "Net-(D199-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 286.964) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 201 "Net-(D198-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 286.964) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 99.358291 75.471214 294.632)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D198 (at 0 -3.5 294.632) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 294.632) (layer F.Fab))
    (fp_text user %R (at 0 0 294.632) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 294.632) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 294.632) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 294.632) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 201 "Net-(D198-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 294.632) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(D197-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 294.632) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 106.183463 82.399174 302.3)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D197 (at 0 -3.5 302.3) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 302.3) (layer F.Fab))
    (fp_text user %R (at 0 0 302.3) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 302.3) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 302.3) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 302.3) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(D197-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 302.3) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 199 "Net-(D196-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 302.3) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 120.152894 88.258019 309.968)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D196 (at 0 -3.5 309.968) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 309.968) (layer F.Fab))
    (fp_text user %R (at 0 0 309.968) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 309.968) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 309.968) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 309.968) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 199 "Net-(D196-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 309.968) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 198 /LEDS/L196))
    (pad 3 smd rect (at 2.45 1.6 309.968) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 109.402017 90.850346 142.364)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D195 (at 0 -3.5 142.364) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 142.364) (layer F.Fab))
    (fp_text user %R (at 0 0 142.364) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 142.364) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 142.364) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 142.364) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 198 /LEDS/L196))
    (pad 4 smd rect (at 2.45 -1.6 142.364) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(D194-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 142.364) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 99.309903 87.150805 134.696)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D194 (at 0 -3.5 134.696) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 134.696) (layer F.Fab))
    (fp_text user %R (at 0 0 134.696) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 134.696) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 134.696) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 134.696) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(D194-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 134.696) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(D193-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 134.696) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 92.574391 81.37888 127.028)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D193 (at 0 -3.5 127.028) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 127.028) (layer F.Fab))
    (fp_text user %R (at 0 0 127.028) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 127.028) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 127.028) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 127.028) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(D193-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 127.028) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(D192-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 127.028) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 88.149141 74.235942 119.36)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D192 (at 0 -3.5 119.36) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 119.36) (layer F.Fab))
    (fp_text user %R (at 0 0 119.36) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 119.36) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 119.36) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 119.36) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(D192-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 119.36) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(D191-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 119.36) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 85.759888 66.171186 111.692)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D191 (at 0 -3.5 111.692) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 111.692) (layer F.Fab))
    (fp_text user %R (at 0 0 111.692) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 111.692) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 111.692) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 111.692) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(D191-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 111.692) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(D190-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 111.692) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 85.306983 57.557217 104.024)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D190 (at 0 -3.5 104.024) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 104.024) (layer F.Fab))
    (fp_text user %R (at 0 0 104.024) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 104.024) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 104.024) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 104.024) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(D190-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 104.024) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 192 "Net-(D189-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 104.024) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 86.732498 48.73351 96.356)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D189 (at 0 -3.5 96.356) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 96.356) (layer F.Fab))
    (fp_text user %R (at 0 0 96.356) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 96.356) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 96.356) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 96.356) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 192 "Net-(D189-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 96.356) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(D188-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 96.356) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 89.975403 40.019688 88.688)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D188 (at 0 -3.5 88.688) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 88.688) (layer F.Fab))
    (fp_text user %R (at 0 0 88.688) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 88.688) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 88.688) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 88.688) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(D188-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 88.688) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(D187-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 88.688) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 94.953278 31.718552 81.02)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D187 (at 0 -3.5 81.02) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 81.02) (layer F.Fab))
    (fp_text user %R (at 0 0 81.02) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 81.02) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 81.02) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 81.02) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(D187-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 81.02) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(D186-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 81.02) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 101.554463 24.114862 73.352)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D186 (at 0 -3.5 73.352) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 73.352) (layer F.Fab))
    (fp_text user %R (at 0 0 73.352) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 73.352) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 73.352) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 73.352) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(D186-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 73.352) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 188 "Net-(D185-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 73.352) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 109.635219 17.472242 65.684)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D185 (at 0 -3.5 65.684) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 65.684) (layer F.Fab))
    (fp_text user %R (at 0 0 65.684) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 65.684) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 65.684) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 65.684) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 188 "Net-(D185-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 65.684) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(D184-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 65.684) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 93.539431 21.658016 258.08)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D183 (at 0 -3.5 258.08) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 258.08) (layer F.Fab))
    (fp_text user %R (at 0 0 258.08) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 258.08) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 258.08) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 258.08) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(D183-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 258.08) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 185 "Net-(D182-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 258.08) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 86.771569 29.947501 265.748)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D182 (at 0 -3.5 265.748) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 265.748) (layer F.Fab))
    (fp_text user %R (at 0 0 265.748) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 265.748) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 265.748) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 265.748) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 185 "Net-(D182-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 265.748) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 184 "Net-(D181-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 265.748) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 81.644836 38.894443 273.416)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D181 (at 0 -3.5 273.416) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 273.416) (layer F.Fab))
    (fp_text user %R (at 0 0 273.416) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 273.416) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 273.416) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 273.416) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 184 "Net-(D181-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 273.416) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 183 /LEDS/L181))
    (pad 3 smd rect (at 2.45 1.6 273.416) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 78.242409 48.21302 281.084)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D180 (at 0 -3.5 281.084) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 281.084) (layer F.Fab))
    (fp_text user %R (at 0 0 281.084) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 281.084) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 281.084) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 281.084) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 183 /LEDS/L181))
    (pad 4 smd rect (at 2.45 -1.6 281.084) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(D179-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 281.084) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 76.60964 57.604485 288.752)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D179 (at 0 -3.5 288.752) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 288.752) (layer F.Fab))
    (fp_text user %R (at 0 0 288.752) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 288.752) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 288.752) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 288.752) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(D179-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 288.752) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(D178-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 288.752) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 76.756021 66.760408 296.42)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D178 (at 0 -3.5 296.42) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 296.42) (layer F.Fab))
    (fp_text user %R (at 0 0 296.42) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 296.42) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 296.42) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 296.42) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(D178-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 296.42) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 180 "Net-(D177-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 296.42) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 78.660129 75.363828 304.088)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D177 (at 0 -3.5 304.088) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 304.088) (layer F.Fab))
    (fp_text user %R (at 0 0 304.088) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 304.088) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 304.088) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 304.088) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 180 "Net-(D177-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 304.088) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(D176-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 304.088) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 82.280014 83.086034 311.756)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D176 (at 0 -3.5 311.756) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 311.756) (layer F.Fab))
    (fp_text user %R (at 0 0 311.756) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 311.756) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 311.756) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 311.756) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(D176-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 311.756) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(D175-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 311.756) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 87.575738 89.573491 319.424)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D175 (at 0 -3.5 319.424) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 319.424) (layer F.Fab))
    (fp_text user %R (at 0 0 319.424) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 319.424) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 319.424) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 319.424) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(D175-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 319.424) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(D174-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 319.424) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 94.566047 94.408508 327.092)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D174 (at 0 -3.5 327.092) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 327.092) (layer F.Fab))
    (fp_text user %R (at 0 0 327.092) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 327.092) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 327.092) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 327.092) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(D174-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 327.092) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 176 "Net-(D173-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 327.092) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 103.517574 96.977183 334.76)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D173 (at 0 -3.5 334.76) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 334.76) (layer F.Fab))
    (fp_text user %R (at 0 0 334.76) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 334.76) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 334.76) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 334.76) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 176 "Net-(D173-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 334.76) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(D172-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 334.76) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 116.134605 95.722832 342.428)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D172 (at 0 -3.5 342.428) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 342.428) (layer F.Fab))
    (fp_text user %R (at 0 0 342.428) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 342.428) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 342.428) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 342.428) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(D172-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 342.428) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 174 "Net-(D171-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 342.428) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 110.747953 103.392485 174.824)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D171 (at 0 -3.5 174.824) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 174.824) (layer F.Fab))
    (fp_text user %R (at 0 0 174.824) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 174.824) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 174.824) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 174.824) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 174 "Net-(D171-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 174.824) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 173 "Net-(D170-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 174.824) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 100.827034 104.964558 167.156)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D170 (at 0 -3.5 167.156) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 167.156) (layer F.Fab))
    (fp_text user %R (at 0 0 167.156) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 167.156) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 167.156) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 167.156) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 173 "Net-(D170-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 167.156) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 172 "Net-(D169-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 167.156) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 92.291545 103.344377 159.488)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D169 (at 0 -3.5 159.488) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 159.488) (layer F.Fab))
    (fp_text user %R (at 0 0 159.488) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 159.488) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 159.488) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 159.488) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 172 "Net-(D169-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 159.488) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 171 "Net-(D168-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 159.488) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 84.879737 99.442552 151.82)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D168 (at 0 -3.5 151.82) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 151.82) (layer F.Fab))
    (fp_text user %R (at 0 0 151.82) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 151.82) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 151.82) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 151.82) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 171 "Net-(D168-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 151.82) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 170 "Net-(D167-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 151.82) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 78.656955 93.727155 144.152)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D167 (at 0 -3.5 144.152) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 144.152) (layer F.Fab))
    (fp_text user %R (at 0 0 144.152) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 144.152) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 144.152) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 144.152) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 170 "Net-(D167-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 144.152) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 169 "Net-(D166-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 144.152) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 73.758924 86.544384 136.484)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D166 (at 0 -3.5 136.484) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 136.484) (layer F.Fab))
    (fp_text user %R (at 0 0 136.484) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 136.484) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 136.484) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 136.484) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 169 "Net-(D166-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 136.484) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 168 /LEDS/L166))
    (pad 3 smd rect (at 2.45 1.6 136.484) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 70.327531 78.201849 128.816)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D165 (at 0 -3.5 128.816) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 128.816) (layer F.Fab))
    (fp_text user %R (at 0 0 128.816) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 128.816) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 128.816) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 128.816) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 168 /LEDS/L166))
    (pad 4 smd rect (at 2.45 -1.6 128.816) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(D164-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 128.816) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 68.486835 68.996894 121.148)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D164 (at 0 -3.5 121.148) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 121.148) (layer F.Fab))
    (fp_text user %R (at 0 0 121.148) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 121.148) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 121.148) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 121.148) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(D164-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 121.148) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 166 "Net-(D163-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 121.148) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 68.331644 59.22641 113.48)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D163 (at 0 -3.5 113.48) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 113.48) (layer F.Fab))
    (fp_text user %R (at 0 0 113.48) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 113.48) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 113.48) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 113.48) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 166 "Net-(D163-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 113.48) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(D162-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 113.48) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 69.921255 49.188919 105.812)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D162 (at 0 -3.5 105.812) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 105.812) (layer F.Fab))
    (fp_text user %R (at 0 0 105.812) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 105.812) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 105.812) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 105.812) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(D162-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 105.812) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(D161-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 105.812) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 73.275881 39.182934 98.144)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D161 (at 0 -3.5 98.144) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 98.144) (layer F.Fab))
    (fp_text user %R (at 0 0 98.144) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 98.144) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 98.144) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 98.144) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(D161-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 98.144) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(D160-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 98.144) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 78.374819 29.503384 90.476)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D160 (at 0 -3.5 90.476) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 90.476) (layer F.Fab))
    (fp_text user %R (at 0 0 90.476) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 90.476) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 90.476) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 90.476) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(D160-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 90.476) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(D159-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 90.476) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 61.857005 51.509325 290.54)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D159 (at 0 -3.5 290.54) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 290.54) (layer F.Fab))
    (fp_text user %R (at 0 0 290.54) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 290.54) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 290.54) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 290.54) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(D159-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 290.54) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(D158-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 290.54) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 60.514604 62.219078 298.208)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D158 (at 0 -3.5 298.208) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 298.208) (layer F.Fab))
    (fp_text user %R (at 0 0 298.208) (layer F.Fab))
    (pad 1 smd rect (at -2.45 -1.6 298.208) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 298.208) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(D158-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 298.208) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(D157-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 298.208) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 60.91453 72.616162 305.876)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D157 (at 0 -3.5 305.876) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 305.876) (layer F.Fab))
    (fp_text user %R (at 0 0 305.876) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 305.876) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 305.876) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 305.876) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(D157-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 305.876) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(D156-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 305.876) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 62.97407 82.415496 313.544)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D156 (at 0 -3.5 313.544) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 313.544) (layer F.Fab))
    (fp_text user %R (at 0 0 313.544) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 313.544) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 313.544) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 313.544) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(D156-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 313.544) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(D155-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 313.544) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 66.571307 91.341932 321.212)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D155 (at 0 -3.5 321.212) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 321.212) (layer F.Fab))
    (fp_text user %R (at 0 0 321.212) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 321.212) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 321.212) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 321.212) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(D155-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 321.212) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(D154-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 321.212) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 71.548315 99.132386 328.88)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D154 (at 0 -3.5 328.88) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 328.88) (layer F.Fab))
    (fp_text user %R (at 0 0 328.88) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 328.88) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 328.88) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 328.88) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(D154-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 328.88) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(D153-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 328.88) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 77.715554 105.535015 336.548)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D153 (at 0 -3.5 336.548) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 336.548) (layer F.Fab))
    (fp_text user %R (at 0 0 336.548) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 336.548) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 336.548) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 336.548) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(D153-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 336.548) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(D152-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 336.548) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 84.858026 110.302761 344.216)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D152 (at 0 -3.5 344.216) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 344.216) (layer F.Fab))
    (fp_text user %R (at 0 0 344.216) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 344.216) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 344.216) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 344.216) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(D152-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 344.216) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(D151-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 344.216) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 92.745046 113.174735 351.884)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D151 (at 0 -3.5 351.884) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 351.884) (layer F.Fab))
    (fp_text user %R (at 0 0 351.884) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 351.884) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 351.884) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 351.884) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(D151-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 351.884) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 153 /LEDS/L151))
    (pad 3 smd rect (at 2.45 1.6 351.884) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 101.150064 113.82606 359.552)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D150 (at 0 -3.5 359.552) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 359.552) (layer F.Fab))
    (fp_text user %R (at 0 0 359.552) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 359.552) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 359.552) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 359.552) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 153 /LEDS/L151))
    (pad 4 smd rect (at 2.45 -1.6 359.552) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(D149-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 359.552) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 109.909433 111.711036 7.22)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D149 (at 0 -3.5 7.22) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 7.22) (layer F.Fab))
    (fp_text user %R (at 0 0 7.22) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 7.22) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 7.22) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 7.22) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(D149-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 7.22) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 151 "Net-(D148-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 7.22) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 119.239432 105.303926 14.888)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D148 (at 0 -3.5 14.888) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 14.888) (layer F.Fab))
    (fp_text user %R (at 0 0 14.888) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 14.888) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 14.888) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 14.888) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 151 "Net-(D148-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 14.888) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(D147-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 14.888) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 126.820218 101.827467 214.952)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D147 (at 0 -3.5 214.952) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 214.952) (layer F.Fab))
    (fp_text user %R (at 0 0 214.952) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 214.952) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 214.952) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 214.952) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(D147-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 214.952) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(D146-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 214.952) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 119.967175 113.965441 207.284)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D146 (at 0 -3.5 207.284) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 207.284) (layer F.Fab))
    (fp_text user %R (at 0 0 207.284) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 207.284) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 207.284) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 207.284) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(D146-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 207.284) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(D145-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 207.284) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 112.478821 119.883243 199.616)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D145 (at 0 -3.5 199.616) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 199.616) (layer F.Fab))
    (fp_text user %R (at 0 0 199.616) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 199.616) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 199.616) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 199.616) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(D145-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 199.616) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(D144-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 199.616) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 104.399966 122.705324 191.948)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D144 (at 0 -3.5 191.948) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 191.948) (layer F.Fab))
    (fp_text user %R (at 0 0 191.948) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 191.948) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 191.948) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 191.948) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(D144-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 191.948) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(D143-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 191.948) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 96.040151 123.116893 184.28)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D143 (at 0 -3.5 184.28) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 184.28) (layer F.Fab))
    (fp_text user %R (at 0 0 184.28) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 184.28) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 184.28) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 184.28) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(D143-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 184.28) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(D142-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 184.28) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 87.715545 121.41695 176.612)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D142 (at 0 -3.5 176.612) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 176.612) (layer F.Fab))
    (fp_text user %R (at 0 0 176.612) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 176.612) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 176.612) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 176.612) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(D142-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 176.612) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(D141-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 176.612) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 79.729727 117.801072 168.944)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D141 (at 0 -3.5 168.944) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 168.944) (layer F.Fab))
    (fp_text user %R (at 0 0 168.944) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 168.944) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 168.944) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 168.944) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(D141-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 168.944) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(D140-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 168.944) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 72.368675 112.441709 161.276)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D140 (at 0 -3.5 161.276) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 161.276) (layer F.Fab))
    (fp_text user %R (at 0 0 161.276) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 161.276) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 161.276) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 161.276) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(D140-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 161.276) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(D139-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 161.276) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 65.896936 105.517638 153.608)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D139 (at 0 -3.5 153.608) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 153.608) (layer F.Fab))
    (fp_text user %R (at 0 0 153.608) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 153.608) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 153.608) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 153.608) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(D139-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 153.608) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(D138-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 153.608) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 60.553683 97.225582 145.94)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D138 (at 0 -3.5 145.94) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 145.94) (layer F.Fab))
    (fp_text user %R (at 0 0 145.94) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 145.94) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 145.94) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 145.94) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(D138-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 145.94) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(D137-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 145.94) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 56.548726 87.78409 138.272)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D137 (at 0 -3.5 138.272) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 138.272) (layer F.Fab))
    (fp_text user %R (at 0 0 138.272) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 138.272) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 138.272) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 138.272) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(D137-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 138.272) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(D136-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 138.272) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 54.058696 77.433446 130.604)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D136 (at 0 -3.5 130.604) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 130.604) (layer F.Fab))
    (fp_text user %R (at 0 0 130.604) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 130.604) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 130.604) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 130.604) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(D136-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 130.604) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 138 /LEDS/L136))
    (pad 3 smd rect (at 2.45 1.6 130.604) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 51.051404 94.13752 323)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D135 (at 0 -3.5 323) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 323) (layer F.Fab))
    (fp_text user %R (at 0 0 323) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 323) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 323) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 323) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 138 /LEDS/L136))
    (pad 4 smd rect (at 2.45 -1.6 323) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 137 "Net-(D134-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 323) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 55.644017 104.006702 330.668)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D134 (at 0 -3.5 330.668) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 330.668) (layer F.Fab))
    (fp_text user %R (at 0 0 330.668) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 330.668) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 330.668) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 330.668) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 137 "Net-(D134-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 330.668) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 136 "Net-(D133-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 330.668) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 61.550196 112.68533 338.336)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D133 (at 0 -3.5 338.336) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 338.336) (layer F.Fab))
    (fp_text user %R (at 0 0 338.336) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 338.336) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 338.336) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 338.336) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 136 "Net-(D133-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 338.336) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 135 "Net-(D132-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 338.336) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 68.547975 119.977466 346.004)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D132 (at 0 -3.5 346.004) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 346.004) (layer F.Fab))
    (fp_text user %R (at 0 0 346.004) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 346.004) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 346.004) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 346.004) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 135 "Net-(D132-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 346.004) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(D131-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 346.004) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 76.387644 125.717156 353.672)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D131 (at 0 -3.5 353.672) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 353.672) (layer F.Fab))
    (fp_text user %R (at 0 0 353.672) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 353.672) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 353.672) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 353.672) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(D131-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 353.672) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(D130-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 353.672) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 84.795663 129.76893 1.34)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D130 (at 0 -3.5 1.34) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 1.34) (layer F.Fab))
    (fp_text user %R (at 0 0 1.34) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 1.34) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 1.34) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 1.34) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(D130-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 1.34) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(D129-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 1.34) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 93.478047 132.02555 9.008)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D129 (at 0 -3.5 9.008) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 9.008) (layer F.Fab))
    (fp_text user %R (at 0 0 9.008) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 9.008) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 9.008) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 9.008) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(D129-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 9.008) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(D128-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 9.008) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 102.122372 132.400917 16.676)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D128 (at 0 -3.5 16.676) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 16.676) (layer F.Fab))
    (fp_text user %R (at 0 0 16.676) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 16.676) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 16.676) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 16.676) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(D128-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 16.676) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(D127-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 16.676) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 110.396587 130.813063 24.344)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D127 (at 0 -3.5 24.344) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 24.344) (layer F.Fab))
    (fp_text user %R (at 0 0 24.344) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 24.344) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 24.344) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 24.344) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(D127-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 24.344) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(D126-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 24.344) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 117.94028 127.14247 32.012)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D126 (at 0 -3.5 32.012) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 32.012) (layer F.Fab))
    (fp_text user %R (at 0 0 32.012) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 32.012) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 32.012) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 32.012) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(D126-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 32.012) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(D125-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 32.012) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 124.334918 121.111201 39.68)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D125 (at 0 -3.5 39.68) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 39.68) (layer F.Fab))
    (fp_text user %R (at 0 0 39.68) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 39.68) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 39.68) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 39.68) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(D125-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 39.68) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(D124-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 39.68) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 128.991578 111.771152 47.348)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D124 (at 0 -3.5 47.348) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 47.348) (layer F.Fab))
    (fp_text user %R (at 0 0 47.348) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 47.348) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 47.348) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 47.348) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(D124-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 47.348) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(D123-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 47.348) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 134.962344 105.823246 247.412)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D123 (at 0 -3.5 247.412) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 247.412) (layer F.Fab))
    (fp_text user %R (at 0 0 247.412) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 247.412) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 247.412) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 247.412) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(D123-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 247.412) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(D122-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 247.412) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 134.787008 117.876236 239.744)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D122 (at 0 -3.5 239.744) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 239.744) (layer F.Fab))
    (fp_text user %R (at 0 0 239.744) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 239.744) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 239.744) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 239.744) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(D122-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 239.744) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(D121-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 239.744) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 131.318613 126.376658 232.076)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D121 (at 0 -3.5 232.076) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 232.076) (layer F.Fab))
    (fp_text user %R (at 0 0 232.076) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 232.076) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 232.076) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 232.076) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(D121-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 232.076) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 123 /LEDS/L121))
    (pad 3 smd rect (at 2.45 1.6 232.076) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 125.808778 132.806934 224.408)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D120 (at 0 -3.5 224.408) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 224.408) (layer F.Fab))
    (fp_text user %R (at 0 0 224.408) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 224.408) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 224.408) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 224.408) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 123 /LEDS/L121))
    (pad 4 smd rect (at 2.45 -1.6 224.408) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(D119-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 224.408) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 118.821876 137.434687 216.74)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D119 (at 0 -3.5 216.74) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 216.74) (layer F.Fab))
    (fp_text user %R (at 0 0 216.74) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 216.74) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 216.74) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 216.74) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(D119-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 216.74) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(D118-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 216.74) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 110.764488 140.299056 209.072)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D118 (at 0 -3.5 209.072) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 209.072) (layer F.Fab))
    (fp_text user %R (at 0 0 209.072) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 209.072) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 209.072) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 209.072) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(D118-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 209.072) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(D117-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 209.072) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 101.988865 141.384591 201.404)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D117 (at 0 -3.5 201.404) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 201.404) (layer F.Fab))
    (fp_text user %R (at 0 0 201.404) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 201.404) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 201.404) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 201.404) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(D117-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 201.404) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(D116-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 201.404) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 92.824382 140.675175 193.736)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D116 (at 0 -3.5 193.736) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 193.736) (layer F.Fab))
    (fp_text user %R (at 0 0 193.736) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 193.736) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 193.736) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 193.736) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(D116-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 193.736) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(D115-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 193.736) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 83.587666 138.17567 186.068)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D115 (at 0 -3.5 186.068) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 186.068) (layer F.Fab))
    (fp_text user %R (at 0 0 186.068) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 186.068) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 186.068) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 186.068) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(D115-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 186.068) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(D114-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 186.068) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 74.584505 133.92178 178.4)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D114 (at 0 -3.5 178.4) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 178.4) (layer F.Fab))
    (fp_text user %R (at 0 0 178.4) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 178.4) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 178.4) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 178.4) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(D114-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 178.4) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(D113-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 178.4) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 66.10809 127.98452 170.732)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D113 (at 0 -3.5 170.732) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 170.732) (layer F.Fab))
    (fp_text user %R (at 0 0 170.732) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 170.732) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 170.732) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 170.732) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(D113-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 170.732) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(D112-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 170.732) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 58.435518 120.471706 163.064)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D112 (at 0 -3.5 163.064) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 163.064) (layer F.Fab))
    (fp_text user %R (at 0 0 163.064) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 163.064) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 163.064) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 163.064) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(D112-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 163.064) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(D111-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 163.064) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 64.965736 136.320021 355.46)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D111 (at 0 -3.5 355.46) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 355.46) (layer F.Fab))
    (fp_text user %R (at 0 0 355.46) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 355.46) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 355.46) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 355.46) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(D111-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 355.46) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(D110-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 355.46) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 74.178871 142.28768 3.128)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D110 (at 0 -3.5 3.128) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 3.128) (layer F.Fab))
    (fp_text user %R (at 0 0 3.128) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 3.128) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 3.128) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 3.128) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(D110-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 3.128) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(D109-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 3.128) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 83.875233 146.546492 10.796)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D109 (at 0 -3.5 10.796) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 10.796) (layer F.Fab))
    (fp_text user %R (at 0 0 10.796) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 10.796) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 10.796) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 10.796) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(D109-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 10.796) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(D108-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 10.796) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 93.763129 149.049886 18.464)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D108 (at 0 -3.5 18.464) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 18.464) (layer F.Fab))
    (fp_text user %R (at 0 0 18.464) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 18.464) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 18.464) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 18.464) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(D108-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 18.464) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(D107-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 18.464) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 103.543822 149.791894 26.132)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D107 (at 0 -3.5 26.132) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 26.132) (layer F.Fab))
    (fp_text user %R (at 0 0 26.132) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 26.132) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 26.132) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 26.132) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(D107-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 26.132) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(D106-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 26.132) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 112.915354 148.805738 33.8)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D106 (at 0 -3.5 33.8) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 33.8) (layer F.Fab))
    (fp_text user %R (at 0 0 33.8) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 33.8) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 33.8) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 33.8) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(D106-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 33.8) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 108 /LEDS/L106))
    (pad 3 smd rect (at 2.45 1.6 33.8) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 121.574672 146.160607 41.468)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D105 (at 0 -3.5 41.468) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 41.468) (layer F.Fab))
    (fp_text user %R (at 0 0 41.468) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 41.468) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 41.468) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 41.468) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 108 /LEDS/L106))
    (pad 4 smd rect (at 2.45 -1.6 41.468) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(D104-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 41.468) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 129.216469 141.955616 49.136)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D104 (at 0 -3.5 49.136) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 49.136) (layer F.Fab))
    (fp_text user %R (at 0 0 49.136) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 49.136) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 49.136) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 49.136) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(D104-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 49.136) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(D103-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 49.136) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 135.525226 136.308442 56.804)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D103 (at 0 -3.5 56.804) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 56.804) (layer F.Fab))
    (fp_text user %R (at 0 0 56.804) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 56.804) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 56.804) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 56.804) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(D103-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 56.804) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(D102-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 56.804) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 140.151264 129.331308 64.472)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D102 (at 0 -3.5 64.472) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 64.472) (layer F.Fab))
    (fp_text user %R (at 0 0 64.472) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 64.472) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 64.472) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 64.472) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(D102-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 64.472) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(D101-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 64.472) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 142.640637 121.067897 72.14)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D101 (at 0 -3.5 72.14) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 72.14) (layer F.Fab))
    (fp_text user %R (at 0 0 72.14) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 72.14) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 72.14) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 72.14) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(D101-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 72.14) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(D100-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 72.14) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 142.176293 111.254125 79.808)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D100 (at 0 -3.5 79.808) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 79.808) (layer F.Fab))
    (fp_text user %R (at 0 0 79.808) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 79.808) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 79.808) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 79.808) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(D100-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 79.808) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(D100-Pad4)"))
    (pad 3 smd rect (at 2.45 1.6 79.808) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 135.26915 96.872849 87.476)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D99 (at 0 -3.5 87.476) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 87.476) (layer F.Fab))
    (fp_text user %R (at 0 0 87.476) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 87.476) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 87.476) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 87.476) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(D100-Pad4)"))
    (pad 4 smd rect (at 2.45 -1.6 87.476) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(D98-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 87.476) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 145.29213 102.889947 279.872)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D98 (at 0 -3.5 279.872) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 279.872) (layer F.Fab))
    (fp_text user %R (at 0 0 279.872) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 279.872) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 279.872) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 279.872) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(D98-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 279.872) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(D97-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 279.872) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 150.431157 112.529265 272.204)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D97 (at 0 -3.5 272.204) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 272.204) (layer F.Fab))
    (fp_text user %R (at 0 0 272.204) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 272.204) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 272.204) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 272.204) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(D97-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 272.204) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(D96-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 272.204) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 151.58782 121.368232 264.536)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D96 (at 0 -3.5 264.536) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 264.536) (layer F.Fab))
    (fp_text user %R (at 0 0 264.536) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 264.536) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 264.536) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 264.536) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(D96-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 264.536) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(D95-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 264.536) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 150.0845 129.643572 256.868)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D95 (at 0 -3.5 256.868) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 256.868) (layer F.Fab))
    (fp_text user %R (at 0 0 256.868) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 256.868) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 256.868) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 256.868) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(D95-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 256.868) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(D94-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 256.868) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 146.443332 137.218818 249.2)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D94 (at 0 -3.5 249.2) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 249.2) (layer F.Fab))
    (fp_text user %R (at 0 0 249.2) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 249.2) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 249.2) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 249.2) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(D94-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 249.2) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(D93-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 249.2) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 140.995335 143.889726 241.532)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D93 (at 0 -3.5 241.532) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 241.532) (layer F.Fab))
    (fp_text user %R (at 0 0 241.532) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 241.532) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 241.532) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 241.532) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(D93-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 241.532) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(D92-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 241.532) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 134.015128 149.446435 233.864)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D92 (at 0 -3.5 233.864) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 233.864) (layer F.Fab))
    (fp_text user %R (at 0 0 233.864) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 233.864) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 233.864) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 233.864) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(D92-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 233.864) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(D91-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 233.864) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 125.764911 153.695086 226.196)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D91 (at 0 -3.5 226.196) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 226.196) (layer F.Fab))
    (fp_text user %R (at 0 0 226.196) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 226.196) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 226.196) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 226.196) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(D91-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 226.196) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 93 /LEDS/L91))
    (pad 3 smd rect (at 2.45 1.6 226.196) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 116.51069 156.468327 218.528)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D90 (at 0 -3.5 218.528) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 218.528) (layer F.Fab))
    (fp_text user %R (at 0 0 218.528) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 218.528) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 218.528) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 218.528) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 93 /LEDS/L91))
    (pad 4 smd rect (at 2.45 -1.6 218.528) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(D89-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 218.528) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 106.527542 157.631676 210.86)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D89 (at 0 -3.5 210.86) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 210.86) (layer F.Fab))
    (fp_text user %R (at 0 0 210.86) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 210.86) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 210.86) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 210.86) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(D89-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 210.86) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(D88-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 210.86) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 96.099754 157.087803 203.192)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D88 (at 0 -3.5 203.192) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 203.192) (layer F.Fab))
    (fp_text user %R (at 0 0 203.192) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 203.192) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 203.192) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 203.192) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(D88-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 203.192) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(D87-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 203.192) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 85.518268 154.779436 195.524)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D87 (at 0 -3.5 195.524) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 195.524) (layer F.Fab))
    (fp_text user %R (at 0 0 195.524) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 195.524) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 195.524) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 195.524) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(D87-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 195.524) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(D86-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 195.524) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 110.761058 164.865633 35.588)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D86 (at 0 -3.5 35.588) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 35.588) (layer F.Fab))
    (fp_text user %R (at 0 0 35.588) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 35.588) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 35.588) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 35.588) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(D86-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 35.588) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(D85-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 35.588) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 121.330583 163.313308 43.256)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D85 (at 0 -3.5 43.256) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 43.256) (layer F.Fab))
    (fp_text user %R (at 0 0 43.256) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 43.256) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 43.256) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 43.256) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(D85-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 43.256) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(D84-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 43.256) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 131.131706 160.169218 50.924)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D84 (at 0 -3.5 50.924) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 50.924) (layer F.Fab))
    (fp_text user %R (at 0 0 50.924) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 50.924) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 50.924) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 50.924) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(D84-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 50.924) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(D83-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 50.924) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 139.909894 155.588062 58.592)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D83 (at 0 -3.5 58.592) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 58.592) (layer F.Fab))
    (fp_text user %R (at 0 0 58.592) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 58.592) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 58.592) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 58.592) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(D83-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 58.592) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(D82-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 58.592) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 147.429645 149.75958 66.26)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D82 (at 0 -3.5 66.26) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 66.26) (layer F.Fab))
    (fp_text user %R (at 0 0 66.26) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 66.26) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 66.26) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 66.26) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(D82-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 66.26) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(D81-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 66.26) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 153.475121 142.904807 73.928)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D81 (at 0 -3.5 73.928) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 73.928) (layer F.Fab))
    (fp_text user %R (at 0 0 73.928) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 73.928) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 73.928) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 73.928) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(D81-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 73.928) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(D80-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 73.928) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 157.847072 135.271851 81.596)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D80 (at 0 -3.5 81.596) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 81.596) (layer F.Fab))
    (fp_text user %R (at 0 0 81.596) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 81.596) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 81.596) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 81.596) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(D80-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 81.596) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(D79-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 81.596) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 160.352555 127.131151 89.264)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D79 (at 0 -3.5 89.264) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 89.264) (layer F.Fab))
    (fp_text user %R (at 0 0 89.264) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 89.264) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 89.264) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 89.264) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(D79-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 89.264) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(D78-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 89.264) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 160.778356 118.76965 96.932)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D78 (at 0 -3.5 96.932) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 96.932) (layer F.Fab))
    (fp_text user %R (at 0 0 96.932) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 96.932) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 96.932) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 96.932) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(D78-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 96.932) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(D77-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 96.932) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 158.819119 110.480682 104.6)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D77 (at 0 -3.5 104.6) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 104.6) (layer F.Fab))
    (fp_text user %R (at 0 0 104.6) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 104.6) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 104.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 104.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(D77-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 104.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(D76-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 104.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 153.832958 102.529567 112.268)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D76 (at 0 -3.5 112.268) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 112.268) (layer F.Fab))
    (fp_text user %R (at 0 0 112.268) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 112.268) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 112.268) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 112.268) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(D76-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 112.268) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 78 /LEDS/L76))
    (pad 3 smd rect (at 2.45 1.6 112.268) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 143.283849 94.851736 119.936)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D75 (at 0 -3.5 119.936) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 119.936) (layer F.Fab))
    (fp_text user %R (at 0 0 119.936) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 119.936) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 119.936) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 119.936) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 78 /LEDS/L76))
    (pad 4 smd rect (at 2.45 -1.6 119.936) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(D74-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 119.936) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 152.707988 93.057327 312.332)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D74 (at 0 -3.5 312.332) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 312.332) (layer F.Fab))
    (fp_text user %R (at 0 0 312.332) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 312.332) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 312.332) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 312.332) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(D74-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 312.332) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(D73-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 312.332) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 161.249854 98.5701 304.664)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D73 (at 0 -3.5 304.664) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 304.664) (layer F.Fab))
    (fp_text user %R (at 0 0 304.664) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 304.664) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 304.664) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 304.664) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(D73-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 304.664) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(D72-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 304.664) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 166.530321 105.509211 296.996)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D72 (at 0 -3.5 296.996) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 296.996) (layer F.Fab))
    (fp_text user %R (at 0 0 296.996) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 296.996) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 296.996) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 296.996) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(D72-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 296.996) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(D71-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 296.996) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 169.414809 113.376756 289.328)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D71 (at 0 -3.5 289.328) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 289.328) (layer F.Fab))
    (fp_text user %R (at 0 0 289.328) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 289.328) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 289.328) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 289.328) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(D71-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 289.328) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(D70-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 289.328) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 170.185645 121.782288 281.66)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D70 (at 0 -3.5 281.66) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 281.66) (layer F.Fab))
    (fp_text user %R (at 0 0 281.66) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 281.66) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 281.66) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 281.66) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(D70-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 281.66) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(D69-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 281.66) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 168.981966 130.378289 273.992)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D69 (at 0 -3.5 273.992) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 273.992) (layer F.Fab))
    (fp_text user %R (at 0 0 273.992) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 273.992) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 273.992) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 273.992) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(D69-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 273.992) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(D68-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 273.992) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 165.909353 138.841768 266.324)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D68 (at 0 -3.5 266.324) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 266.324) (layer F.Fab))
    (fp_text user %R (at 0 0 266.324) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 266.324) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 266.324) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 266.324) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(D68-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 266.324) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(D67-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 266.324) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 161.078376 146.869451 258.656)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D67 (at 0 -3.5 258.656) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 258.656) (layer F.Fab))
    (fp_text user %R (at 0 0 258.656) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 258.656) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 258.656) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 258.656) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(D67-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 258.656) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(D66-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 258.656) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 154.620282 154.178202 250.988)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D66 (at 0 -3.5 250.988) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 250.988) (layer F.Fab))
    (fp_text user %R (at 0 0 250.988) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 250.988) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 250.988) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 250.988) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(D66-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 250.988) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(D65-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 250.988) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 146.693299 160.507685 243.32)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D65 (at 0 -3.5 243.32) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 243.32) (layer F.Fab))
    (fp_text user %R (at 0 0 243.32) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 243.32) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 243.32) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 243.32) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(D65-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 243.32) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(D64-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 243.32) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 137.484295 165.623973 235.652)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D64 (at 0 -3.5 235.652) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 235.652) (layer F.Fab))
    (fp_text user %R (at 0 0 235.652) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 235.652) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 235.652) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 235.652) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(D64-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 235.652) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(D63-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 235.652) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 127.207787 169.323411 227.984)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D63 (at 0 -3.5 227.984) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 227.984) (layer F.Fab))
    (fp_text user %R (at 0 0 227.984) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 227.984) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 227.984) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 227.984) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(D63-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 227.984) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(D62-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 227.984) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 154.197218 164.259643 68.048)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D62 (at 0 -3.5 68.048) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 68.048) (layer F.Fab))
    (fp_text user %R (at 0 0 68.048) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 68.048) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 68.048) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 68.048) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(D62-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 68.048) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(D61-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 68.048) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 162.398342 157.270702 75.716)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D61 (at 0 -3.5 75.716) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 75.716) (layer F.Fab))
    (fp_text user %R (at 0 0 75.716) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 75.716) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 75.716) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 75.716) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(D61-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 75.716) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 63 /LEDS/L61))
    (pad 3 smd rect (at 2.45 1.6 75.716) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 169.102437 149.338009 83.384)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D60 (at 0 -3.5 83.384) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 83.384) (layer F.Fab))
    (fp_text user %R (at 0 0 83.384) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 83.384) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 83.384) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 83.384) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 63 /LEDS/L61))
    (pad 4 smd rect (at 2.45 -1.6 83.384) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(D59-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 83.384) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 174.177914 140.727821 91.052)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D59 (at 0 -3.5 91.052) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 91.052) (layer F.Fab))
    (fp_text user %R (at 0 0 91.052) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 91.052) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 91.052) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 91.052) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(D59-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 91.052) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(D58-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 91.052) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 177.528683 131.725582 98.72)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D58 (at 0 -3.5 98.72) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 98.72) (layer F.Fab))
    (fp_text user %R (at 0 0 98.72) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 98.72) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 98.72) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 98.72) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(D58-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 98.72) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(D57-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 98.72) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 179.093149 122.632233 106.388)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D57 (at 0 -3.5 106.388) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 106.388) (layer F.Fab))
    (fp_text user %R (at 0 0 106.388) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 106.388) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 106.388) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 106.388) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(D57-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 106.388) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(D56-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 106.388) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 178.84026 113.761923 114.056)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D56 (at 0 -3.5 114.056) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 114.056) (layer F.Fab))
    (fp_text user %R (at 0 0 114.056) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 114.056) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 114.056) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 114.056) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(D56-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 114.056) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(D55-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 114.056) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 176.760255 105.442749 121.724)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D55 (at 0 -3.5 121.724) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 121.724) (layer F.Fab))
    (fp_text user %R (at 0 0 121.724) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 121.724) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 121.724) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 121.724) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(D55-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 121.724) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(D54-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 121.724) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 172.844038 98.024235 129.392)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D54 (at 0 -3.5 129.392) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 129.392) (layer F.Fab))
    (fp_text user %R (at 0 0 129.392) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 129.392) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 129.392) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 129.392) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(D54-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 129.392) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(D53-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 129.392) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 167.032186 91.90189 137.06)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D53 (at 0 -3.5 137.06) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 137.06) (layer F.Fab))
    (fp_text user %R (at 0 0 137.06) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 137.06) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 137.06) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 137.06) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(D53-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 137.06) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(D52-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 137.06) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 159.055552 87.596903 144.728)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D52 (at 0 -3.5 144.728) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 144.728) (layer F.Fab))
    (fp_text user %R (at 0 0 144.728) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 144.728) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 144.728) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 144.728) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(D52-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 144.728) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(D51-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 144.728) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 147.60748 86.130034 152.396)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D51 (at 0 -3.5 152.396) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 152.396) (layer F.Fab))
    (fp_text user %R (at 0 0 152.396) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 152.396) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 152.396) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 152.396) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(D51-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 152.396) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(D50-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 152.396) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 139.433594 83.999393 352.46)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D50 (at 0 -3.5 352.46) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 352.46) (layer F.Fab))
    (fp_text user %R (at 0 0 352.46) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 352.46) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 352.46) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 352.46) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(D50-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 352.46) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(D49-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 352.46) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 153.145368 79.30926 344.792)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D49 (at 0 -3.5 344.792) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 344.792) (layer F.Fab))
    (fp_text user %R (at 0 0 344.792) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 344.792) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 344.792) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 344.792) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(D49-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 344.792) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(D48-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 344.792) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 162.758709 79.907083 337.124)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D48 (at 0 -3.5 337.124) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 337.124) (layer F.Fab))
    (fp_text user %R (at 0 0 337.124) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 337.124) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 337.124) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 337.124) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(D48-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 337.124) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(D47-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 337.124) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 170.670811 83.226144 329.456)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D47 (at 0 -3.5 329.456) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 329.456) (layer F.Fab))
    (fp_text user %R (at 0 0 329.456) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 329.456) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 329.456) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 329.456) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(D47-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 329.456) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(D46-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 329.456) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 177.146939 88.528232 321.788)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D46 (at 0 -3.5 321.788) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 321.788) (layer F.Fab))
    (fp_text user %R (at 0 0 321.788) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 321.788) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 321.788) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 321.788) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(D46-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 321.788) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 48 /LEDS/L46))
    (pad 3 smd rect (at 2.45 1.6 321.788) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 182.164534 95.372277 314.12)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D45 (at 0 -3.5 314.12) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 314.12) (layer F.Fab))
    (fp_text user %R (at 0 0 314.12) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 314.12) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 314.12) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 314.12) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 48 /LEDS/L46))
    (pad 4 smd rect (at 2.45 -1.6 314.12) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D44-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 314.12) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 185.6352 103.406135 306.452)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D44 (at 0 -3.5 306.452) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 306.452) (layer F.Fab))
    (fp_text user %R (at 0 0 306.452) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 306.452) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 306.452) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 306.452) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D44-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 306.452) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D43-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 306.452) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 187.466071 112.308084 298.784)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D43 (at 0 -3.5 298.784) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 298.784) (layer F.Fab))
    (fp_text user %R (at 0 0 298.784) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 298.784) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 298.784) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 298.784) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D43-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 298.784) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D42-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 298.784) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 187.583563 121.766857 291.116)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D42 (at 0 -3.5 291.116) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 291.116) (layer F.Fab))
    (fp_text user %R (at 0 0 291.116) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 291.116) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 291.116) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 291.116) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D42-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 291.116) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D41-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 291.116) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 185.944533 131.475404 283.448)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D41 (at 0 -3.5 283.448) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 283.448) (layer F.Fab))
    (fp_text user %R (at 0 0 283.448) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 283.448) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 283.448) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 283.448) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D41-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 283.448) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D40-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 283.448) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 182.54202 141.130579 275.78)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D40 (at 0 -3.5 275.78) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 275.78) (layer F.Fab))
    (fp_text user %R (at 0 0 275.78) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 275.78) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 275.78) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 275.78) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D40-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 275.78) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D39-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 275.78) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 177.408083 150.435698 268.112)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D39 (at 0 -3.5 268.112) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 268.112) (layer F.Fab))
    (fp_text user %R (at 0 0 268.112) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 268.112) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 268.112) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 268.112) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D39-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 268.112) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D38-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 268.112) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 170.614772 159.10456 260.444)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D38 (at 0 -3.5 260.444) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 260.444) (layer F.Fab))
    (fp_text user %R (at 0 0 260.444) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 260.444) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 260.444) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 260.444) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D38-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 260.444) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D37-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 260.444) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 190.887159 140.177224 100.508)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D37 (at 0 -3.5 100.508) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 100.508) (layer F.Fab))
    (fp_text user %R (at 0 0 100.508) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 100.508) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 100.508) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 100.508) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D37-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 100.508) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D36-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 100.508) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 194.14882 129.811164 108.176)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D36 (at 0 -3.5 108.176) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 108.176) (layer F.Fab))
    (fp_text user %R (at 0 0 108.176) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 108.176) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 108.176) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 108.176) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D36-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 108.176) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D35-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 108.176) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 195.638242 119.438429 115.844)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D35 (at 0 -3.5 115.844) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 115.844) (layer F.Fab))
    (fp_text user %R (at 0 0 115.844) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 115.844) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 115.844) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 115.844) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D35-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 115.844) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D34-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 115.844) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 195.386843 109.35357 123.512)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D34 (at 0 -3.5 123.512) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 123.512) (layer F.Fab))
    (fp_text user %R (at 0 0 123.512) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 123.512) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 123.512) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 123.512) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D34-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 123.512) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D33-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 123.512) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 193.466683 99.847847 131.18)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D33 (at 0 -3.5 131.18) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 131.18) (layer F.Fab))
    (fp_text user %R (at 0 0 131.18) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 131.18) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 131.18) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 131.18) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D33-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 131.18) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D32-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 131.18) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 189.987872 91.20629 138.848)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D32 (at 0 -3.5 318.848) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 318.848) (layer F.Fab))
    (fp_text user %R (at 0 0 318.848) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 318.848) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 138.848) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 138.848) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D32-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 138.848) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D31-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 138.848) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 185.094469 83.707193 146.516)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D31 (at 0 -3.5 326.516) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 326.516) (layer F.Fab))
    (fp_text user %R (at 0 0 326.516) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 326.516) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 146.516) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 146.516) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D31-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 146.516) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 33 /LEDS/L31))
    (pad 3 smd rect (at 2.45 1.6 146.516) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 178.958047 77.626256 154.184)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D30 (at 0 -3.5 154.184) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 154.184) (layer F.Fab))
    (fp_text user %R (at 0 0 154.184) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 154.184) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 154.184) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 154.184) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 33 /LEDS/L31))
    (pad 4 smd rect (at 2.45 -1.6 154.184) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D29-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 154.184) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 171.766678 73.250535 161.852)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D29 (at 0 -3.5 161.852) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 161.852) (layer F.Fab))
    (fp_text user %R (at 0 0 161.852) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 161.852) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 161.852) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 161.852) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D29-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 161.852) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D28-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 161.852) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 163.702071 70.916753 169.52)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D28 (at 0 -3.5 169.52) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 169.52) (layer F.Fab))
    (fp_text user %R (at 0 0 169.52) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 169.52) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 169.52) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 169.52) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D28-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 169.52) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D27-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 169.52) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 154.875592 71.126609 177.188)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D27 (at 0 -3.5 177.188) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 177.188) (layer F.Fab))
    (fp_text user %R (at 0 0 177.188) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 177.188) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 177.188) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 177.188) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D27-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 177.188) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D26-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 177.188) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 145.037651 75.037747 184.856)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D26 (at 0 -3.5 184.856) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 184.856) (layer F.Fab))
    (fp_text user %R (at 0 0 184.856) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 184.856) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 184.856) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 184.856) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D26-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 184.856) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D25-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 184.856) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 136.702183 75.67936 24.92)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D25 (at 0 -3.5 24.92) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 24.92) (layer F.Fab))
    (fp_text user %R (at 0 0 24.92) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 24.92) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 24.92) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 24.92) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D25-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 24.92) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D24-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 24.92) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 145.059274 66.58594 17.252)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D24 (at 0 -3.5 17.252) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 17.252) (layer F.Fab))
    (fp_text user %R (at 0 0 17.252) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 17.252) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 17.252) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 17.252) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D24-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 17.252) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D23-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 17.252) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 153.375962 62.548873 9.584)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D23 (at 0 -3.5 -170.416) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 -170.416) (layer F.Fab))
    (fp_text user %R (at 0 0 -170.416) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 -170.416) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 9.584) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 9.584) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D23-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 9.584) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D22-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 9.584) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 161.789034 61.461303 1.916)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D22 (at 0 -3.5 1.916) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 1.916) (layer F.Fab))
    (fp_text user %R (at 0 0 1.916) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 1.916) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 1.916) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 1.916) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D22-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 1.916) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D21-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 1.916) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 170.071377 62.718418 354.248)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D21 (at 0 -3.5 354.248) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 354.248) (layer F.Fab))
    (fp_text user %R (at 0 0 354.248) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 354.248) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 354.248) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 354.248) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D21-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 354.248) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D20-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 354.248) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 177.952057 66.008331 346.58)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D20 (at 0 -3.5 346.58) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 346.58) (layer F.Fab))
    (fp_text user %R (at 0 0 346.58) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 346.58) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 346.58) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 346.58) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D20-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 346.58) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D19-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 346.58) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 185.161825 71.100978 338.912)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D19 (at 0 -3.5 338.912) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 338.912) (layer F.Fab))
    (fp_text user %R (at 0 0 338.912) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 338.912) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 338.912) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 338.912) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D19-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 338.912) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D18-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 338.912) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 191.447301 77.784062 331.244)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D18 (at 0 -3.5 331.244) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 331.244) (layer F.Fab))
    (fp_text user %R (at 0 0 331.244) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 331.244) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 331.244) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 331.244) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D18-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 331.244) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D17-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 331.244) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 196.578435 85.839238 323.576)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D17 (at 0 -3.5 323.576) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 323.576) (layer F.Fab))
    (fp_text user %R (at 0 0 323.576) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 323.576) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 323.576) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 323.576) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D17-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 323.576) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D16-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 323.576) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 200.353872 95.033154 315.908)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D16 (at 0 -3.5 315.908) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 315.908) (layer F.Fab))
    (fp_text user %R (at 0 0 315.908) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 315.908) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 315.908) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 315.908) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D16-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 315.908) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 18 /LEDS/L16))
    (pad 3 smd rect (at 2.45 1.6 315.908) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 202.605318 105.115148 308.24)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D15 (at 0 -3.5 308.24) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 308.24) (layer F.Fab))
    (fp_text user %R (at 0 0 308.24) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 308.24) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 308.24) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 308.24) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 18 /LEDS/L16))
    (pad 4 smd rect (at 2.45 -1.6 308.24) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D14-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 308.24) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 203.201158 115.818413 300.572)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D14 (at 0 -3.5 300.572) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 300.572) (layer F.Fab))
    (fp_text user %R (at 0 0 300.572) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 300.572) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 300.572) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 300.572) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D14-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 300.572) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D13-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 300.572) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 209.087477 99.75556 132.968)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D13 (at 0 -3.5 132.968) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 132.968) (layer F.Fab))
    (fp_text user %R (at 0 0 132.968) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 132.968) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 132.968) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 132.968) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D13-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 132.968) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D12-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 132.968) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 206.316985 89.152825 140.636)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D12 (at 0 -3.5 140.636) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 140.636) (layer F.Fab))
    (fp_text user %R (at 0 0 140.636) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 140.636) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 140.636) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 140.636) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D12-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 140.636) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D11-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 140.636) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 202.03783 79.485681 148.304)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D11 (at 0 -3.5 148.304) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 148.304) (layer F.Fab))
    (fp_text user %R (at 0 0 148.304) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 148.304) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 148.304) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 148.304) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D11-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 148.304) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D10-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 148.304) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 196.433804 70.985544 155.972)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D10 (at 0 -3.5 155.972) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 155.972) (layer F.Fab))
    (fp_text user %R (at 0 0 155.972) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 155.972) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 155.972) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 155.972) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D10-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 155.972) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D10-Pad4)"))
    (pad 3 smd rect (at 2.45 1.6 155.972) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 189.721305 63.858737 163.64)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D9 (at 0 -3.5 163.64) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 163.64) (layer F.Fab))
    (fp_text user %R (at 0 0 163.64) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 163.64) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 163.64) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 163.64) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D10-Pad4)"))
    (pad 4 smd rect (at 2.45 -1.6 163.64) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D8-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 163.64) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 182.145568 58.285025 171.308)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D8 (at 0 -3.5 171.308) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 171.308) (layer F.Fab))
    (fp_text user %R (at 0 0 171.308) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 171.308) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 171.308) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 171.308) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D8-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 171.308) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D7-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 171.308) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 173.976922 54.418681 178.976)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D7 (at 0 -3.5 358.976) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 358.976) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 358.976) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 358.976) (layer F.Fab))
    (pad 3 smd rect (at 2.45 1.6 178.976) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 4 smd rect (at 2.45 -1.6 178.976) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D6-Pad2)"))
    (pad 2 smd rect (at -2.45 1.6 178.976) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D7-Pad2)"))
    (pad 1 smd rect (at -2.45 -1.6 178.976) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 157.049805 52.33957 194.312)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D5 (at 0 -3.5 194.312) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 194.312) (layer F.Fab))
    (fp_text user %R (at 0 0 194.312) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 194.312) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 194.312) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 194.312) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D5-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 194.312) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 194.312) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 148.937426 54.413853 201.98)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D4 (at 0 -3.5 21.98) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 21.98) (layer F.Fab))
    (fp_text user %R (at 0 0 21.98) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 21.98) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 201.98) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 201.98) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 201.98) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 201.98) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 141.53478 58.904199 209.648)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D3 (at 0 -3.5 29.648) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 29.648) (layer F.Fab))
    (fp_text user %R (at 0 0 29.648) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 29.648) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 209.648) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 209.648) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 209.648) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 209.648) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 135.265194 66.606033 217.316)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D2 (at 0 -3.5 37.316) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 37.316) (layer F.Fab))
    (fp_text user %R (at 0 0 37.316) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 37.316) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 217.316) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 217.316) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 217.316) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6 217.316) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 130.618251 82.956013 224.984)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D1 (at 0 -3.5 44.984) (layer F.SilkS) hide)
    (fp_text value WS2812B (at 0 4 44.984) (layer F.Fab))
    (fp_text user %R (at 0 0 44.984) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 44.984) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.45 -1.6 224.984) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.45 1.6 224.984) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6 224.984) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 3 /DIN))
    (pad 3 smd rect (at 2.45 1.6 224.984) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 111.22406 172.78858 -12) (layer B.SilkS))
  (gr_text 5V (at 134.76986 174.7647 2) (layer B.SilkS))
  (gr_text r1.0 (at 128.72212 5.31114 180) (layer F.SilkS))
  (gr_text "Holes: R=81.5 Angles=27, 164, 269" (at 130.1496 0.33782) (layer Cmts.User))
  (gr_text DIN (at 48.66132 87.06104 90) (layer B.SilkS))
  (gr_text DIN (at 49.34204 87.48776 270) (layer F.SilkS))
  (gr_text GND (at 46.62932 92.1258) (layer F.SilkS))
  (gr_text GND (at 46.64456 92.28836) (layer B.SilkS))
  (gr_text 5V (at 46.24324 82.23504) (layer B.SilkS))
  (gr_text 5V (at 46.1518 82.2452) (layer F.SilkS))
  (gr_text DOUT (at 210.98256 87.884 90) (layer B.SilkS))
  (gr_text GND (at 212.36432 92.9386) (layer B.SilkS))
  (gr_text 5V (at 213.65972 81.72196) (layer B.SilkS))
  (gr_text DOUT (at 211.455 87.8967 90) (layer F.SilkS))
  (gr_text GND (at 213.1822 93.2942) (layer F.SilkS))
  (gr_text 5V (at 213.5124 81.6483) (layer F.SilkS))
  (gr_circle (center 130 90) (end 216 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 222.5294 2.4003) (xy 228.5873 192.7098) (xy 34.6202 185.3692) (xy 37.7698 0.7366)
      )
    )
  )
  (zone (net 1) (net_name VDD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 225.5139 2.5527) (xy 226.0092 191.5541) (xy 33.7693 182.4609) (xy 40.1066 1.8542)
      )
    )
  )
)
