<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="10.16" x2="0" y2="0.02" width="0" layer="20"/>
<wire x1="0" y1="0.02" x2="35.23" y2="0.02" width="0" layer="20"/>
<wire x1="35.23" y1="0.02" x2="35.23" y2="10.16" width="0" layer="20"/>
<wire x1="35.23" y1="10.16" x2="0" y2="10.16" width="0" layer="20"/>
<text>ISP</text>
<text>1</text>
<text>Eifel-Modellbau.de</text>
<text>QFN-Adapter</text>
<text>ATmega</text>
<text>48/88/168/328</text>
</plain>
<libraries>
<library name="Erics-Sachen2">
<packages>
<package name="QFN50P500X500X100-33N">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X14">
</package>
<package name="AVR_MINI_PROG">
</package>
</packages>
</library>
<library name="Testing">
<packages>
<package name="RESONATOR-SMD-1:1">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="Erics-Sachen2" package="QFN50P500X500X100-33N" value="ATMEGA328P-MU">
<attribute name="PACKAGE" value="QFN-32"/>
<attribute name="OC_NEWARK" value="26R2526"/>
<attribute name="MPN" value="ATMEGA328P-MU"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="OC_FARNELL" value="1748522"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X14" value="M14"/>
<element name="JP2" library="SparkFun-Connectors" package="1X14" value="M14"/>
<element name="U$1" library="SparkFun-Connectors" package="AVR_MINI_PROG" value="AVR_MINI_PROGSMD"/>
<element name="Q1" library="Testing" package="RESONATOR-SMD-1:1" value="8/16/20MHz"/>
</elements>
<signals>
<signal name="AVCC">
<contactref element="U1" pad="18"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
<contactref element="JP2" pad="7"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="AREF">
<contactref element="U1" pad="20"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="B0">
<contactref element="U1" pad="12"/>
<contactref element="JP2" pad="14"/>
</signal>
<signal name="B1">
<contactref element="U1" pad="13"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="B2">
<contactref element="U1" pad="14"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="B3">
<contactref element="U1" pad="15"/>
<contactref element="JP1" pad="3"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="B4">
<contactref element="U1" pad="16"/>
<contactref element="JP1" pad="4"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="B5">
<contactref element="U1" pad="17"/>
<contactref element="JP1" pad="5"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="B6">
<contactref element="U1" pad="7"/>
<contactref element="Q1" pad="1"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="B7">
<contactref element="U1" pad="8"/>
<contactref element="Q1" pad="3"/>
<contactref element="JP2" pad="10"/>
</signal>
<signal name="C6">
<contactref element="U1" pad="29"/>
<contactref element="JP2" pad="1"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="C5">
<contactref element="U1" pad="28"/>
<contactref element="JP1" pad="14"/>
</signal>
<signal name="C4">
<contactref element="U1" pad="27"/>
<contactref element="JP1" pad="13"/>
</signal>
<signal name="C3">
<contactref element="U1" pad="26"/>
<contactref element="JP1" pad="12"/>
</signal>
<signal name="C2">
<contactref element="U1" pad="25"/>
<contactref element="JP1" pad="11"/>
</signal>
<signal name="C1">
<contactref element="U1" pad="24"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="C0">
<contactref element="U1" pad="23"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="D7">
<contactref element="U1" pad="11"/>
<contactref element="JP2" pad="13"/>
</signal>
<signal name="D6">
<contactref element="U1" pad="10"/>
<contactref element="JP2" pad="12"/>
</signal>
<signal name="D5">
<contactref element="U1" pad="9"/>
<contactref element="JP2" pad="11"/>
</signal>
<signal name="D4">
<contactref element="U1" pad="2"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="D3">
<contactref element="U1" pad="1"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="D1">
<contactref element="U1" pad="31"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="D2">
<contactref element="U1" pad="32"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="D0">
<contactref element="U1" pad="30"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="33"/>
<contactref element="Q1" pad="2"/>
<contactref element="JP2" pad="8"/>
<contactref element="JP1" pad="8"/>
<contactref element="U$1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
