(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 368)
    (zones 0)
    (modules 39)
    (nets 43)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3 3)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 38.1 38.1)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 "Net-(D1-Pad1)")
  (net 3 "Net-(D1-Pad3)")
  (net 4 "Net-(D1-Pad4)")
  (net 5 "Net-(D2-Pad1)")
  (net 6 "Net-(D2-Pad3)")
  (net 7 "Net-(D3-Pad1)")
  (net 8 "Net-(D29-Pad1)")
  (net 9 "Net-(D4-Pad1)")
  (net 10 "Net-(D5-Pad1)")
  (net 11 "Net-(D6-Pad1)")
  (net 12 "Net-(D10-Pad3)")
  (net 13 "Net-(D11-Pad3)")
  (net 14 "Net-(D12-Pad3)")
  (net 15 "Net-(D10-Pad1)")
  (net 16 "Net-(D11-Pad1)")
  (net 17 "Net-(D12-Pad1)")
  (net 18 "Net-(D13-Pad1)")
  (net 19 "Net-(D14-Pad1)")
  (net 20 "Net-(D15-Pad1)")
  (net 21 "Net-(D16-Pad1)")
  (net 22 "Net-(D17-Pad1)")
  (net 23 "Net-(D18-Pad1)")
  (net 24 "Net-(D19-Pad1)")
  (net 25 "Net-(D20-Pad1)")
  (net 26 "Net-(D21-Pad1)")
  (net 27 "Net-(D22-Pad1)")
  (net 28 "Net-(D23-Pad1)")
  (net 29 "Net-(D24-Pad1)")
  (net 30 "Net-(D25-Pad1)")
  (net 31 "Net-(D26-Pad1)")
  (net 32 "Net-(D27-Pad1)")
  (net 33 "Net-(J1-Pad1)")
  (net 34 "Net-(R3-Pad1)")
  (net 35 "Net-(R3-Pad2)")
  (net 36 "Net-(R4-Pad1)")
  (net 37 "Net-(R4-Pad2)")
  (net 38 "Net-(R5-Pad2)")
  (net 39 "Net-(R5-Pad1)")
  (net 40 "Net-(R7-Pad2)")
  (net 41 "Net-(R7-Pad1)")
  (net 42 "Net-(D4-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D1-Pad4)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D10-Pad3)")
    (add_net "Net-(D11-Pad1)")
    (add_net "Net-(D11-Pad3)")
    (add_net "Net-(D12-Pad1)")
    (add_net "Net-(D12-Pad3)")
    (add_net "Net-(D13-Pad1)")
    (add_net "Net-(D14-Pad1)")
    (add_net "Net-(D15-Pad1)")
    (add_net "Net-(D16-Pad1)")
    (add_net "Net-(D17-Pad1)")
    (add_net "Net-(D18-Pad1)")
    (add_net "Net-(D19-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad3)")
    (add_net "Net-(D20-Pad1)")
    (add_net "Net-(D21-Pad1)")
    (add_net "Net-(D22-Pad1)")
    (add_net "Net-(D23-Pad1)")
    (add_net "Net-(D24-Pad1)")
    (add_net "Net-(D25-Pad1)")
    (add_net "Net-(D26-Pad1)")
    (add_net "Net-(D27-Pad1)")
    (add_net "Net-(D29-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad3)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R7-Pad2)")
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 53.261 34.877 57)
    (fp_text reference D1 (at 0.25 2 57) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 57) (layer F.Fab))
    (pad 2 smd rect (at -0.475 -0.475 57) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at 0.475 -0.475 57) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 3 smd rect (at -0.475 0.475 57) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad3)"))
    (pad 4 smd rect (at 0.475 0.475 57) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 27.728 26.581 177)
    (fp_text reference D2 (at 0.25 2 177) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 177) (layer F.Fab))
    (pad 2 smd rect (at -0.475 -0.475 177) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at 0.475 -0.475 177) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 3 smd rect (at -0.475 0.475 177) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad3)"))
    (pad 4 smd rect (at 0.475 0.475 177) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 33.31 52.841 297)
    (fp_text reference D3 (at 0.25 2 297) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 297) (layer F.Fab))
    (pad 2 smd rect (at -0.475 -0.475001 297) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at 0.475001 -0.475 297) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D3-Pad1)"))
    (pad 3 smd rect (at -0.475001 0.475 297) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D29-Pad1)"))
    (pad 4 smd rect (at 0.475 0.475001 297) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 52.26 31.796 69)
    (fp_text reference D4 (at 0.25 2 69) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 69) (layer F.Fab))
    (pad 2 smd rect (at -0.475 -0.475 69) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at 0.475 -0.475 69) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D4-Pad1)"))
    (pad 3 smd rect (at -0.475 0.475 69) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D4-Pad3)"))
    (pad 4 smd rect (at 0.475 0.475 69) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 25.56 28.989 189)
    (fp_text reference D5 (at 0.25 2 189) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 189) (layer F.Fab))
    (pad 4 smd rect (at 0.475 0.475 189) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
    (pad 3 smd rect (at -0.475 0.475 189) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 1 smd rect (at 0.475 -0.475 189) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at -0.475 -0.475 189) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 36.48 53.515 309)
    (fp_text reference D6 (at 0.25 2 309) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 309) (layer F.Fab))
    (pad 4 smd rect (at 0.475 0.475 309) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
    (pad 3 smd rect (at -0.475 0.475 309) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D3-Pad1)"))
    (pad 1 smd rect (at 0.475 -0.475 309) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at -0.475 -0.475 309) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 50.64 28.989 81)
    (fp_text reference D7 (at 0.25 2 81) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 81) (layer F.Fab))
    (pad 4 smd rect (at 0.475 0.475 81) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
    (pad 3 smd rect (at -0.475 0.475 81) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D4-Pad1)"))
    (pad 1 smd rect (at 0.475 -0.475 81) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D10-Pad3)"))
    (pad 2 smd rect (at -0.475 -0.475 81) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 23.94 31.796 201)
    (fp_text reference D8 (at 0.25 2 201) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 201) (layer F.Fab))
    (pad 2 smd rect (at -0.475 -0.475 201) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at 0.475 -0.475 201) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D11-Pad3)"))
    (pad 3 smd rect (at -0.475 0.475 201) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D5-Pad1)"))
    (pad 4 smd rect (at 0.475 0.475 201) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 39.72 53.515 321)
    (fp_text reference D9 (at 0.25 2 321) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 321) (layer F.Fab))
    (pad 2 smd rect (at -0.475 -0.475 321) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at 0.475 -0.475 321) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D12-Pad3)"))
    (pad 3 smd rect (at -0.475 0.475 321) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D6-Pad1)"))
    (pad 4 smd rect (at 0.475 0.475 321) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 48.472 26.581 93)
    (fp_text reference D10 (at 0.25 2 93) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 93) (layer F.Fab))
    (pad 2 smd rect (at -0.475 -0.475 93) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at 0.475 -0.475 93) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D10-Pad1)"))
    (pad 3 smd rect (at -0.475 0.475 93) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D10-Pad3)"))
    (pad 4 smd rect (at 0.475 0.475 93) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 22.939 34.877 213)
    (fp_text reference D11 (at 0.25 2 213) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 213) (layer F.Fab))
    (pad 4 smd rect (at 0.475 0.475 213) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
    (pad 3 smd rect (at -0.475 0.475 213) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D11-Pad3)"))
    (pad 1 smd rect (at 0.475 -0.475 213) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D11-Pad1)"))
    (pad 2 smd rect (at -0.475 -0.475 213) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 42.89 52.841 333)
    (fp_text reference D12 (at 0.25 2 333) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 333) (layer F.Fab))
    (pad 4 smd rect (at 0.475001 0.475 333) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
    (pad 3 smd rect (at -0.475 0.475001 333) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D12-Pad3)"))
    (pad 1 smd rect (at 0.475 -0.475001 333) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D12-Pad1)"))
    (pad 2 smd rect (at -0.475001 -0.475 333) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 45.85 24.677 105)
    (fp_text reference D13 (at 0.25 2 105) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 105) (layer F.Fab))
    (pad 4 smd rect (at 0.475 0.475 105) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
    (pad 3 smd rect (at -0.475 0.475 105) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D10-Pad1)"))
    (pad 1 smd rect (at 0.475 -0.475 105) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D13-Pad1)"))
    (pad 2 smd rect (at -0.475 -0.475 105) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 22.6 38.1 225)
    (fp_text reference D14 (at 0.25 2 225) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 225) (layer F.Fab))
    (pad 4 smd rect (at 0.475 0.475 225) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
    (pad 3 smd rect (at -0.475 0.475 225) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D11-Pad1)"))
    (pad 1 smd rect (at 0.475 -0.475 225) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D14-Pad1)"))
    (pad 2 smd rect (at -0.475 -0.475 225) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 45.85 51.523 345)
    (fp_text reference D15 (at 0.25 2 345) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 345) (layer F.Fab))
    (pad 2 smd rect (at -0.475 -0.475 345) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at 0.475 -0.475 345) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D15-Pad1)"))
    (pad 3 smd rect (at -0.475 0.475 345) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D12-Pad1)"))
    (pad 4 smd rect (at 0.475 0.475 345) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 42.89 23.359 117)
    (fp_text reference D16 (at 0.25 2 117) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 117) (layer F.Fab))
    (pad 2 smd rect (at -0.475 -0.475001 117) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at 0.475001 -0.475 117) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D16-Pad1)"))
    (pad 3 smd rect (at -0.475001 0.475 117) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D13-Pad1)"))
    (pad 4 smd rect (at 0.475 0.475001 117) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 22.939 41.323 237)
    (fp_text reference D17 (at 0.25 2 237) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 237) (layer F.Fab))
    (pad 2 smd rect (at -0.475 -0.475 237) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at 0.475 -0.475 237) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D17-Pad1)"))
    (pad 3 smd rect (at -0.475 0.475 237) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D14-Pad1)"))
    (pad 4 smd rect (at 0.475 0.475 237) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 48.472 49.619 357)
    (fp_text reference D18 (at 0.25 2 357) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 357) (layer F.Fab))
    (pad 4 smd rect (at 0.475 0.475 357) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
    (pad 3 smd rect (at -0.475 0.475 357) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D15-Pad1)"))
    (pad 1 smd rect (at 0.475 -0.475 357) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D18-Pad1)"))
    (pad 2 smd rect (at -0.475 -0.475 357) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 39.72 22.685 129)
    (fp_text reference D19 (at 0.25 2 129) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 129) (layer F.Fab))
    (pad 4 smd rect (at 0.475 0.475 129) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
    (pad 3 smd rect (at -0.475 0.475 129) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D16-Pad1)"))
    (pad 1 smd rect (at 0.475 -0.475 129) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D19-Pad1)"))
    (pad 2 smd rect (at -0.475 -0.475 129) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 23.94 44.404 249)
    (fp_text reference D20 (at 0.25 2 249) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 249) (layer F.Fab))
    (pad 2 smd rect (at -0.475 -0.475 249) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at 0.475 -0.475 249) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D20-Pad1)"))
    (pad 3 smd rect (at -0.475 0.475 249) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D17-Pad1)"))
    (pad 4 smd rect (at 0.475 0.475 249) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 50.64 47.211 9)
    (fp_text reference D21 (at 0.25 2 9) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 9) (layer F.Fab))
    (pad 2 smd rect (at -0.475 -0.475 9) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at 0.475 -0.475 9) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D21-Pad1)"))
    (pad 3 smd rect (at -0.475 0.475 9) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D18-Pad1)"))
    (pad 4 smd rect (at 0.475 0.475 9) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 36.48 22.685 141)
    (fp_text reference D22 (at 0.25 2 141) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 141) (layer F.Fab))
    (pad 2 smd rect (at -0.475 -0.475 141) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at 0.475 -0.475 141) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D22-Pad1)"))
    (pad 3 smd rect (at -0.475 0.475 141) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D19-Pad1)"))
    (pad 4 smd rect (at 0.475 0.475 141) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 25.56 47.211 261)
    (fp_text reference D23 (at 0.25 2 261) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 261) (layer F.Fab))
    (pad 4 smd rect (at 0.475 0.475 261) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
    (pad 3 smd rect (at -0.475 0.475 261) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D20-Pad1)"))
    (pad 1 smd rect (at 0.475 -0.475 261) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D23-Pad1)"))
    (pad 2 smd rect (at -0.475 -0.475 261) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 52.26 44.404 21)
    (fp_text reference D24 (at 0.25 2 21) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 21) (layer F.Fab))
    (pad 4 smd rect (at 0.475 0.475 21) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
    (pad 3 smd rect (at -0.475 0.475 21) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D21-Pad1)"))
    (pad 1 smd rect (at 0.475 -0.475 21) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D24-Pad1)"))
    (pad 2 smd rect (at -0.475 -0.475 21) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 33.31 23.359 153)
    (fp_text reference D25 (at 0.25 2 153) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 153) (layer F.Fab))
    (pad 4 smd rect (at 0.475001 0.475 153) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
    (pad 3 smd rect (at -0.475 0.475001 153) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D22-Pad1)"))
    (pad 1 smd rect (at 0.475 -0.475001 153) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D25-Pad1)"))
    (pad 2 smd rect (at -0.475001 -0.475 153) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 27.728 49.619 273)
    (fp_text reference D26 (at 0.25 2 273) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 273) (layer F.Fab))
    (pad 2 smd rect (at -0.475 -0.475 273) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at 0.475 -0.475 273) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D26-Pad1)"))
    (pad 3 smd rect (at -0.475 0.475 273) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D23-Pad1)"))
    (pad 4 smd rect (at 0.475 0.475 273) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 53.261 41.323 33)
    (fp_text reference D27 (at 0.25 2 33) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 33) (layer F.Fab))
    (pad 2 smd rect (at -0.475 -0.475 33) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at 0.475 -0.475 33) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D27-Pad1)"))
    (pad 3 smd rect (at -0.475 0.475 33) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D24-Pad1)"))
    (pad 4 smd rect (at 0.475 0.475 33) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 30.35 24.677 165)
    (fp_text reference D28 (at 0.25 2 165) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 165) (layer F.Fab))
    (pad 4 smd rect (at 0.475 0.475 165) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
    (pad 3 smd rect (at -0.475 0.475 165) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D25-Pad1)"))
    (pad 1 smd rect (at 0.475 -0.475 165) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad3)"))
    (pad 2 smd rect (at -0.475 -0.475 165) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 30.35 51.523 285)
    (fp_text reference D29 (at 0.25 2 285) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 285) (layer F.Fab))
    (pad 4 smd rect (at 0.475 0.475 285) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
    (pad 3 smd rect (at -0.475 0.475 285) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D26-Pad1)"))
    (pad 1 smd rect (at 0.475 -0.475 285) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D29-Pad1)"))
    (pad 2 smd rect (at -0.475 -0.475 285) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
  )
  (module lightsaber_footprints:sk6805ec (layer F.Cu) (tedit 5E670C2C)
    (at 53.6 38.1 45)
    (fp_text reference D30 (at 0.25 2 45) (layer F.SilkS) hide)
    (fp_text value SK6805 (at 0.25 -2.25 45) (layer F.Fab))
    (pad 4 smd rect (at 0.475 0.475 45) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad4)"))
    (pad 3 smd rect (at -0.475 0.475 45) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D27-Pad1)"))
    (pad 1 smd rect (at 0.475 -0.475 45) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad3)"))
    (pad 2 smd rect (at -0.475 -0.475 45) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer B.Cu) (tedit 5E670CEC)
    (at 48.006 28.194)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference J1 (at 0 3.81) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 0 -6.35) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 3 3) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(J1-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer B.Cu) (tedit 5E670CD1)
    (at 44.45 26.162 180)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference J2 (at 0 3.81 180) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 0 -6.35 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at 0 0 180) (size 3 3) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(D1-Pad2)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer B.Cu) (tedit 5E670CE6)
    (at 47.244 47.244)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference J3 (at 0 3.81) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 0 -6.35) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 3 3) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(D1-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer B.Cu) (tedit 5E670CDC)
    (at 50.038 31.75)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference J4 (at 0 3.81) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 0 -6.35) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 3 3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D1-Pad4)"))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 45.72 30.48 315)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 1.43 315) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.43 315) (layer B.Fab))
    (fp_text user %R (at 0 0 315) (layer B.Fab))
    (pad 1 smd roundrect (at -0.874999 0 315) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(J1-Pad1)"))
    (pad 2 smd roundrect (at 0.874999 0 315) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(D4-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 25.4 41.402 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 1.43 180) (layer B.SilkS))
    (fp_text value R (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(R3-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 25.4 34.798)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 1.43) (layer B.SilkS))
    (fp_text value R (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(R4-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 34.798 50.8 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 1.43 270) (layer B.SilkS))
    (fp_text value R (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(R5-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(R5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 34.798 25.4 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 1.43 270) (layer B.SilkS))
    (fp_text value R (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(R7-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_circle (center 38.1 38.1) (end 47.2 38.1) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 38.1 38.1) (end 55.1 38.1) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.6 35.6) (xy 58.1 35.6) (xy 58.1 40.6) (xy 40.6 40.6) (xy 40.6 58.1)
        (xy 35.6 58.1) (xy 35.6 40.6) (xy 18.1 40.6) (xy 18.1 35.6) (xy 35.6 35.6)
        (xy 35.6 18.1) (xy 40.6 18.1)
      )
    )
  )
)
