(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu16.04.1)
  (general
    (links 173)
    (no_connects 0)
    (area 98.150001 44.671 215.9326 150.700001)
    (thickness 1.6)
    (drawings 30)
    (tracks 983)
    (zones 0)
    (modules 73)
    (nets 45)
  )
  (page A4)
  (title_block
    (title "Dual Monitoring and Protection Unit")
    (date 2018-05-23)
    (rev 1)
    (company Arqiva)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010ff_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/home/clive/Servers/DOCUMENTS/KiCAD shematics/MHUGHES-M+P/"))
  )
  (net 0 "")
  (net 1 GNDPWR)
  (net 2 "Net-(C6-Pad1)")
  (net 3 "Net-(C7-Pad1)")
  (net 4 "Net-(C8-Pad1)")
  (net 5 "Net-(C9-Pad1)")
  (net 6 "Net-(C10-Pad1)")
  (net 7 "Net-(C11-Pad2)")
  (net 8 "Net-(C12-Pad2)")
  (net 9 "Net-(C13-Pad1)")
  (net 10 "Net-(C14-Pad1)")
  (net 11 "Net-(C15-Pad1)")
  (net 12 "Net-(C16-Pad1)")
  (net 13 "Net-(C17-Pad1)")
  (net 14 "Net-(C19-Pad1)")
  (net 15 "Net-(C20-Pad1)")
  (net 16 "Net-(C21-Pad1)")
  (net 17 "Net-(D4-Pad1)")
  (net 18 "Net-(D4-Pad2)")
  (net 19 "Net-(LK1-Pad1)")
  (net 20 "Net-(LK1-Pad3)")
  (net 21 "Net-(LK1-Pad5)")
  (net 22 "Net-(LK2-Pad2)")
  (net 23 "Net-(LK2-Pad4)")
  (net 24 "Net-(LK2-Pad6)")
  (net 25 "Net-(LK3-Pad2)")
  (net 26 "Net-(LK3-Pad4)")
  (net 27 "Net-(LK3-Pad6)")
  (net 28 "Net-(LK4-Pad1)")
  (net 29 "Net-(LK4-Pad3)")
  (net 30 "Net-(LK4-Pad5)")
  (net 31 "Net-(LK5-Pad1)")
  (net 32 "Net-(LK6-Pad2)")
  (net 33 "Net-(LK9-Pad2)")
  (net 34 "Net-(LK11-Pad1)")
  (net 35 "Net-(Q1-Pad1)")
  (net 36 "Net-(Q2-Pad1)")
  (net 37 "Net-(R12-Pad1)")
  (net 38 Unreg)
  (net 39 12vReg)
  (net 40 8v)
  (net 41 12vOut)
  (net 42 Ext12v)
  (net 43 "Net-(LK13-Pad2)")
  (net 44 "Net-(C22-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(LK1-Pad1)")
    (add_net "Net-(LK1-Pad3)")
    (add_net "Net-(LK1-Pad5)")
    (add_net "Net-(LK11-Pad1)")
    (add_net "Net-(LK13-Pad2)")
    (add_net "Net-(LK2-Pad2)")
    (add_net "Net-(LK2-Pad4)")
    (add_net "Net-(LK2-Pad6)")
    (add_net "Net-(LK3-Pad2)")
    (add_net "Net-(LK3-Pad4)")
    (add_net "Net-(LK3-Pad6)")
    (add_net "Net-(LK4-Pad1)")
    (add_net "Net-(LK4-Pad3)")
    (add_net "Net-(LK4-Pad5)")
    (add_net "Net-(LK5-Pad1)")
    (add_net "Net-(LK6-Pad2)")
    (add_net "Net-(LK9-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(R12-Pad1)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.75)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 12vOut)
    (add_net 12vReg)
    (add_net 8v)
    (add_net Ext12v)
    (add_net GNDPWR)
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C20-Pad1)")
    (add_net Unreg)
  )
  (module TO-252-2aaaaaa (layer F.Cu) (tedit 5B0547C2)
    (at 176.6824 77.47 270)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference Q1p (at 0 -4.5 270) (layer F.SilkS))
    (fp_text value Q_NMOS_GDS (at 0 4.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 2.1844 0 270) (layer F.Fab))
    (pad 1 smd rect (at -4.2 -2.28 270) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -4.2 2.28 270) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C11-Pad2)"))
    (pad 3 smd rect (at 2.1 0 270) (size 6.4 5.8) (layers F.Cu F.Mask)
      (net 15 "Net-(C20-Pad1)"))
    (pad 3 smd rect (at 3.775 1.525 270) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 15 "Net-(C20-Pad1)"))
    (pad 3 smd rect (at 0.425 -1.525 270) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 15 "Net-(C20-Pad1)"))
    (pad 3 smd rect (at 3.775 -1.525 270) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 15 "Net-(C20-Pad1)"))
    (pad 3 smd rect (at 0.425 1.525 270) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 15 "Net-(C20-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 188.0776 65.5744 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 10u (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 Unreg))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 201.0776 65.5744 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 10u (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 39 12vReg))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 188.0776 72.3244 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 38 Unreg))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 201.0776 72.3244 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 39 12vReg))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B057443)
    (at 119.3276 87.0744 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 3.5544 -0.0476 180) (layer F.SilkS))
    (fp_text value 100n (at -4.1672 -0.0476 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 41 12vOut))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B056F23)
    (at 199.0776 84.5744 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 3.4976 -0.3886 180) (layer F.SilkS))
    (fp_text value 10n (at -3.7414 0.2464 180) (layer F.Fab))
    (fp_text user %R (at 2.2276 0.1194 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B056F26)
    (at 199.0776 86.8244 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 3.4976 -0.2976 180) (layer F.SilkS))
    (fp_text value 10n (at -3.8684 0.2104 180) (layer F.Fab))
    (fp_text user %R (at 2.2276 0.0834 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B056F28)
    (at 199.0776 89.0744 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 3.4976 -0.0796 180) (layer F.SilkS))
    (fp_text value 10n (at -3.7414 -0.0796 180) (layer F.Fab))
    (fp_text user %R (at 2.2276 -0.0796 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B056F2B)
    (at 199.0776 91.3244 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 3.3706 -0.2426 180) (layer F.SilkS))
    (fp_text value 10n (at -3.8684 0.0114 180) (layer F.Fab))
    (fp_text user %R (at 2.1006 0.1384 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B05682B)
    (at 179.7536 123.8624 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 5.6254 0.0784 90) (layer F.SilkS))
    (fp_text value 1n (at 3.3394 0.0784 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B2B6C35)
    (at 148.7424 74.6252 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 0.254 1.6764 90) (layer F.SilkS))
    (fp_text value 10n (at 0.3048 2.9972 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 41 12vOut))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C11-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B2B6C84)
    (at 197.1548 123.8504 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 3.9116 1.3208 180) (layer F.SilkS))
    (fp_text value 10n (at 3.8264 -0.1332 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 41 12vOut))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C12-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B0571DE)
    (at 190.5776 134.0744 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 1.6388 1.7004 90) (layer F.SilkS))
    (fp_text value 10n (at -1.8664 1.5988 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B056823)
    (at 177.2536 123.8624 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at 5.6254 0.0384 90) (layer F.SilkS))
    (fp_text value 1n (at 3.3394 0.0384 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 153.5176 129.9464 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 10n (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B056F6B)
    (at 208.5776 103.8244 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C16 (at 2.4566 1.5894 180) (layer F.SilkS))
    (fp_text value 10n (at -2.1154 1.7164 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B05681C)
    (at 174.7536 123.8624 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C17 (at 5.7524 0.2524 90) (layer F.SilkS))
    (fp_text value 1n (at 3.3394 0.1254 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B05745E)
    (at 126.5776 68.3244 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C18 (at 3.7068 0.2192 90) (layer F.SilkS))
    (fp_text value 10n (at -3.5576 -0.0856 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 40 8v))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B2B6C51)
    (at 141.0776 66.8244 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C19 (at 0.0224 -1.5808 90) (layer F.SilkS))
    (fp_text value 10n (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C19-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B2B6C44)
    (at 143.5608 72.644 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C20 (at 3.6576 1.9304 90) (layer F.SilkS))
    (fp_text value 10n (at 3.6068 0.5588 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C20-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 190.0776 95.0744 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C21 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 10n (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C21-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5B2B6C10)
    (at 141.2748 72.6948 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 0.8636 -1.6764 90) (layer F.SilkS))
    (fp_text value D_Small (at -5.1264 -0.5366 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C20-Pad1)"))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5B2B6C1E)
    (at 146.4564 74.6252 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at -1.7272 -1.7272 90) (layer F.SilkS))
    (fp_text value D_Small (at 0 2.1 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 41 12vOut))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C11-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5B2B6C7D)
    (at 197.2056 126.0348 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D3 (at 3.4036 -0.4572 180) (layer F.SilkS))
    (fp_text value D_Small (at -5.3772 -0.0936 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2 180) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 41 12vOut))
    (pad 2 smd rect (at 1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C12-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5B057198)
    (at 185.5776 128.9244 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D4 (at 0 -2 90) (layer F.SilkS))
    (fp_text value D_Small (at 0 2.1 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5B05734A)
    (at 136.5376 92.5744)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference LK1 (at 5.4992 -0.5756) (layer F.SilkS))
    (fp_text value CONN_3X2 (at 1.27 7.41) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(LK1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C6-Pad1)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(LK1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C6-Pad1)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(LK1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5B057368)
    (at 120.6176 97.6544 180)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference LK2 (at -2.9788 5.6556 180) (layer F.SilkS))
    (fp_text value CONN_3X2 (at 1.27 7.41 180) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C7-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(LK2-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C7-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(LK2-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C7-Pad1)"))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(LK2-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5B057350)
    (at 120.5776 110.1544 180)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference LK3 (at -3.0188 5.7096 180) (layer F.SilkS))
    (fp_text value CONN_3X2 (at 1.27 7.41 180) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C8-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(LK3-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C8-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(LK3-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C8-Pad1)"))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(LK3-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5B057356)
    (at 136.5776 105.0744)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference LK4 (at 5.4592 -0.5788) (layer F.SilkS))
    (fp_text value CONN_3X2 (at 1.27 7.41) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(LK4-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C9-Pad1)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(LK4-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C9-Pad1)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(LK4-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5B056EF9)
    (at 188.5376 89.5744 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference LK5 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_2 (at 0 4.87 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(LK5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 8v))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5B056849)
    (at 162.0376 99.5744 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference LK6 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_3 (at 0 7.41 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C6-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(LK6-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5B056856)
    (at 162.0376 90.0744 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference LK7 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_3 (at 0 7.41 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C7-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(C16-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5B056845)
    (at 161.9976 106.5744 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference LK8 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_3 (at 0 7.41 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C8-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(C21-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5B05683D)
    (at 161.9976 114.5744 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference LK9 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_3 (at 0 7.41 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C9-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(LK9-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5B056EF5)
    (at 188.5376 106.5744 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference LK10 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_2 (at 0 4.87 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.114 1.472 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(C13-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5B056EF0)
    (at 188.5776 98.5744 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference LK11 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_2 (at 0 4.87 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(LK11-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 8v))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5B056E52)
    (at 161.9976 83.0744 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference LK12 (at 2.0484 2.4674 180) (layer F.SilkS))
    (fp_text value CONN_3 (at 0 7.41 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 Ext12v))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 12vOut))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 12vReg))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2 (layer F.Cu) (tedit 5B053609)
    (at 179.0526 68.9994 90)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference Q1n (at 0 -4.5 90) (layer F.SilkS))
    (fp_text value Q_NMOS_GDS (at 0 4.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.6226 0.119 90) (layer F.Fab))
    (pad 1 smd rect (at -4.2 -2.28 90) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q1-Pad1)"))
    (pad 3 smd rect (at -4.2 2.28 90) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C20-Pad1)"))
    (pad 2 smd rect (at 2.1 0 90) (size 6.4 5.8) (layers F.Cu F.Mask)
      (net 7 "Net-(C11-Pad2)"))
    (pad 2 smd rect (at 3.775 1.525 90) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 7 "Net-(C11-Pad2)"))
    (pad 2 smd rect (at 0.425 -1.525 90) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 7 "Net-(C11-Pad2)"))
    (pad 2 smd rect (at 3.775 -1.525 90) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 7 "Net-(C11-Pad2)"))
    (pad 2 smd rect (at 0.425 1.525 90) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 7 "Net-(C11-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2 (layer F.Cu) (tedit 5B056850)
    (at 180.1876 102.5144 270)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference Q2 (at 0 -4.5 270) (layer F.SilkS))
    (fp_text value Q_NMOS_GDS (at 0 4.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -4.2 -2.28 270) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(Q2-Pad1)"))
    (pad 3 smd rect (at -4.2 2.28 270) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (pad 2 smd rect (at 2.1 0 270) (size 6.4 5.8) (layers F.Cu F.Mask)
      (net 8 "Net-(C12-Pad2)"))
    (pad 2 smd rect (at 3.775 1.525 270) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 8 "Net-(C12-Pad2)"))
    (pad 2 smd rect (at 0.425 -1.525 270) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 8 "Net-(C12-Pad2)"))
    (pad 2 smd rect (at 3.775 -1.525 270) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 8 "Net-(C12-Pad2)"))
    (pad 2 smd rect (at 0.425 1.525 270) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 8 "Net-(C12-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B056F5D)
    (at 208.5776 109.0744 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 2.8376 -0.1456 180) (layer F.SilkS))
    (fp_text value 47K (at -1.9884 -1.4156 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C22-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B0571EB)
    (at 188.0776 134.1744 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -2.7824 -0.8288 90) (layer F.SilkS))
    (fp_text value 47K (at -2.376 1.1016 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B0571FB)
    (at 188.0776 128.9744 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 1.48 -1.4572 270) (layer F.SilkS))
    (fp_text value 47K (at -1.1616 -1.4572 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B057187)
    (at 185.5776 134.0744 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -0.7244 1.4276 270) (layer F.SilkS))
    (fp_text value 1k (at 1.8156 1.4276 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C13-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B056835)
    (at 172.0596 123.8504 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 5.3594 0.1524 90) (layer F.SilkS))
    (fp_text value 1k (at 3.3274 0.1524 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(LK13-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 185.5776 123.5744 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value 1k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 192.1776 76.5744 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 8v))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 12vOut))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B056F65)
    (at 208.5776 107.0744 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 2.8376 1.2834 180) (layer F.SilkS))
    (fp_text value 10k (at -0.8454 1.5374 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(LK11-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 190.1776 92.5744 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C21-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(LK5-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 163.6776 76.6064)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 6k8 (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 12vOut))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B057260)
    (at 140.3096 129.6924 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at -6.4008 0.1524 90) (layer F.SilkS))
    (fp_text value 1k (at -3.6068 0.1524 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 41 12vOut))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B056915)
    (at 159.0776 79.5744)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at -2.9946 1.5786) (layer F.SilkS))
    (fp_text value 2k7 (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R12-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B056926)
    (at 159.1056 76.6064 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 2.8956 1.5494 180) (layer F.SilkS))
    (fp_text value 2k7 (at -0.5334 1.5494 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Multicomp:Multicomp_MC9A12-1034_2x05x2.54mm_Straight (layer F.Cu) (tedit 5B2B6D09)
    (at 207.5776 85.5744 270)
    (descr http://www.farnell.com/datasheets/1520732.pdf)
    (tags "connector multicomp MC9A MC9A12")
    (fp_text reference SK1 (at -3.5832 4.1744 270) (layer F.SilkS))
    (fp_text value HE10-10 (at 5.08 5 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C7-Pad1)"))
    (pad 4 thru_hole circle (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
    (pad 5 thru_hole circle (at 5.08 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C8-Pad1)"))
    (pad 6 thru_hole circle (at 5.08 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
    (pad 7 thru_hole circle (at 7.62 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C9-Pad1)"))
    (pad 8 thru_hole circle (at 7.62 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
    (pad 9 thru_hole circle (at 10.16 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(R12-Pad1)"))
    (pad 10 thru_hole circle (at 10.16 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
  )
  (module Connectors_Multicomp:Multicomp_MC9A12-1034_2x05x2.54mm_Straight (layer F.Cu) (tedit 5B2B6CFC)
    (at 207.5776 116.5744 270)
    (descr http://www.farnell.com/datasheets/1520732.pdf)
    (tags "connector multicomp MC9A MC9A12")
    (fp_text reference SK2 (at -3.5444 4.1744 270) (layer F.SilkS))
    (fp_text value HE10-10 (at 5.08 5 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(C16-Pad1)"))
    (pad 2 thru_hole circle (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(LK6-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(C21-Pad1)"))
    (pad 4 thru_hole circle (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(LK9-Pad2)"))
    (pad 5 thru_hole circle (at 5.08 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(C19-Pad1)"))
    (pad 6 thru_hole circle (at 5.08 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
    (pad 7 thru_hole circle (at 7.62 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(C22-Pad1)"))
    (pad 8 thru_hole circle (at 7.62 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
    (pad 9 thru_hole circle (at 10.16 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(C10-Pad1)"))
    (pad 10 thru_hole circle (at 10.16 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
  )
  (module Connectors_Multicomp:Multicomp_MC9A12-1034_2x05x2.54mm_Straight (layer F.Cu) (tedit 5B2B6D4B)
    (at 117.9576 69.4944 270)
    (descr http://www.farnell.com/datasheets/1520732.pdf)
    (tags "connector multicomp MC9A MC9A12")
    (fp_text reference SK3 (at -3.3528 -6.9596 270) (layer F.SilkS))
    (fp_text value HE10-10 (at 5.08 5 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(LK2-Pad2)"))
    (pad 2 thru_hole circle (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(LK1-Pad1)"))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(LK2-Pad4)"))
    (pad 4 thru_hole circle (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(LK1-Pad3)"))
    (pad 5 thru_hole circle (at 5.08 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(LK2-Pad6)"))
    (pad 6 thru_hole circle (at 5.08 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(LK1-Pad5)"))
    (pad 7 thru_hole circle (at 7.62 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
    (pad 8 thru_hole circle (at 7.62 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
    (pad 9 thru_hole circle (at 10.16 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 12vOut))
    (pad 10 thru_hole circle (at 10.16 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 12vOut))
  )
  (module Connectors_Multicomp:Multicomp_MC9A12-1034_2x05x2.54mm_Straight (layer F.Cu) (tedit 5B2B6D3A)
    (at 117.9576 120.9144 270)
    (descr http://www.farnell.com/datasheets/1520732.pdf)
    (tags "connector multicomp MC9A MC9A12")
    (fp_text reference SK4 (at 12.9944 -7.0612 450) (layer F.SilkS))
    (fp_text value HE10-10 (at 5.08 5 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(LK3-Pad2)"))
    (pad 2 thru_hole circle (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(LK4-Pad1)"))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(LK3-Pad4)"))
    (pad 4 thru_hole circle (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(LK4-Pad3)"))
    (pad 5 thru_hole circle (at 5.08 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(LK3-Pad6)"))
    (pad 6 thru_hole circle (at 5.08 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(LK4-Pad5)"))
    (pad 7 thru_hole circle (at 7.62 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
    (pad 8 thru_hole circle (at 7.62 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
    (pad 9 thru_hole circle (at 10.16 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 12vOut))
    (pad 10 thru_hole circle (at 10.16 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 12vOut))
  )
  (module Connectors_JST:JST_EH_S02B-EH_02x2.50mm_Angled (layer F.Cu) (tedit 5B05670F)
    (at 163.7176 70.0024)
    (descr "JST EH series connector, S02B-EH, 2.50mm pitch, side entry")
    (tags "connector jst eh side horizontal angled")
    (fp_text reference SK5 (at 1.25 3) (layer F.SilkS))
    (fp_text value CONN_2 (at 1.25 -8) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 -2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 38 Unreg))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
    (model Connectors_JST.3dshapes/JST_EH_S02B-EH_02x2.50mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_EH_S02B-EH_02x2.50mm_Angled (layer F.Cu) (tedit 5B2B6BF1)
    (at 149.9616 70.0024)
    (descr "JST EH series connector, S02B-EH, 2.50mm pitch, side entry")
    (tags "connector jst eh side horizontal angled")
    (fp_text reference SK6 (at -4.6228 -6.1976) (layer F.SilkS))
    (fp_text value CONN_2 (at 1.25 -8) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 -2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 42 Ext12v))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
    (model Connectors_JST.3dshapes/JST_EH_S02B-EH_02x2.50mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_EH_S02B-EH_02x2.50mm_Angled (layer F.Cu) (tedit 5B2B6C77)
    (at 198.5264 129.6924 180)
    (descr "JST EH series connector, S02B-EH, 2.50mm pitch, side entry")
    (tags "connector jst eh side horizontal angled")
    (fp_text reference SK7 (at -4.318 -4.0132 180) (layer F.SilkS))
    (fp_text value CONN_2 (at 1.25 -8 180) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 -2 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 41 12vOut))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(C12-Pad2)"))
    (model Connectors_JST.3dshapes/JST_EH_S02B-EH_02x2.50mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_EH_S04B-EH_04x2.50mm_Angled (layer F.Cu) (tedit 5B33636A)
    (at 179.5596 129.6924 180)
    (descr "JST EH series connector, S04B-EH, 2.50mm pitch, side entry")
    (tags "connector jst eh side horizontal angled")
    (fp_text reference SK9 (at -0.3504 3.0824 180) (layer F.SilkS))
    (fp_text value CONN_4 (at 3.75 -8 180) (layer F.Fab) hide)
    (fp_text user %R (at 3.75 -2 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(C14-Pad1)"))
    (pad 3 thru_hole circle (at 5 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 "Net-(C17-Pad1)"))
    (pad 4 thru_hole circle (at 7.5 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
    (model Connectors_JST.3dshapes/JST_EH_S04B-EH_04x2.50mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_EH_S03B-EH_03x2.50mm_Angled (layer F.Cu) (tedit 5B2B6BE6)
    (at 131.0776 70.0744)
    (descr "JST EH series connector, S03B-EH, 2.50mm pitch, side entry")
    (tags "connector jst eh side horizontal angled")
    (fp_text reference SK11 (at -1.436 2.8236) (layer F.SilkS))
    (fp_text value CONN_3 (at 2.5 -8) (layer F.Fab) hide)
    (fp_text user %R (at 2.5 -2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 40 8v))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(C19-Pad1)"))
    (pad 3 thru_hole circle (at 5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
    (model Connectors_JST.3dshapes/JST_EH_S03B-EH_03x2.50mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2 (layer F.Cu) (tedit 590079C0)
    (at 194.0776 69.0744 90)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference U1 (at 0 -4.5 90) (layer F.SilkS))
    (fp_text value L7812 (at 0 4.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.2 -2.28 90) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 38 Unreg))
    (pad 3 smd rect (at -4.2 2.28 90) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 39 12vReg))
    (pad 2 smd rect (at 2.1 0 90) (size 6.4 5.8) (layers F.Cu F.Mask)
      (net 1 GNDPWR))
    (pad 2 smd rect (at 3.775 1.525 90) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 1 GNDPWR))
    (pad 2 smd rect (at 0.425 -1.525 90) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 1 GNDPWR))
    (pad 2 smd rect (at 3.775 -1.525 90) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 1 GNDPWR))
    (pad 2 smd rect (at 0.425 1.525 90) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 1 GNDPWR))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0805 (layer F.Cu) (tedit 590CE9A4)
    (at 197.0776 76.5744)
    (descr "Diode SMD in 0805 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (attr smd)
    (fp_text reference ZD1 (at 0 -1.6) (layer F.SilkS))
    (fp_text value 8v2 (at 0 1.7) (layer F.Fab))
    (fp_text user %R (at 0 -1.6) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 8v))
    (pad 2 smd rect (at 1.05 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_EH_S02B-EH_02x2.50mm_Angled (layer F.Cu) (tedit 5B05671E)
    (at 206.8576 66.9544 270)
    (descr "JST EH series connector, S02B-EH, 2.50mm pitch, side entry")
    (tags "connector jst eh side horizontal angled")
    (fp_text reference SK10 (at 1.25 3 270) (layer F.SilkS))
    (fp_text value CONN_2 (at 1.25 -8 270) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 -2 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 38 Unreg))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
    (model Connectors_JST.3dshapes/JST_EH_S02B-EH_02x2.50mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_EH_S02B-EH_02x2.50mm_Angled (layer F.Cu) (tedit 5B05679B)
    (at 147.6756 129.4384 180)
    (descr "JST EH series connector, S02B-EH, 2.50mm pitch, side entry")
    (tags "connector jst eh side horizontal angled")
    (fp_text reference SK8 (at 1.25 3 180) (layer F.SilkS))
    (fp_text value CONN_2 (at 1.25 -8 180) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 -2 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(C15-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
    (model Connectors_JST.3dshapes/JST_EH_S02B-EH_02x2.50mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5B058B53)
    (at 177.3936 85.1154 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference LK13 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_3 (at 0 7.41 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(C20-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(LK13-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(C22-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5B057452)
    (at 130 77)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at -0.3584 -2.7304) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5B0572C9)
    (at 130 121)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 3.9088 -5.684) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5B056EE8)
    (at 201 99)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at -5.42 2.6) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 180.3908 92.2528 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C22 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 10n (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C22-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_EH_B02B-EH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5B2B6CD5)
    (at 141.732 81.4324 180)
    (descr "JST EH series connector, B02B-EH-A, 2.50mm pitch, top entry")
    (tags "connector jst eh top vertical straight")
    (fp_text reference SK12 (at 1.27 -2.8956 180) (layer F.SilkS))
    (fp_text value CONN_2 (at 1.25 3.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 -3 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(C20-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GNDPWR))
    (model Connectors_JST.3dshapes/JST_EH_B02B-EH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_EH_B02B-EH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5B2B6201)
    (at 151.1808 81.3308 180)
    (descr "JST EH series connector, B02B-EH-A, 2.50mm pitch, top entry")
    (tags "connector jst eh top vertical straight")
    (fp_text reference SK13 (at 1.25 -3 180) (layer F.SilkS))
    (fp_text value CONN_2 (at 1.25 3.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 -3 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 41 12vOut))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(C11-Pad2)"))
    (model Connectors_JST.3dshapes/JST_EH_B02B-EH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text CDT2018 (at 145.9484 100.076 270) (layer F.SilkS))
  (gr_text "Monitoring and Protection\n  Dual Monitor Mk1" (at 154.8384 98.9584 270) (layer F.SilkS))
  (gr_text "FWD\nPWR\nSET" (at 134.4676 75.2348) (layer F.SilkS))
  (gr_text Detectors (at 124.9172 119.9388 90) (layer F.SilkS))
  (gr_text Detectors (at 125.0696 79.5528 90) (layer F.SilkS))
  (gr_text " Range\nSelector" (at 128.4732 99.2124) (layer F.SilkS))
  (gr_text "Trip RLY" (at 204.5716 136.0932) (layer F.SilkS))
  (gr_text "Dehydrator ALM in" (at 146.7612 124.1044) (layer F.SilkS))
  (gr_text LEDs (at 171.98 126.87) (layer F.SilkS))
  (gr_text "Link\nQ1=N" (at 140.462 87.5792) (layer F.SilkS))
  (gr_text "Link\nQ1=P" (at 149.86 87.5284) (layer F.SilkS))
  (gr_text "   MOXA \nCONNECTORS" (at 212.344 106.2228 90) (layer F.SilkS))
  (gr_text "UNREG in" (at 161.544 85.09) (layer F.SilkS))
  (gr_text "12v in" (at 167.005 85.09) (layer F.SilkS))
  (gr_text "EXT 12v in" (at 156.6164 68.1736 270) (layer F.SilkS))
  (gr_text "EXT PWR" (at 170.434 67.31 270) (layer F.SilkS))
  (dimension 101.6 (width 0.3) (layer Dwgs.User)
    (gr_text "4.0000 in" (at 163.703 46.021) (layer Dwgs.User))
    (feature1 (pts (xy 112.903 61.849) (xy 112.903 44.671)))
    (feature2 (pts (xy 214.503 61.849) (xy 214.503 44.671)))
    (crossbar (pts (xy 214.503 47.371) (xy 112.903 47.371)))
    (arrow1a (pts (xy 112.903 47.371) (xy 114.029504 46.784579)))
    (arrow1b (pts (xy 112.903 47.371) (xy 114.029504 47.957421)))
    (arrow2a (pts (xy 214.503 47.371) (xy 213.376496 46.784579)))
    (arrow2b (pts (xy 214.503 47.371) (xy 213.376496 47.957421)))
  )
  (dimension 101.6 (width 0.3) (layer Dwgs.User)
    (gr_text "101.600 mm" (at 163.703 54.657) (layer Dwgs.User))
    (feature1 (pts (xy 112.903 61.849) (xy 112.903 53.307)))
    (feature2 (pts (xy 214.503 61.849) (xy 214.503 53.307)))
    (crossbar (pts (xy 214.503 56.007) (xy 112.903 56.007)))
    (arrow1a (pts (xy 112.903 56.007) (xy 114.029504 55.420579)))
    (arrow1b (pts (xy 112.903 56.007) (xy 114.029504 56.593421)))
    (arrow2a (pts (xy 214.503 56.007) (xy 213.376496 55.420579)))
    (arrow2b (pts (xy 214.503 56.007) (xy 213.376496 56.593421)))
  )
  (dimension 17 (width 0.3) (layer Dwgs.User)
    (gr_text "17.000 mm" (at 104.65 129.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 130 138) (xy 103.3 138)))
    (feature2 (pts (xy 130 121) (xy 103.3 121)))
    (crossbar (pts (xy 106 121) (xy 106 138)))
    (arrow1a (pts (xy 106 138) (xy 105.413579 136.873496)))
    (arrow1b (pts (xy 106 138) (xy 106.586421 136.873496)))
    (arrow2a (pts (xy 106 121) (xy 105.413579 122.126504)))
    (arrow2b (pts (xy 106 121) (xy 106.586421 122.126504)))
  )
  (dimension 71 (width 0.3) (layer Dwgs.User)
    (gr_text "71.000 mm" (at 165.5 149.35) (layer Dwgs.User))
    (feature1 (pts (xy 130 99) (xy 130 150.7)))
    (feature2 (pts (xy 201 99) (xy 201 150.7)))
    (crossbar (pts (xy 201 148) (xy 130 148)))
    (arrow1a (pts (xy 130 148) (xy 131.126504 147.413579)))
    (arrow1b (pts (xy 130 148) (xy 131.126504 148.586421)))
    (arrow2a (pts (xy 201 148) (xy 199.873496 147.413579)))
    (arrow2b (pts (xy 201 148) (xy 199.873496 148.586421)))
  )
  (dimension 44 (width 0.3) (layer Dwgs.User)
    (gr_text "44.000 mm" (at 105.65 99 90) (layer Dwgs.User))
    (feature1 (pts (xy 130 77) (xy 104.3 77)))
    (feature2 (pts (xy 130 121) (xy 104.3 121)))
    (crossbar (pts (xy 107 121) (xy 107 77)))
    (arrow1a (pts (xy 107 77) (xy 107.586421 78.126504)))
    (arrow1b (pts (xy 107 77) (xy 106.413579 78.126504)))
    (arrow2a (pts (xy 107 121) (xy 107.586421 119.873496)))
    (arrow2b (pts (xy 107 121) (xy 106.413579 119.873496)))
  )
  (gr_line (start 112.8776 61.8744) (end 214.4776 61.8744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.8776 138.0744) (end 112.8776 61.8744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 214.4776 138.0744) (end 112.8776 138.0744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 214.4776 61.8744) (end 214.4776 138.0744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Unreg\nPWR" (at 210.5776 74.5744) (layer F.SilkS))
  (gr_line (start 112.8776 138.0744) (end 112.8776 61.8744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 214.4776 138.0744) (end 112.8776 138.0744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 214.4776 61.8744) (end 214.4776 138.0744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.8776 61.8744) (end 214.4776 61.8744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GNDPWR) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 214.4776 138.0744) (xy 112.8776 138.0744) (xy 112.8776 61.8744) (xy 214.4776 61.8744)
      )
    )
  )
  (zone (net 1) (net_name GNDPWR) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 214.4776 138.0744) (xy 112.8776 138.0744) (xy 112.8776 61.8744) (xy 214.4776 61.8744)
      )
    )
  )
)
