(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-1")
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 16)
    (zones 0)
    (modules 7)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.762)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.762)
    (via_size 1.016)
    (via_drill 0.635)
    (via_min_size 0.254)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 76.2 127)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(SW1-Pad1)")
  (net 4 "Net-(SW1-Pad2)")
  (net 5 "Net-(XBT1-Pad2)")
  (net 6 "Net-(XBT2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.762)
    (via_dia 1.016)
    (via_drill 0.635)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.762)
    (diff_pair_gap 0.25)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(SW1-Pad1)")
    (add_net "Net-(SW1-Pad2)")
    (add_net "Net-(XBT1-Pad2)")
    (add_net "Net-(XBT2-Pad2)")
  )
  (module IPC_MFG:KEYSTONE_1294 (layer F.Cu) (tedit 5D3495A6)
    (at 92.71 71.755)
    (fp_text reference XBT3 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 1249 (at 16.51 38.735 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 11.9126 37.465) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -11.9126 37.465) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 11.9126 15.24) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -11.9126 15.24) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 6.35 0) (size 3.81 3.81) (drill 2.159) (layers *.Cu *.Mask)
      (net 6 "Net-(XBT2-Pad2)"))
    (pad 2 thru_hole circle (at -6.35 0) (size 3.81 3.81) (drill 2.159) (layers *.Cu *.Mask)
      (net 4 "Net-(SW1-Pad2)"))
  )
  (module IPC_MFG:KEYSTONE_1294 (layer F.Cu) (tedit 5D3495A6)
    (at 163.83 71.755)
    (fp_text reference XBT1 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 1249 (at 16.51 51.435 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 11.9126 37.465) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -11.9126 37.465) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 11.9126 15.24) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -11.9126 15.24) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 6.35 0) (size 3.81 3.81) (drill 2.159) (layers *.Cu *.Mask)
      (net 3 "Net-(SW1-Pad1)"))
    (pad 2 thru_hole circle (at -6.35 0) (size 3.81 3.81) (drill 2.159) (layers *.Cu *.Mask)
      (net 5 "Net-(XBT1-Pad2)"))
  )
  (module IPC_MFG:KEYSTONE_1294 (layer F.Cu) (tedit 5D3495A6)
    (at 133.35 71.755)
    (fp_text reference XBT2 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 1249 (at -16.51 38.735 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 11.9126 37.465) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -11.9126 37.465) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 11.9126 15.24) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -11.9126 15.24) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 6.35 0) (size 3.81 3.81) (drill 2.159) (layers *.Cu *.Mask)
      (net 5 "Net-(XBT1-Pad2)"))
    (pad 2 thru_hole circle (at -6.35 0) (size 3.81 3.81) (drill 2.159) (layers *.Cu *.Mask)
      (net 6 "Net-(XBT2-Pad2)"))
  )
  (module MountingHole:MountingHole_5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 184.15 76.2)
    (descr "Mounting Hole 5mm, no annular")
    (tags "mounting hole 5mm no annular")
    (attr virtual)
    (fp_text reference H2 (at 0 -6) (layer F.SilkS))
    (fp_text value MountingHole (at 0 6) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 5 5) (drill 5) (layers *.Cu *.Mask))
  )
  (module Connector_Pheonix_MSTBA:PheonixContact_MSTBA_1x02_P5.08_Horizontal (layer F.Cu) (tedit 5D32800B)
    (at 193.675 81.28 90)
    (fp_text reference J1 (at 0 -3.5 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 0 11.5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 4.508 4.508) (drill 2.8) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 4.508 4.508) (drill 2.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
  )
  (module IPC_MFG:CKSWITCHES_DF62J12S2AHQA (layer F.Cu) (tedit 5D33B574)
    (at 199.39 110.49 180)
    (fp_text reference SW1 (at 7.62 -13.97) (layer F.SilkS))
    (fp_text value DPST (at 7.62 13.97) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 -11.3792 180) (size 2.764 2.764) (drill 1.905) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 12.7254 -5.9436 180) (size 2.764 2.764) (drill 1.905) (layers *.Cu *.Mask)
      (net 3 "Net-(SW1-Pad1)"))
    (pad 1A thru_hole circle (at 12.7254 5.9436 180) (size 2.764 2.764) (drill 1.905) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 17.6784 -5.9436 180) (size 2.764 2.764) (drill 1.905) (layers *.Cu *.Mask)
      (net 4 "Net-(SW1-Pad2)"))
    (pad 2A thru_hole circle (at 17.6784 5.9436 180) (size 2.764 2.764) (drill 1.905) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 4 thru_hole circle (at 0 11.3792 180) (size 2.764 2.764) (drill 1.905) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 113.03 119.38)
    (descr "Mounting Hole 5mm, no annular")
    (tags "mounting hole 5mm no annular")
    (attr virtual)
    (fp_text reference H1 (at 0 -6) (layer F.SilkS))
    (fp_text value MountingHole (at 0 6) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 5 5) (drill 5) (layers *.Cu *.Mask))
  )
  (gr_text "BATTERY PACK - 27 VDC" (at 133.35 123.19) (layer B.SilkS))
  (gr_line (start 201.93 127) (end 76.2 127) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 201.93 68.58) (end 201.93 127) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 76.2 68.58) (end 201.93 68.58) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 76.2 127) (end 76.2 68.58) (layer Edge.Cuts) (width 0.05))
)
