<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="36.068" y1="18.796" x2="0.33" y2="18.796" width="0" layer="20"/>
<wire x1="0.33" y1="18.796" x2="0.33" y2="0.518" width="0" layer="20"/>
<wire x1="0.33" y1="0.518" x2="36.068" y2="0.518" width="0" layer="20"/>
<wire x1="36.068" y1="0.518" x2="36.068" y2="18.796" width="0" layer="20"/>
<text>PiTAG-AVR</text>
<text>false.ekta.is 2013</text>
<text>(OpenOCD sysfs adapter)</text>
<text>##STM32</text>
</plain>
<libraries>
<library name="karl-raspi-header">
<packages>
<package name="RASBERRYPI_SHIELD">
</package>
</packages>
</library>
<library name="cortex_10pin">
<packages>
<package name="2X10-50MIL-JTAG">
<description>2x5 50mil (1.27mm) AVR-JTAG pinout
&lt;p/&gt;
Should also work for cortex debug, same size, but different pinout</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$3" library="karl-raspi-header" package="RASBERRYPI_SHIELD" value="RASPBERRYPI_BB"/>
<element name="U$1" library="cortex_10pin" package="2X10-50MIL-JTAG" value="JTAG-AVR"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$3" pad="6"/>
<contactref element="U$1" pad="P$2"/>
<contactref element="U$1" pad="P$10"/>
</signal>
<signal name="TMS">
<contactref element="U$3" pad="22"/>
<contactref element="U$1" pad="P$5"/>
</signal>
<signal name="TCK">
<contactref element="U$3" pad="23"/>
<contactref element="U$1" pad="P$1"/>
</signal>
<signal name="TDO">
<contactref element="U$3" pad="21"/>
<contactref element="U$1" pad="P$3"/>
</signal>
<signal name="TDI">
<contactref element="U$3" pad="19"/>
<contactref element="U$1" pad="P$9"/>
</signal>
<signal name="SRST">
<contactref element="U$3" pad="18"/>
<contactref element="U$1" pad="P$6"/>
</signal>
<signal name="TRST">
<contactref element="U$3" pad="26"/>
<contactref element="U$1" pad="P$8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
