<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="103.81" y2="0" width="0" layer="20"/>
<wire x1="103.81" y1="0" x2="103.81" y2="8.88" width="0" layer="20"/>
<wire x1="103.81" y1="8.88" x2="0" y2="8.88" width="0" layer="20"/>
<wire x1="0" y1="8.88" x2="0" y2="0" width="0" layer="20"/>
<text>www.TelescopeLab.com</text>
<hole x="8.89" y="3.302" drill="1.6"/>
<hole x="94.742" y="5.08" drill="1.6"/>
<hole x="46.482" y="6.096" drill="1.6"/>
<text>USE APPROPRIATE RESISTORS
       FOR VOLTAGE</text>
<text>5.1v (USB) 220ohm
14v (Car Batt) 620ohm</text>
<text>SPAC Optical Lab</text>
</plain>
<libraries>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,17/1,3">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="led" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="led" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="led" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="led" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+" library="wirepad" package="3,17/1,3" value="WIREPAD3,17/1,3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="-" library="wirepad" package="3,17/1,3" value="WIREPAD3,17/1,3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$5">
<contactref element="R5" pad="P$2"/>
<contactref element="LED5" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="P$2"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="P$2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="P$2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="5V">
<contactref element="+" pad="1"/>
<contactref element="R1" pad="P$1"/>
<contactref element="R5" pad="P$1"/>
<contactref element="R4" pad="P$1"/>
<contactref element="R3" pad="P$1"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="GND">
<contactref element="-" pad="1"/>
<contactref element="LED1" pad="K"/>
<contactref element="LED5" pad="K"/>
<contactref element="LED4" pad="K"/>
<contactref element="LED3" pad="K"/>
<contactref element="LED2" pad="K"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="P$2"/>
<contactref element="LED1" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
