(kicad_pcb (version 20171130) (host pcbnew "(5.1.0)-1")
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 745)
    (zones 0)
    (modules 54)
    (nets 57)
  )
  (page A4)
  (title_block
    (title "AM 3090")
    (rev v01)
    (comment 4 "Author: Tristan Neugebauer")
  )
  (layers
    (0 F.Cu signal)
    (1 GND signal)
    (2 PWR signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFDFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(AM1-Pad1)")
  (net 3 "Net-(AM1-Pad2)")
  (net 4 "Net-(AM1-Pad3)")
  (net 5 "Net-(AM1-Pad4)")
  (net 6 "Net-(AM1-Pad5)")
  (net 7 "Net-(AM1-Pad6)")
  (net 8 "Net-(AM1-Pad8)")
  (net 9 "Net-(AM1-Pad9)")
  (net 10 "Net-(AM1-Pad10)")
  (net 11 "Net-(AM1-Pad11)")
  (net 12 "Net-(AM1-Pad12)")
  (net 13 "Net-(AM1-Pad13)")
  (net 14 "Net-(AM1-Pad16)")
  (net 15 "Net-(AM1-Pad18)")
  (net 16 "Net-(AM1-Pad19)")
  (net 17 "Net-(AM1-Pad21)")
  (net 18 "Net-(AM1-Pad22)")
  (net 19 "Net-(AM1-Pad23)")
  (net 20 "Net-(AM1-Pad24)")
  (net 21 "Net-(AM1-Pad25)")
  (net 22 "Net-(AM1-Pad26)")
  (net 23 "Net-(AM1-Pad27)")
  (net 24 "Net-(AM1-Pad28)")
  (net 25 "Net-(AM1-Pad29)")
  (net 26 "Net-(AM1-Pad30)")
  (net 27 "Net-(AM1-Pad31)")
  (net 28 "Net-(AM1-Pad32)")
  (net 29 "Net-(AM1-Pad33)")
  (net 30 "Net-(AM1-Pad34)")
  (net 31 "Net-(AM1-Pad37)")
  (net 32 "Net-(AM1-Pad39)")
  (net 33 "Net-(AM1-Pad40)")
  (net 34 "Net-(C5-Pad1)")
  (net 35 "Net-(C6-Pad1)")
  (net 36 "Net-(C7-Pad1)")
  (net 37 "Net-(C8-Pad1)")
  (net 38 "Net-(C9-Pad1)")
  (net 39 "Net-(C16-Pad1)")
  (net 40 "Net-(C17-Pad1)")
  (net 41 "Net-(C18-Pad1)")
  (net 42 "Net-(C19-Pad1)")
  (net 43 "Net-(C20-Pad1)")
  (net 44 "Net-(R1-Pad2)")
  (net 45 "Net-(R2-Pad2)")
  (net 46 "Net-(R3-Pad2)")
  (net 47 "Net-(R4-Pad2)")
  (net 48 "Net-(R5-Pad2)")
  (net 49 "Net-(R11-Pad1)")
  (net 50 "Net-(R12-Pad1)")
  (net 51 "Net-(R13-Pad1)")
  (net 52 "Net-(R14-Pad1)")
  (net 53 "Net-(R15-Pad1)")
  (net 54 "Net-(5V2-Pad1)")
  (net 55 "Net-(5V3-Pad1)")
  (net 56 "Net-(5V1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(5V1-Pad1)")
    (add_net "Net-(AM1-Pad1)")
    (add_net "Net-(AM1-Pad10)")
    (add_net "Net-(AM1-Pad11)")
    (add_net "Net-(AM1-Pad12)")
    (add_net "Net-(AM1-Pad13)")
    (add_net "Net-(AM1-Pad18)")
    (add_net "Net-(AM1-Pad19)")
    (add_net "Net-(AM1-Pad2)")
    (add_net "Net-(AM1-Pad21)")
    (add_net "Net-(AM1-Pad22)")
    (add_net "Net-(AM1-Pad23)")
    (add_net "Net-(AM1-Pad24)")
    (add_net "Net-(AM1-Pad25)")
    (add_net "Net-(AM1-Pad26)")
    (add_net "Net-(AM1-Pad27)")
    (add_net "Net-(AM1-Pad28)")
    (add_net "Net-(AM1-Pad29)")
    (add_net "Net-(AM1-Pad3)")
    (add_net "Net-(AM1-Pad30)")
    (add_net "Net-(AM1-Pad31)")
    (add_net "Net-(AM1-Pad32)")
    (add_net "Net-(AM1-Pad33)")
    (add_net "Net-(AM1-Pad34)")
    (add_net "Net-(AM1-Pad39)")
    (add_net "Net-(AM1-Pad4)")
    (add_net "Net-(AM1-Pad40)")
    (add_net "Net-(AM1-Pad5)")
    (add_net "Net-(AM1-Pad6)")
    (add_net "Net-(AM1-Pad8)")
    (add_net "Net-(AM1-Pad9)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R14-Pad1)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
  )
  (net_class RF ""
    (clearance 0.68)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(5V2-Pad1)")
    (add_net "Net-(5V3-Pad1)")
    (add_net "Net-(AM1-Pad16)")
    (add_net "Net-(AM1-Pad37)")
  )
  (module AM3090:ICM3090-PDIP (layer F.Cu) (tedit 5CB73B84)
    (at 145.52 158.34)
    (fp_text reference AM1 (at -5.22 -2.24) (layer F.SilkS))
    (fp_text value 3090 (at 0 3.81) (layer F.Fab))
    (pad 41 smd rect (at 0 0) (size 6.65 2.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 40 smd rect (at -3.9 1.25) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(AM1-Pad40)"))
    (pad 39 smd rect (at -3.9 0.75) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(AM1-Pad39)"))
    (pad 38 smd rect (at -3.9 0.25) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 37 smd rect (at -3.9 -0.25) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(AM1-Pad37)"))
    (pad 36 smd rect (at -3.9 -0.75) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 35 smd rect (at -3.9 -1.25) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 34 smd rect (at -3.25 -1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(AM1-Pad34)"))
    (pad 33 smd rect (at -2.75 -1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(AM1-Pad33)"))
    (pad 32 smd rect (at -2.25 -1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(AM1-Pad32)"))
    (pad 31 smd rect (at -1.75 -1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(AM1-Pad31)"))
    (pad 30 smd rect (at -1.25 -1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(AM1-Pad30)"))
    (pad 29 smd rect (at -0.75 -1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(AM1-Pad29)"))
    (pad 28 smd rect (at -0.25 -1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(AM1-Pad28)"))
    (pad 27 smd rect (at 0.25 -1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(AM1-Pad27)"))
    (pad 26 smd rect (at 0.75 -1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(AM1-Pad26)"))
    (pad 25 smd rect (at 1.25 -1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(AM1-Pad25)"))
    (pad 24 smd rect (at 1.75 -1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(AM1-Pad24)"))
    (pad 23 smd rect (at 2.25 -1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(AM1-Pad23)"))
    (pad 22 smd rect (at 2.75 -1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(AM1-Pad22)"))
    (pad 21 smd rect (at 3.25 -1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(AM1-Pad21)"))
    (pad 20 smd rect (at 3.9 -1.25) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 19 smd rect (at 3.9 -0.75) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(AM1-Pad19)"))
    (pad 18 smd rect (at 3.9 -0.25) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(AM1-Pad18)"))
    (pad 17 smd rect (at 3.9 0.25) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at 3.9 0.75) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(AM1-Pad16)"))
    (pad 15 smd rect (at 3.9 1.25) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at 3.25 1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at 2.75 1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(AM1-Pad13)"))
    (pad 12 smd rect (at 2.25 1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(AM1-Pad12)"))
    (pad 11 smd rect (at 1.75 1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(AM1-Pad11)"))
    (pad 10 smd rect (at 1.25 1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(AM1-Pad10)"))
    (pad 9 smd rect (at 0.75 1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(AM1-Pad9)"))
    (pad 8 smd rect (at 0.25 1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(AM1-Pad8)"))
    (pad 7 smd rect (at -0.25 1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -0.75 1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(AM1-Pad6)"))
    (pad 5 smd rect (at -1.25 1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(AM1-Pad5)"))
    (pad 4 smd rect (at -1.75 1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(AM1-Pad4)"))
    (pad 3 smd rect (at -2.25 1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(AM1-Pad3)"))
    (pad 2 smd rect (at -2.75 1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(AM1-Pad2)"))
    (pad 1 smd rect (at -3.25 1.9) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(AM1-Pad1)"))
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 150.95 157.565 90)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L7 (at 1.415 0 180) (layer F.SilkS))
    (fp_text value 68nH (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(AM1-Pad18)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(AM1-Pad19)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:0603 (layer F.Cu) (tedit 595EA1C0)
    (at 146.9 151.75 270)
    (fp_text reference FB6 (at -2.5 0) (layer F.SilkS))
    (fp_text value 2.2kOHM (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(5V1-Pad1)"))
    (pad 2 smd rect (at 0.7 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(AM1-Pad28)"))
  )
  (module digikey-footprints:RF_SMA_BoardEdge_142-0701-801 (layer F.Cu) (tedit 5CADFB52)
    (at 121.24 158.1885 90)
    (descr https://belfuse.com/resources/Johnson/productinformation/pi-142-0701-801.pdf)
    (fp_text reference RF2 (at -0.8615 6.76 180) (layer F.SilkS))
    (fp_text value Conn_Coaxial_Power (at 0 6.36 90) (layer F.Fab))
    (fp_text user %R (at 0 -3.7 90) (layer F.Fab))
    (pad 2 smd rect (at -4.3815 2.54 90) (size 2.413 5.08) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 4.3815 2.54 90) (size 2.413 5.08) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 4.3815 2.54 90) (size 2.413 5.08) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 2.54 90) (size 2.286 5.08) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(5V3-Pad1)"))
    (pad 2 smd rect (at -4.3815 2.54 90) (size 2.413 5.08) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module digikey-footprints:RF_SMA_BoardEdge_142-0701-801 (layer F.Cu) (tedit 5CADFB52)
    (at 168.76 159.04 270)
    (descr https://belfuse.com/resources/Johnson/productinformation/pi-142-0701-801.pdf)
    (fp_text reference RF1 (at 0.86 6.61) (layer F.SilkS))
    (fp_text value Conn_Coaxial_Power (at 0 6.36 270) (layer F.Fab))
    (fp_text user %R (at 0 -3.7 270) (layer F.Fab))
    (pad 2 smd rect (at -4.3815 2.54 270) (size 2.413 5.08) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 4.3815 2.54 270) (size 2.413 5.08) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 4.3815 2.54 270) (size 2.413 5.08) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 2.54 270) (size 2.286 5.08) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(5V2-Pad1)"))
    (pad 2 smd rect (at -4.3815 2.54 270) (size 2.413 5.08) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module digikey-footprints:RF_SMA_BoardEdge_142-0701-801 (layer F.Cu) (tedit 5CADFB52)
    (at 145 125.62)
    (descr https://belfuse.com/resources/Johnson/productinformation/pi-142-0701-801.pdf)
    (fp_text reference 5V1 (at -7.95 0.33 180) (layer F.SilkS))
    (fp_text value Conn_Coaxial_Power (at 0 6.36) (layer F.Fab))
    (fp_text user %R (at 0 -3.7) (layer F.Fab))
    (pad 2 smd rect (at -4.3815 2.54) (size 2.413 5.08) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 2.54) (size 2.286 5.08) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(5V1-Pad1)"))
    (pad 2 smd rect (at 4.3815 2.54) (size 2.413 5.08) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 4.3815 2.54) (size 2.413 5.08) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -4.3815 2.54) (size 2.413 5.08) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 163.375 145.95 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0.575 0.9) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 156.785 145.85 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0.385 0.9) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 153.755 145.84 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0.405 0.94) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(C7-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 150.675 145.85 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0.375 0.9) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(C8-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 147.605 145.81 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0.605 0.96) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(C9-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 142.35 152.015 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 1.165 -1.2 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(AM1-Pad30)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 145.5 152.035 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 2.535 -0.5) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 -90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(AM1-Pad28)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 151.6 152.015 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at -2.885 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(AM1-Pad23)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 154.8 152 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 1.55 1.15 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(AM1-Pad21)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 159.695 159.05)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 0.005 -1.45 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 "Net-(5V2-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(AM1-Pad16)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 130.575 158.2)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at -0.125 -1.65 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(AM1-Pad37)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(5V3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 137.765 145.93 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 0.315 0.93) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(C16-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 131.225 145.96 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at 0.225 0.91) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(C17-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 128.095 145.97 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at 0.145 0.92) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(C18-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 125.035 145.97 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at 0.185 0.92) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(C19-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 122.035 145.92 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at 0.335 0.87) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(C20-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:0603 (layer F.Cu) (tedit 595EA1C0)
    (at 143.7 151.7 270)
    (fp_text reference FB5 (at -2 1.75) (layer F.SilkS))
    (fp_text value 2.2kOHM (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(5V1-Pad1)"))
    (pad 2 smd rect (at 0.7 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(AM1-Pad30)"))
  )
  (module digikey-footprints:0603 (layer F.Cu) (tedit 595EA1C0)
    (at 150.2 151.7 270)
    (fp_text reference FB7 (at -2 -1.55) (layer F.SilkS))
    (fp_text value 2.2kOHM (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(5V1-Pad1)"))
    (pad 2 smd rect (at 0.7 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(AM1-Pad23)"))
  )
  (module digikey-footprints:0603 (layer F.Cu) (tedit 595EA1C0)
    (at 153.45 151.7 270)
    (fp_text reference FB8 (at -2.05 -1.1) (layer F.SilkS))
    (fp_text value 2.2kOHM (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(AM1-Pad21)"))
    (pad 1 smd rect (at -0.7 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(5V1-Pad1)"))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 164.9 144.245 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0.645 -1.15 180) (layer F.SilkS))
    (fp_text value 100OHM (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(C5-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 158.32 144.295 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0.495 -1.07 180) (layer F.SilkS))
    (fp_text value 100OHM (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(R2-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.28 144.285 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0.085 -0.98 180) (layer F.SilkS))
    (fp_text value 100OHM (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 152.21 144.255 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0.705 -1.06 180) (layer F.SilkS))
    (fp_text value 100OHM (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(C8-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 149.14 144.24 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0.69 -1.14 180) (layer F.SilkS))
    (fp_text value 100OHM (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(R5-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 164.92 147.625 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -1.175 -1.17 180) (layer F.SilkS))
    (fp_text value 100OHM (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(AM1-Pad22)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 158.36 147.485 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at -0.215 -1.01 180) (layer F.SilkS))
    (fp_text value 100OHM (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(C6-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(AM1-Pad24)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.28 147.375 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at -0.025 -1.03 180) (layer F.SilkS))
    (fp_text value 100OHM (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(C7-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(AM1-Pad25)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 152.21 147.375 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at -0.225 -1.11 180) (layer F.SilkS))
    (fp_text value 100OHM (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(AM1-Pad26)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 149.14 147.385 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at -0.615 -1.29 180) (layer F.SilkS))
    (fp_text value 100OHM (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(AM1-Pad27)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 139.3 144.235 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at -1.385 -0.2) (layer F.SilkS))
    (fp_text value 100OHM (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(R11-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(C16-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 132.77 144.305 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at -0.605 1.27) (layer F.SilkS))
    (fp_text value 100OHM (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 "Net-(R12-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 129.69 144.235 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at -0.585 1.29) (layer F.SilkS))
    (fp_text value 100OHM (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(C18-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 "Net-(R13-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 126.64 144.305 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at -0.605 1.29) (layer F.SilkS))
    (fp_text value 100OHM (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R14-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(C19-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 123.61 144.275 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at -0.625 1.26) (layer F.SilkS))
    (fp_text value 100OHM (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(R15-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(C20-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 139.28 147.695 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 0.655 1.33) (layer F.SilkS))
    (fp_text value 100OHM (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(AM1-Pad29)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(C16-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 132.76 147.615 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 0.635 1.31) (layer F.SilkS))
    (fp_text value 100OHM (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(AM1-Pad31)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 129.72 147.585 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at 0.615 1.27) (layer F.SilkS))
    (fp_text value 100OHM (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(AM1-Pad32)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(C18-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 126.58 147.625 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at 0.075 1.28) (layer F.SilkS))
    (fp_text value 100OHM (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(C19-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(AM1-Pad33)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 123.57 147.645 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at 0.555 1.37) (layer F.SilkS))
    (fp_text value 100OHM (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(AM1-Pad34)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(C20-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_DIP_SPSTx05_Slide_9.78x14.88mm_W8.61mm_P2.54mm (layer F.Cu) (tedit 5A4E1405)
    (at 160.1 135.02 270)
    (descr "SMD 5x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x14.88mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD")
    (tags "SMD DIP Switch SPST Slide 8.61mm 338mil SMD")
    (attr smd)
    (fp_text reference SW1 (at -0.02 9.45) (layer F.SilkS))
    (fp_text value SW_DIP_x05 (at 0 8.5 270) (layer F.Fab))
    (fp_text user on (at 1.3075 -6.5775 270) (layer F.Fab))
    (fp_text user %R (at 1.3 9.62) (layer F.Fab))
    (pad 10 smd rect (at 4.305 -5.08 270) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R1-Pad2)"))
    (pad 5 smd rect (at -4.305 5.08 270) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(5V1-Pad1)"))
    (pad 9 smd rect (at 4.305 -2.54 270) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R2-Pad2)"))
    (pad 4 smd rect (at -4.305 2.54 270) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(5V1-Pad1)"))
    (pad 8 smd rect (at 4.305 0 270) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R3-Pad2)"))
    (pad 3 smd rect (at -4.305 0 270) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(5V1-Pad1)"))
    (pad 7 smd rect (at 4.305 2.54 270) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R4-Pad2)"))
    (pad 2 smd rect (at -4.305 -2.54 270) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(5V1-Pad1)"))
    (pad 6 smd rect (at 4.305 5.08 270) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(R5-Pad2)"))
    (pad 1 smd rect (at -4.305 -5.08 270) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(5V1-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_DIP_SPSTx05_Slide_9.78x14.88mm_W8.61mm_P2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Button_Switch_SMD:SW_DIP_SPSTx05_Slide_9.78x14.88mm_W8.61mm_P2.54mm (layer F.Cu) (tedit 5A4E1405)
    (at 129.89 134.94 270)
    (descr "SMD 5x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x14.88mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD")
    (tags "SMD DIP Switch SPST Slide 8.61mm 338mil SMD")
    (attr smd)
    (fp_text reference SW2 (at 0.01 -9.5) (layer F.SilkS))
    (fp_text value SW_DIP_x05 (at 0 8.5 270) (layer F.Fab))
    (fp_text user %R (at 1.28 -9.29) (layer F.Fab))
    (fp_text user on (at 1.3075 -6.5775 270) (layer F.Fab))
    (pad 1 smd rect (at -4.305 -5.08 270) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(5V1-Pad1)"))
    (pad 6 smd rect (at 4.305 5.08 270) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(R15-Pad1)"))
    (pad 2 smd rect (at -4.305 -2.54 270) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(5V1-Pad1)"))
    (pad 7 smd rect (at 4.305 2.54 270) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(R14-Pad1)"))
    (pad 3 smd rect (at -4.305 0 270) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(5V1-Pad1)"))
    (pad 8 smd rect (at 4.305 0 270) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R13-Pad1)"))
    (pad 4 smd rect (at -4.305 2.54 270) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(5V1-Pad1)"))
    (pad 9 smd rect (at 4.305 -2.54 270) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R12-Pad1)"))
    (pad 5 smd rect (at -4.305 5.08 270) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(5V1-Pad1)"))
    (pad 10 smd rect (at 4.305 -5.08 270) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R11-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_DIP_SPSTx05_Slide_9.78x14.88mm_W8.61mm_P2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 147.6 162.115 270)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L1 (at 1.435 0) (layer F.SilkS))
    (fp_text value 56nH (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(AM1-Pad10)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(AM1-Pad11)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 143.05 162.115 90)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L2 (at -1.435 0 180) (layer F.SilkS))
    (fp_text value 27nH (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(AM1-Pad4)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(AM1-Pad3)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 149.4 162.115 270)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L3 (at 1.485 0.05) (layer F.SilkS))
    (fp_text value 56nH (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(AM1-Pad13)"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(AM1-Pad12)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 146.2 162.115 270)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L4 (at 1.435 0.05) (layer F.SilkS))
    (fp_text value 68nH (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(AM1-Pad8)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(AM1-Pad9)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 144.45 162.115 270)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L5 (at 1.435 0) (layer F.SilkS))
    (fp_text value 24nH (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(AM1-Pad5)"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(AM1-Pad6)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 141.6 162.115 270)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L6 (at 1.435 0.05) (layer F.SilkS))
    (fp_text value 27nH (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(AM1-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(AM1-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 140.52 159.925 270)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L8 (at 1.425 0.07) (layer F.SilkS))
    (fp_text value 24nH (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(AM1-Pad40)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(AM1-Pad39)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "AM3090 Eval Board Rev 01" (at 145 141.95) (layer B.SilkS))
  (gr_line (start 120.01 164.95) (end 170.01 164.95) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 170.01 124.95) (end 170.01 164.95) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 120.01 124.95) (end 170.01 124.95) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 120.01 164.95) (end 120.01 124.95) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer GND) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.21 165.85) (xy 119.09 124.09) (xy 170.8 124.15) (xy 170.9 165.73)
      )
    )
  )
  (zone (net 56) (net_name "Net-(5V1-Pad1)") (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.03 164.01) (xy 121.42 126.34) (xy 168.75 126.48) (xy 169.12 164.01)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.5 123.6) (xy 171 123.55) (xy 171.15 166.5) (xy 118.65 166.65)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.95 123.1) (xy 171.45 123) (xy 171.55 167) (xy 118.3 167)
      )
    )
  )
)
