<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="3.81" y1="0" x2="28.88" y2="0" width="0" layer="20"/>
<wire x1="28.88" y1="0" x2="28.88" y2="29.2" width="0" layer="20"/>
<wire x1="28.88" y1="29.2" x2="3.81" y2="29.2" width="0" layer="20"/>
<wire x1="3.81" y1="29.2" x2="3.81" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="elechouse-mine">
<packages>
<package name="ELECHOUSE-PINS">
<description>Single-row, 8-pin Pin Header (Male) Straight, 2.54 mm (0.10 in) col pitch, 5.84 mm mating length, 10.16 X 5.08 X 8.38 mm body
&lt;p&gt;Single-row (1X8), 8-pin Pin Header (Male) Straight package with 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.00 mm tail length and 5.84 mm mating length with overall size 10.16 X 5.08 X 8.38 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
<package name="ESP32-POE-UEXT-PINS">
<description>Double-row, 10-pin Receptacle Header (Female) Straight, 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 2.54 mm insulator length, 10.16 X 5.08 X 2.54 mm body
&lt;p&gt;Double-row (2X5), 10-pin Receptacle Header (Female) Straight package with 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.00 mm tail length and 2.54 mm insulator length with overall size 10.16 X 5.08 X 2.54 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X02" value="BUT1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X02" value="BUT2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="NFC" library="elechouse-mine" package="ELECHOUSE-PINS" value="NFC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ESP32" library="elechouse-mine" package="ESP32-POE-UEXT-PINS" value="ESP32">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="J1" pad="1"/>
<contactref element="ESP32" pad="B1"/>
</signal>
<signal name="N$2">
<contactref element="ESP32" pad="B2"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="J2" pad="2"/>
<contactref element="ESP32" pad="GND"/>
<contactref element="J1" pad="2"/>
<contactref element="NFC" pad="GND"/>
</signal>
<signal name="N$4">
<contactref element="ESP32" pad="3.3V"/>
<contactref element="NFC" pad="VCC"/>
</signal>
<signal name="N$6">
<contactref element="NFC" pad="IRQ"/>
<contactref element="ESP32" pad="IRQ"/>
</signal>
<signal name="N$7">
<contactref element="NFC" pad="SS"/>
<contactref element="ESP32" pad="SS"/>
</signal>
<signal name="N$8">
<contactref element="ESP32" pad="MOSI"/>
<contactref element="NFC" pad="MOSI"/>
</signal>
<signal name="N$9">
<contactref element="NFC" pad="MISO"/>
<contactref element="ESP32" pad="MISO"/>
</signal>
<signal name="N$10">
<contactref element="ESP32" pad="CLK"/>
<contactref element="NFC" pad="SCK"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
