(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 32)
    (no_connects 0)
    (area 136.718983 69.269877 179.511017 106.730001)
    (thickness 1.6)
    (drawings 42)
    (tracks 127)
    (zones 0)
    (modules 17)
    (nets 12)
  )
  (page USLetter)
  (title_block
    (date 2000-12-31)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.3)
    (user_trace_width 0.35)
    (user_trace_width 0.4)
    (user_trace_width 0.45)
    (user_trace_width 0.5)
    (user_trace_width 0.55)
    (user_trace_width 0.6)
    (user_trace_width 0.65)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.3)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.5 0.4)
    (user_via 0.6 0.5)
    (user_via 0.7 0.6)
    (user_via 0.8 0.7)
    (user_via 0.9 0.8)
    (user_via 1 0.9)
    (user_via 1.1 1)
    (user_via 6.1 6)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 13 7)
    (pad_drill 0.1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 148.4 102.23)
    (visible_elements FFFFF97F)
    (pcbplotparams
      (layerselection 0x01030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory TinyRobot/))
  )
  (net 0 "")
  (net 1 VIN)
  (net 2 GND)
  (net 3 "Net-(D1-Pad2)")
  (net 4 PB5)
  (net 5 PB0)
  (net 6 "Net-(IC1-Pad2)")
  (net 7 PB1)
  (net 8 "Net-(IC1-Pad3)")
  (net 9 "Net-(IC1-Pad7)")
  (net 10 "Net-(M1-Pad1)")
  (net 11 "Net-(M2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(M1-Pad1)")
    (add_net "Net-(M2-Pad1)")
    (add_net PB0)
    (add_net PB1)
    (add_net PB5)
    (add_net VIN)
  )
  (net_class Large ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Medium ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module "Robot Parts:Motor_Holder" (layer F.Cu) (tedit 5925E0F5)
    (at 172.085 102.235)
    (fp_text reference REF** (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value "Motor Holder" (at 0 -7.62) (layer F.Fab) hide)
    (pad "" thru_hole oval (at 0 0) (size 13 7) (drill oval 0.1) (layers *.Cu *.Mask))
  )
  (module "Robot Parts:Motor_Holder" (layer F.Cu) (tedit 5925E0C1)
    (at 144.145 102.235)
    (fp_text reference REF** (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value "Motor Holder" (at 0 -7.62) (layer F.Fab) hide)
    (pad "" thru_hole oval (at 0 0) (size 13 7) (drill oval 0.1) (layers *.Cu *.Mask)
      (die_length 10))
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5923C21F)
    (at 152.4 82.55)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference IC1 (at 3.81 3.175) (layer F.SilkS))
    (fp_text value ATTINY85 (at 3.81 10.01) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 PB5))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 PB0))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(IC1-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 PB1))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(IC1-Pad3)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(IC1-Pad7)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VIN))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Robot Parts:CR2032_Battery_Holder" (layer F.Cu) (tedit 5925DB39)
    (at 163.195 100.33 270)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference P1 (at 3.175 10.16 360) (layer F.SilkS) hide)
    (fp_text value BATT (at 1.27 12.49 270) (layer F.Fab) hide)
    (fp_text user BATT (at 0 5.08 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VIN))
    (pad 3 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VIN))
    (pad 2 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x05_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_THT:C_Rect_L4.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 59263013)
    (at 155.575 93.98)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C1 (at 4.635 0.46) (layer F.SilkS))
    (fp_text value 10uf (at 1.25 2.31) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VIN))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-5MM (layer F.Cu) (tedit 5924F56B)
    (at 157.48 73.66)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference D1 (at 1.27 1.905) (layer F.SilkS))
    (fp_text value "Red LED" (at 1.524 -3.937) (layer F.Fab) hide)
    (fp_text user K (at -1.905 1.905) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5924F3C7)
    (at 165.1 82.55)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference ISP1 (at 1.27 -2.33) (layer F.SilkS) hide)
    (fp_text value AVR-ISP-6 (at 1.27 7.41) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -2.33) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 PB1))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VIN))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(IC1-Pad7)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 PB0))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 PB5))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5924F8B9)
    (at 144.145 93.345)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference M1 (at 1.27 -2.54) (layer F.SilkS))
    (fp_text value Left (at 0 4.87) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(M1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VIN))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5924F8C0)
    (at 172.72 93.345)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference M2 (at -1.27 -2.54) (layer F.SilkS))
    (fp_text value Right (at 0 4.87) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(M2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VIN))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 5924F529)
    (at 161.925 77.47)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference Q1 (at 3.175 2.54) (layer F.SilkS))
    (fp_text value Right (at 1.3 -2.9) (layer F.Fab) hide)
    (fp_text user K (at -1.69 1.74) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 VIN))
    (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 9 "Net-(IC1-Pad7)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 5924F52E)
    (at 152.4 77.47)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference Q2 (at 0 2.54) (layer F.SilkS))
    (fp_text value Left (at 1.3 -2.9) (layer F.Fab) hide)
    (fp_text user K (at -1.69 1.74) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 VIN))
    (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 6 "Net-(IC1-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 5924F945)
    (at 151.765 94.615 180)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q3 (at 3.81 -2.54 180) (layer F.SilkS))
    (fp_text value BS170 (at 1.27 2.79 180) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -3.56 180) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 1.27 -1.27 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 7 PB1))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 10 "Net-(M1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 5926300A)
    (at 167.64 94.615 180)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q4 (at -1.51 -2.615 180) (layer F.SilkS))
    (fp_text value BS170 (at 1.27 2.79 180) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -3.56 180) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 1.27 -1.27 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 5 PB0))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 11 "Net-(M2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer F.Cu) (tedit 5924F930)
    (at 148.59 84.455 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0.95 1.86 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 PB5))
    (pad 2 thru_hole oval (at 1.9 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 VIN))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer F.Cu) (tedit 5924F521)
    (at 164.465 90.805)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 3.81 0) (layer F.SilkS))
    (fp_text value 10k (at 0.95 1.86) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(IC1-Pad7)"))
    (pad 2 thru_hole oval (at 1.9 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer F.Cu) (tedit 5924F4C4)
    (at 148.59 87.63 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at 3.81 0 360) (layer F.SilkS))
    (fp_text value 10k (at 0.95 1.86 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(IC1-Pad2)"))
    (pad 2 thru_hole oval (at 1.9 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer F.Cu) (tedit 5923C93C)
    (at 157.48 79.375)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R4 (at 0.95 -1.86) (layer F.SilkS))
    (fp_text value 330 (at 0.95 1.86) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(IC1-Pad3)"))
    (pad 2 thru_hole oval (at 1.9 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 179 100.2) (end 179.2 100.6) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 174.6 95.2) (end 179 100.2) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 174.6 90.8) (end 174.6 95.2) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.24 90.8) (end 146.68 87.64) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.44 73) (end 170.18 80.01) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 158.76 73) (end 155.08 73.03) (angle 180.4670748) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.685 80.01) (end 155.08 73.03) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 174.62 90.81) (end 170.18 87.63) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.4 102.2) (end 142 102.2) (angle 90) (layer Edge.Cuts) (width 6))
  (gr_text - (at 159.75 102.75) (layer F.SilkS))
  (gr_text + (at 161.5 99.75) (layer F.SilkS))
  (gr_text + (at 154.5 99.75) (layer F.SilkS))
  (gr_line (start 174.15 102.25) (end 169.75 102.25) (angle 90) (layer Edge.Cuts) (width 6))
  (gr_text github.com/chappy1978/Tiny-Robot (at 158.25 97.75) (layer F.SilkS))
  (gr_line (start 142.24 90.805) (end 142.24 95.25) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 141.605 102.235) (end 139.7 106.68) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.16 100.33) (end 142.24 95.25) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 174.625 102.235) (end 179.07 100.33) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.225 106.68) (end 139.7 106.68) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 150.495 105.41) (end 149.225 106.68) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 167.005 106.68) (end 176.53 106.68) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.735 105.41) (end 167.005 106.68) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.685 80.01) (end 146.685 87.63) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.18 80.01) (end 170.18 87.63) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 150.495 105.41) (end 165.735 105.41) (angle 90) (layer Edge.Cuts) (width 0.1))
)
