(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 116)
    (no_connects 2)
    (area 79.921196 36.741196 196.938804 153.758804)
    (thickness 1.6)
    (drawings 17)
    (tracks 437)
    (zones 0)
    (modules 48)
    (nets 79)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.35)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.6)
    (via_drill 0.6)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.5 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4 4)
    (pad_drill 3.5)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 158.77 72.39)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x01000_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerbers/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C2-Pad2)")
  (net 5 VDD)
  (net 6 GND)
  (net 7 /SRV)
  (net 8 "Net-(P4-Pad1)")
  (net 9 "Net-(P4-Pad2)")
  (net 10 "Net-(P5-Pad1)")
  (net 11 "Net-(P5-Pad2)")
  (net 12 "Net-(P5-Pad3)")
  (net 13 "Net-(P5-Pad4)")
  (net 14 "Net-(P6-Pad1)")
  (net 15 "Net-(P6-Pad2)")
  (net 16 "Net-(P6-Pad3)")
  (net 17 "Net-(P6-Pad4)")
  (net 18 /LED)
  (net 19 "Net-(R5-Pad1)")
  (net 20 "Net-(R6-Pad1)")
  (net 21 "Net-(R11-Pad1)")
  (net 22 "Net-(R12-Pad1)")
  (net 23 +3V3)
  (net 24 "Net-(U1-Pad36)")
  (net 25 "Net-(U1-Pad35)")
  (net 26 "Net-(U1-Pad34)")
  (net 27 "Net-(U1-Pad33)")
  (net 28 "Net-(U1-Pad32)")
  (net 29 "Net-(U1-Pad30)")
  (net 30 "Net-(U1-Pad29)")
  (net 31 "Net-(U1-Pad28)")
  (net 32 /RadInt)
  (net 33 "Net-(U1-Pad2)")
  (net 34 "Net-(U1-Pad4)")
  (net 35 "Net-(U1-Pad5)")
  (net 36 "Net-(U1-Pad7)")
  (net 37 "Net-(U1-Pad8)")
  (net 38 "Net-(U1-Pad9)")
  (net 39 /RadCS)
  (net 40 /MOSI)
  (net 41 /MISO)
  (net 42 /SCK)
  (net 43 "Net-(U1-Pad14)")
  (net 44 "Net-(U1-Pad15)")
  (net 45 /DIR2)
  (net 46 /DIR1)
  (net 47 /STEP2)
  (net 48 /STEP1)
  (net 49 "Net-(U1-Pad25)")
  (net 50 "Net-(U2-Pad7)")
  (net 51 "Net-(U2-Pad10)")
  (net 52 "Net-(U2-Pad12)")
  (net 53 "Net-(U2-Pad13)")
  (net 54 "Net-(U2-Pad14)")
  (net 55 "Net-(U2-Pad16)")
  (net 56 "Net-(U5-Pad1)")
  (net 57 "Net-(U5-Pad4)")
  (net 58 "Net-(U5-Pad5)")
  (net 59 "Net-(U6-Pad1)")
  (net 60 "Net-(U6-Pad4)")
  (net 61 "Net-(U6-Pad5)")
  (net 62 "Net-(U5-Pad10)")
  (net 63 "Net-(U6-Pad10)")
  (net 64 "Net-(P7-Pad3)")
  (net 65 "Net-(P7-Pad4)")
  (net 66 "Net-(P8-Pad3)")
  (net 67 "Net-(P8-Pad4)")
  (net 68 "Net-(P9-Pad1)")
  (net 69 "Net-(P9-Pad2)")
  (net 70 /Reset)
  (net 71 "Net-(U2-Pad6)")
  (net 72 ref_filter)
  (net 73 /Sen1)
  (net 74 /Sen2)
  (net 75 /FFT1)
  (net 76 /Vref)
  (net 77 /FFT2)
  (net 78 3v3f)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 1.6)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /DIR1)
    (add_net /DIR2)
    (add_net /FFT1)
    (add_net /FFT2)
    (add_net /LED)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RadCS)
    (add_net /RadInt)
    (add_net /Reset)
    (add_net /SCK)
    (add_net /SRV)
    (add_net /STEP1)
    (add_net /STEP2)
    (add_net /Sen1)
    (add_net /Sen2)
    (add_net /Vref)
    (add_net 3v3f)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P5-Pad3)")
    (add_net "Net-(P5-Pad4)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P6-Pad2)")
    (add_net "Net-(P6-Pad3)")
    (add_net "Net-(P6-Pad4)")
    (add_net "Net-(P7-Pad3)")
    (add_net "Net-(P7-Pad4)")
    (add_net "Net-(P8-Pad3)")
    (add_net "Net-(P8-Pad4)")
    (add_net "Net-(P9-Pad1)")
    (add_net "Net-(P9-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad33)")
    (add_net "Net-(U1-Pad34)")
    (add_net "Net-(U1-Pad35)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U5-Pad1)")
    (add_net "Net-(U5-Pad10)")
    (add_net "Net-(U5-Pad4)")
    (add_net "Net-(U5-Pad5)")
    (add_net "Net-(U6-Pad1)")
    (add_net "Net-(U6-Pad10)")
    (add_net "Net-(U6-Pad4)")
    (add_net "Net-(U6-Pad5)")
    (add_net VDD)
    (add_net ref_filter)
  )
  (net_class Production ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module custom_footprints:DRV8834Breakout (layer F.Cu) (tedit 594BE73F)
    (at 100.33 85.09 180)
    (descr "footprint for drv8834 pololu breakout")
    (fp_text reference U5 (at 7.62 1.27 180) (layer F.SilkS))
    (fp_text value DRV8834_Breakout (at 7.62 -21.59 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.27 -19.05 180) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(U5-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 -16.51 180) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(P7-Pad3)"))
    (pad 3 thru_hole circle (at 1.27 -13.97 180) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(P7-Pad4)"))
    (pad 4 thru_hole circle (at 1.27 -11.43 180) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(U5-Pad4)"))
    (pad 5 thru_hole circle (at 1.27 -8.89 180) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(U5-Pad5)"))
    (pad 6 thru_hole circle (at 1.27 -6.35 180) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 +3V3))
    (pad 7 thru_hole circle (at 1.27 -3.81 180) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /STEP1))
    (pad 8 thru_hole circle (at 1.27 -1.27 180) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /DIR1))
    (pad 9 thru_hole rect (at 13.97 -1.27 180) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 10 thru_hole circle (at 13.97 -3.81 180) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(U5-Pad10)"))
    (pad 11 thru_hole circle (at 13.97 -6.35 180) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P5-Pad4)"))
    (pad 12 thru_hole circle (at 13.97 -8.89 180) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P5-Pad3)"))
    (pad 13 thru_hole circle (at 13.97 -11.43 180) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P5-Pad2)"))
    (pad 14 thru_hole circle (at 13.97 -13.97 180) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P5-Pad1)"))
    (pad 15 thru_hole circle (at 13.97 -16.51 180) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 16 thru_hole circle (at 13.97 -19.05 180) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 VDD))
  )
  (module custom_footprints:RFM69Breakout (layer F.Cu) (tedit 594BE7D6)
    (at 144.78 133.35)
    (fp_text reference U2 (at 12.7 2.54) (layer F.SilkS))
    (fp_text value RFM69_Breakout (at 12.7 -20.32) (layer F.Fab))
    (fp_text user ANT (at 22.86 -2.54) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 -17.78) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /MISO))
    (pad 2 thru_hole circle (at 0 -15.24) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /MOSI))
    (pad 3 thru_hole circle (at 0 -12.7) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /SCK))
    (pad 4 thru_hole circle (at 0 -10.16) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /RadCS))
    (pad 5 thru_hole circle (at 0 -7.62) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 /Reset))
    (pad 6 thru_hole circle (at 0 -5.08) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(U2-Pad6)"))
    (pad 7 thru_hole circle (at 0 -2.54) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(U2-Pad7)"))
    (pad 8 thru_hole circle (at 0 0) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 +3V3))
    (pad 9 thru_hole rect (at 25.4 0) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 10 thru_hole circle (at 25.4 -2.54) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(U2-Pad10)"))
    (pad 11 thru_hole circle (at 25.4 -5.08) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 12 thru_hole circle (at 25.4 -7.62) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(U2-Pad12)"))
    (pad 13 thru_hole circle (at 25.4 -10.16) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(U2-Pad13)"))
    (pad 14 thru_hole circle (at 25.4 -12.7) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(U2-Pad14)"))
    (pad 15 thru_hole circle (at 25.4 -15.24) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /RadInt))
    (pad 16 thru_hole circle (at 25.4 -17.78) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(U2-Pad16)"))
  )
  (module Mounting_Holes:MountingHole_3.5mm_Pad (layer F.Cu) (tedit 594AA380)
    (at 163.83 52.07)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS))
    (fp_text value Mount (at 0 4.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm_Pad (layer F.Cu) (tedit 594AA380)
    (at 113.03 52.07)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS))
    (fp_text value Mount (at 0 4.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm_Pad (layer F.Cu) (tedit 594AA370)
    (at 113.03 142.24)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS))
    (fp_text value Mount (at 0 4.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Connect:1pin (layer F.Cu) (tedit 594A9D23)
    (at 138.43 75.75)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS))
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.778) (layers *.Cu *.Mask))
  )
  (module Connect:1pin (layer F.Cu) (tedit 594A9CD4)
    (at 138.43 104.4)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS))
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.778) (layers *.Cu *.Mask))
  )
  (module Capacitors_ThroughHole:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5920C254)
    (at 102.87 85.09 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C1 (at 2.5 -2.01 90) (layer F.SilkS))
    (fp_text value 0.47uF (at 2.5 2.01 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5920C254)
    (at 148.59 57.15)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C2 (at 2.5 -2.01) (layer F.SilkS))
    (fp_text value 0.47uF (at 2.5 2.01) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 5920C255)
    (at 147.32 45.72)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C3 (at 2.5 -6.06) (layer F.SilkS))
    (fp_text value 470uF (at 2.5 6.06) (layer F.Fab))
    (fp_text user %R (at 2.4 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 VDD))
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 121.92 49.53)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference P1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value SEN (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 /Sen1))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 /Sen2))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 86.36 110.49)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference P2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value SRV (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 VDD))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /SRV))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_2pol (layer F.Cu) (tedit 0)
    (at 139.7 40.64 180)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P3 (at 1.27 -4.50088 180) (layer F.SilkS))
    (fp_text value PWR (at 1.27 4.50088 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 5 VDD))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 6 GND))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_2pol.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC5)
    (at 118.11 140.97 270)
    (descr "Through hole straight pin header, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x01 2.54mm double row")
    (fp_text reference P4 (at 1.27 -2.33 270) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.33 270) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(P4-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(P4-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x01_Pitch2.54mm.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 82.55 99.06 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P5 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value M1 (at 0 9.95 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(P5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(P5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(P5-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(P5-Pad4)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 194.31 91.44)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P6 (at 0 -2.33) (layer F.SilkS))
    (fp_text value M2 (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(P6-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(P6-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(P6-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(P6-Pad4)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 58CE52AF)
    (at 127 146.05 90)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 2.54 -3.56 270) (layer F.SilkS))
    (fp_text value 5LN01SP (at 2.54 2.79 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.56 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(P4-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /LED))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 106.68 73.66 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.81 -2.31 90) (layer F.SilkS))
    (fp_text value 20k (at 3.81 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 /FFT1))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 106.68 86.36 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 3.81 -2.31 90) (layer F.SilkS))
    (fp_text value 1M (at 3.81 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 114.3 90.17 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 3.81 -2.31 180) (layer F.SilkS))
    (fp_text value 20k (at 3.81 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(R5-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 128.27 87.63 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 3.81 -2.31 90) (layer F.SilkS))
    (fp_text value 20k (at 3.81 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R6-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(R5-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 152.4 77.47 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 3.81 -2.31 270) (layer F.SilkS))
    (fp_text value 20k (at 3.81 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 /FFT2))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 147.32 60.96)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R10 (at 3.81 -2.31) (layer F.SilkS))
    (fp_text value 1M (at 3.81 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 147.32 72.39 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R11 (at 3.81 -2.31 90) (layer F.SilkS))
    (fp_text value 20k (at 3.81 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R11-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 147.32 85.09 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R12 (at 3.81 -2.31 90) (layer F.SilkS))
    (fp_text value 20k (at 3.81 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(R12-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R11-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 144.78 142.24 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R13 (at 3.81 -2.31 180) (layer F.SilkS))
    (fp_text value 10R (at 3.81 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 +3V3))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(P4-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 124.46 59.69 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference Rc1 (at 3.81 -2.31 180) (layer F.SilkS))
    (fp_text value 36k (at 3.81 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R6-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 /Sen1))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 156.21 85.09)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference Rc2 (at 3.81 -2.31) (layer F.SilkS))
    (fp_text value 36k (at 3.81 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(R12-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 /Sen2))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 118.11 99.06 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference Rd1 (at 3.81 -2.31 90) (layer F.SilkS))
    (fp_text value 6.2k (at 3.81 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 +3V3))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 /Vref))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 124.46 91.44 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference Rd2 (at 3.81 -2.31 270) (layer F.SilkS))
    (fp_text value 1.5k (at 3.81 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 /Vref))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 102.87 59.69)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference Rf1 (at 3.81 -2.31) (layer F.SilkS))
    (fp_text value 68k (at 3.81 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 /FFT1))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 /Sen1))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 128.27 62.23 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference Rf2 (at 3.81 -2.31 270) (layer F.SilkS))
    (fp_text value 68k (at 3.81 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 /FFT2))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 /Sen2))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Teensy-3.1:Teensy-3.1 (layer F.Cu) (tedit 57C2CCF9)
    (at 102.87 132.08)
    (fp_text reference U1 (at -5.08 -7.62 90) (layer F.SilkS))
    (fp_text value Teensy_3.1 (at 5.08 -10.16) (layer F.Fab))
    (pad 36 thru_hole circle (at 10.16 -12.7) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(U1-Pad36)"))
    (pad 35 thru_hole circle (at 7.62 -12.7) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(U1-Pad35)"))
    (pad 34 thru_hole circle (at 5.08 -12.7) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(U1-Pad34)"))
    (pad 33 thru_hole circle (at 0 -12.7) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(U1-Pad33)"))
    (pad 32 thru_hole circle (at 30.48 -2.54) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(U1-Pad32)"))
    (pad 31 thru_hole circle (at 30.48 -5.08) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 +3V3))
    (pad 30 thru_hole circle (at 30.48 -7.62) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(U1-Pad30)"))
    (pad 29 thru_hole circle (at 30.48 -10.16) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(U1-Pad29)"))
    (pad 28 thru_hole circle (at 30.48 -12.7) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(U1-Pad28)"))
    (pad 0 thru_hole circle (at 0 0) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /RadInt))
    (pad 1 thru_hole circle (at 2.54 0) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 /Reset))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(U1-Pad2)"))
    (pad 3 thru_hole circle (at 7.62 0) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SRV))
    (pad 4 thru_hole circle (at 10.16 0) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(U1-Pad4)"))
    (pad 5 thru_hole circle (at 12.7 0) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at 15.24 0) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /LED))
    (pad 7 thru_hole circle (at 17.78 0) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(U1-Pad7)"))
    (pad 8 thru_hole circle (at 20.32 0) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(U1-Pad8)"))
    (pad 9 thru_hole circle (at 22.86 0) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(U1-Pad9)"))
    (pad 10 thru_hole circle (at 25.4 0) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /RadCS))
    (pad 11 thru_hole circle (at 27.94 0) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /MOSI))
    (pad 12 thru_hole circle (at 30.48 0) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /MISO))
    (pad 13 thru_hole circle (at 30.48 -15.24) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /SCK))
    (pad 14 thru_hole circle (at 27.94 -15.24) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(U1-Pad14)"))
    (pad 15 thru_hole circle (at 25.4 -15.24) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(U1-Pad15)"))
    (pad 16 thru_hole circle (at 22.86 -15.24) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 75 /FFT1))
    (pad 17 thru_hole circle (at 20.32 -15.24) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 77 /FFT2))
    (pad 18 thru_hole circle (at 17.78 -15.24) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(P9-Pad1)"))
    (pad 19 thru_hole circle (at 15.24 -15.24) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(P9-Pad2)"))
    (pad 20 thru_hole circle (at 12.7 -15.24) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /DIR2))
    (pad 21 thru_hole circle (at 10.16 -15.24) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /DIR1))
    (pad 22 thru_hole circle (at 7.62 -15.24) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 /STEP2))
    (pad 23 thru_hole circle (at 5.08 -15.24) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /STEP1))
    (pad 24 thru_hole circle (at 2.54 -15.24) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 +3V3))
    (pad 25 thru_hole circle (at 0 -15.24) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(U1-Pad25)"))
    (pad 26 thru_hole circle (at -2.54 -15.24) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 VDD))
    (pad 27 thru_hole circle (at -2.54 0) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC5)
    (at 104.14 97.79 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference P7 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(P7-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(P7-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 +3V3))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC5)
    (at 172.72 88.9 270)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference P8 (at 1.27 -2.33 270) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 1.27 7.41 270) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(P8-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(P8-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 +3V3))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:MountingHole_3.5mm_Pad (layer F.Cu) (tedit 594AA36A)
    (at 163.83 142.24)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS))
    (fp_text value Mount (at 0 4.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module custom_footprints:DRV8834Breakout (layer F.Cu) (tedit 594BE73F)
    (at 176.53 105.41)
    (descr "footprint for drv8834 pololu breakout")
    (fp_text reference U6 (at 7.62 1.27) (layer F.SilkS))
    (fp_text value DRV8834_Breakout (at 7.62 -21.59) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.27 -19.05) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(U6-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 -16.51) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(P8-Pad3)"))
    (pad 3 thru_hole circle (at 1.27 -13.97) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(P8-Pad4)"))
    (pad 4 thru_hole circle (at 1.27 -11.43) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(U6-Pad4)"))
    (pad 5 thru_hole circle (at 1.27 -8.89) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(U6-Pad5)"))
    (pad 6 thru_hole circle (at 1.27 -6.35) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 +3V3))
    (pad 7 thru_hole circle (at 1.27 -3.81) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 /STEP2))
    (pad 8 thru_hole circle (at 1.27 -1.27) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /DIR2))
    (pad 9 thru_hole rect (at 13.97 -1.27) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 10 thru_hole circle (at 13.97 -3.81) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(U6-Pad10)"))
    (pad 11 thru_hole circle (at 13.97 -6.35) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P6-Pad4)"))
    (pad 12 thru_hole circle (at 13.97 -8.89) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P6-Pad3)"))
    (pad 13 thru_hole circle (at 13.97 -11.43) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P6-Pad2)"))
    (pad 14 thru_hole circle (at 13.97 -13.97) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P6-Pad1)"))
    (pad 15 thru_hole circle (at 13.97 -16.51) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 16 thru_hole circle (at 13.97 -19.05) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 VDD))
  )
  (module Pin_Headers:Pin_Header_Straight_2x01_Pitch2.54mm (layer F.Cu) (tedit 5966877B)
    (at 121.92 46.99 90)
    (descr "Through hole straight pin header, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x01 2.54mm double row")
    (fp_text reference P9 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Range (at 1.27 2.54 90) (layer F.Fab))
    (fp_text user %R (at 1.27 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(P9-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(P9-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 114.3 72.39 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 10u (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 78 3v3f))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 121.92 71.12 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 10u (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 72 ref_filter))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 160.02 72.39 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 1.75 180) (layer B.SilkS))
    (fp_text value 10u (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 78 3v3f))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 160.02 69.85 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 1.75 180) (layer B.SilkS))
    (fp_text value 10u (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 72 ref_filter))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 114.3 78.74 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 1.45 270) (layer B.SilkS))
    (fp_text value 500 (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 78 3v3f))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 23 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 128.27 77.47)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 1.45) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 72 ref_filter))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 76 /Vref))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 158.75 76.2 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 1.45 270) (layer B.SilkS))
    (fp_text value 500 (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 78 3v3f))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 23 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 152.4 69.85 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 72 ref_filter))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 76 /Vref))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_footprints:DIP-14_W7.62mm_Socket (layer F.Cu) (tedit 5A96D943)
    (at 116.84 67.31)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U3 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value MCP6004 (at 3.81 17.57) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 75 /FFT1))
    (pad 8 thru_hole oval (at 7.62 15.24) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(R6-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 73 /Sen1))
    (pad 9 thru_hole oval (at 7.62 12.7) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(R5-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 72 ref_filter))
    (pad 10 thru_hole oval (at 7.62 10.16) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 72 ref_filter))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 78 3v3f))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 72 ref_filter))
    (pad 12 thru_hole oval (at 7.62 5.08) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 72 ref_filter))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 13 thru_hole oval (at 7.62 2.54) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 74 /Sen2))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 14 thru_hole oval (at 7.62 0) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 77 /FFT2))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_footprints:DIP-14_W7.62mm_Socket (layer F.Cu) (tedit 5A96D943)
    (at 156.21 64.77)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U4 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value MCP6004 (at 3.81 17.57) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 8 thru_hole oval (at 7.62 15.24) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 12.7) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 72 ref_filter))
    (pad 10 thru_hole oval (at 7.62 10.16) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 78 3v3f))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 72 ref_filter))
    (pad 12 thru_hole oval (at 7.62 5.08) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(R11-Pad1)"))
    (pad 13 thru_hole oval (at 7.62 2.54) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "Net-(R12-Pad1)"))
    (pad 14 thru_hole oval (at 7.62 0) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 141.625 84.455) (end 135.275 84.455) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.625 89.535) (end 141.625 84.455) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.895 90.805) (end 141.625 89.535) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.275 89.535) (end 135.275 84.455) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.005 90.805) (end 135.275 89.535) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 138.45 95.25) (end 134.005 99.695) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 138.45 95.25) (end 142.895 90.805) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 138.45 95.25) (end 142.895 99.695) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 35.56 (width 0.3) (layer F.Fab)
    (gr_text "35.560 mm" (at 199.47 113.03 270) (layer F.Fab))
    (feature1 (pts (xy 170.18 130.81) (xy 200.82 130.81)))
    (feature2 (pts (xy 170.18 95.25) (xy 200.82 95.25)))
    (crossbar (pts (xy 198.12 95.25) (xy 198.12 130.81)))
    (arrow1a (pts (xy 198.12 130.81) (xy 197.533579 129.683496)))
    (arrow1b (pts (xy 198.12 130.81) (xy 198.706421 129.683496)))
    (arrow2a (pts (xy 198.12 95.25) (xy 197.533579 96.376504)))
    (arrow2b (pts (xy 198.12 95.25) (xy 198.706421 96.376504)))
  )
  (dimension 31.75 (width 0.3) (layer F.Fab)
    (gr_text "31.750 mm" (at 154.305 109.14) (layer F.Fab))
    (feature1 (pts (xy 170.18 130.81) (xy 170.18 107.79)))
    (feature2 (pts (xy 138.43 130.81) (xy 138.43 107.79)))
    (crossbar (pts (xy 138.43 110.49) (xy 170.18 110.49)))
    (arrow1a (pts (xy 170.18 110.49) (xy 169.053496 111.076421)))
    (arrow1b (pts (xy 170.18 110.49) (xy 169.053496 109.903579)))
    (arrow2a (pts (xy 138.43 110.49) (xy 139.556504 111.076421)))
    (arrow2b (pts (xy 138.43 110.49) (xy 139.556504 109.903579)))
  )
  (dimension 90.17 (width 0.3) (layer F.Fab)
    (gr_text "90.170 mm" (at 208.36 97.155 90) (layer F.Fab))
    (feature1 (pts (xy 163.83 52.07) (xy 209.71 52.07)))
    (feature2 (pts (xy 163.83 142.24) (xy 209.71 142.24)))
    (crossbar (pts (xy 207.01 142.24) (xy 207.01 52.07)))
    (arrow1a (pts (xy 207.01 52.07) (xy 207.596421 53.196504)))
    (arrow1b (pts (xy 207.01 52.07) (xy 206.423579 53.196504)))
    (arrow2a (pts (xy 207.01 142.24) (xy 207.596421 141.113496)))
    (arrow2b (pts (xy 207.01 142.24) (xy 206.423579 141.113496)))
  )
  (dimension 46.99 (width 0.3) (layer F.Fab)
    (gr_text "46.990 mm" (at 202.01 118.745 270) (layer F.Fab))
    (feature1 (pts (xy 138.43 142.24) (xy 203.36 142.24)))
    (feature2 (pts (xy 138.43 95.25) (xy 203.36 95.25)))
    (crossbar (pts (xy 200.66 95.25) (xy 200.66 142.24)))
    (arrow1a (pts (xy 200.66 142.24) (xy 200.073579 141.113496)))
    (arrow1b (pts (xy 200.66 142.24) (xy 201.246421 141.113496)))
    (arrow2a (pts (xy 200.66 95.25) (xy 200.073579 96.376504)))
    (arrow2b (pts (xy 200.66 95.25) (xy 201.246421 96.376504)))
  )
  (dimension 50.8 (width 0.3) (layer F.Fab)
    (gr_text "50.800 mm" (at 138.43 163.91) (layer F.Fab))
    (feature1 (pts (xy 163.83 142.24) (xy 163.83 165.26)))
    (feature2 (pts (xy 113.03 142.24) (xy 113.03 165.26)))
    (crossbar (pts (xy 113.03 162.56) (xy 163.83 162.56)))
    (arrow1a (pts (xy 163.83 162.56) (xy 162.703496 163.146421)))
    (arrow1b (pts (xy 163.83 162.56) (xy 162.703496 161.973579)))
    (arrow2a (pts (xy 113.03 162.56) (xy 114.156504 163.146421)))
    (arrow2b (pts (xy 113.03 162.56) (xy 114.156504 161.973579)))
  )
  (gr_text "Ian D. Miller 2017" (at 158.75 102.87) (layer F.SilkS))
  (gr_text v1.2 (at 167.64 99.06) (layer F.SilkS))
  (gr_text swarmR (at 156.21 99.06) (layer F.SilkS))
  (gr_circle (center 138.43 95.25) (end 196.85 93.98) (layer Edge.Cuts) (width 0.15))
  (zone (net 6) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.24 54.61) (xy 167.64 54.61) (xy 167.64 83.82) (xy 147.32 110.49) (xy 130.81 110.49)
        (xy 114.3 101.6) (xy 114.3 92.71) (xy 104.14 92.71) (xy 104.14 87.63) (xy 100.33 87.63)
        (xy 100.33 83.82) (xy 97.79 83.82) (xy 97.79 60.96) (xy 101.6 57.15) (xy 102.87 49.53)
        (xy 111.76 44.45) (xy 124.46 39.37) (xy 130.81 38.1) (xy 142.24 38.1)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.55 83.82) (xy 96.52 83.82) (xy 96.52 90.17) (xy 101.6 90.17) (xy 101.6 96.52)
        (xy 111.76 96.52) (xy 111.76 102.87) (xy 130.81 113.03) (xy 147.32 113.03) (xy 170.18 83.82)
        (xy 170.18 52.07) (xy 143.51 52.07) (xy 143.51 38.1) (xy 160.02 41.91) (xy 179.07 54.61)
        (xy 190.5 71.12) (xy 194.31 85.09) (xy 195.58 93.98) (xy 194.31 107.95) (xy 189.23 120.65)
        (xy 181.61 133.35) (xy 168.91 143.51) (xy 152.4 151.13) (xy 124.46 151.13) (xy 102.87 139.7)
        (xy 90.17 125.73) (xy 82.55 106.68) (xy 81.28 93.98)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.02 41.91) (xy 179.07 54.61) (xy 190.5 71.12) (xy 195.58 93.98) (xy 194.31 107.95)
        (xy 189.23 120.65) (xy 181.61 133.35) (xy 168.91 143.51) (xy 152.4 151.13) (xy 124.46 151.13)
        (xy 102.87 139.7) (xy 90.17 125.73) (xy 82.55 106.68) (xy 81.28 93.98) (xy 82.55 83.82)
        (xy 96.52 83.82) (xy 96.52 90.17) (xy 101.6 90.17) (xy 101.6 96.52) (xy 111.76 96.52)
        (xy 111.76 102.87) (xy 130.81 113.03) (xy 147.32 113.03) (xy 170.18 83.82) (xy 170.18 52.07)
        (xy 143.51 52.07) (xy 143.51 38.1)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.24 54.61) (xy 167.64 54.61) (xy 167.64 83.82) (xy 147.32 110.49) (xy 130.81 110.49)
        (xy 114.3 101.6) (xy 114.3 92.71) (xy 104.14 92.71) (xy 104.14 87.63) (xy 100.33 87.63)
        (xy 100.33 83.82) (xy 97.79 83.82) (xy 97.79 60.96) (xy 101.6 57.15) (xy 102.87 49.53)
        (xy 111.76 44.45) (xy 124.46 39.37) (xy 130.81 38.1) (xy 142.24 38.1)
      )
    )
  )
)
