<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="2.54" x2="25.38" y2="2.54" width="0" layer="20"/>
<wire x1="25.38" y1="2.54" x2="25.507" y2="40.437" width="0" layer="20"/>
<wire x1="25.507" y1="40.437" x2="0.127" y2="40.437" width="0" layer="20"/>
<wire x1="0.127" y1="40.437" x2="0" y2="2.54" width="0" layer="20"/>
<text>+15V</text>
<text>-15V</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>INL</text>
<text>INR</text>
<text>OL</text>
<text>OR</text>
<text>GND</text>
<text>GND</text>
<text>1646</text>
<text>1646</text>
<text>10uf</text>
<text>10uf</text>
<text>0.1uf</text>
<text>HA - MK1</text>
<hole x="0.889" y="39.624" drill="1"/>
<hole x="0.762" y="3.429" drill="1"/>
<hole x="24.638" y="3.429" drill="1"/>
<hole x="24.638" y="39.624" drill="1"/>
</plain>
<libraries>
<library name="capacitor-wima">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C5B3">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 7.5 x 3 mm, grid 5.08 mm</description>
</package>
<package name="C7.5B6">
<description>&lt;B&gt;MKS3&lt;/B&gt;, 10 x 6 mm, grid 7.62 mm</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="JP2">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="that-corp">
<description>&lt;b&gt;THAT Corporation&lt;/b&gt; - v1.04 (05/05/2011)&lt;p&gt;
Pro Audio IC's and Components&lt;p&gt;
source: http://www.thatcorp.com
&lt;p&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;
USE AT YOUR OWN RISK!&lt;p&gt;
&lt;author&gt;Copyright (C) 2008-2010, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;&lt;/author&gt;&lt;p&gt;
History:&lt;p&gt;
1.02 (05/01/2010) - Corrected bug in THAT320 where pins 5 &amp; 7 were swapped.&lt;p&gt;
1.03 (09/27/2010) - Corrected bug in THAT4305, power pins 8 &amp; 9 were swapped.</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="capacitor-wima" package="C5B3" value="0.1uf"/>
<element name="C2" library="capacitor-wima" package="C5B3" value="0.1uf"/>
<element name="C3" library="capacitor-wima" package="C7.5B6" value="10uf"/>
<element name="C4" library="capacitor-wima" package="C5B3" value="0.1uf"/>
<element name="C5" library="capacitor-wima" package="C5B3" value="0.1uf"/>
<element name="C6" library="capacitor-wima" package="C7.5B6" value="10uf"/>
<element name="JP1" library="jumper" package="JP1" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="jumper" package="JP1" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="jumper" package="JP1" value="">
<attribute name="VALUE"/>
</element>
<element name="JP4" library="jumper" package="JP2" value="">
<attribute name="VALUE"/>
</element>
<element name="JP5" library="jumper" package="JP1" value="">
<attribute name="VALUE"/>
</element>
<element name="U1" library="that-corp" package="DIL08" value="THAT1646P08-U"/>
<element name="U2" library="that-corp" package="DIL08" value="THAT1646P08-U"/>
</elements>
<signals>
<signal name="+15V">
<contactref element="U1" pad="6"/>
<contactref element="C2" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="U2" pad="6"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="-15V">
<contactref element="U1" pad="5"/>
<contactref element="C1" pad="1"/>
<contactref element="JP4" pad="2"/>
<contactref element="U2" pad="5"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="3"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP4" pad="3"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP5" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="OUT">
<contactref element="U1" pad="8"/>
<contactref element="C3" pad="2"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="IN">
<contactref element="U1" pad="4"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$1">
<contactref element="C6" pad="1"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="OUT2">
<contactref element="U2" pad="8"/>
<contactref element="C6" pad="2"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="IN2">
<contactref element="U2" pad="4"/>
<contactref element="JP2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
