(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (grid_origin 116.0124 80.3094)
    (pcbplotparams
      (layerselection 0x000100c_7ffffffe)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "VCC")
  (net 3 "/GATE")
  (net 4 "/VRAW1")
  (net 5 "/DTR")
  (net 6 "/RESET")
  (net 7 "/CS_SHIFT_REG")
  (net 8 "/AVCC")
  (net 9 "/AGND")
  (net 10 "/VBAT")
  (net 11 "/HALL0_~{SLEEP}")
  (net 12 "/HALL0_OUTPUT")
  (net 13 "/HALL1_~{SLEEP}")
  (net 14 "/HALL1_OUTPUT")
  (net 15 "/HALL2_~{SLEEP}")
  (net 16 "/HALL2_OUTPUT")
  (net 17 "/HALL3_~{SLEEP}")
  (net 18 "/HALL3_OUTPUT")
  (net 19 "/HALL4_~{SLEEP}")
  (net 20 "/HALL4_OUTPUT")
  (net 21 "/HALL5_~{SLEEP}")
  (net 22 "/HALL5_OUTPUT")
  (net 23 "/HALL6_~{SLEEP}")
  (net 24 "/HALL6_OUTPUT")
  (net 25 "/HALL7_~{SLEEP}")
  (net 26 "/HALL7_OUTPUT")
  (net 27 "/HALL8_~{SLEEP}")
  (net 28 "/HALL8_OUTPUT")
  (net 29 "/HALL9_~{SLEEP}")
  (net 30 "/HALL9_OUTPUT")
  (net 31 "/HALL10_~{SLEEP}")
  (net 32 "/HALL10_OUTPUT")
  (net 33 "/HALL11_~{SLEEP}")
  (net 34 "/HALL11_OUTPUT")
  (net 35 "/HALL12_~{SLEEP}")
  (net 36 "/HALL12_OUTPUT")
  (net 37 "/HALL13_~{SLEEP}")
  (net 38 "/HALL13_OUTPUT")
  (net 39 "/HALL14_~{SLEEP}")
  (net 40 "/HALL14_OUTPUT")
  (net 41 "/HALL15_~{SLEEP}")
  (net 42 "/HALL15_OUTPUT")
  (net 43 "/MISO")
  (net 44 "/SCK")
  (net 45 "/MOSI")
  (net 46 "/TO_FTDI_TX")
  (net 47 "/TO_FTDI_RX")
  (net 48 "Net-(LED1-PadA)")
  (net 49 "Net-(LED2-PadA)")
  (net 50 "/SCL")
  (net 51 "/SDA")
  (net 52 "/PB7")
  (net 53 "/LED_RED")
  (net 54 "/LED_GRN")
  (net 55 "/32KHZ")
  (net 56 "/SHIFT_CLEAR")
  (net 57 "/ANALOG_0")
  (net 58 "/MUX_~{EN}")
  (net 59 "/BATT_MONITOR")
  (net 60 "/BATT_MONITOR_EN")
  (net 61 "Net-(BJT0-B)")
  (net 62 "Net-(P-FET0-D)")
  (net 63 "/CS_SD")
  (net 64 "/MUX_S0")
  (net 65 "/MUX_S1")
  (net 66 "/MUX_S3")
  (net 67 "/MUX_S2")
  (net 68 "/BUTTON1")
  (net 69 "/BUTTON2")
  (net 70 "/AREF")
  (net 71 "unconnected-(BUTTON2-PadP)")
  (net 72 "unconnected-(BUTTON2-PadS)")
  (net 73 "unconnected-(BUTTON1-PadP)")
  (net 74 "unconnected-(BUTTON1-PadS)")
  (net 75 "Net-(U$1-DAT2_RES)")
  (net 76 "Net-(U$1-DAT1_NC)")
  (net 77 "unconnected-(RESET0-P-PadP$1)")
  (net 78 "unconnected-(RESET0-S-PadP$3)")
  (net 79 "Net-(SHIFT_0-QH*)")
  (net 80 "unconnected-(SHIFT_1-QH*-Pad9)")
  (net 81 "unconnected-(U$1-CARD_DETECT-PadCARD_DETECT1)")
  (net 82 "unconnected-(U$1-CARD_DETECT1-PadCARD_DETECT2)")
  (net 83 "unconnected-(U2-~{NT{slash}SQW}-Pad3)")
  (net 84 "unconnected-(U2-~{RST}-Pad4)")
  (net 85 "unconnected-(U2-N.C.-Pad10)")
  (net 86 "unconnected-(U3-~{INT}{slash}SQW-Pad3)")
  (net 87 "unconnected-(U3-~{RST}-Pad4)")
  (net 88 "unconnected-(UNK2,1MM_JACK0-GNDBREAK-PadP$3)")
  (footprint "MusselGapeTracker_RevE:SOT95P237X112-3N" (layer "F.Cu")
    (at 114.975 78.375 90)
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "MCP1700T-3302" (at -1.9812 -2.159 90) (layer "F.SilkS") hide)
    (fp_text value "MCP1700T-3302E/TT" (at -1.651 2.9718 90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -0.9398 1.0414 90) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.9398 1.0414 90) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "VOUT") (pintype "output") (solder_mask_margin 0.0762))
    (pad "3" smd rect (at 0 -1.0414 90) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/VRAW1") (pinfunction "VIN") (pintype "input") (solder_mask_margin 0.0762))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 121.975 95.475 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at 1.8356 -0.3826 180) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "/32KHZ") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 134.8105 117.3101)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at -0.0281 -0.9707) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at 0.0619 1.1393) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/CS_SHIFT_REG") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MusselGapeTracker_RevE:1X01_SMALL" (layer "F.Cu")
    (at 130.3655 132.6771)
    (descr "0.035\" (0.89 mm) diameter drill, 0.055\" (1.397mm) copper diameter<br>\nThis hole should be barely large enough for standard 0.1\" pitch header pins.")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U$3" (at -1.3162 -1.2688) (layer "F.SilkS") hide)
    (fp_text value "PINHD-1X1SMALL" (at -1.26 1.915) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 1.397 1.397) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 6 "/RESET") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:STAND-OFF" (layer "F.Cu")
    (at 102.6795 106.1341)
    (descr "<b>Stand Off</b><p>\nThis is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447\nOuter keepout is 0.127\" radius (0.254\" diameter).")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "STANDOFF2" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "STAND-OFF4-40" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.302 3.302) (drill 3.302) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MusselGapeTracker_RevE:PUSHBUTTON_DPST_SMD" (layer "F.Cu")
    (at 105.3846 115.2652)
    (descr "PUSHBUTTON Omron B3S-1000 SMD DPST")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "BUTTON2" (at -3.8722 -3.3658) (layer "F.SilkS") hide)
    (fp_text value "PUSHBUTTON_DPST_SMDSTANDARD" (at -3.81 5.08) (layer "F.Fab") hide)
    (pad "P" smd rect (at 3.975 2.25) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "unconnected-(BUTTON2-PadP)") (pinfunction "P") (pintype "passive+no_connect") (solder_mask_margin 0.0762))
    (pad "P$1" smd rect (at -3.975 2.25) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "/BUTTON2") (pinfunction "P1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "S" smd rect (at 3.975 -2.25) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "unconnected-(BUTTON2-PadS)") (pinfunction "S") (pintype "passive+no_connect") (solder_mask_margin 0.0762))
    (pad "S$1" smd rect (at -3.975 -2.25) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "S1") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:JST-PH-4-THM" (layer "F.Cu")
    (at 152.5905 100.2921)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL6" (at -5 3) (layer "F.SilkS") hide)
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "/HALL6_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "/HALL6_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:1X01_SMALL" (layer "F.Cu")
    (at 132.6515 104.2291)
    (descr "0.035\" (0.89 mm) diameter drill, 0.055\" (1.397mm) copper diameter<br>\nThis hole should be barely large enough for standard 0.1\" pitch header pins.")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U$10" (at -1.3162 -1.2688) (layer "F.SilkS") hide)
    (fp_text value "PINHD-1X1SMALL" (at -1.26 1.915) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 1.397 1.397) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 57 "/ANALOG_0") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:JST-PH-4-THM" (layer "F.Cu")
    (at 164.7825 109.8171)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL9" (at -5 3) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "/HALL9_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "/HALL9_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:SO16" (layer "F.Cu")
    (at 141.5415 123.6601)
    (descr "<b>Small Outline package</b> 150 mil")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "SHIFT_1" (at -5.461 1.778 90) (layer "F.SilkS") hide)
    (fp_text value "74HC595D" (at -4.064 0.635) (layer "F.SilkS"))
    (pad "1" smd rect (at -4.445 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/HALL9_~{SLEEP}") (pinfunction "QB") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at -3.175 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/HALL10_~{SLEEP}") (pinfunction "QC") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "3" smd rect (at -1.905 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/HALL11_~{SLEEP}") (pinfunction "QD") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "4" smd rect (at -0.635 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "/HALL12_~{SLEEP}") (pinfunction "QE") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "5" smd rect (at 0.635 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "/HALL13_~{SLEEP}") (pinfunction "QF") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "6" smd rect (at 1.905 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/HALL14_~{SLEEP}") (pinfunction "QG") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "7" smd rect (at 3.175 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "/HALL15_~{SLEEP}") (pinfunction "QH") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "8" smd rect (at 4.445 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "9" smd rect (at 4.445 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "unconnected-(SHIFT_1-QH*-Pad9)") (pinfunction "QH*") (pintype "tri_state+no_connect") (solder_mask_margin 0.0762))
    (pad "10" smd rect (at 3.175 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/SHIFT_CLEAR") (pinfunction "~{SRCLR}") (pintype "input") (solder_mask_margin 0.0762))
    (pad "11" smd rect (at 1.905 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "/SCK") (pinfunction "SRCLK") (pintype "input") (solder_mask_margin 0.0762))
    (pad "12" smd rect (at 0.635 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/CS_SHIFT_REG") (pinfunction "RCLK") (pintype "input") (solder_mask_margin 0.0762))
    (pad "13" smd rect (at -0.635 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "~{OE}") (pintype "input") (solder_mask_margin 0.0762))
    (pad "14" smd rect (at -1.905 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "Net-(SHIFT_0-QH*)") (pinfunction "SER") (pintype "input") (solder_mask_margin 0.0762))
    (pad "15" smd rect (at -3.175 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/HALL8_~{SLEEP}") (pinfunction "QA") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "16" smd rect (at -4.445 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:PANASONIC_B" (layer "F.Cu")
    (at 112.1 81.425 90)
    (descr "<b>Panasonic Aluminium Electrolytic Capacitor VS-Serie Package B</b>")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C1" (at 1.4956 -1.2376 90) (layer "F.SilkS"))
    (fp_text value "1µF" (at -0.9144 1.8024 90) (layer "F.SilkS"))
    (pad "+" smd rect (at 2.0064 0 90) (size 2.667 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/VRAW1") (pinfunction "+") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "-" smd rect (at -2.0064 0 90) (size 2.667 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "-") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 134.9375 120.4851 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at -0.3843 -1.0351 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at -0.1743 1.0649 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 130.81 102.4636 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at 0.1676 -1.1958 180) (layer "F.SilkS"))
    (fp_text value "10k" (at -2.4324 0.2542 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "/SHIFT_CLEAR") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MusselGapeTracker_RevE:JST-PH-4-THM" (layer "F.Cu")
    (at 152.5905 116.8021)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL10" (at -5 3) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "/HALL10_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "/HALL10_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:CHIPLED_0805" (layer "F.Cu")
    (at 111.1885 99.4031 90)
    (descr "Surface mount LED 0805 footprint with marker for positive (anode) terminal")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "LED2" (at -1.27 1.27 180) (layer "F.SilkS") hide)
    (fp_text value "GREEN_LED" (at 1.27 1.27 180) (layer "F.Fab") hide)
    (fp_text user "+" (at -0.1778 1.651 90) (layer "F.Fab"))
    (pad "A" smd rect (at 0 1.05 90) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "Net-(LED2-PadA)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "C" smd rect (at 0 -1.05 90) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:PUSHBUTTON_DPST_SMD" (layer "F.Cu")
    (at 110.7948 107.0102)
    (descr "PUSHBUTTON Omron B3S-1000 SMD DPST")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "BUTTON1" (at -3.81 -3.81) (layer "F.SilkS") hide)
    (fp_text value "PUSHBUTTON_DPST_SMDSTANDARD" (at -3.81 5.08) (layer "F.Fab") hide)
    (pad "P" smd rect (at 3.975 2.25) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "unconnected-(BUTTON1-PadP)") (pinfunction "P") (pintype "passive+no_connect") (solder_mask_margin 0.0762))
    (pad "P$1" smd rect (at -3.975 2.25) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "/BUTTON1") (pinfunction "P1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "S" smd rect (at 3.975 -2.25) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "unconnected-(BUTTON1-PadS)") (pinfunction "S") (pintype "passive+no_connect") (solder_mask_margin 0.0762))
    (pad "S$1" smd rect (at -3.975 -2.25) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "S1") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:2X3" (layer "F.Cu")
    (at 127.9779 117.5133 180)
    (descr "ISP programming header for Arduino<br>\nKeepout area gives approximate footprint of connector from AVR MKII ISP")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "J1" (at -3.81 -4.445 180) (layer "F.SilkS") hide)
    (fp_text value "AVR_SPI_PRG_6PTH" (at -3.81 3.175 180) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at -2.54 0 180) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 43 "/MISO") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole roundrect (at -2.54 -2.54 180) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 2 "VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole roundrect (at 0 0 180) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 44 "/SCK") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole roundrect (at 0 -2.54 180) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 45 "/MOSI") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "5" thru_hole roundrect (at 2.54 0 180) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 6 "/RESET") (pinfunction "5") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "6" thru_hole roundrect (at 2.54 -2.54 180) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 1 "GND") (pinfunction "6") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:STAND-OFF_M2" (layer "F.Cu")
    (at 112.25 88.775)
    (descr "M2 stand-off hole<p>\nDrill diam = 2.2mm <br>\nOuter keepout diameter = 3.175mm (0.125\")")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "STANDOFF5_M2" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "STAND-OFFM2" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MusselGapeTracker_RevE:1X01_SMALL" (layer "F.Cu")
    (at 130.7 88.55)
    (descr "0.035\" (0.89 mm) diameter drill, 0.055\" (1.397mm) copper diameter<br>\nThis hole should be barely large enough for standard 0.1\" pitch header pins.")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U$17" (at -1.3162 -1.2688) (layer "F.SilkS") hide)
    (fp_text value "PINHD-1X1SMALL" (at -1.26 1.915) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 1.397 1.397) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 70 "/AREF") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:JST-PH-4-THM" (layer "F.Cu")
    (at 164.7825 116.8021)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL11" (at -5 3) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "/HALL11_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "/HALL11_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:JST-PH-4-THM" (layer "F.Cu")
    (at 164.7825 130.7721)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL15" (at -5 3) (layer "F.SilkS") hide)
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 41 "/HALL15_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 42 "/HALL15_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 135.6868 103.9751 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at -0.5343 -1.1244 90) (layer "F.SilkS"))
    (fp_text value "100k" (at -0.6043 1.0156 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "/ANALOG_0") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MusselGapeTracker_RevE:1X01_SMALL" (layer "F.Cu")
    (at 99.3775 108.9281)
    (descr "0.035\" (0.89 mm) diameter drill, 0.055\" (1.397mm) copper diameter<br>\nThis hole should be barely large enough for standard 0.1\" pitch header pins.")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U$6" (at -1.3162 -1.2688) (layer "F.SilkS") hide)
    (fp_text value "PINHD-1X1SMALL" (at -1.26 1.915) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 1.397 1.397) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 68 "/BUTTON1") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:1X01_SMALL" (layer "F.Cu")
    (at 99.3775 111.4681)
    (descr "0.035\" (0.89 mm) diameter drill, 0.055\" (1.397mm) copper diameter<br>\nThis hole should be barely large enough for standard 0.1\" pitch header pins.")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U$7" (at -1.3162 -1.2688) (layer "F.SilkS") hide)
    (fp_text value "PINHD-1X1SMALL" (at -1.26 1.915) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 1.397 1.397) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 1 "GND") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 122.1613 131.2547 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0.3753 -1.2689 90) (layer "F.SilkS"))
    (fp_text value "100k Ω" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "Net-(U$1-DAT2_RES)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 113.4106 85.904)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R32" (at 0.5118 -1.1546) (layer "F.SilkS"))
    (fp_text value "10k" (at 0.7418 1.1854) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "/BATT_MONITOR_EN") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MusselGapeTracker_RevE:1X01_SMALL" (layer "F.Cu")
    (at 119.5705 132.6771)
    (descr "0.035\" (0.89 mm) diameter drill, 0.055\" (1.397mm) copper diameter<br>\nThis hole should be barely large enough for standard 0.1\" pitch header pins.")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "PB7" (at -1.3162 -1.2688) (layer "F.SilkS"))
    (fp_text value "PINHD-1X1SMALL" (at -1.26 1.915) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 1.397 1.397) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 52 "/PB7") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 109.8546 85.904 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R33" (at -0.1178 1.1446 180) (layer "F.SilkS"))
    (fp_text value "10k" (at 2.4622 -0.7954 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/GATE") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/VRAW1") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MusselGapeTracker_RevE:1X04_LOCK" (layer "F.Cu")
    (at 124.12 87.623)
    (descr "0.035\" drills, 0.056\" pad width<br>\nStaggered holes to help hold header in position while soldering.")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "OLED" (at -1.4876 -2.5636) (layer "F.SilkS"))
    (fp_text value "PINHD-1X4LOCK" (at -5.08 2.54) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at -3.81 -0.127 90) (size 1.4224 1.4224) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 1 "GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole roundrect (at -1.27 0.127 90) (size 1.4224 1.4224) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 2 "VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole roundrect (at 1.27 -0.127 90) (size 1.4224 1.4224) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 50 "/SCL") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole roundrect (at 3.81 0.127 90) (size 1.4224 1.4224) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 51 "/SDA") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:CHIPLED_0805" (layer "F.Cu")
    (at 111.1885 97.4981 90)
    (descr "Surface mount LED 0805 footprint with marker for positive (anode) terminal")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "LED1" (at -1.27 1.27 180) (layer "F.SilkS") hide)
    (fp_text value "RED_LED" (at 1.27 1.27 180) (layer "F.Fab") hide)
    (fp_text user "+" (at -0.1778 1.651 90) (layer "F.Fab"))
    (pad "A" smd rect (at 0 1.05 90) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "Net-(LED1-PadA)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "C" smd rect (at 0 -1.05 90) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:STAND-OFF" (layer "F.Cu")
    (at 138.6205 131.4071)
    (descr "<b>Stand Off</b><p>\nThis is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447\nOuter keepout is 0.127\" radius (0.254\" diameter).")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "STANDOFF3" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "STAND-OFF4-40" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.302 3.302) (drill 3.302) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MusselGapeTracker_RevE:PANASONIC_B" (layer "F.Cu")
    (at 118.325 81.45 90)
    (descr "<b>Panasonic Aluminium Electrolytic Capacitor VS-Serie Package B</b>")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C2" (at -1.3594 -2.0926 90) (layer "F.SilkS"))
    (fp_text value "1µF" (at -0.8394 1.8074 270) (layer "F.SilkS"))
    (pad "+" smd rect (at 2.0064 0 90) (size 2.667 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "+") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "-" smd rect (at -2.0064 0 90) (size 2.667 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "-") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:JST-PH-4-THM" (layer "F.Cu")
    (at 152.5905 79.3371)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL0" (at -5 3) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "/HALL0_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "/HALL0_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 133.4897 107.2263)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C23" (at 0.8927 -0.9669) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 3.1227 0.5231) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/AVCC") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/AGND") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 117.1575 107.5311 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0.0051 1.1417 180) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0 1.43 180) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MusselGapeTracker_RevE:JST-PH-4-THM" (layer "F.Cu")
    (at 152.5905 123.7871)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL12" (at -5 3) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "/HALL12_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "/HALL12_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 135.4455 113.2461 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R28" (at -0.0233 -1.0331 90) (layer "F.SilkS"))
    (fp_text value "10kΩ" (at -2.0933 -0.1531 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "/MUX_~{EN}") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MusselGapeTracker_RevE:CR1220_BATTERY_HOLDER_SMD" (layer "F.Cu")
    (at 137.4775 83.1471)
    (descr "CR1220 Battery Holder, SMD\nKeystone Part # 3000")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "CR1220_BATTERY0" (at -2.54 8.89) (layer "F.SilkS") hide)
    (fp_text value "CR1220_BATTERY_HOLDERSMD" (at 0 0) (layer "F.Fab") hide)
    (pad "GND" smd rect (at 0 0) (size 4.064 4.064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "P$1" smd rect (at -7.62 0) (size 3.429 3.429) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/VBAT") (pinfunction "VBAT") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 7.62 0) (size 3.429 3.429) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/VBAT") (pinfunction "P$2") (pintype "power_in") (solder_mask_margin 0.0762))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 115.7 95.575 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 1.9456 -0.0176 180) (layer "F.SilkS"))
    (fp_text value "10k Ω" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/RESET") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MusselGapeTracker_RevE:1X01_SMALL" (layer "F.Cu")
    (at 99.3775 114.0081)
    (descr "0.035\" (0.89 mm) diameter drill, 0.055\" (1.397mm) copper diameter<br>\nThis hole should be barely large enough for standard 0.1\" pitch header pins.")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U$8" (at -1.3162 -1.2688) (layer "F.SilkS") hide)
    (fp_text value "PINHD-1X1SMALL" (at -1.26 1.915) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 1.397 1.397) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 69 "/BUTTON2") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:JST-PH-4-THM" (layer "F.Cu")
    (at 152.5905 109.8171)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL8" (at -5 3) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "/HALL8_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 28 "/HALL8_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:JST-PH-4-THM" (layer "F.Cu")
    (at 152.5905 86.3221)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL2" (at -5 3) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "/HALL2_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "/HALL2_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 117.1956 101.346 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0.0934 -1.43) (layer "F.SilkS"))
    (fp_text value "100 Ω" (at 0 1.43 -90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(LED1-PadA)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "/LED_RED") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 120.5992 91.567 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R29" (at -0.2276 -1.3332 -90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0.0124 0.9968 -90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "/BATT_MONITOR") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 137.3505 112.3571 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 1.9077 0.0019 180) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at -2.1123 0.1319 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 124.6251 125.3111 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.43 -90) (layer "F.SilkS"))
    (fp_text value "100k Ω" (at 0 1.43 -90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(U$1-DAT1_NC)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MusselGapeTracker_RevE:1X06-RIGHT_ANGLE" (layer "F.Cu")
    (at 105.7275 102.0701 90)
    (descr "1x06 0.1\" spacing right angle header<p>\nExample: Sullins PPPC061LGBN-RC, Digikey PN S5481-ND")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "JP1" (at -0.7993 -1.7551 90) (layer "F.SilkS"))
    (fp_text value "FTDI_HEADER" (at -1.27 2.54 90) (layer "F.Fab") hide)
    (fp_text user "2" (at 2.54 -8.89 90) (layer "F.Fab"))
    (fp_text user "3" (at 5.08 -8.89 90) (layer "F.Fab"))
    (fp_text user "6" (at 12.7 -8.89 90) (layer "F.Fab"))
    (fp_text user "5" (at 10.16 -8.89 90) (layer "F.Fab"))
    (fp_text user "1" (at 0 -8.89 90) (layer "F.Fab"))
    (fp_text user "4" (at 7.62 -8.89 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 180) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 1 "GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole roundrect (at 2.54 0 180) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 1 "GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole roundrect (at 5.08 0 180) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 2 "VCC") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole roundrect (at 7.62 0 180) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 46 "/TO_FTDI_TX") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "5" thru_hole roundrect (at 10.16 0 180) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 47 "/TO_FTDI_RX") (pinfunction "5") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "6" thru_hole roundrect (at 12.7 0 180) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 5 "/DTR") (pinfunction "6") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 117.975 95.5 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 1.8306 0.1074 180) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "/SCL") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MusselGapeTracker_RevE:1X01_SMALL" (layer "F.Cu")
    (at 99.3775 116.5481)
    (descr "0.035\" (0.89 mm) diameter drill, 0.055\" (1.397mm) copper diameter<br>\nThis hole should be barely large enough for standard 0.1\" pitch header pins.")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U$9" (at -1.3162 -1.2688) (layer "F.SilkS") hide)
    (fp_text value "PINHD-1X1SMALL" (at -1.26 1.915) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 1.397 1.397) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 1 "GND") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:SO16" (layer "F.Cu")
    (at 141.7955 99.2761)
    (descr "<b>Small Outline package</b> 150 mil")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "SHIFT_0" (at -5.461 1.778 90) (layer "F.SilkS") hide)
    (fp_text value "74HC595D" (at -4.0331 1.3333) (layer "F.SilkS"))
    (pad "1" smd rect (at -4.445 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/HALL1_~{SLEEP}") (pinfunction "QB") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at -3.175 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/HALL2_~{SLEEP}") (pinfunction "QC") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "3" smd rect (at -1.905 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/HALL3_~{SLEEP}") (pinfunction "QD") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "4" smd rect (at -0.635 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/HALL4_~{SLEEP}") (pinfunction "QE") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "5" smd rect (at 0.635 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/HALL5_~{SLEEP}") (pinfunction "QF") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "6" smd rect (at 1.905 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/HALL6_~{SLEEP}") (pinfunction "QG") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "7" smd rect (at 3.175 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "/HALL7_~{SLEEP}") (pinfunction "QH") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "8" smd rect (at 4.445 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "9" smd rect (at 4.445 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "Net-(SHIFT_0-QH*)") (pinfunction "QH*") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "10" smd rect (at 3.175 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/SHIFT_CLEAR") (pinfunction "~{SRCLR}") (pintype "input") (solder_mask_margin 0.0762))
    (pad "11" smd rect (at 1.905 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "/SCK") (pinfunction "SRCLK") (pintype "input") (solder_mask_margin 0.0762))
    (pad "12" smd rect (at 0.635 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/CS_SHIFT_REG") (pinfunction "RCLK") (pintype "input") (solder_mask_margin 0.0762))
    (pad "13" smd rect (at -0.635 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "~{OE}") (pintype "input") (solder_mask_margin 0.0762))
    (pad "14" smd rect (at -1.905 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/MOSI") (pinfunction "SER") (pintype "input") (solder_mask_margin 0.0762))
    (pad "15" smd rect (at -3.175 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/HALL0_~{SLEEP}") (pinfunction "QA") (pintype "tri_state") (solder_mask_margin 0.0762))
    (pad "16" smd rect (at -4.445 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:SOT23-3" (layer "F.Cu")
    (at 108.9 88.75 180)
    (descr "SOT23-3 package<br>\nPad size 0.8 x 0.9mm")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "P-FET0" (at -1.6624 -0.4394) (layer "F.SilkS"))
    (fp_text value "MOSFET-PCHANNELBSH203" (at -1.016 0.1905) (layer "F.Fab") hide)
    (fp_text user "1" (at -1.24 0.53) (layer "F.Fab"))
    (fp_text user "2" (at 1.02 0.54) (layer "F.Fab"))
    (fp_text user "3" (at -0.1 -0.28) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 1 180) (size 0.8 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/GATE") (pinfunction "G") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.95 1 180) (size 0.8 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/VRAW1") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" smd rect (at 0 -1.1 180) (size 0.8 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "Net-(P-FET0-D)") (pinfunction "D") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:1X01_SMALL" (layer "F.Cu")
    (at 125.2855 132.6771)
    (descr "0.035\" (0.89 mm) diameter drill, 0.055\" (1.397mm) copper diameter<br>\nThis hole should be barely large enough for standard 0.1\" pitch header pins.")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U$4" (at -1.3162 -1.2688) (layer "F.SilkS") hide)
    (fp_text value "PINHD-1X1SMALL" (at -1.26 1.915) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 1.397 1.397) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 1 "GND") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 119.975 95.475 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 1.8356 0.0174 180) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "/SDA") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MusselGapeTracker_RevE:STAND-OFF_M2" (layer "F.Cu")
    (at 112.275 112.55)
    (descr "M2 stand-off hole<p>\nDrill diam = 2.2mm <br>\nOuter keepout diameter = 3.175mm (0.125\")")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "STANDOFF4_M2" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "STAND-OFFM2" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers "F&B.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 135.8138 100.4316 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at 2.5922 0.0686 180) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.4822 1.4386 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MusselGapeTracker_RevE:22-23-2021" (layer "F.Cu")
    (at 124.175 79.025 90)
    (descr ".100\" (2.54mm) Center Headers - 2 Pin")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "MOLEX_KK0" (at -2.54 -3.81 90) (layer "F.SilkS") hide)
    (fp_text value "22-23-2021" (at -2.54 5.08 90) (layer "F.Fab") hide)
    (pad "1" thru_hole oval (at -1.27 0 180) (size 3 1.5) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole oval (at 1.27 0 180) (size 3 1.5) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "/VRAW1") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:PUSHBUTTON_SPST_PTS525_SERIES" (layer "F.Cu")
    (at 130.1115 127.7239 90)
    (descr "C&K PTS525 series tactile switch<br>\nSmall surface mount switches")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "RESET0" (at -3.81 -3.175 90) (layer "F.SilkS"))
    (fp_text value "PUSHBUTTON_DPST_SMDSMALL" (at -3.81 3.81 90) (layer "F.Fab") hide)
    (fp_text user "2" (at 2.72 -1.845 90) (layer "F.Fab"))
    (fp_text user "3" (at -2.78 2.005 90) (layer "F.Fab"))
    (fp_text user "4" (at 2.58 2.04 90) (layer "F.Fab"))
    (fp_text user "1" (at -2.73 -1.785 90) (layer "F.Fab"))
    (pad "P$1" smd rect (at -3.2 -1.9 90) (size 1.6 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "unconnected-(RESET0-P-PadP$1)") (pinfunction "P") (pintype "passive+no_connect") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 3.2 -1.9 90) (size 1.6 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "P1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$3" smd rect (at -3.2 1.9 90) (size 1.6 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "unconnected-(RESET0-S-PadP$3)") (pinfunction "S") (pintype "passive+no_connect") (solder_mask_margin 0.0762))
    (pad "P$4" smd rect (at 3.2 1.9 90) (size 1.6 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/RESET") (pinfunction "S1") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:JST-PH-4-THM" (layer "F.Cu")
    (at 164.7825 100.2921)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL7" (at -5 3) (layer "F.SilkS") hide)
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "/HALL7_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 26 "/HALL7_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:SOT23" (layer "F.Cu")
    (at 116.9 88.9 180)
    (descr "<b>SOT-23</b>")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "BJT0" (at 1.0676 -0.6494) (layer "F.SilkS"))
    (fp_text value "KSC1623_BJT_TRANSISTOR" (at -1.645 2.585) (layer "F.Fab") hide)
    (fp_text user "2" (at 1.04 0.52) (layer "F.Fab"))
    (fp_text user "1" (at -1.25 0.52) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 1.1 180) (size 1 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "Net-(BJT0-B)") (pinfunction "B") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.95 1.1 180) (size 1 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "E") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" smd rect (at 0 -1.1 180) (size 1 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/GATE") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:JST-PH-4-THM" (layer "F.Cu")
    (at 164.7825 123.7871)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL13" (at -5 3) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 37 "/HALL13_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 38 "/HALL13_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:MICROSD_SOCKET_MOLEX_REVERSEMOUNT" (layer "F.Cu")
    (at 113.3475 132.2707 90)
    (descr "<b>Molex micro SD card slot, push-push spring-loaded style \"reverse mount\"</b><br>\nMolex PN 5027740891<br>\nDigikey PN WM24066CT-ND<br>\nThis version has the surface mount pins easily accessible at the rear of the housing rather than underneath it like most other sockets.")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U$1" (at 5.2313 -0.9751 90) (layer "F.SilkS"))
    (fp_text value "MICROSD_MOLEX_REVERSECURRENT" (at 0 0 90) (layer "F.Fab") hide)
    (fp_text user "RSV8" (at 1.524 1.524 180) (layer "F.Fab"))
    (fp_text user "GND" (at -0.254 1.524 180) (layer "F.Fab"))
    (fp_text user "MOSI" (at 6.985 1.524 180) (layer "F.Fab"))
    (fp_text user "SCK" (at 4.699 1.524 180) (layer "F.Fab"))
    (fp_text user "GND" (at -0.254 -13.462 180) (layer "F.Fab"))
    (fp_text user "RSV1" (at 9.144 1.524 180) (layer "F.Fab"))
    (fp_text user "GND" (at 12.954 -13.462 180) (layer "F.Fab"))
    (fp_text user "GND" (at 3.556 1.524 180) (layer "F.Fab"))
    (fp_text user "CS" (at 8.001 1.524 180) (layer "F.Fab"))
    (fp_text user "VDD" (at 5.715 1.524 180) (layer "F.Fab"))
    (fp_text user "CD1" (at -0.762 -7.874 90) (layer "F.Fab"))
    (fp_text user "CD2" (at -0.762 -0.508 90) (layer "F.Fab"))
    (fp_text user "MISO" (at 2.54 1.524 180) (layer "F.Fab"))
    (fp_text user "GND" (at 12.446 1.524 180) (layer "F.Fab"))
    (pad "CARD_DETECT1" smd rect (at -0.645 -8.12 90) (size 1.29 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "unconnected-(U$1-CARD_DETECT-PadCARD_DETECT1)") (pinfunction "CARD_DETECT") (pintype "passive+no_connect") (solder_mask_margin 0.0762))
    (pad "CARD_DETECT2" smd rect (at -0.645 -0.65 90) (size 1.29 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "unconnected-(U$1-CARD_DETECT1-PadCARD_DETECT2)") (pinfunction "CARD_DETECT1") (pintype "passive+no_connect") (solder_mask_margin 0.0762))
    (pad "CS2" smd rect (at 7.8 0.84 90) (size 0.8 1.68) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/CS_SD") (pinfunction "CS") (pintype "input") (solder_mask_margin 0.0762))
    (pad "GND6" smd rect (at 3.4 0.84 90) (size 0.8 1.68) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS_GND") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "MISO7" smd rect (at 2.3 0.84 90) (size 0.8 1.68) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "/MISO") (pinfunction "DATA_OUT_MISO") (pintype "output") (solder_mask_margin 0.0762))
    (pad "MNT1" smd rect (at -0.2 0.93 270) (size 1.6 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND1") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "MNT2" smd rect (at 12.45 0.93 90) (size 1.7 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND2") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "MNT3" smd rect (at -0.54 -13.92 90) (size 1.5 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND3") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "MNT4" smd rect (at 12.75 -13.92 90) (size 1.5 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND4") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "MOSI3" smd rect (at 6.7 0.84 90) (size 0.8 1.68) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/MOSI") (pinfunction "DATA_IN_MOSI") (pintype "input") (solder_mask_margin 0.0762))
    (pad "NC1" smd rect (at 8.9 0.84 90) (size 0.8 1.68) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "Net-(U$1-DAT1_NC)") (pinfunction "DAT1_NC") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "RES8" smd rect (at 1.2 0.84 90) (size 0.8 1.68) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "Net-(U$1-DAT2_RES)") (pinfunction "DAT2_RES") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "SCK5" smd rect (at 4.5 0.84 90) (size 0.8 1.68) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "/SCK") (pinfunction "SCLK") (pintype "input") (solder_mask_margin 0.0762))
    (pad "VDD4" smd rect (at 5.6 0.84 90) (size 0.8 1.68) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:STAND-OFF" (layer "F.Cu")
    (at 143.4465 91.7831)
    (descr "<b>Stand Off</b><p>\nThis is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447\nOuter keepout is 0.127\" radius (0.254\" diameter).")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "STANDOFF1" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "STAND-OFF4-40" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.302 3.302) (drill 3.302) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 121.7295 127.5971 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at -0.0377 3.2071 -90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0 1.43 -90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MusselGapeTracker_RevE:JST-PH-4-THM" (layer "F.Cu")
    (at 152.5905 93.3071)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL4" (at -5 3) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "/HALL4_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "/HALL4_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:1X01_SMALL" (layer "F.Cu")
    (at 117.0305 132.6771)
    (descr "0.035\" (0.89 mm) diameter drill, 0.055\" (1.397mm) copper diameter<br>\nThis hole should be barely large enough for standard 0.1\" pitch header pins.")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "GND0" (at -1.3162 -1.2688) (layer "F.SilkS"))
    (fp_text value "PINHD-1X1SMALL" (at -1.26 1.915) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 1.397 1.397) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 1 "GND") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:JST-PH-4-THM" (layer "F.Cu")
    (at 164.7825 79.3371)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL1" (at -5 3) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "/HALL1_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "/HALL1_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:I_0805" (layer "F.Cu")
    (at 133.4643 110.0965)
    (descr "<b>0805 (2012) Inductor footprint<br></b>\nExample:\nTaiyo Yuden inductor # LBR2012T100K<br>\nDigikey PN 587-2045-1-ND")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "INDUCTOR0" (at -2 -0.8471) (layer "F.SilkS"))
    (fp_text value "10µH" (at -0.3319 1.6429) (layer "F.SilkS"))
    (pad "P$1" smd rect (at -0.85 0) (size 0.7 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/AVCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$2" smd rect (at 0.85 0) (size 0.7 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:1X01_SMALL" (layer "F.Cu")
    (at 145.2245 131.9151)
    (descr "0.035\" (0.89 mm) diameter drill, 0.055\" (1.397mm) copper diameter<br>\nThis hole should be barely large enough for standard 0.1\" pitch header pins.")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U$11" (at -1.5121 -1.3657) (layer "F.SilkS") hide)
    (fp_text value "PINHD-1X1SMALL" (at -1.26 1.915) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0) (size 1.397 1.397) (drill 0.9) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 9 "/AGND") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:JST-PH-4-THM" (layer "F.Cu")
    (at 152.5905 130.7721)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL14" (at -5 3) (layer "F.SilkS") hide)
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 39 "/HALL14_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 40 "/HALL14_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 114.225 91.5 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R30" (at -0.1306 -1.2774 -90) (layer "F.SilkS"))
    (fp_text value "15k" (at -0.0706 1.1126 -90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "/BATT_MONITOR") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(P-FET0-D)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MusselGapeTracker_RevE:POWER_JACK_DC_2,1MM" (layer "F.Cu")
    (at 106.8705 80.6071 180)
    (descr "2.1 mm DC power jack. Digikey PN CP-202AH-ND")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "UNK2,1MM_JACK0" (at 8.89 -5.08 180) (layer "F.SilkS") hide)
    (fp_text value "POWER_JACK_2,1MM" (at 8.89 6.35 180) (layer "F.Fab") hide)
    (fp_text user "GND" (at 7.9681 2.2777 180) (layer "F.SilkS"))
    (fp_text user "+" (at -0.7219 2.0377 180) (layer "F.SilkS"))
    (pad "P$1" thru_hole circle (at 0 0 270) (size 4.572 4.572) (drill 3.175) (layers "*.Cu" "*.Mask")
      (net 4 "/VRAW1") (pinfunction "PWR") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$2" thru_hole rect (at 6.096 0 180) (size 4.191 4.191) (drill 3.175) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P$3" thru_hole rect (at 3.048 -4.826 180) (size 3.816 3.816) (drill 2.8) (layers "*.Cu" "*.Mask")
      (net 88 "unconnected-(UNK2,1MM_JACK0-GNDBREAK-PadP$3)") (pinfunction "GNDBREAK") (pintype "bidirectional+no_connect") (solder_mask_margin 0.0762))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 112.2553 94.9073)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at -1.5129 -1.3379) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/DTR") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/RESET") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 117.0305 127.5971 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at 0.0923 -6.2119 -90) (layer "F.SilkS"))
    (fp_text value "10µF" (at -0.0877 -3.3319 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 122.3824 99.3144 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 0.04 -1.445 180) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0 1.43 180) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 114.554 101.3714 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0.088 1.4016) (layer "F.SilkS"))
    (fp_text value "100 Ω" (at 0 1.43 -90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(LED2-PadA)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "/LED_GRN") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (at 129.6924 96.1644)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "±5ppm, I2C Real-Time Clock SOIC-8")
    (property "ki_keywords" "RTC TCXO Realtime Time Clock MEMS I2C")
    (attr smd)
    (fp_text reference "U3" (at -0.01 -3.075) (layer "F.SilkS"))
    (fp_text value "DS3231MZ" (at 0 3.4) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "/32KHZ") (pinfunction "32KHZ") (pintype "open_collector"))
    (pad "2" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (pad "3" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "unconnected-(U3-~{INT}{slash}SQW-Pad3)") (pinfunction "~{INT}/SQW") (pintype "open_collector+no_connect"))
    (pad "4" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "unconnected-(U3-~{RST}-Pad4)") (pinfunction "~{RST}") (pintype "bidirectional+no_connect"))
    (pad "5" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "6" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/VBAT") (pinfunction "VBAT") (pintype "power_in"))
    (pad "7" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "/SCL") (pinfunction "SCL") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm" (layer "F.Cu")
    (at 142.5575 111.9761 -90)
    (descr "TSSOP, 24 Pin (JEDEC MO-153 Var AD https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U$2" (at 0 -4.85 90) (layer "F.SilkS"))
    (fp_text value "74HC4067" (at -0.3067 -0.7349 180) (layer "F.SilkS"))
    (pad "1" smd roundrect (at -2.8625 -3.575 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "/ANALOG_0") (pinfunction "COM") (pintype "output"))
    (pad "2" smd roundrect (at -2.8625 -2.925 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/HALL7_OUTPUT") (pinfunction "X7") (pintype "input"))
    (pad "3" smd roundrect (at -2.8625 -2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/HALL6_OUTPUT") (pinfunction "X6") (pintype "input"))
    (pad "4" smd roundrect (at -2.8625 -1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/HALL5_OUTPUT") (pinfunction "X5") (pintype "input"))
    (pad "5" smd roundrect (at -2.8625 -0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/HALL4_OUTPUT") (pinfunction "X4") (pintype "input"))
    (pad "6" smd roundrect (at -2.8625 -0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/HALL3_OUTPUT") (pinfunction "X3") (pintype "input"))
    (pad "7" smd roundrect (at -2.8625 0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/HALL2_OUTPUT") (pinfunction "X2") (pintype "input"))
    (pad "8" smd roundrect (at -2.8625 0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/HALL1_OUTPUT") (pinfunction "X1") (pintype "input"))
    (pad "9" smd roundrect (at -2.8625 1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/HALL0_OUTPUT") (pinfunction "X0") (pintype "input"))
    (pad "10" smd roundrect (at -2.8625 2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/MUX_S0") (pinfunction "S0") (pintype "input"))
    (pad "11" smd roundrect (at -2.8625 2.925 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "/MUX_S1") (pinfunction "S1") (pintype "input"))
    (pad "12" smd roundrect (at -2.8625 3.575 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "13" smd roundrect (at 2.8625 3.575 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "/MUX_S3") (pinfunction "S3") (pintype "input"))
    (pad "14" smd roundrect (at 2.8625 2.925 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "/MUX_S2") (pinfunction "S2") (pintype "input"))
    (pad "15" smd roundrect (at 2.8625 2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "/MUX_~{EN}") (pinfunction "~{E}") (pintype "input"))
    (pad "16" smd roundrect (at 2.8625 1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/HALL15_OUTPUT") (pinfunction "X15") (pintype "input"))
    (pad "17" smd roundrect (at 2.8625 0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/HALL14_OUTPUT") (pinfunction "X14") (pintype "input"))
    (pad "18" smd roundrect (at 2.8625 0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/HALL13_OUTPUT") (pinfunction "X13") (pintype "input"))
    (pad "19" smd roundrect (at 2.8625 -0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/HALL12_OUTPUT") (pinfunction "X12") (pintype "input"))
    (pad "20" smd roundrect (at 2.8625 -0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/HALL11_OUTPUT") (pinfunction "X11") (pintype "input"))
    (pad "21" smd roundrect (at 2.8625 -1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/HALL10_OUTPUT") (pinfunction "X10") (pintype "input"))
    (pad "22" smd roundrect (at 2.8625 -2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/HALL9_OUTPUT") (pinfunction "X9") (pintype "input"))
    (pad "23" smd roundrect (at 2.8625 -2.925 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/HALL8_OUTPUT") (pinfunction "X8") (pintype "input"))
    (pad "24" smd roundrect (at 2.8625 -3.575 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-24_4.4x7.8mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MusselGapeTracker_RevE:JST-PH-4-THM" (layer "F.Cu")
    (at 164.7825 86.3221)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL3" (at -5 3) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 17 "/HALL3_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 18 "/HALL3_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "DS3231M_TRL:SOIC127P1032X265-16N" (layer "F.Cu")
    (at 129.525 95.7 90)
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at -1.6494 -0.1726 180) (layer "F.SilkS"))
    (fp_text value "DS3231M+TRL" (at 6.85 6.062 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -4.655 -4.445 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 55 "/32KHZ") (pinfunction "32KHZ") (pintype "output"))
    (pad "2" smd roundrect (at -4.655 -3.175 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (pad "3" smd roundrect (at -4.655 -1.905 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 83 "unconnected-(U2-~{NT{slash}SQW}-Pad3)") (pinfunction "~{NT/SQW}") (pintype "output+no_connect"))
    (pad "4" smd roundrect (at -4.655 -0.635 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 84 "unconnected-(U2-~{RST}-Pad4)") (pinfunction "~{RST}") (pintype "bidirectional+no_connect"))
    (pad "5" smd roundrect (at -4.655 0.635 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 85 "unconnected-(U2-N.C.-Pad10)") (pinfunction "N.C.") (pintype "bidirectional+no_connect"))
    (pad "6" smd roundrect (at -4.655 1.905 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 85 "unconnected-(U2-N.C.-Pad10)") (pinfunction "N.C.") (pintype "bidirectional+no_connect"))
    (pad "7" smd roundrect (at -4.655 3.175 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 85 "unconnected-(U2-N.C.-Pad10)") (pinfunction "N.C.") (pintype "bidirectional+no_connect"))
    (pad "8" smd roundrect (at -4.655 4.445 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 85 "unconnected-(U2-N.C.-Pad10)") (pinfunction "N.C.") (pintype "bidirectional+no_connect"))
    (pad "9" smd roundrect (at 4.655 4.445 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 85 "unconnected-(U2-N.C.-Pad10)") (pinfunction "N.C.") (pintype "bidirectional+no_connect"))
    (pad "10" smd roundrect (at 4.655 3.175 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 85 "unconnected-(U2-N.C.-Pad10)") (pinfunction "N.C.") (pintype "bidirectional+no_connect"))
    (pad "11" smd roundrect (at 4.655 1.905 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 85 "unconnected-(U2-N.C.-Pad10)") (pinfunction "N.C.") (pintype "bidirectional+no_connect"))
    (pad "12" smd roundrect (at 4.655 0.635 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 85 "unconnected-(U2-N.C.-Pad10)") (pinfunction "N.C.") (pintype "bidirectional+no_connect"))
    (pad "13" smd roundrect (at 4.655 -0.635 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "14" smd roundrect (at 4.655 -1.905 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 10 "/VBAT") (pinfunction "VBAT") (pintype "power_in"))
    (pad "15" smd roundrect (at 4.655 -3.175 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 51 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "16" smd roundrect (at 4.655 -4.445 90) (size 2.05 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 50 "/SCL") (pinfunction "SCL") (pintype "input"))
  )
  (footprint "MusselGapeTracker_RevE:JST-PH-4-THM" (layer "F.Cu")
    (at 164.7825 93.3071)
    (descr "<b>JST PH series 4-pin male header, shrouded<br></b>\nJST PN B4B-PH-K-S")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "HALL5" (at -5 3) (layer "F.SilkS"))
    (fp_text value "JST-4PINTH_STRAIGHT" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at 3 -1) (layer "F.Fab"))
    (fp_text user "4" (at -3 -1) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "2" thru_hole circle (at 1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "/AGND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "3" thru_hole circle (at -1 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "/HALL5_~{SLEEP}") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "4" thru_hole circle (at -3 0 180) (size 1.4224 1.4224) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "/HALL5_OUTPUT") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (footprint "MusselGapeTracker_RevE:TQFP32-08" (layer "F.Cu")
    (at 125.4125 107.9121)
    (descr "<B>Thin Plasic Quad Flat Package</B> Grid 0.8 mm")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U1" (at -3.175 -5.08) (layer "F.SilkS"))
    (fp_text value "ATMEGA328P" (at -2.1301 -1.3527) (layer "F.SilkS"))
    (pad "1" smd rect (at -4.2926 -2.8) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "/BUTTON2") (pinfunction "PD3(INT1)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at -4.2926 -2) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "/LED_RED") (pinfunction "PD4(XCK/T0)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "3" smd rect (at -4.2926 -1.2) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND@1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "4" smd rect (at -4.2926 -0.4) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "VCC@1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "5" smd rect (at -4.2926 0.4) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND@2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "6" smd rect (at -4.2926 1.2) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "VCC@2") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "7" smd rect (at -4.2926 2) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/32KHZ") (pinfunction "PB6(XTAL1/TOSC1)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "8" smd rect (at -4.2926 2.8) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "/PB7") (pinfunction "PB7(XTAL2/TOSC2)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "9" smd rect (at -2.8 4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "/MUX_S1") (pinfunction "PD5(T1)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "10" smd rect (at -2 4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "/MUX_S2") (pinfunction "PD6(AIN0)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "11" smd rect (at -1.2 4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "/MUX_S3") (pinfunction "PD7(AIN1)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "12" smd rect (at -0.4 4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "/MUX_~{EN}") (pinfunction "PB0(ICP)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "13" smd rect (at 0.4 4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/MUX_S0") (pinfunction "PB1(OC1A)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "14" smd rect (at 1.2 4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/CS_SD") (pinfunction "PB2(SS/OC1B)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "15" smd rect (at 2 4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/MOSI") (pinfunction "PB3(MOSI/OC2)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "16" smd rect (at 2.8 4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "/MISO") (pinfunction "PB4(MISO)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "17" smd rect (at 4.2926 2.8) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "/SCK") (pinfunction "PB5(SCK)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "18" smd rect (at 4.2926 2) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/AVCC") (pinfunction "AVCC") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "19" smd rect (at 4.2926 1.2) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "/BATT_MONITOR") (pinfunction "ADC6") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "20" smd rect (at 4.2926 0.4) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/AREF") (pinfunction "AREF") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "21" smd rect (at 4.2926 -0.4) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/AGND") (pinfunction "AGND") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "22" smd rect (at 4.2926 -1.2) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "/ANALOG_0") (pinfunction "ADC7") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "23" smd rect (at 4.2926 -2) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "/BATT_MONITOR_EN") (pinfunction "PC0(ADC0)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "24" smd rect (at 4.2926 -2.8) (size 1.27 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/SHIFT_CLEAR") (pinfunction "PC1(ADC1)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "25" smd rect (at 2.8 -4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/CS_SHIFT_REG") (pinfunction "PC2(ADC2)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "26" smd rect (at 2 -4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "/LED_GRN") (pinfunction "PC3(ADC3)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "27" smd rect (at 1.2 -4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "/SDA") (pinfunction "PC4(ADC4/SDA)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "28" smd rect (at 0.4 -4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "/SCL") (pinfunction "PC5(ADC5/SCL)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "29" smd rect (at -0.4 -4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/RESET") (pinfunction "PC6(/RESET)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "30" smd rect (at -1.2 -4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/TO_FTDI_TX") (pinfunction "PD0(RXD)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "31" smd rect (at -2 -4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "/TO_FTDI_RX") (pinfunction "PD1(TXD)") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "32" smd rect (at -2.8 -4.2926) (size 0.5588 1.27) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "/BUTTON1") (pinfunction "PD2(INT0)") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 116.8396 85.904)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R31" (at -0.3172 -1.1546) (layer "F.SilkS"))
    (fp_text value "10k" (at 2.0128 -0.0546 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "/BATT_MONITOR_EN") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(BJT0-B)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MusselGapeTracker_RevE:SJ_2S-TRACE" (layer "B.Cu")
    (at 133.6744 109.6594)
    (descr "Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.")
    (property "Sheetfile" "MusselGapeTracker_RevG.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "GROUND_CON0" (at -0.9525 1.27 180) (layer "B.SilkS"))
    (fp_text value "SOLDER_JUMPER_TRACESTANDARD" (at -0.9525 -1.651 180) (layer "B.Fab") hide)
    (pad "1" smd rect (at -0.508 0) (size 0.635 1.27) (layers "B.Cu" "B.Mask")
      (net 1 "GND") (pinfunction "P$1") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "2" smd rect (at 0.508 0) (size 0.635 1.27) (layers "B.Cu" "B.Mask")
      (net 9 "/AGND") (pinfunction "P$2") (pintype "bidirectional") (solder_mask_margin 0.0762))
  )
  (gr_line (start 97.9805 133.9471) (end 170.4721 133.9471)
    (layer "Edge.Cuts"))
  (gr_line (start 97.9805 76.1621) (end 97.9805 133.9471)
    (layer "Edge.Cuts"))
  (gr_line (start 170.4724 133.9494) (end 170.4724 76.1644)
    (layer "Edge.Cuts"))
  (gr_line (start 170.4721 76.1621) (end 97.9805 76.1621)
    (layer "Edge.Cuts"))
  (gr_text "VCC" (at 167.7035 81.3691 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 165.7985 88.4811 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 151.4475 125.6921 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 163.6395 81.3691 -90) (layer "B.SilkS"))
  (gr_text "SCK" (at 129.0955 115.4051) (layer "B.SilkS"))
  (gr_text "VCC" (at 169.1005 100.1651 -90) (layer "B.SilkS"))
  (gr_text "BUTTON1" (at 103.8824 109.4094) (layer "B.SilkS"))
  (gr_text "OUT" (at 149.5425 81.2421 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 149.5425 128.7401 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 151.5745 102.1971 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 151.5745 118.7071 -90) (layer "B.SilkS"))
  (gr_text "MOSI" (at 128.9685 121.8821) (layer "B.SilkS"))
  (gr_text "RX" (at 99.3775 90.8941 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 99.3775 100.4191 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 155.5115 128.6131 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 161.8615 111.7221 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 153.6065 88.4811 -90) (layer "B.SilkS"))
  (gr_text "HALL13" (at 167.5765 122.2885) (layer "B.SilkS"))
  (gr_text "-" (at 122.6024 79.2444 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 165.7985 81.3691 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 165.7985 95.2121 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 161.7345 118.5801 -90) (layer "B.SilkS"))
  (gr_text "+" (at 110.0824 78.5694) (layer "B.SilkS"))
  (gr_text "HALL14" (at 155.1305 132.6771) (layer "B.SilkS"))
  (gr_text "GND" (at 165.7985 102.1971 -90) (layer "B.SilkS"))
  (gr_text "HALL8" (at 154.7495 108.6741) (layer "B.SilkS"))
  (gr_text "GND" (at 153.6065 111.8491 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 155.5115 111.9761 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 161.7345 128.6131 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 161.6075 81.3691 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 99.3775 97.7521 -90) (layer "B.SilkS"))
  (gr_text "POWER" (at 120.2724 77.0994 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 149.5425 111.8491 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 121.2524 89.7094) (layer "B.SilkS"))
  (gr_text "SLP" (at 163.7665 88.2271 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 167.7035 125.6921 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 167.7035 111.9761 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 151.5745 88.3541 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 155.6385 118.7071 -90) (layer "B.SilkS"))
  (gr_text "MISO" (at 132.1435 115.4051) (layer "B.SilkS"))
  (gr_text "VCC" (at 167.7035 128.6131 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 102.5525 116.9291) (layer "B.SilkS"))
  (gr_text "GND" (at 153.6065 95.0851 -90) (layer "B.SilkS"))
  (gr_text "BUTTON2" (at 103.8024 114.5894) (layer "B.SilkS"))
  (gr_text "VCC" (at 167.7035 118.7071 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 165.7985 128.7401 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 165.7985 111.9761 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 153.6065 118.7071 -90) (layer "B.SilkS"))
  (gr_text "HALL6" (at 154.3685 98.8951) (layer "B.SilkS"))
  (gr_text "GND" (at 153.6065 102.1971 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 161.7345 102.0701 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 163.7665 95.2121 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 155.5115 81.3691 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 163.7665 102.1971 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 151.5745 81.2421 -90) (layer "B.SilkS"))
  (gr_text "HALL10" (at 154.1145 115.0241) (layer "B.SilkS"))
  (gr_text "SLP" (at 163.7665 111.9761 -90) (layer "B.SilkS"))
  (gr_text "RST" (at 123.1011 118.1991 -90) (layer "B.SilkS"))
  (gr_text "4-40\nscrew" (at 107.1624 106.1894 90) (layer "B.SilkS"))
  (gr_text "millerlp@gmail.com" (at 102.6033 95.6185 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 151.5745 111.9761 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 165.6715 125.6921 -90) (layer "B.SilkS"))
  (gr_text "HALL15" (at 167.4495 132.6771) (layer "B.SilkS"))
  (gr_text "SLP" (at 163.7665 128.7401 -90) (layer "B.SilkS"))
  (gr_text "+" (at 122.7874 78.6094) (layer "B.SilkS"))
  (gr_text "VCC" (at 155.5115 88.4811 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 153.6065 125.6921 -90) (layer "B.SilkS"))
  (gr_text "HALL11" (at 167.5765 115.2781) (layer "B.SilkS"))
  (gr_text "GND" (at 165.7985 118.7071 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 155.6385 102.0701 -90) (layer "B.SilkS"))
  (gr_text "HALL5" (at 167.1955 91.9101) (layer "B.SilkS"))
  (gr_text "SLP" (at 151.5745 95.2121 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 123.7742 89.7094) (layer "B.SilkS"))
  (gr_text "HALL2" (at 154.8765 84.9251) (layer "B.SilkS"))
  (gr_text "VCC" (at 155.5115 125.5651 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 149.5425 88.3541 -90) (layer "B.SilkS"))
  (gr_text "HALL9" (at 166.8145 108.6741) (layer "B.SilkS"))
  (gr_text "GND" (at 99.3775 103.2131 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 123.8885 121.8567 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 161.7345 125.5651 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 131.8624 121.3694 -90) (layer "B.SilkS"))
  (gr_text "TX" (at 108.0135 93.6881 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 151.5745 128.7401 -90) (layer "B.SilkS"))
  (gr_text "TX" (at 99.3775 93.4341 -90) (layer "B.SilkS"))
  (gr_text "SCL" (at 126.3124 89.6344) (layer "B.SilkS"))
  (gr_text "GND" (at 102.5525 111.7221) (layer "B.SilkS"))
  (gr_text "HALL7" (at 167.1955 98.8951) (layer "B.SilkS"))
  (gr_text "VCC" (at 167.8305 88.3541 -90) (layer "B.SilkS"))
  (gr_text "RX" (at 108.2675 91.0211 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 149.5425 118.5801 -90) (layer "B.SilkS"))
  (gr_text "Mussel\nGape\nTracker\nRev H" (at 104.7115 122.1361) (layer "B.SilkS"))
  (gr_text "GND" (at 128.4605 133.5661) (layer "B.SilkS"))
  (gr_text "VCC" (at 155.5115 95.2121 -90) (layer "B.SilkS"))
  (gr_text "HALL12" (at 154.2161 122.2377) (layer "B.SilkS"))
  (gr_text "VCC" (at 167.7035 95.2121 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 163.7665 125.5651 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 149.5425 95.0851 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 163.6395 118.7071 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 102.7324 78.3294) (layer "B.SilkS"))
  (gr_text "DTR" (at 99.3775 88.1001 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 161.7345 95.2121 -90) (layer "B.SilkS"))
  (gr_text "HALL0" (at 154.8765 77.8131) (layer "B.SilkS"))
  (gr_text "SDA" (at 128.8124 89.6594) (layer "B.SilkS"))
  (gr_text "RESET" (at 135.0645 133.5661) (layer "B.SilkS"))
  (gr_text "L P MILLER\n2023" (at 104.7115 127.9781) (layer "B.SilkS"))
  (gr_text "HALL3" (at 167.3225 84.9251) (layer "B.SilkS"))
  (gr_text "GND" (at 153.6065 128.7401 -90) (layer "B.SilkS"))
  (gr_text "HALL4" (at 153.8605 91.6561) (layer "B.SilkS"))
  (gr_text "GND" (at 153.6065 81.3691 -90) (layer "B.SilkS"))
  (gr_text "HALL1" (at 166.9415 77.9401) (layer "B.SilkS"))
  (gr_text "OUT" (at 161.7345 88.3541 -90) (layer "B.SilkS"))
  (gr_text "OUT" (at 149.5425 125.5651 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 121.7624 89.8794) (layer "F.SilkS"))
  (gr_text "SDA" (at 128.9024 89.0694) (layer "F.SilkS"))
  (gr_text "GRN" (at 114.1124 99.2761) (layer "F.SilkS"))
  (gr_text "+" (at 113.2205 100.1651) (layer "F.SilkS"))
  (gr_text "HALL10" (at 147.3835 118.6594 90) (layer "F.SilkS"))
  (gr_text "GND" (at 107.3023 100.8001 90) (layer "F.SilkS"))
  (gr_text "GND" (at 98.3624 104.8294) (layer "F.SilkS"))
  (gr_text "VREG" (at 115.189 80.4926) (layer "F.SilkS"))
  (gr_text "GND" (at 100.0374 115.9131) (layer "F.SilkS"))
  (gr_text "HALL7" (at 162.9624 103.6094) (layer "F.SilkS"))
  (gr_text "GND" (at 121.5124 85.3894) (layer "F.SilkS"))
  (gr_text "DTR" (at 98.7424 87.6794) (layer "F.SilkS"))
  (gr_text "RST" (at 123.8631 118.1991 90) (layer "F.SilkS"))
  (gr_text "POWER" (at 130.5374 80.9844 90) (layer "F.SilkS"))
  (gr_text "°" (at 125.7624 94.3344) (layer "F.SilkS"))
  (gr_text "New Molex \nmicroSD\n502774-0891" (at 108.2675 125.5651 90) (layer "F.SilkS"))
  (gr_text "CR1220" (at 134.6835 77.5591) (layer "F.SilkS"))
  (gr_text "100k Ω" (at 123.9824 126.0694 90) (layer "F.SilkS"))
  (gr_text "GND" (at 108.1405 98.3871 90) (layer "F.SilkS"))
  (gr_text "RED" (at 114.0124 97.4981) (layer "F.SilkS"))
  (gr_text "AGND" (at 144.0815 132.6771 90) (layer "F.SilkS"))
  (gr_text "HALL4" (at 147.3835 93.8151 90) (layer "F.SilkS"))
  (gr_text "4-40\nscrew" (at 139.4024 92.8194) (layer "F.SilkS"))
  (gr_text "0.1µF" (at 118.4924 108.3494) (layer "F.SilkS"))
  (gr_text "10k" (at 121.2324 97.7194) (layer "F.SilkS"))
  (gr_text "AREF" (at 130.9624 87.0094) (layer "F.SilkS"))
  (gr_text "0.1µF" (at 115.8424 127.5994 90) (layer "F.SilkS"))
  (gr_text "GND" (at 121.2724 89.0394) (layer "F.SilkS"))
  (gr_text "GND" (at 126.4285 133.5661) (layer "F.SilkS"))
  (gr_text "MISO" (at 129.6035 115.4051) (layer "F.SilkS"))
  (gr_text "100Ω" (at 115.4874 103.0344) (layer "F.SilkS"))
  (gr_text "10k" (at 115.0124 97.8394) (layer "F.SilkS"))
  (gr_text "HALL0" (at 147.2565 80.9881 90) (layer "F.SilkS"))
  (gr_text "HALL14" (at 147.3374 132.2344 90) (layer "F.SilkS"))
  (gr_text "0.1µF" (at 121.3824 98.6994) (layer "F.SilkS"))
  (gr_text "°" (at 124.206 100.8634) (layer "F.SilkS"))
  (gr_text "SCL" (at 126.4524 89.0894) (layer "F.SilkS"))
  (gr_text "4.7k" (at 117.1524 97.7694) (layer "F.SilkS"))
  (gr_text "M2->" (at 109.2624 92.8794 45) (layer "F.SilkS"))
  (gr_text "Mussel\nGape\nTracker\nRev H" (at 118.8374 120.4844) (layer "F.SilkS"))
  (gr_text "BUTTON1" (at 100.5124 109.7694) (layer "F.SilkS"))
  (gr_text "FTDI 3.3V ONLY!" (at 109.1057 101.7399 90) (layer "F.SilkS"))
  (gr_text "+" (at 127.0624 78.4094) (layer "F.SilkS"))
  (gr_text "ICSP\nHEADER" (at 124.1124 114.5344) (layer "F.SilkS"))
  (gr_text "4-40\nscrew" (at 135.4224 130.7594) (layer "F.SilkS"))
  (gr_text "-" (at 129.4924 81.4594 90) (layer "F.SilkS"))
  (gr_text "DTR" (at 108.0024 91.4394 90) (layer "F.SilkS"))
  (gr_text "RX" (at 108.4224 92.8394 90) (layer "F.SilkS"))
  (gr_text "LP MILLER\n2023" (at 117.2874 114.8344) (layer "F.SilkS"))
  (gr_text "VCC" (at 122.0524 86.2594) (layer "F.SilkS"))
  (gr_text "ADC7" (at 130.6324 105.9594) (layer "F.SilkS"))
  (gr_text "HALL15" (at 162.1155 133.6931) (layer "F.SilkS"))
  (gr_text "1" (at 107.4928 107.7468 90) (layer "F.SilkS"))
  (gr_text "100Ω" (at 118.1608 103.0986) (layer "F.SilkS"))
  (gr_text "HALL14" (at 150.0505 133.6931) (layer "F.SilkS"))
  (gr_text "RTC" (at 129.1224 95.8594) (layer "F.SilkS"))
  (gr_text "4-40" (at 100.7224 108.1194 90) (layer "F.SilkS"))
  (gr_text "2" (at 110.6874 116.1344 90) (layer "F.SilkS"))
  (gr_text "HALL6" (at 150.4874 103.4094) (layer "F.SilkS"))
  (gr_text "0.1µF" (at 112.141 93.98) (layer "F.SilkS"))
  (gr_text "TX" (at 108.1405 95.0851 90) (layer "F.SilkS"))
  (gr_text "VCC" (at 132.7785 121.3741 90) (layer "F.SilkS"))
  (gr_text "B2" (at 100.6724 114.6494) (layer "F.SilkS"))
  (gr_text "+" (at 113.2205 98.2601) (layer "F.SilkS"))
  (gr_text "100k Ω" (at 123.6824 132.8994 90) (layer "F.SilkS"))
  (gr_text "I2C HEADER" (at 124.9426 86.0806) (layer "F.SilkS"))
  (gr_text "GND" (at 100.2665 111.0094) (layer "F.SilkS"))
  (gr_text "RESET" (at 131.6355 133.5661) (layer "F.SilkS"))
  (gr_text "HALL9" (at 162.8874 106.2844) (layer "F.SilkS"))
  (gr_text "VCC" (at 108.1405 95.7201 90) (layer "F.SilkS"))
  (gr_text "4.7k" (at 118.9424 97.7694) (layer "F.SilkS"))
  (gr_text "SCK" (at 126.9365 115.4051) (layer "F.SilkS"))
  (gr_text "HALL2" (at 147.2565 89.1094 90) (layer "F.SilkS"))
  (gr_text "M2->" (at 112.7924 117.9494 90) (layer "F.SilkS"))
  (gr_text "HALL8" (at 150.4624 106.6344) (layer "F.SilkS"))
  (gr_text "GND" (at 123.9393 121.8821 90) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.0889) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2278) (thermal_bridge_width 0.2278))
    (polygon
      (pts
        (xy 142.6102 106.1922)
        (xy 133.7202 106.1922)
        (xy 133.7202 116.1744)
        (xy 142.6102 116.1744)
        (xy 142.6102 132.6844)
        (xy 143.8802 132.6844)
        (xy 143.8802 134.1322)
        (xy 97.9824 134.1322)
        (xy 97.9824 76.1694)
        (xy 142.6102 76.1694)
      )
    )
  )
  (zone (net 9) (net_name "/AGND") (layer "B.Cu") (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.0889) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2278) (thermal_bridge_width 0.2278))
    (polygon
      (pts
        (xy 170.4494 134.1422)
        (xy 144.8716 134.1422)
        (xy 144.8716 113.8222)
        (xy 134.7116 113.8222)
        (xy 134.7116 107.2944)
        (xy 143.6016 107.2944)
        (xy 143.6016 76.1794)
        (xy 170.4494 76.1794)
      )
    )
  )
)
